(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0001000_7fffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/")
    )
  )
  (net 0 "")
  (net 1 "Net-(TP1-Pad1)")
  (net 2 "Net-(U1A--)")
  (net 3 "Net-(U1A-+)")
  (net 4 "Net-(U1C-V-)")
  (net 5 "Net-(TP7-Pad1)")
  (net 6 "Net-(U1C-V+)")
  (net 7 "Net-(U1B-+)")
  (net 8 "Net-(U1B--)")
  (footprint "t_misc:TP_SQ_120_H25" (layer "F.Cu")
    (at 148.844 105.791)
    (property "Sheetfile" "Two_wire_Opamp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP8" (at 0 -2.286) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.05 -1.375) (layer "F.SilkS") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 3.048 3.048) (drill 0.635) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1666666667)
      (net 6 "Net-(U1C-V+)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "t_misc:TP_SQ_120_H25" (layer "F.Cu")
    (at 132.08 105.791)
    (property "Sheetfile" "Two_wire_Opamp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP2" (at 0 -2.286) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.05 -1.375) (layer "F.SilkS") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 3.048 3.048) (drill 0.635) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1666666667)
      (net 2 "Net-(U1A--)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "t_misc:TP_SQ_120_H25" (layer "F.Cu")
    (at 148.717 109.601)
    (property "Sheetfile" "Two_wire_Opamp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP5" (at 0 2.413) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.05 -1.375) (layer "F.SilkS") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 3.048 3.048) (drill 0.635) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1666666667)
      (net 7 "Net-(U1B-+)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "t_misc:TP_SQ_120_H25" (layer "F.Cu")
    (at 128.016 105.791)
    (property "Sheetfile" "Two_wire_Opamp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP1" (at 0 -2.286) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.05 -1.375) (layer "F.SilkS") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 3.048 3.048) (drill 0.635) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1666666667)
      (net 1 "Net-(TP1-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_SO:VSSOP-8_3.0x3.0mm_P0.65mm" (layer "F.Cu")
    (at 138.303 107.696)
    (descr "VSSOP-8 3.0 x 3.0, http://www.ti.com/lit/ds/symlink/lm75b.pdf")
    (tags "VSSOP-8 3.0 x 3.0")
    (property "Sheetfile" "Two_wire_Opamp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Dual 36V, Precision, Rail-to-Rail Input/Output, Low Offset Voltage, Operational Amplifier, VSSOP-8")
    (property "ki_keywords" "dual opamp rtor")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "OPA2197xDGK" (at 0.02 2.73) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.2 -0.975 270) (size 0.45 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(TP1-Pad1)") (pintype "output"))
    (pad "2" smd rect (at -2.2 -0.325 270) (size 0.45 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(U1A--)") (pinfunction "-") (pintype "input"))
    (pad "3" smd rect (at -2.2 0.325 270) (size 0.45 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(U1A-+)") (pinfunction "+") (pintype "input"))
    (pad "4" smd rect (at -2.2 0.975 270) (size 0.45 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U1C-V-)") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd rect (at 2.2 0.975 270) (size 0.45 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(U1B-+)") (pinfunction "+") (pintype "input"))
    (pad "6" smd rect (at 2.2 0.325 270) (size 0.45 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(U1B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd rect (at 2.2 -0.325 270) (size 0.45 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(TP7-Pad1)") (pintype "output"))
    (pad "8" smd rect (at 2.2 -0.975 270) (size 0.45 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(U1C-V+)") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/VSSOP-8_3.0x3.0mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "t_misc:TP_SQ_120_H25" (layer "F.Cu")
    (at 132.08 109.601)
    (property "Sheetfile" "Two_wire_Opamp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP3" (at -0.127 2.413) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.05 -1.375) (layer "F.SilkS") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 3.048 3.048) (drill 0.635) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1666666667)
      (net 3 "Net-(U1A-+)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "t_misc:TP_SQ_120_H25" (layer "F.Cu")
    (at 144.78 109.601)
    (property "Sheetfile" "Two_wire_Opamp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP6" (at 0 2.413) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.05 -1.375) (layer "F.SilkS") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 3.048 3.048) (drill 0.635) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1666666667)
      (net 8 "Net-(U1B--)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "t_misc:TP_SQ_120_H25" (layer "F.Cu")
    (at 128.143 109.601)
    (property "Sheetfile" "Two_wire_Opamp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP4" (at -0.127 2.413) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.05 -1.375) (layer "F.SilkS") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 3.048 3.048) (drill 0.635) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1666666667)
      (net 4 "Net-(U1C-V-)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "t_misc:TP_SQ_120_H25" (layer "F.Cu")
    (at 144.78 105.791)
    (property "Sheetfile" "Two_wire_Opamp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP7" (at 0 -2.286) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.05 -1.375) (layer "F.SilkS") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 3.048 3.048) (drill 0.635) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1666666667)
      (net 5 "Net-(TP7-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (gr_rect (start 125.73 102.616) (end 151.13 112.776)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "1" (at 135.509 105.41) (layer "F.Cu"))
)
