(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 13)
    (zones 0)
    (modules 4)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net VCC)
  )
  (module Battery:BatteryHolder_Keystone_3034_1x20mm (layer B.Cu) (tedit 5CA58061)
    (at 144.6784 118 180)
    (descr "Keystone 3034 SMD battery holder for 2020, 2025 and 2032 coincell batteries. http://www.keyelco.com/product-pdf.cfm?p=798")
    (tags "Keystone type 3034 coin cell retainer")
    (attr smd)
    (fp_text reference BT1 (at 0 11.5 180) (layer F.Fab))
    (fp_text value Battery (at 0 -11.5 180) (layer B.Fab))
    (fp_text user %R (at 0 2.9 180) (layer B.Fab))
    (pad 2 smd rect (at 0 0 180) (size 3.96 3.96) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 10.985 0 180) (size 1.27 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -10.985 0 180) (size 1.27 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_3034_1x20mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FancyFeast:PinHeader_2x03_P2.54mm_Vertical (layer B.Cu) (tedit 5BAD67E7)
    (at 142.06 102.36 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J1 (at 1.269999 2.33 270) (layer B.Fab))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 -7.41 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -2.54 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module andnxor:lapel-pin-5mm (layer B.Cu) (tedit 5B8371A3)
    (at 144.6 95)
    (fp_text reference g1 (at 0 -4.3) (layer Dwgs.User))
    (fp_text value pin (at 0 3.8) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 5 5) (layers B.Cu B.Paste B.Mask))
  )
  (module manbearpig:ANDnXOR1 (layer F.Cu) (tedit 0)
    (at 144.6 117)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (dimension 44 (width 0.3) (layer F.Fab)
    (gr_text "44.000 mm" (at 120.9 110 270) (layer F.Fab))
    (feature1 (pts (xy 145 132) (xy 122.413579 132)))
    (feature2 (pts (xy 145 88) (xy 122.413579 88)))
    (crossbar (pts (xy 123 88) (xy 123 132)))
    (arrow1a (pts (xy 123 132) (xy 122.413579 130.873496)))
    (arrow1b (pts (xy 123 132) (xy 123.586421 130.873496)))
    (arrow2a (pts (xy 123 88) (xy 122.413579 89.126504)))
    (arrow2b (pts (xy 123 88) (xy 123.586421 89.126504)))
  )
  (dimension 25 (width 0.3) (layer F.Fab)
    (gr_text "25.000 mm" (at 144.5 141.1) (layer F.Fab))
    (feature1 (pts (xy 157 119) (xy 157 139.586421)))
    (feature2 (pts (xy 132 119) (xy 132 139.586421)))
    (crossbar (pts (xy 132 139) (xy 157 139)))
    (arrow1a (pts (xy 157 139) (xy 155.873496 139.586421)))
    (arrow1b (pts (xy 157 139) (xy 155.873496 138.413579)))
    (arrow2a (pts (xy 132 139) (xy 133.126504 139.586421)))
    (arrow2b (pts (xy 132 139) (xy 133.126504 138.413579)))
  )
  (gr_text "Header goes on other side" (at 144.6 107.3) (layer B.SilkS))
  (gr_text "Keystone 3034" (at 144.6 122.5) (layer B.SilkS))
  (gr_arc (start 144.5 119) (end 132.000002 119.000001) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157 100.5) (end 157 119) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.5 100.5) (end 157 100.5) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132 119) (end 132 100.5) (layer Edge.Cuts) (width 0.15))
  (gr_text "SAO v1.169bis" (at 144.6 98.6) (layer F.SilkS))
  (gr_text "AND!XOR SAO\nShitty Brooch" (at 144.6 94.7) (layer F.SilkS))
)
