<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="-0.626240625" y1="20.3570125" x2="12.86498125" y2="20.3427875" width="0" layer="20"/>
<wire x1="12.86498125" y1="20.3427875" x2="12.878634375" y2="34.05495625" width="0" layer="20"/>
<wire x1="12.878634375" y1="34.05495625" x2="-0.6261125" y2="34.057115625" width="0" layer="20"/>
<wire x1="-0.6261125" y1="34.057115625" x2="-0.626240625" y2="20.3570125" width="0" layer="20"/>
<text>Micro LiPo 
Charger v1</text>
</plain>
<libraries>
<library name="TP4056">
<packages>
<package name="SOP-8">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="micro usb B - sparkfun - china - hole 4LEGS TEST">
<packages>
<package name="MICRO_USB_4_LEGS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="TP4056" package="SOP-8" value="TP4056">
<attribute name="NAME"/>
</element>
<element name="USB" library="micro usb B - sparkfun - china - hole 4LEGS TEST" package="MICRO_USB_4_LEGS" value="MICRO-USB-B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+" library="SparkFun-Connectors" package="1X02" value="BAT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RPROG" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LEDR" library="led" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LEDG" library="led" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="eagle-ltspice" package="C0603" value="">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="eagle-ltspice" package="C0603" value="">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="2"/>
<contactref element="RPROG" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="LEDR" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="2"/>
<contactref element="LEDG" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="7"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="6"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="USB" pad="VCC"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="8"/>
<contactref element="LEDR" pad="A"/>
<contactref element="LEDG" pad="A"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="5"/>
<contactref element="+" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="1"/>
<contactref element="USB" pad="GND" route="any" routetag="G$1.GND"/>
<contactref element="+" pad="2"/>
<contactref element="IC1" pad="9"/>
<contactref element="RPROG" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
