<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<text>SPI</text>
<text>I2C</text>
<text>Analog I/O</text>
<text>Digital In/Out</text>
<text>CI Test Shield
v0.1.0
mbed.org/cishield</text>
<text>Tests
Analog I/O - A0-5 mesh
Digital I/O - D0-D9 loopback
UART - D0/1 loopback
SPI - micoSD W/R
I2C - Flash / Temp Sensor
PWM - Loopback
Interrupt In - Loopback</text>
<text>TMP102</text>
<text>Flash</text>
<wire x1="38.1" y1="22.86" x2="46.99" y2="13.97" width="0" layer="20"/>
<wire x1="46.99" y1="13.97" x2="87.63" y2="13.97" width="0" layer="20"/>
<wire x1="87.63" y1="13.97" x2="90.17" y2="16.51" width="0" layer="20"/>
<wire x1="90.17" y1="16.51" x2="90.17" y2="64.77" width="0" layer="20"/>
<wire x1="90.17" y1="64.77" x2="87.63" y2="67.31" width="0" layer="20"/>
<wire x1="87.63" y1="67.31" x2="40.64" y2="67.31" width="0" layer="20"/>
<wire x1="40.64" y1="67.31" x2="38.1" y2="64.77" width="0" layer="20"/>
<wire x1="38.1" y1="64.77" x2="38.1" y2="22.86" width="0" layer="20"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="MICROSD">
</package>
<package name="ARDUINOR3-BPLACE">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT563">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C025-025X050" value="0.01uF"/>
<element name="R1" library="adafruit" package="0204/7" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0204/7" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0204/7" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0204/7" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="0204/7" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="0204/7" value="10K">
<attribute name="VALUE"/>
</element>
<element name="SCL_PULLUP" library="adafruit" package="0204/7" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SDA_PULLUP" library="adafruit" package="0204/7" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UART" library="jumper" package="SJ" value=""/>
<element name="SJ2" library="jumper" package="SJ" value=""/>
<element name="SJ3" library="jumper" package="SJ" value=""/>
<element name="SJ4" library="jumper" package="SJ" value=""/>
<element name="SJ5" library="jumper" package="SJ" value=""/>
<element name="SCL1" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SDA1" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SDA2" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SCL2" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MICRO-SD" library="adafruit" package="MICROSD" value="MICROSD">
<attribute name="NAME"/>
</element>
<element name="U1" library="adafruit" package="ARDUINOR3-BPLACE" value="ARDUINOR3-BPLACE"/>
<element name="U2" library="SparkFun-Sensors" package="SOT563" value="TMP102">
<attribute name="PROD_ID" value="IC-09303"/>
</element>
<element name="EEPROM" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="EEPROM-I2CEIAJ"/>
<element name="C2" library="adafruit" package="C025-025X050" value="0.01uF"/>
<element name="C3" library="adafruit" package="C025-025X050" value="0.01uF"/>
</elements>
<signals>
<signal name="VIN">
<contactref element="U1" pad="VIN"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="5V"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="A0"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="A1"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="A2"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="A3"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="A4"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="A5"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="D0"/>
<contactref element="UART" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="D1"/>
<contactref element="UART" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="D2"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="D3"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="D4"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="D5"/>
<contactref element="SJ3" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="D6"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="D7"/>
<contactref element="SJ4" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="D8"/>
<contactref element="SJ5" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="D9"/>
<contactref element="SJ5" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="SCL"/>
<contactref element="SCL_PULLUP" pad="2"/>
<contactref element="SCL1" pad="1"/>
<contactref element="SCL2" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="SDA"/>
<contactref element="SDA_PULLUP" pad="2"/>
<contactref element="SDA1" pad="1"/>
<contactref element="SDA2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="EEPROM" pad="1"/>
<contactref element="EEPROM" pad="4"/>
<contactref element="EEPROM" pad="3"/>
<contactref element="EEPROM" pad="2"/>
<contactref element="U1" pad="GND2"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="EEPROM" pad="7"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="MICRO-SD" pad="MT2"/>
<contactref element="MICRO-SD" pad="MT1"/>
<contactref element="MICRO-SD" pad="6"/>
<contactref element="U1" pad="GND"/>
<contactref element="U1" pad="GND1"/>
</signal>
<signal name="N$20">
<contactref element="U2" pad="6"/>
<contactref element="SDA2" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U2" pad="1"/>
<contactref element="SCL2" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="EEPROM" pad="6"/>
<contactref element="SCL1" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="EEPROM" pad="5"/>
<contactref element="SDA1" pad="2"/>
</signal>
<signal name="SD_NCS">
<contactref element="U1" pad="D10"/>
<contactref element="MICRO-SD" pad="2"/>
</signal>
<signal name="SD_SCLK">
<contactref element="U1" pad="D13"/>
<contactref element="MICRO-SD" pad="5"/>
</signal>
<signal name="SD_MOSI">
<contactref element="U1" pad="D11"/>
<contactref element="MICRO-SD" pad="3"/>
</signal>
<signal name="SD_MISO">
<contactref element="U1" pad="D12"/>
<contactref element="MICRO-SD" pad="7"/>
</signal>
<signal name="+3.3V">
<contactref element="U1" pad="3V"/>
<contactref element="U2" pad="5"/>
<contactref element="EEPROM" pad="8"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="SDA_PULLUP" pad="1"/>
<contactref element="SCL_PULLUP" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="MICRO-SD" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
