(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 50)
    (zones 0)
    (modules 9)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 2.5)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 2 1)
    (user_via 3.81 3.2004)
    (user_via 4 3.2)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 135.9746 89.4224)
    (grid_origin 53.00472 53.42128)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /TEC2-)
  (net 3 /LD-)
  (net 4 /LD+)
  (net 5 /TEC2+)
  (net 6 /TEC1-)
  (net 7 /LEDInd-)
  (net 8 /LEDInd+)
  (net 9 /Therm2-)
  (net 10 /Therm2+)
  (net 11 /Therm1-)
  (net 12 /Therm1+)
  (net 13 /TEC1+)
  (net 14 "Net-(DSubOut1-Pad10)")
  (net 15 "Net-(DSubOut1-Pad12)")
  (net 16 "Net-(DSubOut1-Pad14)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LD+)
    (add_net /LD-)
    (add_net /LEDInd+)
    (add_net /LEDInd-)
    (add_net /TEC1+)
    (add_net /TEC1-)
    (add_net /TEC2+)
    (add_net /TEC2-)
    (add_net /Therm1+)
    (add_net /Therm1-)
    (add_net /Therm2+)
    (add_net /Therm2-)
    (add_net GND)
    (add_net "Net-(DSubOut1-Pad10)")
    (add_net "Net-(DSubOut1-Pad12)")
    (add_net "Net-(DSubOut1-Pad14)")
  )
  (module MyFootprints:Mountinghole (layer F.Cu) (tedit 5DFA669C)
    (at 36.34232 53.42128)
    (zone_connect 2)
    (fp_text reference J1 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module MyFootprints:Dsub15pin (layer F.Cu) (tedit 5DF10A79)
    (at 53 52)
    (fp_text reference DSubOut1 (at 0 -2) (layer F.SilkS))
    (fp_text value Conn_01x15_Female (at 0 -0.5) (layer F.Fab))
    (pad 9 thru_hole circle (at 8.2296 0) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 2 /TEC2-))
    (pad 10 thru_hole circle (at 5.4864 0) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 14 "Net-(DSubOut1-Pad10)"))
    (pad 11 thru_hole circle (at 2.7432 0) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 3 /LD-))
    (pad 12 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 15 "Net-(DSubOut1-Pad12)"))
    (pad 13 thru_hole circle (at -2.7432 0) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 4 /LD+))
    (pad 14 thru_hole circle (at -5.4864 0) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 16 "Net-(DSubOut1-Pad14)"))
    (pad 15 thru_hole circle (at -8.2296 0) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 5 /TEC2+))
    (pad 1 thru_hole circle (at 9.6012 2.8448) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 6 /TEC1-))
    (pad 2 thru_hole circle (at 6.858 2.8448) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 7 /LEDInd-))
    (pad 3 thru_hole circle (at 4.1148 2.8448) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 8 /LEDInd+))
    (pad 4 thru_hole circle (at 1.3716 2.8448) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 9 /Therm2-))
    (pad 5 thru_hole circle (at -1.3716 2.8448) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 10 /Therm2+))
    (pad 6 thru_hole circle (at -4.1148 2.8448) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 11 /Therm1-))
    (pad 7 thru_hole circle (at -6.858 2.8448) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 12 /Therm1+))
    (pad 8 thru_hole circle (at -9.6012 2.8448) (size 2.4 2.4) (drill 1.0922) (layers *.Cu *.Mask)
      (net 13 /TEC1+))
    (model "R:/Cuprite/CAD/Innolume laser design/Electronics box/171-015-213.STEP"
      (offset (xyz -19.6 4.88 -9))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (module MyFootprints:QLMLogo (layer F.Cu) (tedit 0)
    (at 38.00472 45.42128)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 55 45)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference LDPair1 (at 1.27 -4.12) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 4 /LD+))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 /LD-))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 59 62)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference LEDIndicator1 (at 2 4) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /LEDInd-))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 8 /LEDInd+))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 52 70)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference TEC1 (at -4 2) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 /TEC1-))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 13 /TEC1+))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 48 45)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference TEC2 (at 1.27 -4.12) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /TEC2-))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 5 /TEC2+))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 45 62)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference Therm1 (at 1.27 -4.12) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 12 /Therm1+))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 /Therm1-))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 52 62)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference Therm2 (at 1.27 -4.12) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 10 /Therm2+))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /Therm2-))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 33.00472 75.42128) (end 33.00472 39.42128) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.00472 75.42128) (end 33.00472 75.42128) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.00472 39.42128) (end 73.00472 75.42128) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 33.00472 39.42128) (end 73.00472 39.42128) (layer Edge.Cuts) (width 0.1))
  (gr_text 8 (at 41.00472 55.42128) (layer F.SilkS))
  (gr_text 15 (at 42.00472 50.42128) (layer F.SilkS))
  (gr_text 9 (at 63.00472 50.42128) (layer F.SilkS))
  (gr_text 1 (at 65.00472 54.42128) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33.00472 39.42128) (xy 73.00472 39.42128) (xy 73.00472 75.42128) (xy 33.00472 75.42128)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33.00472 39.42128) (xy 73.00472 39.42128) (xy 73.00472 75.42128) (xy 33.00472 75.42128)
      )
    )
  )
)
