(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 110)
    (tracks 186)
    (zones 0)
    (modules 5)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.127)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.6096)
    (via_min_drill 0.3048)
    (user_via 0.6096 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 100.965 121.285)
    (grid_origin 100.965 121.285)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad20)")
  (net 2 "Net-(J1-Pad19)")
  (net 3 "Net-(J1-Pad18)")
  (net 4 "Net-(J1-Pad17)")
  (net 5 "Net-(J1-Pad16)")
  (net 6 "Net-(J1-Pad15)")
  (net 7 "Net-(J1-Pad14)")
  (net 8 "Net-(J1-Pad13)")
  (net 9 "Net-(J1-Pad12)")
  (net 10 "Net-(J1-Pad11)")
  (net 11 "Net-(J1-Pad10)")
  (net 12 "Net-(J1-Pad9)")
  (net 13 "Net-(J1-Pad8)")
  (net 14 "Net-(J1-Pad7)")
  (net 15 "Net-(J1-Pad6)")
  (net 16 "Net-(J1-Pad5)")
  (net 17 "Net-(J1-Pad4)")
  (net 18 "Net-(J1-Pad3)")
  (net 19 "Net-(J1-Pad2)")
  (net 20 "Net-(J1-Pad1)")
  (net 21 "Net-(J2-Pad24)")
  (net 22 "Net-(J2-Pad23)")
  (net 23 "Net-(J2-Pad22)")
  (net 24 "Net-(J2-Pad21)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad24)")
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 600062E0)
    (at 114.046 70.993)
    (fp_text reference REF** (at -2.032 0.127) (layer F.SilkS) hide)
    (fp_text value TP (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad20)"))
  )
  (module t_logos:Thales_15x2_Cu (layer F.Cu) (tedit 0)
    (at 109.9185 96.3295 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module "t_connectors:FH12A-24S-0.5SH(55)_flex_connector" (layer B.Cu) (tedit 6000628D)
    (at 124.3203 116.1796 270)
    (attr smd)
    (fp_text reference J2 (at -4.3688 -1.8542 270) (layer B.SilkS))
    (fp_text value "Conn_FH12A-24S-0.5SH(55)" (at -4.6482 -3.3782 270) (layer B.Fab))
    (pad 25 smd rect (at 2.4384 3.3528 270) (size 2 2.4) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad20)"))
    (pad 26 smd rect (at -13.4112 3.302 270) (size 2 2.4) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad20)"))
    (pad 24 smd oval (at -11.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J2-Pad24)"))
    (pad 23 smd oval (at -10.7364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J2-Pad23)"))
    (pad 22 smd oval (at -10.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J2-Pad22)"))
    (pad 21 smd oval (at -9.7364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J2-Pad21)"))
    (pad 20 smd oval (at -9.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad20)"))
    (pad 19 smd oval (at -8.7364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad19)"))
    (pad 18 smd oval (at -8.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad18)"))
    (pad 17 smd oval (at -7.7364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad17)"))
    (pad 16 smd oval (at -7.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad16)"))
    (pad 15 smd oval (at -6.7364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad15)"))
    (pad 14 smd oval (at -6.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad14)"))
    (pad 13 smd oval (at -5.7364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad13)"))
    (pad 12 smd oval (at -5.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad12)"))
    (pad 11 smd oval (at -4.7364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J1-Pad11)"))
    (pad 10 smd oval (at -4.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J1-Pad10)"))
    (pad 9 smd oval (at -3.7364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J1-Pad9)"))
    (pad 8 smd oval (at -3.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J1-Pad8)"))
    (pad 7 smd oval (at -2.7364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J1-Pad7)"))
    (pad 6 smd oval (at -2.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J1-Pad6)"))
    (pad 5 smd oval (at -1.7364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J1-Pad5)"))
    (pad 4 smd oval (at -1.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J1-Pad4)"))
    (pad 3 smd oval (at -0.7364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J1-Pad3)"))
    (pad 2 smd oval (at -0.2364 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at 0.2636 0 270) (size 0.3 1.32) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J1-Pad1)"))
    (model ${T_LIBS}/3d/t_connectors/FH12A-24S-0.5SH.stp
      (offset (xyz -26 22 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module t_connectors:AXK5S20047Y_socket (layer B.Cu) (tedit 600061E8)
    (at 106.2228 76.1746 180)
    (attr smd)
    (fp_text reference J1 (at -6.5786 -2.667) (layer B.SilkS))
    (fp_text value AXK520147YG_socket (at 0 0) (layer B.Fab))
    (pad 20 smd oval (at 2.54 -2 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad20)"))
    (pad 19 smd oval (at 2.5146 1.9812 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad19)"))
    (pad 18 smd oval (at 1.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad18)"))
    (pad 17 smd oval (at 1.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad17)"))
    (pad 16 smd oval (at 1.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad16)"))
    (pad 15 smd oval (at 1.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad15)"))
    (pad 14 smd oval (at 0.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad14)"))
    (pad 13 smd oval (at 0.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad13)"))
    (pad 12 smd oval (at 0.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad12)"))
    (pad 11 smd oval (at 0.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J1-Pad11)"))
    (pad 10 smd oval (at -0.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J1-Pad10)"))
    (pad 9 smd oval (at -0.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J1-Pad9)"))
    (pad 8 smd oval (at -0.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J1-Pad8)"))
    (pad 7 smd oval (at -0.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J1-Pad7)"))
    (pad 6 smd oval (at -1.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J1-Pad6)"))
    (pad 5 smd oval (at -1.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J1-Pad5)"))
    (pad 4 smd oval (at -1.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J1-Pad4)"))
    (pad 3 smd oval (at -1.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J1-Pad3)"))
    (pad 2 smd oval (at -2.5146 -2.032 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -2.5146 1.9812 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J1-Pad1)"))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 107.95 82.8294)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_Pad_TopBottom (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 5.4 5.4) (layers B.Cu B.Mask))
    (pad 1 connect circle (at 0 0) (size 5.4 5.4) (layers F.Cu F.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask))
  )
  (gr_text SK1597 (at 112.903 78.486 90) (layer F.SilkS))
  (gr_text "Keyboard Adapter" (at 115.189 95.758 90) (layer F.Cu))
  (gr_text GND (at 112.268 70.993 90) (layer F.SilkS))
  (gr_text "Jan 2021" (at 115.57 78.232 90) (layer F.SilkS))
  (gr_text "JAVLIIN MVP" (at 112.649 96.266 90) (layer F.Cu))
  (gr_line (start 127 119.38) (end 125.095 121.285) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.87 69.215) (end 100.965 71.12) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.745 71.12) (end 116.84 69.215) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.745 96.52) (end 118.745 71.12) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.65 98.425) (end 118.745 96.52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.095 98.425) (end 120.65 98.425) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 100.33) (end 125.095 98.425) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 107.315 119.38) (end 109.22 121.285) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 107.315 94.615) (end 107.315 119.38) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100.965 88.265) (end 107.315 94.615) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.22 121.285) (end 125.095 121.285) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.87 69.215) (end 116.84 69.215) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 100.33) (end 127 119.38) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100.965 88.265) (end 100.965 71.12) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name "Net-(J1-Pad20)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.127))
    (polygon
      (pts
        (xy 118.11 71.12) (xy 118.11 73.025) (xy 118.11 97.155) (xy 120.015 99.06) (xy 125.095 99.06)
        (xy 126.365 100.33) (xy 126.365 119.38) (xy 125.095 120.65) (xy 109.22 120.65) (xy 107.95 119.38)
        (xy 107.95 93.98) (xy 101.6 87.63) (xy 101.6 71.755) (xy 103.505 69.85) (xy 116.84 69.85)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pad20)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.127))
    (polygon
      (pts
        (xy 118.11 71.12) (xy 118.11 73.025) (xy 118.11 97.155) (xy 120.015 99.06) (xy 125.095 99.06)
        (xy 126.365 100.33) (xy 126.365 119.38) (xy 125.095 120.65) (xy 109.22 120.65) (xy 107.95 119.38)
        (xy 107.95 93.98) (xy 101.6 87.63) (xy 101.6 71.755) (xy 103.505 69.85) (xy 116.84 69.85)
      )
    )
  )
)
