(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 9)
    (no_connects 8)
    (area 123.165761 102.693361 150.443001 119.709039)
    (thickness 1.6)
    (drawings 13)
    (tracks 33)
    (zones 0)
    (modules 3)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(M1-Pad1)")
  (net 2 /CS)
  (net 3 /MOSI)
  (net 4 /+3V)
  (net 5 /SCK)
  (net 6 GND)
  (net 7 /MISO)
  (net 8 "Net-(M1-Pad8)")
  (net 9 "Net-(M1-Pad9)")
  (net 10 "Net-(M1-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+3V)
    (add_net /CS)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M1-Pad10)")
    (add_net "Net-(M1-Pad8)")
    (add_net "Net-(M1-Pad9)")
  )
  (module dics-exotic-footprints:MOLEX_MicroSD (layer F.Cu) (tedit 5A5AE296)
    (at 135.2072 105.911 180)
    (fp_text reference M1 (at 4.5496 -10.2686 270) (layer F.SilkS))
    (fp_text value Molex_Micro-SDCARD (at -1.27 -17.78 180) (layer F.Fab) hide)
    (fp_text user molex (at -6.3754 -8.5598 180) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 0.85 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(M1-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 0.85 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 /CS))
    (pad 3 smd rect (at -2.2 0 180) (size 0.85 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /MOSI))
    (pad 4 smd rect (at -3.3 0 180) (size 0.85 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /+3V))
    (pad 5 smd rect (at -4.4 0 180) (size 0.85 1.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCK))
    (pad 6 smd rect (at -5.5 0 180) (size 0.85 1.4) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 7 smd rect (at -6.6 0 180) (size 0.85 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /MISO))
    (pad 7 smd rect (at -6.6 0 180) (size 0.85 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /MISO))
    (pad 8 smd rect (at -7.65 0 180) (size 0.75 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(M1-Pad8)"))
    (pad "" smd rect (at -8.86 -0.35 180) (size 1.17 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -6.855 -10.675 180) (size 1.9 1.35) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -0.885 -10.675 180) (size 1.9 1.35) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 2.46 -0.125 180) (size 1.55 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.635 -6.15 180) (size 1.2 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(M1-Pad9)"))
    (pad 10 smd rect (at 2.635 -9.85 180) (size 1.2 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(M1-Pad10)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5A5AE299)
    (at 148.5011 105.0036)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -2.7305 13.3096 90) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /+3V))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SCK))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /MISO))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /MOSI))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /CS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5A5AE29D)
    (at 128.9812 109.4232)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0.1778 -2.6416) (layer F.SilkS))
    (fp_text value CARD_SELECT (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(M1-Pad9)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(M1-Pad10)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "molex\n104031\nseries" (at 135.9408 111.1504 90) (layer F.SilkS))
  (gr_text "card\ndetect" (at 125.5776 110.5408 90) (layer F.SilkS))
  (gr_text "SPI\nuSD Card\n32bit.fun" (at 135.5852 111.2774 90) (layer B.SilkS))
  (gr_arc (start 131.6736 111.2012) (end 131.699 119.634) (angle 180.1725771) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.368 119.634) (end 131.699 119.634) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.368 102.7684) (end 150.368 119.634) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.6736 102.7684) (end 150.368 102.7684) (layer Edge.Cuts) (width 0.15))
  (gr_text CS (at 145.796 117.7036) (layer B.SilkS))
  (gr_text "MOSI\n" (at 144.9324 115.1636) (layer B.SilkS))
  (gr_text MISO (at 144.9324 112.4458) (layer B.SilkS))
  (gr_text SCK (at 145.2372 110.1344) (layer B.SilkS))
  (gr_text +3.3V (at 144.6022 107.5436) (layer B.SilkS))
  (gr_text GND (at 145.2372 105.0544) (layer B.SilkS))
)
