<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="15.24" y2="0" width="0.254" layer="20"/>
<wire x1="15.24" y1="0" x2="15.24" y2="15.24" width="0.254" layer="20"/>
<wire x1="15.24" y1="15.24" x2="0" y2="15.24" width="0.254" layer="20"/>
<wire x1="0" y1="15.24" x2="0" y2="0" width="0.254" layer="20"/>
<text>KD0GLS 2017</text>
<text>H</text>
<text>L</text>
<text>S</text>
<text>D</text>
<text>P</text>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="0805">
</package>
<package name="CONN_BREAKAWAY_1X5_100">
</package>
<package name="SWITCH_PANASONIC_EVQQ2">
</package>
<package name="SOT23-6">
<description>Revised pad sizes and positions per SN74LVC1T45DBVR data sheet.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="kd0gls" package="0805" value="0.1uF"/>
<element name="J1" library="kd0gls" package="CONN_BREAKAWAY_1X5_100" value="CONN_BREAKAWAY_1X5_100"/>
<element name="SW1" library="kd0gls" package="SWITCH_PANASONIC_EVQQ2" value="SWITCH_PANASONIC_EVQQ2"/>
<element name="U1" library="kd0gls" package="SOT23-6" value="PIC10F222/OT"/>
</elements>
<signals>
<signal name="+5V">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="SW1" pad="B"/>
<contactref element="SW1" pad="B'"/>
</signal>
<signal name="ICSPDAT">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="ICSPCLK">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="VPP">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="1"/>
<contactref element="SW1" pad="A"/>
<contactref element="SW1" pad="A'"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
