<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<board>
<plain>
<wire x1="97.5868" y1="54.9021" x2="98.056421875" y2="54.908715625" width="0.254" layer="20"/>
<wire x1="98.056421875" y1="54.908715625" x2="99.070490625" y2="53.90375625" width="0.254" layer="20" curve="-91.090349"/>
<wire x1="99.070490625" y1="53.90375625" x2="99.06" y2="51.816" width="0.254" layer="20"/>
<wire x1="99.06" y1="40.386" x2="99.534503125" y2="39.911496875" width="0.254" layer="20"/>
<wire x1="99.534503125" y1="39.911496875" x2="99.720490625" y2="39.4649625" width="0.254" layer="20" curve="-44.776401"/>
<wire x1="99.720490625" y1="39.4649625" x2="99.73300625" y2="3.470025" width="0.254" layer="20"/>
<wire x1="99.73300625" y1="3.470025" x2="99.542725" y2="3.013615625" width="0.254" layer="20" curve="-45.749369"/>
<wire x1="99.542725" y1="3.013615625" x2="99.06" y2="2.54" width="0.254" layer="20"/>
<wire x1="99.06" y1="2.54" x2="99.06" y2="-0.5621" width="0.254" layer="20"/>
<wire x1="99.06" y1="-0.5621" x2="98.06" y2="-1.5621" width="0.254" layer="20" curve="-90"/>
<wire x1="98.06" y1="-1.5621" x2="1" y2="-1.5621" width="0.254" layer="20"/>
<wire x1="1" y1="-1.5621" x2="0" y2="-0.5621" width="0.254" layer="20" curve="-90"/>
<wire x1="0" y1="-0.5621" x2="0" y2="53.914996875" width="0.254" layer="20"/>
<wire x1="0" y1="53.914996875" x2="1.000134375" y2="54.914996875" width="0.254" layer="20" curve="-90.007699"/>
<wire x1="1.000134375" y1="54.914996875" x2="97.5868" y2="54.9021" width="0.254" layer="20"/>
<wire x1="99.06" y1="51.816" x2="99.06" y2="40.386" width="0.254" layer="20"/>
<text>AREF</text>
<text>GND</text>
<text>TX1</text>
<text>RX1</text>
<text>Arduino-</text>
<text>RESET</text>
<text>3V3</text>
<text>5V</text>
<text>VIN</text>
<text>GND</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>6</text>
<text>A7</text>
<text>1</text>
<text>A8</text>
<text>A9</text>
<text>A10</text>
<text>A11</text>
<text>A12</text>
<text>A13</text>
<text>A14</text>
<text>A15</text>
<text>A16</text>
<text>A17</text>
<text>A20</text>
<text>24</text>
<text>25</text>
<text>32</text>
<text>33</text>
<text>PGM</text>
<text>5V</text>
<text>Teensy</text>
<text>SDA</text>
<text>SCL</text>
<text>IOREF</text>
<hole x="96.52" y="2.54" drill="3.2"/>
<hole x="15.24" y="50.8" drill="3.2"/>
<hole x="90.17" y="50.8" drill="3.2"/>
<hole x="13.97" y="2.54" drill="3.2"/>
<hole x="66.04" y="35.56" drill="3.2"/>
<hole x="66.04" y="7.62" drill="3.2"/>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>GND</text>
<text>ESP-GPIO</text>
<text>NRF24L01+</text>
<text>VUSB</text>
<text>CS</text>
<text>ESP-SPI0</text>
<text>5V</text>
<text>GND</text>
<text>6 - 16VDC</text>
<text>VIN Voltage</text>
<text>4/2017</text>
<text>REV 4.3</text>
<text>SERIAL</text>
<text>1</text>
<text>COMMS:</text>
<text>NRF24L01 : TEENSY SPI</text>
<text>ESP-12 : RX1/TX1</text>
<text>3V3</text>
<text>RX</text>
<text>TX</text>
<text>ENA</text>
<text>R4.3</text>
<text>ESP</text>
<text>TX2</text>
<text>RX2</text>
<text>TX3</text>
<text>RX3</text>
<text>3V3_ByP</text>
<text>KEY</text>
<text>3V3</text>
<text>GND</text>
<text>KEY</text>
<text>RX3</text>
<text>TX3</text>
<text>D24</text>
<text>RST</text>
<text>HC05/06 : RX3/TX3 + D24</text>
<text>TX1</text>
<text>IO16</text>
<text>RX1</text>
<text>IO14</text>
<text>IO2</text>
<text>IO4</text>
<text>IO12</text>
<text>IO15</text>
<text>IO13</text>
<text>IO5</text>
<text>ADC</text>
<text>+ESP-12E</text>
<text>3V3</text>
<text>ESP-GPIO</text>
<text>HC-05/06</text>
<text>NRF24L01+</text>
<text>D2</text>
<text>D12</text>
<text>D13</text>
<text>D11</text>
<text>RX2</text>
<text>TX2</text>
<text>GND</text>
<text>3V3</text>
<text>1</text>
<text>RN7</text>
<text>Q1</text>
<text>Q2</text>
<text>RN1</text>
<text>RN3</text>
<text>RN6</text>
<text>RN9</text>
<text>RN8</text>
<text>Q3</text>
<text>L1</text>
<text>D1</text>
<text>C1</text>
<text>R1</text>
<text>RN5</text>
<text>RN4</text>
<text>C8</text>
<text>STATE</text>
<text>F1</text>
<text>C5</text>
<text>R3</text>
<text>R4</text>
<text>IC1</text>
<text>D2</text>
<text>D3</text>
<text>L2</text>
<text>C7</text>
<text>C6</text>
<text>F2</text>
<text>C2</text>
<text>R2</text>
<text>IC2</text>
<text>C9</text>
<text>R5</text>
<text>C10</text>
<text>C3</text>
<text>(P)</text>
<text>(P)</text>
<text>(T)</text>
<text>(T)</text>
<text>(P)</text>
<text>(T)</text>
<text>(P)</text>
<text>(T)</text>
<text>(T)</text>
<text>(T)</text>
<text>(T)</text>
<text>(P)</text>
<text>(P)</text>
<text>(P)</text>
<text>(P)</text>
<text>(P)</text>
<text>(P)</text>
<text>(P)</text>
<text>(P)</text>
<text>(T)</text>
<text>(T)</text>
<text>(T)</text>
<text>(T)</text>
<text>(T)</text>
<text>DAC</text>
<text>-</text>
<text>+</text>
<text>CAN-RX</text>
<text>CAN-TX</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>3V3</text>
<text>VBAT</text>
<text>PGM</text>
<text>3V3</text>
<text>3.2_RST</text>
<text>3.1_RST</text>
<text>/EN</text>
<text>CS0</text>
<text>SCK</text>
<text>MISO</text>
<text>IO10</text>
<text>MOSI</text>
<text>IO9</text>
<text>GND</text>
<text>ESP-SPI0</text>
<text>VUSB</text>
<text>Q4</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
<package name="SMC_B">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="MINIMELF">
<description>&lt;b&gt;Mini Melf Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SmartPrj">
<packages>
<package name="R0603-ROUND">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="2X18">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="POWERSUPPLY_DC-21MM">
<description>DC 2.1mm Jack</description>
</package>
<package name="C0603-ROUND">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
<package name="DO220AAL">
</package>
<package name="SRR0604">
</package>
</packages>
</library>
<library name="resistor-dil">
<packages>
<package name="CAT16">
<description>&lt;b&gt;BOURNS&lt;/b&gt; Chip Resistor Array&lt;p&gt;
Source: RS Component / BUORNS</description>
</package>
<package name="EXB34V">
<description>&lt;b&gt;Chip Resistor Array 0603x2&lt;/b&gt; 2 resistors in 1.6 mm x 1.6 mm size (EXB34V, V4V)&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
</packages>
</library>
<library name="wuerth-elektronik">
<packages>
<package name="0805">
<description>Multilayer SMD</description>
</package>
</packages>
</library>
<library name="Teensy_3_and_LC_Series_Boards_v1.1">
<packages>
<package name="TEENSY3_ALL_PINS_&amp;_PADS">
</package>
</packages>
</library>
<library name="switch-tact">
<description>&lt;b&gt;Diptronics THMD &amp; SMD tact switches&lt;/b&gt;
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;DTS-3: 3.5x6mm THMD tact switch
&lt;li&gt;DTS-6, DTS-64: 6x6mm THMD tact switch
&lt;li&gt;DTSM-3: 3.5x6mm SMD tact switch
&lt;li&gt;DTSM-6, DTSM-64: 6x6mm SMD tact switch
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="DTSM-6">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X01-CLEANBIG">
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="PTC-1206">
</package>
<package name="1X02_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
</packages>
</library>
<library name="transistor-fet">
<description>&lt;b&gt;Field Effect Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
Symbols changed according to IEC617&lt;p&gt; 
All types, packages and assignment to symbols and pins checked&lt;p&gt;
Package outlines partly checked&lt;p&gt;
&lt;p&gt;
JFET = junction FET&lt;p&gt;
IGBT-x = insulated gate bipolar transistor&lt;p&gt;
x=N: NPN; x=P: PNP&lt;p&gt;
IGFET-mc-nnn; (IGFET=insulated gate field effect transistor)&lt;P&gt;
m=D: depletion mode (Verdr&amp;auml;ngungstyp)&lt;p&gt;
m=E: enhancement mode (Anreicherungstyp)&lt;p&gt;
c: N=N-channel; P=P-Channel&lt;p&gt;
GDSB: gate, drain, source, bulk&lt;p&gt;
&lt;p&gt;
by R. Vogg  15.March.2002</description>
<packages>
<package name="SOT363_INFINEON">
<description>&lt;b&gt;Small Outline Transistor; 6 leads&lt;/b&gt; Reflow soldering&lt;p&gt;
INFINEON, www.infineon.com/cmc_upload/0/000/010/257/eh_db_5b.pdf</description>
</package>
</packages>
</library>
<library name="ESP8266-ESP12E">
<packages>
<package name="ESP8266-ESP12E">
<description>
&lt;b&gt;ESP8266-12E with additional I/O and GPIO04/05 corrected&lt;/b&gt;&lt;p&gt;
The author cannot warrant that this library is free from error
or will meet your specific requirements.&lt;p&gt;
&lt;author&gt;Created by PuceBaboon.com. Komagane, Nagano, JAPAN&lt;/author&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_20MM_4LEGS">
</package>
</packages>
</library>
<library name="my-custom-lib">
<packages>
<package name="SOC89-L3">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SUPER-SOT3">
<description>&lt;b&gt;MOLDED PACKAGE SUPERSOT, 3 LEAD&lt;/b&gt; MKT-MAO3B&lt;p&gt;
Source: http://www.fairchildsemi.com/dwg/MA/MA03B.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SPI" library="SmartPrj" package="2X03" value="3x2M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SmartPrj" package="1X08" value="8x1F-H8.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SmartPrj" package="1X10" value="10x1F-H8.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="PANASONIC_D" value="47u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="PANASONIC_D" value="47u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="SmartPrj" package="POWERSUPPLY_DC-21MM" value="POWERSUPPLY_DC21MMX">
<attribute name="VALUE"/>
</element>
<element name="JP11" library="SmartPrj" package="1X08" value="8x1F-H8.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="SmartPrj" package="1X08" value="8x1F-H8.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SmartPrj" package="1X08" value="8x1F-H8.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="SmartPrj" package="1X08" value="8x1F-H8.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SmartPrj" package="2X18" value="18x2F-H8.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="wuerth-elektronik" package="0805" value="MH2029-300Y">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SmartPrj" package="SOT23-6" value="LM2734Y">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="SMC_B" value="10u Ceramic, 1206 or 1210">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SmartPrj" package="C0603-ROUND" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SmartPrj" package="R0603-ROUND" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SmartPrj" package="R0603-ROUND" value="52K3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="MINIMELF" value="CD1206-S01575">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SmartPrj" package="DO220AAL" value="SS1P3L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="SmartPrj" package="SRR0604" value="10u SRR0604-100ML">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SmartPrj" package="DO220AAL" value="SS1P3L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TEENSY_3.1/3.2" library="Teensy_3_and_LC_Series_Boards_v1.1" package="TEENSY3_ALL_PINS_&amp;_PADS" value="TEENSY_3.1_ALL_PINS_AND_PADS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="switch-tact" package="DTSM-6" value="DTSM-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD1" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="ESP-RST" library="switch-tact" package="DTSM-6" value="DTSM-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ESP-PGM" library="switch-tact" package="DTSM-6" value="DTSM-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HC-PGM" library="switch-tact" package="DTSM-6" value="DTSM-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3.2_RST" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3.1_RST" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN3" library="resistor-dil" package="CAT16" value="10k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="RN1" library="resistor-dil" package="CAT16" value="1k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="D13" library="adafruit" package="CHIPLED_0805" value="red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="adafruit" package="CHIPLED_0805" value="green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RXD1" library="adafruit" package="CHIPLED_0805" value="amber">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TXD1" library="adafruit" package="CHIPLED_0805" value="amber">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TXD2" library="adafruit" package="CHIPLED_0805" value="amber">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RXD2" library="adafruit" package="CHIPLED_0805" value="amber">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TXD3" library="adafruit" package="CHIPLED_0805" value="amber">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RXD3" library="adafruit" package="CHIPLED_0805" value="amber">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED10" library="adafruit" package="CHIPLED_0805" value="Yellow">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ4" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-fet" package="SOT363_INFINEON" value="BSD223P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor-fet" package="SOT363_INFINEON" value="BSD223P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="transistor-fet" package="SOT363_INFINEON" value="BSD223P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="SparkFun" package="PTC-1206" value=".5A/1A (0ZCJ0050FF2G)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VIN" library="SparkFun" package="1X02_LOCK_LONGPADS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0805" value="10uf Tantalum, 1206 package (F920J106MPA)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SmartPrj" package="C0603-ROUND" value=".1uf ceramic">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN6" library="resistor-dil" package="CAT16" value="22K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SJ5" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ6" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN7" library="resistor-dil" package="CAT16" value="1k">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="RN8" library="resistor-dil" package="EXB34V" value="10K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="RN9" library="resistor-dil" package="EXB34V" value="22K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="MDL1" library="ESP8266-ESP12E" package="ESP8266-ESP12E" value="ESP8266-12E)"/>
<element name="CR2032" library="SparkFun-Electromechanical" package="BATTCON_20MM_4LEGS" value="20mm coincell">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="BATT-10373"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="SMC_B" value="220uf Tantalum, 1206 or 1210 or SMC_B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN4" library="resistor-dil" package="EXB34V" value="10K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="RN5" library="resistor-dil" package="EXB34V" value="10K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="F2" library="SparkFun" package="PTC-1206" value=".5A/1A (0ZCJ0050FF2G)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SmartPrj" package="C0603-ROUND" value="1u ceramic, 0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SmartPrj" package="C0603-ROUND" value="1u ceramic">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0603" value="0-Ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="my-custom-lib" package="SOC89-L3" value="AP7215AP7215-SOC89-L3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HC-05/06" library="pinhead" package="1X06" value="PPPC061LFBN-RC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="transistor-power" package="SUPER-SOT3" value="FDN340P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+5V">
<contactref element="D2" pad="A"/>
<contactref element="L2" pad="P$2"/>
<contactref element="R3" pad="1"/>
<contactref element="C5" pad="+"/>
<contactref element="PAD1" pad="1"/>
<contactref element="F1" pad="1"/>
<contactref element="F2" pad="1"/>
<contactref element="Q4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="SPI" pad="6"/>
<contactref element="C5" pad="-"/>
<contactref element="C1" pad="-"/>
<contactref element="JP4" pad="7"/>
<contactref element="X1" pad="3"/>
<contactref element="JP11" pad="7"/>
<contactref element="JP11" pad="6"/>
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="R4" pad="2"/>
<contactref element="D3" pad="P$2"/>
<contactref element="RESET" pad="2"/>
<contactref element="TEENSY_3.1/3.2" pad="GND2"/>
<contactref element="TEENSY_3.1/3.2" pad="GND"/>
<contactref element="TEENSY_3.1/3.2" pad="GND1"/>
<contactref element="TEENSY_3.1/3.2" pad="AGND"/>
<contactref element="LED10" pad="C"/>
<contactref element="SJ1" pad="1"/>
<contactref element="SJ2" pad="1"/>
<contactref element="SJ3" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="JP8" pad="35"/>
<contactref element="JP8" pad="36"/>
<contactref element="D13" pad="C"/>
<contactref element="CR2032" pad="NEGATIVE"/>
<contactref element="ESP-PGM" pad="4"/>
<contactref element="MDL1" pad="9"/>
<contactref element="ESP-RST" pad="2"/>
<contactref element="C8" pad="-"/>
<contactref element="RN4" pad="3"/>
<contactref element="JP8" pad="25"/>
<contactref element="C9" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="HC-05/06" pad="4"/>
<contactref element="PWR" pad="C"/>
<contactref element="JP8" pad="24"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="JP11" pad="8"/>
<contactref element="C1" pad="+"/>
<contactref element="IC1" pad="5"/>
<contactref element="C2" pad="+"/>
<contactref element="D1" pad="P$1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="JP11" pad="4"/>
<contactref element="JP11" pad="2"/>
<contactref element="JP8" pad="4"/>
<contactref element="TEENSY_3.1/3.2" pad="3.3V2"/>
<contactref element="TEENSY_3.1/3.2" pad="3.3V"/>
<contactref element="TEENSY_3.1/3.2" pad="3.3V1"/>
<contactref element="HC-PGM" pad="2"/>
<contactref element="Q1" pad="4"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q2" pad="4"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q3" pad="4"/>
<contactref element="Q3" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="SPI" pad="2"/>
<contactref element="SJ5" pad="2"/>
<contactref element="SJ6" pad="1"/>
<contactref element="JP8" pad="26"/>
<contactref element="RN1" pad="4"/>
<contactref element="R5" pad="1"/>
<contactref element="HC-05/06" pad="5"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="AD2">
<contactref element="JP9" pad="3"/>
<contactref element="TEENSY_3.1/3.2" pad="16/A2"/>
</signal>
<signal name="AD3">
<contactref element="JP9" pad="4"/>
<contactref element="TEENSY_3.1/3.2" pad="17/A3"/>
</signal>
<signal name="AD6/CS1">
<contactref element="JP9" pad="7"/>
<contactref element="TEENSY_3.1/3.2" pad="20/A6"/>
</signal>
<signal name="AD7">
<contactref element="JP9" pad="8"/>
<contactref element="TEENSY_3.1/3.2" pad="21/A7"/>
</signal>
<signal name="SCL0-3/A5/D19">
<contactref element="TEENSY_3.1/3.2" pad="19/A5"/>
<contactref element="JP9" pad="6"/>
</signal>
<signal name="SDA0-3/A4/D18">
<contactref element="TEENSY_3.1/3.2" pad="18/A4"/>
<contactref element="JP9" pad="5"/>
</signal>
<signal name="AD17">
<contactref element="JP6" pad="2"/>
<contactref element="TEENSY_3.1/3.2" pad="28"/>
</signal>
<signal name="AD16">
<contactref element="JP6" pad="1"/>
<contactref element="TEENSY_3.1/3.2" pad="27"/>
</signal>
<signal name="AD20">
<contactref element="JP6" pad="3"/>
<contactref element="TEENSY_3.1/3.2" pad="31"/>
</signal>
<signal name="SDA1/A19/D30">
<contactref element="JP4" pad="9"/>
<contactref element="TEENSY_3.1/3.2" pad="30"/>
</signal>
<signal name="SCL1/A18/D29">
<contactref element="JP4" pad="10"/>
<contactref element="TEENSY_3.1/3.2" pad="29"/>
</signal>
<signal name="D11/DOUT/MOSI">
<contactref element="JP4" pad="4"/>
<contactref element="TEENSY_3.1/3.2" pad="11"/>
<contactref element="SPI" pad="4"/>
<contactref element="JP8" pad="30"/>
</signal>
<signal name="D12/DIN/MISO">
<contactref element="JP4" pad="5"/>
<contactref element="TEENSY_3.1/3.2" pad="12"/>
<contactref element="SPI" pad="1"/>
<contactref element="JP8" pad="31"/>
</signal>
<signal name="PWM9/RX2">
<contactref element="JP4" pad="2"/>
<contactref element="TEENSY_3.1/3.2" pad="9"/>
<contactref element="RN3" pad="3"/>
<contactref element="JP8" pad="27"/>
</signal>
<signal name="D8/TX3/A-MISO">
<contactref element="JP4" pad="1"/>
<contactref element="TEENSY_3.1/3.2" pad="8"/>
<contactref element="RN8" pad="3"/>
<contactref element="HC-05/06" pad="2"/>
</signal>
<signal name="PWM7/RX3/A-MOSI">
<contactref element="JP5" pad="8"/>
<contactref element="TEENSY_3.1/3.2" pad="7"/>
<contactref element="RN8" pad="1"/>
<contactref element="HC-05/06" pad="3"/>
</signal>
<signal name="PWM6/CS0">
<contactref element="JP5" pad="7"/>
<contactref element="TEENSY_3.1/3.2" pad="6"/>
<contactref element="SPI" pad="5"/>
</signal>
<signal name="D2">
<contactref element="JP5" pad="3"/>
<contactref element="TEENSY_3.1/3.2" pad="2"/>
<contactref element="JP8" pad="32"/>
</signal>
<signal name="PWM5">
<contactref element="JP5" pad="6"/>
<contactref element="TEENSY_3.1/3.2" pad="5"/>
</signal>
<signal name="TEENSY_RX1">
<contactref element="JP5" pad="1"/>
<contactref element="TEENSY_3.1/3.2" pad="0"/>
<contactref element="RN3" pad="1"/>
<contactref element="MDL1" pad="16"/>
<contactref element="JP8" pad="6"/>
</signal>
<signal name="TEENSY_TX1">
<contactref element="JP5" pad="2"/>
<contactref element="TEENSY_3.1/3.2" pad="1"/>
<contactref element="RN3" pad="2"/>
<contactref element="MDL1" pad="15"/>
<contactref element="JP8" pad="8"/>
</signal>
<signal name="AD1">
<contactref element="JP9" pad="2"/>
<contactref element="TEENSY_3.1/3.2" pad="15/A1"/>
</signal>
<signal name="AD0/A-SCK">
<contactref element="JP9" pad="1"/>
<contactref element="TEENSY_3.1/3.2" pad="14/A0"/>
</signal>
<signal name="AD8">
<contactref element="JP10" pad="1"/>
<contactref element="TEENSY_3.1/3.2" pad="22/A8"/>
</signal>
<signal name="AD9">
<contactref element="JP10" pad="2"/>
<contactref element="TEENSY_3.1/3.2" pad="23/A9"/>
</signal>
<signal name="AD10">
<contactref element="JP10" pad="3"/>
<contactref element="TEENSY_3.1/3.2" pad="A10"/>
</signal>
<signal name="AREF">
<contactref element="JP4" pad="8"/>
<contactref element="TEENSY_3.1/3.2" pad="AREF"/>
</signal>
<signal name="VIN+">
<contactref element="X1" pad="2"/>
<contactref element="L1" pad="2"/>
<contactref element="VIN" pad="2"/>
</signal>
<signal name="MASTER-RESET">
<contactref element="JP11" pad="3"/>
<contactref element="RESET" pad="3"/>
<contactref element="3.1_RST" pad="1"/>
<contactref element="3.2_RST" pad="1"/>
</signal>
<signal name="AD14/DAC">
<contactref element="TEENSY_3.1/3.2" pad="RESET/DAC"/>
<contactref element="JP10" pad="7"/>
</signal>
<signal name="CANTX/PWM3">
<contactref element="TEENSY_3.1/3.2" pad="3"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="AD13">
<contactref element="JP10" pad="6"/>
<contactref element="TEENSY_3.1/3.2" pad="A13"/>
</signal>
<signal name="D32">
<contactref element="JP6" pad="6"/>
<contactref element="TEENSY_3.1/3.2" pad="32"/>
</signal>
<signal name="AD11">
<contactref element="JP10" pad="4"/>
<contactref element="TEENSY_3.1/3.2" pad="A11"/>
</signal>
<signal name="PWM10/TX2">
<contactref element="JP4" pad="3"/>
<contactref element="TEENSY_3.1/3.2" pad="10"/>
<contactref element="JP8" pad="28"/>
<contactref element="RN3" pad="4"/>
</signal>
<signal name="D13/SCK">
<contactref element="JP4" pad="6"/>
<contactref element="TEENSY_3.1/3.2" pad="13"/>
<contactref element="SPI" pad="3"/>
<contactref element="RN1" pad="8"/>
<contactref element="JP8" pad="29"/>
</signal>
<signal name="BOOST">
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="SW">
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="D3" pad="P$1"/>
<contactref element="L2" pad="P$1"/>
</signal>
<signal name="FB">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="EN">
<contactref element="IC1" pad="4"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="L1" pad="1"/>
<contactref element="D1" pad="P$2"/>
</signal>
<signal name="VUSB">
<contactref element="TEENSY_3.1/3.2" pad="VUSB"/>
<contactref element="PAD2" pad="1"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="CANRX/PWM4">
<contactref element="JP5" pad="5"/>
<contactref element="TEENSY_3.1/3.2" pad="4"/>
</signal>
<signal name="VBAT">
<contactref element="TEENSY_3.1/3.2" pad="VBAT"/>
<contactref element="CR2032" pad="POSITIVE@3"/>
<contactref element="CR2032" pad="POSITIVE@2"/>
<contactref element="CR2032" pad="POSITIVE@1"/>
<contactref element="CR2032" pad="POSITIVE@4"/>
</signal>
<signal name="AD12">
<contactref element="JP10" pad="5"/>
<contactref element="TEENSY_3.1/3.2" pad="A12"/>
</signal>
<signal name="AD15">
<contactref element="JP10" pad="8"/>
<contactref element="TEENSY_3.1/3.2" pad="26"/>
</signal>
<signal name="D33">
<contactref element="TEENSY_3.1/3.2" pad="33"/>
<contactref element="JP6" pad="7"/>
</signal>
<signal name="D25">
<contactref element="TEENSY_3.1/3.2" pad="25"/>
<contactref element="JP6" pad="5"/>
</signal>
<signal name="D24">
<contactref element="TEENSY_3.1/3.2" pad="24"/>
<contactref element="JP6" pad="4"/>
<contactref element="SJ4" pad="1"/>
<contactref element="HC-05/06" pad="1"/>
</signal>
<signal name="PGM">
<contactref element="TEENSY_3.1/3.2" pad="PGM"/>
<contactref element="JP6" pad="8"/>
</signal>
<signal name="HC-KEY">
<contactref element="HC-PGM" pad="4"/>
<contactref element="HC-05/06" pad="6"/>
</signal>
<signal name="TX2L">
<contactref element="Q2" pad="6"/>
<contactref element="RN7" pad="6"/>
</signal>
<signal name="TX3L">
<contactref element="Q3" pad="6"/>
<contactref element="RN1" pad="7"/>
</signal>
<signal name="RX2L">
<contactref element="Q2" pad="3"/>
<contactref element="RN7" pad="5"/>
</signal>
<signal name="RX3L">
<contactref element="Q3" pad="3"/>
<contactref element="RN1" pad="6"/>
</signal>
<signal name="SER1_TRC">
<contactref element="SJ1" pad="2"/>
<contactref element="TXD1" pad="C"/>
<contactref element="RXD1" pad="C"/>
</signal>
<signal name="SER2_TRC">
<contactref element="SJ2" pad="2"/>
<contactref element="TXD2" pad="C"/>
<contactref element="RXD2" pad="C"/>
</signal>
<signal name="SER3_TRC">
<contactref element="SJ3" pad="2"/>
<contactref element="TXD3" pad="C"/>
<contactref element="RXD3" pad="C"/>
</signal>
<signal name="STA_LED_RES">
<contactref element="LED10" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="STA_LED_TRC">
<contactref element="SJ4" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="TX1_Q1A_GATE">
<contactref element="RN3" pad="7"/>
<contactref element="Q1" pad="2"/>
<contactref element="RN6" pad="6"/>
</signal>
<signal name="RX1_Q1B_GATE">
<contactref element="Q1" pad="5"/>
<contactref element="RN3" pad="8"/>
<contactref element="RN6" pad="5"/>
</signal>
<signal name="RX1L">
<contactref element="Q1" pad="3"/>
<contactref element="RN7" pad="7"/>
</signal>
<signal name="TX1L">
<contactref element="Q1" pad="6"/>
<contactref element="RN7" pad="8"/>
</signal>
<signal name="TX2_Q2A_GATE">
<contactref element="Q2" pad="2"/>
<contactref element="RN3" pad="5"/>
<contactref element="RN6" pad="8"/>
</signal>
<signal name="RX2_Q2B_GATE">
<contactref element="Q2" pad="5"/>
<contactref element="RN3" pad="6"/>
<contactref element="RN6" pad="7"/>
</signal>
<signal name="TX3_Q3A_GATE">
<contactref element="Q3" pad="2"/>
<contactref element="RN8" pad="2"/>
<contactref element="RN9" pad="3"/>
</signal>
<signal name="RX3_Q3B_GATE">
<contactref element="Q3" pad="5"/>
<contactref element="RN8" pad="4"/>
<contactref element="RN9" pad="4"/>
</signal>
<signal name="N$1">
</signal>
<signal name="5V-FUSE">
<contactref element="F1" pad="2"/>
<contactref element="JP11" pad="5"/>
<contactref element="TEENSY_3.1/3.2" pad="VIN"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="VIN2_GND">
<contactref element="VIN" pad="1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="RX1_TX1_RX2_TX2_PU_SJ">
<contactref element="RN6" pad="4"/>
<contactref element="RN6" pad="3"/>
<contactref element="RN6" pad="2"/>
<contactref element="RN6" pad="1"/>
<contactref element="SJ5" pad="1"/>
</signal>
<signal name="TX3_RX3_PU_SJ">
<contactref element="RN9" pad="1"/>
<contactref element="SJ6" pad="2"/>
<contactref element="RN9" pad="2"/>
</signal>
<signal name="TX1_LED_RES">
<contactref element="RN7" pad="1"/>
<contactref element="TXD1" pad="A"/>
</signal>
<signal name="RX1_LED_RES">
<contactref element="RXD1" pad="A"/>
<contactref element="RN7" pad="2"/>
</signal>
<signal name="TX2_LED_RES">
<contactref element="TXD2" pad="A"/>
<contactref element="RN7" pad="3"/>
</signal>
<signal name="RX2_LED_RES">
<contactref element="RXD2" pad="A"/>
<contactref element="RN7" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="RN1" pad="1"/>
<contactref element="D13" pad="A"/>
</signal>
<signal name="RX3_LED_RES">
<contactref element="RXD3" pad="A"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="TX3_LED_RES">
<contactref element="TXD3" pad="A"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="GPIO15">
<contactref element="MDL1" pad="10"/>
<contactref element="RN4" pad="2"/>
<contactref element="JP8" pad="16"/>
</signal>
<signal name="GPIO0">
<contactref element="MDL1" pad="12"/>
<contactref element="RN4" pad="1"/>
<contactref element="ESP-PGM" pad="2"/>
</signal>
<signal name="GPIO2">
<contactref element="MDL1" pad="11"/>
<contactref element="JP8" pad="14"/>
</signal>
<signal name="GPIO4">
<contactref element="MDL1" pad="13"/>
<contactref element="JP8" pad="12"/>
</signal>
<signal name="GPIO5">
<contactref element="MDL1" pad="14"/>
<contactref element="JP8" pad="10"/>
</signal>
<signal name="GPIO13">
<contactref element="MDL1" pad="7"/>
<contactref element="JP8" pad="15"/>
</signal>
<signal name="GPIO12">
<contactref element="MDL1" pad="6"/>
<contactref element="JP8" pad="13"/>
</signal>
<signal name="GPIO14">
<contactref element="MDL1" pad="5"/>
<contactref element="JP8" pad="11"/>
</signal>
<signal name="GPIO16">
<contactref element="MDL1" pad="4"/>
<contactref element="JP8" pad="9"/>
</signal>
<signal name="ADC">
<contactref element="MDL1" pad="2"/>
<contactref element="JP8" pad="7"/>
</signal>
<signal name="ESP-RST">
<contactref element="RN5" pad="2"/>
<contactref element="MDL1" pad="1"/>
<contactref element="ESP-RST" pad="4"/>
<contactref element="JP8" pad="5"/>
</signal>
<signal name="CH_PD">
<contactref element="MDL1" pad="3"/>
<contactref element="JP8" pad="23"/>
<contactref element="RN5" pad="1"/>
</signal>
<signal name="ESP_SPI0_CSO">
<contactref element="MDL1" pad="17"/>
<contactref element="JP8" pad="18"/>
</signal>
<signal name="ESP_SPI0_MISO">
<contactref element="MDL1" pad="18"/>
<contactref element="JP8" pad="22"/>
</signal>
<signal name="GPIO9">
<contactref element="MDL1" pad="19"/>
<contactref element="JP8" pad="21"/>
</signal>
<signal name="GPIO10">
<contactref element="MDL1" pad="20"/>
<contactref element="JP8" pad="17"/>
</signal>
<signal name="ESP_SPI0__MOSI">
<contactref element="MDL1" pad="21"/>
<contactref element="JP8" pad="19"/>
</signal>
<signal name="ESP_SPI0_SCLK">
<contactref element="MDL1" pad="22"/>
<contactref element="JP8" pad="20"/>
</signal>
<signal name="3V3_ESP_DED">
<contactref element="RN5" pad="3"/>
<contactref element="RN4" pad="4"/>
<contactref element="MDL1" pad="8"/>
<contactref element="C8" pad="+"/>
<contactref element="RN5" pad="4"/>
<contactref element="C10" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="5V_FUSE_TO_3V3_REG">
<contactref element="F2" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="RN1" pad="5"/>
<contactref element="PWR" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
