(kicad_pcb (version 20171130) (host pcbnew 5.1.6+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 1)
    (zones 0)
    (modules 8)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.7)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad4)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J3-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J3-Pad3)")
  )
  (module MountingHole:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 112.649 85.979)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference M2 (at 0 -2.921 180) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module KiCAD:oshw3mm (layer B.Cu) (tedit 0)
    (at 112.141 78.613 270)
    (fp_text reference "" (at 0 0 90) (layer B.SilkS))
    (fp_text value "" (at 0 0 90) (layer B.SilkS))
  )
  (module KiCAD:oshw3mm (layer F.Cu) (tedit 0)
    (at 112.141 78.613 90)
    (fp_text reference "" (at 0 0 90) (layer F.SilkS))
    (fp_text value "" (at 0 0 90) (layer F.SilkS))
  )
  (module Symbol:Symbol_Barrel_Polarity (layer B.Cu) (tedit 5765E9A7)
    (at 106.299 94.869)
    (descr "Barrel connector polarity indicator")
    (tags "barrel polarity")
    (attr virtual)
    (fp_text reference REF** (at 0 2 180) (layer B.SilkS) hide)
    (fp_text value Symbol_Barrel_Polarity (at 0 -2 180) (layer B.Fab))
  )
  (module Symbol:Symbol_Barrel_Polarity (layer F.Cu) (tedit 5765E9A7)
    (at 106.299 94.869 180)
    (descr "Barrel connector polarity indicator")
    (tags "barrel polarity")
    (attr virtual)
    (fp_text reference REF** (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Symbol_Barrel_Polarity (at 0 2) (layer F.Fab))
  )
  (module Connector_BarrelJack:BarrelJack_Horizontal (layer F.Cu) (tedit 5A1DBF6A)
    (at 113.38 93.599 180)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J3 (at -6.223 5.588) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at -6.2 -5.5) (layer F.Fab))
    (fp_text user %R (at -3 -2.95) (layer F.Fab))
    (pad 3 thru_hole roundrect (at -3 4.7 180) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J3-Pad3)"))
    (pad 2 thru_hole roundrect (at -6 0 180) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MC_HighVoltage:PhoenixContact_MCV_1,5_2-G-5.08_1x02_P5.08mm_Vertical (layer F.Cu) (tedit 5B784ED3)
    (at 118.364 78.867 270)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-5.08; number of pins: 02; pin pitch: 5.08mm; Vertical || order number: 1836299 8A 320V")
    (tags "phoenix_contact connector MCV_01x02_G_5.08mm")
    (fp_text reference J2 (at 2.54 -5.55 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 2.54 4.1 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.65 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 4 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC_HighVoltage.3dshapes/PhoenixContact_MCV_1,5_2-G-5.08_1x02_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_A_Molex_67643_Horizontal (layer F.Cu) (tedit 5EA03975)
    (at 107.823 81.28 270)
    (descr "USB type A, Horizontal, https://www.molex.com/pdm_docs/sd/676433910_sd.pdf")
    (tags "USB_A Female Connector receptacle")
    (fp_text reference J1 (at 11.557 0 180) (layer F.SilkS) hide)
    (fp_text value USB_A (at 3.5 14.5 90) (layer F.Fab))
    (fp_text user %R (at 3.5 3.7 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 7 0 270) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 4.5 0 270) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.5) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 5 thru_hole circle (at 10.07 2.71 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 5 thru_hole circle (at -3.07 2.71 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_Molex_67643_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "M2\n" (at 112.649 82.931 180) (layer B.SilkS))
  (gr_text + (at 103.251 94.869 90) (layer F.SilkS))
  (gr_text + (at 109.22 94.869 90) (layer B.SilkS))
  (gr_text "5V\n" (at 114.3 78.867 90) (layer B.SilkS))
  (gr_text Gnd (at 114.3 83.058 90) (layer F.SilkS))
  (gr_text Gnd (at 114.3 83.058 90) (layer B.SilkS))
  (gr_text "5V\n" (at 114.3 78.867 90) (layer F.SilkS))
  (gr_arc (start 101.6 95.758) (end 100.33 95.758) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 122.047 77.089) (end 123.317 77.089) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 122.047 95.758) (end 122.047 97.028) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 101.6 77.089) (end 101.6 75.819) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100.33 95.758) (end 100.33 77.089) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.047 97.028) (end 101.6 97.028) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.317 77.089) (end 123.317 95.758) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.6 75.819) (end 122.047 75.819) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name "Net-(J1-Pad4)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.317 97.028) (xy 100.33 97.028) (xy 100.33 75.819) (xy 123.317 75.819)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.317 97.028) (xy 100.33 97.028) (xy 100.33 75.819) (xy 123.317 75.819)
      )
    )
  )
)
