(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 80)
    (zones 0)
    (modules 23)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(J2_1-Pad1)")
  (net 4 "Net-(J2_2-Pad1)")
  (net 5 "Net-(J2_3-Pad1)")
  (net 6 "Net-(J2_4-Pad1)")
  (net 7 "Net-(J1_1-Pad1)")
  (net 8 "Net-(J1_2-Pad1)")
  (net 9 "Net-(J1_3-Pad1)")
  (net 10 "Net-(U1-Pad2)")
  (net 11 "Net-(D1-Pad2)")
  (net 12 "Net-(D1-Pad1)")
  (net 13 "Net-(D2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1_1-Pad1)")
    (add_net "Net-(J1_2-Pad1)")
    (add_net "Net-(J1_3-Pad1)")
    (add_net "Net-(J2_1-Pad1)")
    (add_net "Net-(J2_2-Pad1)")
    (add_net "Net-(J2_3-Pad1)")
    (add_net "Net-(J2_4-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net VCC)
  )
  (module Package_SO:VSSOP-8_2.4x2.1mm_P0.5mm (layer F.Cu) (tedit 60069151)
    (at 99.695 69.85 180)
    (descr http://www.ti.com/lit/ml/mpds050d/mpds050d.pdf)
    (tags "VSSOP DCU R-PDSO-G8 Pitch0.5mm")
    (attr smd)
    (fp_text reference U1 (at -3.175 -1.27 180) (layer F.SilkS))
    (fp_text value 74LVC2G32 (at 0 2.413 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.65 -0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1_3-Pad1)"))
    (pad 2 smd rect (at -1.65 -0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -1.65 0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad2)"))
    (pad 4 smd rect (at -1.65 0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.65 0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1_1-Pad1)"))
    (pad 6 smd rect (at 1.65 0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1_2-Pad1)"))
    (pad 7 smd rect (at 1.65 -0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad1)"))
    (pad 8 smd rect (at 1.65 -0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/VSSOP-8_2.4x2.1mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 95.885 73.533)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 1.905 -1.143) (layer F.SilkS))
    (fp_text value 3k3 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5)
    (at 101.12 73.66 180)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (attr smd)
    (fp_text reference D2 (at 0 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.75 0 180) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.75 0 180) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5)
    (at 101.12 76.2 180)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (attr smd)
    (fp_text reference D1 (at 0 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.75 0 180) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.75 0 180) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 96.52 62.23 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.54 0) (layer F.SilkS))
    (fp_text value 470R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2_2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 95.885 76.2 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -1.905 1.27) (layer F.SilkS))
    (fp_text value 33k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J2_4-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 95.25 70.1525 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.2075 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "ZX Speccy:logo-speccypl" (layer B.Cu) (tedit 0)
    (at 99.06 67.31 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 105.41 58.42)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1_1 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value R (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1_1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 105.41 62.23)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1_2 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value G (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1_2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 105.41 66.04)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1_3 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value B (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1_3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 105.41 76.2)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1_4 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value I (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 92.71 73.66)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1_5 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value +5V (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 105.41 71.12)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1_6 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value GND (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 92.71 58.42)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J2_1 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value RED (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2_1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 92.71 62.23)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J2_2 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value GREEN (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2_2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 92.71 71.12)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J2_3 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value BLUE (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2_3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 92.71 76.2)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J2_4 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value BRIGHT (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2_4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 102.235 58.42 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2_1-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(J1_1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 102.235 62.23 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -1.905 1.905) (layer F.SilkS))
    (fp_text value 5k6 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(J1_2-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2_2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 102.235 66.04 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 2.54 0) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2_3-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(J1_3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 96.52 58.42 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -2.54 0) (layer F.SilkS))
    (fp_text value 470R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2_1-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 96.52 66.04 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 2.54 0) (layer F.SilkS))
    (fp_text value 470R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2_3-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 5.08 (width 0.15) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 113.06 68.58 270) (layer Dwgs.User))
    (feature1 (pts (xy 107.315 71.12) (xy 112.346421 71.12)))
    (feature2 (pts (xy 107.315 66.04) (xy 112.346421 66.04)))
    (crossbar (pts (xy 111.76 66.04) (xy 111.76 71.12)))
    (arrow1a (pts (xy 111.76 71.12) (xy 111.173579 69.993496)))
    (arrow1b (pts (xy 111.76 71.12) (xy 112.346421 69.993496)))
    (arrow2a (pts (xy 111.76 66.04) (xy 111.173579 67.166504)))
    (arrow2b (pts (xy 111.76 66.04) (xy 112.346421 67.166504)))
  )
  (dimension 15.24 (width 0.15) (layer Dwgs.User)
    (gr_text "0.6000 in" (at 99.06 50.77) (layer Dwgs.User))
    (feature1 (pts (xy 106.68 53.975) (xy 106.68 51.483579)))
    (feature2 (pts (xy 91.44 53.975) (xy 91.44 51.483579)))
    (crossbar (pts (xy 91.44 52.07) (xy 106.68 52.07)))
    (arrow1a (pts (xy 106.68 52.07) (xy 105.553496 52.656421)))
    (arrow1b (pts (xy 106.68 52.07) (xy 105.553496 51.483579)))
    (arrow2a (pts (xy 91.44 52.07) (xy 92.566504 52.656421)))
    (arrow2b (pts (xy 91.44 52.07) (xy 92.566504 51.483579)))
  )
  (dimension 20.32 (width 0.15) (layer Dwgs.User)
    (gr_text "0.8000 in" (at 83.155 67.31 90) (layer Dwgs.User))
    (feature1 (pts (xy 86.36 57.15) (xy 83.868579 57.15)))
    (feature2 (pts (xy 86.36 77.47) (xy 83.868579 77.47)))
    (crossbar (pts (xy 84.455 77.47) (xy 84.455 57.15)))
    (arrow1a (pts (xy 84.455 57.15) (xy 85.041421 58.276504)))
    (arrow1b (pts (xy 84.455 57.15) (xy 83.868579 58.276504)))
    (arrow2a (pts (xy 84.455 77.47) (xy 85.041421 76.343496)))
    (arrow2b (pts (xy 84.455 77.47) (xy 83.868579 76.343496)))
  )
  (dimension 5.08 (width 0.15) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 110.52 73.66 270) (layer Dwgs.User))
    (feature1 (pts (xy 107.315 76.2) (xy 109.806421 76.2)))
    (feature2 (pts (xy 107.315 71.12) (xy 109.806421 71.12)))
    (crossbar (pts (xy 109.22 71.12) (xy 109.22 76.2)))
    (arrow1a (pts (xy 109.22 76.2) (xy 108.633579 75.073496)))
    (arrow1b (pts (xy 109.22 76.2) (xy 109.806421 75.073496)))
    (arrow2a (pts (xy 109.22 71.12) (xy 108.633579 72.246504)))
    (arrow2b (pts (xy 109.22 71.12) (xy 109.806421 72.246504)))
  )
  (dimension 2.54 (width 0.15) (layer Dwgs.User)
    (gr_text "0.1000 in" (at 87.6 72.39 90) (layer Dwgs.User))
    (feature1 (pts (xy 90.805 71.12) (xy 88.313579 71.12)))
    (feature2 (pts (xy 90.805 73.66) (xy 88.313579 73.66)))
    (crossbar (pts (xy 88.9 73.66) (xy 88.9 71.12)))
    (arrow1a (pts (xy 88.9 71.12) (xy 89.486421 72.246504)))
    (arrow1b (pts (xy 88.9 71.12) (xy 88.313579 72.246504)))
    (arrow2a (pts (xy 88.9 73.66) (xy 89.486421 72.533496)))
    (arrow2b (pts (xy 88.9 73.66) (xy 88.313579 72.533496)))
  )
  (dimension 3.81 (width 0.15) (layer Dwgs.User)
    (gr_text "0.1500 in" (at 87.6 60.325 90) (layer Dwgs.User))
    (feature1 (pts (xy 90.805 58.42) (xy 88.313579 58.42)))
    (feature2 (pts (xy 90.805 62.23) (xy 88.313579 62.23)))
    (crossbar (pts (xy 88.9 62.23) (xy 88.9 58.42)))
    (arrow1a (pts (xy 88.9 58.42) (xy 89.486421 59.546504)))
    (arrow1b (pts (xy 88.9 58.42) (xy 88.313579 59.546504)))
    (arrow2a (pts (xy 88.9 62.23) (xy 89.486421 61.103496)))
    (arrow2b (pts (xy 88.9 62.23) (xy 88.313579 61.103496)))
  )
  (dimension 3.81 (width 0.15) (layer Dwgs.User)
    (gr_text "0.1500 in" (at 110.52 64.135 270) (layer Dwgs.User))
    (feature1 (pts (xy 107.315 66.04) (xy 109.806421 66.04)))
    (feature2 (pts (xy 107.315 62.23) (xy 109.806421 62.23)))
    (crossbar (pts (xy 109.22 62.23) (xy 109.22 66.04)))
    (arrow1a (pts (xy 109.22 66.04) (xy 108.633579 64.913496)))
    (arrow1b (pts (xy 109.22 66.04) (xy 109.806421 64.913496)))
    (arrow2a (pts (xy 109.22 62.23) (xy 108.633579 63.356504)))
    (arrow2b (pts (xy 109.22 62.23) (xy 109.806421 63.356504)))
  )
  (gr_text "TC2068 NoBRIGHT BLK" (at 99.06 64.135) (layer F.SilkS))
  (gr_line (start 92.075 57.15) (end 91.44 57.785) (layer Edge.Cuts) (width 0.05))
  (dimension 17.78 (width 0.15) (layer Dwgs.User)
    (gr_text "0.7000 in" (at 115.6 67.31 270) (layer Dwgs.User))
    (feature1 (pts (xy 111.76 76.2) (xy 114.886421 76.2)))
    (feature2 (pts (xy 111.76 58.42) (xy 114.886421 58.42)))
    (crossbar (pts (xy 114.3 58.42) (xy 114.3 76.2)))
    (arrow1a (pts (xy 114.3 76.2) (xy 113.713579 75.073496)))
    (arrow1b (pts (xy 114.3 76.2) (xy 114.886421 75.073496)))
    (arrow2a (pts (xy 114.3 58.42) (xy 113.713579 59.546504)))
    (arrow2b (pts (xy 114.3 58.42) (xy 114.886421 59.546504)))
  )
  (dimension 12.7 (width 0.15) (layer Dwgs.User)
    (gr_text "0.5000 in" (at 99.06 81.309986) (layer Dwgs.User))
    (feature1 (pts (xy 105.41 77.47) (xy 105.41 80.596407)))
    (feature2 (pts (xy 92.71 77.47) (xy 92.71 80.596407)))
    (crossbar (pts (xy 92.71 80.009986) (xy 105.41 80.009986)))
    (arrow1a (pts (xy 105.41 80.009986) (xy 104.283496 80.596407)))
    (arrow1b (pts (xy 105.41 80.009986) (xy 104.283496 79.423565)))
    (arrow2a (pts (xy 92.71 80.009986) (xy 93.836504 80.596407)))
    (arrow2b (pts (xy 92.71 80.009986) (xy 93.836504 79.423565)))
  )
  (gr_line (start 91.44 77.47) (end 91.44 57.785) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.68 77.47) (end 91.44 77.47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.68 57.15) (end 106.68 77.47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.075 57.15) (end 106.68 57.15) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.68 77.47) (xy 91.44 77.47) (xy 92.075 57.15) (xy 106.68 57.15)
      )
    )
  )
)
