(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 40)
    (tracks 25)
    (zones 0)
    (modules 2)
    (nets 4)
  )
  (page A4)
  (title_block
    (title "Phoenix Connector Audio Adapter")
    (date 2018-03-30)
    (rev 0.1)
    (company "db Electronics")
    (comment 1 "Licensed Under The CERN OHL v.1.2")
    (comment 2 https://github.com/db-electronics/phoenix-audio-adapter-kicad)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.635)
    (trace_clearance 0.1778)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1778)
    (via_size 0.6096)
    (via_drill 0.3048)
    (via_min_size 0.6096)
    (via_min_drill 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 139.7 114.3)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/0.1/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /LEFT)
  (net 3 /RIGHT)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.635)
    (via_dia 0.6096)
    (via_drill 0.3048)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LEFT)
    (add_net /RIGHT)
    (add_net GND)
  )
  (module db-thparts:RCJ-2223 (layer B.Cu) (tedit 5ABD818D)
    (at 139.7 107.3 180)
    (solder_mask_margin 0.1016)
    (fp_text reference CON101 (at 5.08 -1.1) (layer B.SilkS))
    (fp_text value RCJ-2223 (at -4.6 2.3) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 -7 180) (size 1.778 1.778) (drill 1.1938) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -4 -10.25 180) (size 1.778 1.778) (drill 1.1938) (layers *.Cu *.Mask)
      (net 2 /LEFT))
    (pad 3 thru_hole circle (at 4 -11.5 180) (size 1.778 1.778) (drill 1.1938) (layers *.Cu *.Mask)
      (net 3 /RIGHT))
  )
  (module db-artwork:db-logo_7.5mm (layer F.Cu) (tedit 0)
    (at 143.5 109.5)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text db-electronics.ca (at 141.4 111.9) (layer F.SilkS))
  (gr_text L+ (at 146.7 120.5) (layer F.SilkS))
  (gr_text L- (at 143.4 120.5) (layer F.SilkS))
  (gr_text G (at 139.7 120.5) (layer F.SilkS))
  (gr_text R+ (at 136.7 120.5) (layer F.SilkS))
  (gr_text R- (at 133.2 120.5) (layer F.SilkS))
  (gr_line (start 147.3 121.3) (end 147.8 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.8 121.3) (end 146.1 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.3 121.3) (end 142.6 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.8 121.3) (end 139.1 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.3 121.3) (end 135.6 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.6 121.3) (end 132.1 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.6 127.3) (end 143.8 127.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.8 127.3) (end 143.8 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.3 127.3) (end 147.3 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.1 121.3) (end 146.1 127.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.1 127.3) (end 147.3 127.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.6 121.3) (end 142.6 127.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.3 127.3) (end 133.3 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.1 127.3) (end 133.3 127.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.1 121.3) (end 132.1 127.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.8 127.3) (end 136.8 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.6 127.3) (end 136.8 127.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.6 121.3) (end 135.6 127.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.3 127.3) (end 140.3 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.1 127.3) (end 140.3 127.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.1 121.3) (end 139.1 127.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.8 118.8) (end 147.8 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.8 116.3) (end 147.8 118.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.1 116.3) (end 147.8 116.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.1 113.3) (end 146.1 116.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.8 113.3) (end 146.1 113.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.8 107.3) (end 147.8 113.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.6 107.3) (end 147.8 107.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.6 118.8) (end 131.6 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.6 116.3) (end 131.6 118.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.3 116.3) (end 131.6 116.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.3 113.3) (end 133.3 116.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.6 113.3) (end 133.3 113.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.6 107.3) (end 131.6 113.3) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.1 122.3) (xy 132.1 127.3) (xy 133.3 127.3) (xy 133.3 122.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.6 122.3) (xy 135.6 127.3) (xy 136.8 127.3) (xy 136.8 122.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.1 122.3) (xy 139.1 127.3) (xy 140.3 127.3) (xy 140.3 122.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.6 122.3) (xy 142.6 127.3) (xy 143.8 127.3) (xy 143.8 122.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.1 122.3) (xy 146.1 127.3) (xy 147.3 127.3) (xy 147.3 122.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.1 122.3) (xy 132.1 127.3) (xy 133.3 127.3) (xy 133.3 122.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.6 122.3) (xy 135.6 127.3) (xy 136.8 127.3) (xy 136.8 122.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.1 122.3) (xy 139.1 127.3) (xy 140.3 127.3) (xy 140.3 122.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.6 122.3) (xy 142.6 127.3) (xy 143.8 127.3) (xy 143.8 122.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.1 122.3) (xy 146.1 127.3) (xy 147.3 127.3) (xy 147.3 122.3)
      )
    )
  )
)
