<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0.0136" y1="0.0216" x2="17.8936" y2="0.0216" width="0" layer="20"/>
<wire x1="17.8936" y1="0.0216" x2="17.8936" y2="15.0216" width="0" layer="20"/>
<wire x1="17.8936" y1="15.0216" x2="0.0136" y2="15.0216" width="0" layer="20"/>
<wire x1="0.0136" y1="15.0216" x2="0.0136" y2="0.0216" width="0" layer="20"/>
<text>Battery</text>
<text>+     -</text>
<text>+     -</text>
<text>Solar</text>
<text>Remove
C1 and D1
Jumper for Ver 1</text>
<text>Rev B  2/23/2019</text>
<text>LED Driver/Solar Chg V1/V2</text>
<text>A</text>
<text>C</text>
<text>Red   Black</text>
<text>Yellow  Violet</text>
<text>Bud PB-1560</text>
<text>Potting Box</text>
<text>Orange  Green</text>
<text>LED</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="1X02">
<description>Pitch: 0.1" (2.54mm)&lt;br&gt;Drill: 0.040" dia</description>
</package>
<package name="1/4W_AXIAL_RESISTOR_3.5MIL(V2)">
<description>Axial 1/4Watt Resistor&lt;p&gt;Pitch: 0.35"</description>
</package>
<package name="QX5252F">
<description>LED Driver/Solar Battery Charger&lt;br&gt;&lt;a href="https://www.mikrocontroller.net/attachment/158139/QX5252.pdf"&gt;Data Sheet&lt;/a&gt;</description>
</package>
<package name="GENERIC_0100_DEVICE_100_SPACING">
<description>Pitch: 0.1" (2.54mm)</description>
</package>
<package name="DIODE-1N4148(NEW)">
<description>Pitch: 0.2"</description>
</package>
<package name="ART_CHEROKEE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="J2" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="L1" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="a-lib" package="QX5252F" value="">
<attribute name="NAME"/>
</element>
<element name="C1" library="a-lib" package="GENERIC_0100_DEVICE_100_SPACING" value="0.1UF">
<attribute name="MARKING" value="104 (100nF)"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="a-lib" package="DIODE-1N4148(NEW)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="U$1" library="a-lib" package="ART_CHEROKEE" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="P$2"/>
<contactref element="L1" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="L1" pad="2"/>
<contactref element="U1" pad="P$4"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="P$3"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="P$1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="C1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="J3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
