(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 87)
    (no_connects 0)
    (area 35.726679 37.81514 109.081442 185.081601)
    (thickness 1.6002)
    (drawings 25)
    (tracks 1005)
    (zones 0)
    (modules 185)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.35)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.127)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 2.032)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.1)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000007)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../IF Module/Gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(ANT501-Pad1)")
  (net 2 "Net-(C504-Pad2)")
  (net 3 "Net-(C101-Pad2)")
  (net 4 "Net-(C103-Pad1)")
  (net 5 "Net-(C103-Pad2)")
  (net 6 "Net-(R101-Pad2)")
  (net 7 "Net-(T501-Pad4)")
  (net 8 "Net-(J105-Pad1)")
  (net 9 "Net-(J103-Pad1)")
  (net 10 "Net-(J104-Pad1)")
  (net 11 "Net-(C105-Pad2)")
  (net 12 "Net-(J108-Pad1)")
  (net 13 GNDA)
  (net 14 PIN_Switch_2)
  (net 15 "Net-(C106-Pad2)")
  (net 16 PIN_Switch_3)
  (net 17 "Net-(C107-Pad2)")
  (net 18 "Net-(C108-Pad2)")
  (net 19 PIN_Switch_1)
  (net 20 GND)
  (net 21 "Net-(J106-Pad1)")
  (net 22 "Net-(JP103-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(ANT501-Pad1)")
    (add_net "Net-(C101-Pad2)")
    (add_net "Net-(C103-Pad1)")
    (add_net "Net-(C103-Pad2)")
    (add_net "Net-(C105-Pad2)")
    (add_net "Net-(C106-Pad2)")
    (add_net "Net-(C107-Pad2)")
    (add_net "Net-(C108-Pad2)")
    (add_net "Net-(C504-Pad2)")
    (add_net "Net-(J103-Pad1)")
    (add_net "Net-(J104-Pad1)")
    (add_net "Net-(J105-Pad1)")
    (add_net "Net-(J106-Pad1)")
    (add_net "Net-(J108-Pad1)")
    (add_net "Net-(JP103-Pad1)")
    (add_net "Net-(R101-Pad2)")
    (add_net "Net-(T501-Pad4)")
    (add_net PIN_Switch_1)
    (add_net PIN_Switch_2)
    (add_net PIN_Switch_3)
  )
  (net_class Power.35 ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power.5 ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power.75 ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power1.0 ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Mounting_Holes:MountingHole_5mm locked (layer F.Cu) (tedit 5A90BA5E)
    (at 95.88 45.29)
    (descr "Mounting hole, Befestigungsbohrung, 5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -6.49986) (layer F.SilkS) hide)
    (fp_text value MountingHole_5mm (at 0 7.00024) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers))
  )
  (module Mounting_Holes:MountingHole_5mm locked (layer F.Cu) (tedit 5A90BA5E)
    (at 48.84 45.29)
    (descr "Mounting hole, Befestigungsbohrung, 5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -6.49986) (layer F.SilkS) hide)
    (fp_text value MountingHole_5mm (at 0 7.00024) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 155.72)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A940CBE)
    (at 90.5 131.39)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J106 (at 0.08 -2.39) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J106-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_2-5mm locked (layer F.Cu) (tedit 5A90BA37)
    (at 97.7 160.35)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_5mm locked (layer F.Cu) (tedit 5A90BA4D)
    (at 95.88 136)
    (descr "Mounting hole, Befestigungsbohrung, 5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -6.49986) (layer F.SilkS) hide)
    (fp_text value MountingHole_5mm (at 0 7.00024) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 71.27 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 84.97 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Connect:BNC_Right_Angle locked (layer F.Cu) (tedit 5A8F75E7)
    (at 72.28 151 180)
    (descr file:///Users/Charles/Downloads/ENG_CD_5227677_A1.pdf)
    (tags "	\r5227677-1")
    (fp_text reference P501 (at -0.36 -6.02 180) (layer F.SilkS))
    (fp_text value "BNC ANT OUT ~~50Ω" (at -3.81 11.43 180) (layer F.Fab))
    (fp_text user CTR (at 1.5494 -2.032 180) (layer F.SilkS))
    (fp_text user GND (at -2.2987 -2.032 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at -5.08 -5.08 180) (size 3 3) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(JP103-Pad1)") (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 16 PIN_Switch_3))
    (pad 2 thru_hole rect (at -2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(JP103-Pad1)") (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
    (pad 2 thru_hole circle (at 5.08 -5.08 180) (size 3 3) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(JP103-Pad1)") (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 61.14 142.98)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 64.77 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 163.04)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 162.31)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 161.58)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 160.85)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.89 160.12)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 159.39)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 158.65)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 157.92)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 157.18)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 156.42)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 155.69)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 154.95)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 154.23)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 153.5)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 152.76)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 152.03)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 151.29)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 150.55)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 149.83)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 149.1)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 148.37)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 147.64)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 146.9)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 146.17)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 145.43)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 144.69)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.88 143.95)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A905B81)
    (at 85.5 146.24)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J103 (at 2.77 0.61) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J103-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 144)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 144.74)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 145.48)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 146.22)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 146.95)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 147.69)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 148.42)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 149.15)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 149.88)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 150.6)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 151.34)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 152.08)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 152.81)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 153.55)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 154.28)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 155)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 156.47)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 157.23)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 157.97)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 158.7)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 159.44)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.31 160.17)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 160.9)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 161.63)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 162.36)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.3 163.09)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A94141E)
    (at 72.44 145.43)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J107 (at -2.88 0.67) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 PIN_Switch_3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A940C12)
    (at 58.06 156.17)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J106 (at -2.43 0.7) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J106-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A9336EC)
    (at 74.96 140.57)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference GNDA (at 1.09 -2.23) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GNDA) (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A9414B2)
    (at 74.98 145.43)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J109 (at 2.67 0.8) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(JP103-Pad1)") (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A940C1B)
    (at 58.12 148.64)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J105 (at -2.66 0.67) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J105-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 100.83 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 100.11 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 99.38 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 98.66 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 97.94 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 97.22 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 96.5 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 95.78 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 95.06 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 94.34 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 93.62 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 92.9 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 92.18 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 91.46 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 90.74 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 90.02 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 89.3 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 88.57 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 87.85 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 87.13 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 86.41 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 85.69 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 84.25 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 83.53 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.81 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 82.08 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 81.36 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 80.64 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 79.92 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 79.2 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 78.48 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 77.76 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 77.04 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 76.32 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 75.6 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 74.16 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 73.44 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 72.71 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 71.99 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 70.55 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 69.83 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 69.11 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 68.39 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 67.67 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 66.95 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 66.23 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 65.5 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 64.04 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 63.32 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 62.59 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 61.86 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 60.41 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 59.68 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 58.23 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 56.78 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 56.05 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 55.32 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 54.59 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 53.87 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 53.15 142.99)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 52.43 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 51.71 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 50.99 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 50.27 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 49.55 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 48.83 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 48.1 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 47.37 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 46.66 143.02)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 45.94 143.01)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 45.22 143.01)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 44.5 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Oddities:Rod_Attachment locked (layer F.Cu) (tedit 589680DA)
    (at 72.25 94.24)
    (descr "Through hole pin header")
    (tags "pin header")
    (clearance 0.1)
    (fp_text reference ANT501 (at 0.2 -38.4) (layer F.SilkS))
    (fp_text value "15-cm Rod" (at 0.4445 -5.2324) (layer F.Fab))
    (pad "" np_thru_hole circle (at 4.02 -27.68) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -4.01 -27.68) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 1.8 -36) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.8 -36) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.8 -45.1485) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad 1 smd rect (at 0 -25.4127) (size 5 15) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(ANT501-Pad1)"))
    (pad "" np_thru_hole circle (at 1.8 -45) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58991CBB)
    (at 72.25 111.79 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C501 (at 0.07 -1.37 180) (layer B.SilkS))
    (fp_text value 3900pF (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C103-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C103-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:KNOWLES-JZ500_Handsolder (layer B.Cu) (tedit 58973C0F)
    (at 72.6 77.53 180)
    (fp_text reference C502 (at 0 0 180) (layer B.SilkS))
    (fp_text value 8-50pF (at 0 -2.54 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.4 0 180) (size 1.9 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(ANT501-Pad1)"))
    (pad 2 smd rect (at 2.4 0 180) (size 1.9 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 GNDA))
  )
  (module Oddities:Large_Loop_Attachment locked (layer B.Cu) (tedit 58967F2F)
    (at 72.2 93.62 180)
    (clearance 0.07)
    (fp_text reference L502 (at 0 -14 180) (layer B.SilkS))
    (fp_text value "~~0.49uH (22cm dia. loop)" (at 0.4445 5.2324 180) (layer B.Fab))
    (pad "" np_thru_hole circle (at 8.3033 -5.0939 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at 24.8097 -20.3558 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at 18.5097 -21.4558 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at 14.732 -4.0005 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at 12.25 -22.58 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at 21.3033 -2.7939 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -12.2097 -22.5558 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -8.3033 -5.0939 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -18.5097 -21.4558 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -14.732 -4.0005 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -24.8097 -20.3558 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad 2 smd rect (at 15.113 -12.9921 170) (size 25 15) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C103-Pad2)"))
    (pad 1 smd rect (at -15.113 -12.9921 190) (size 25 15) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C103-Pad1)"))
    (pad "" np_thru_hole circle (at -21.3033 -2.7939 190) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
  )
  (module Oddities:Trace_Loop_SM locked (layer B.Cu) (tedit 58973EFF)
    (at 72.54 93.08 180)
    (tags "loop antenna")
    (fp_text reference L501 (at 0.04 1.8 180) (layer B.SilkS))
    (fp_text value "PCB Trace" (at 0.4445 5.2324 180) (layer B.Fab))
    (pad 1 smd rect (at -2 -3 180) (size 1.7272 7) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C101-Pad2)"))
    (pad 2 smd rect (at 2 -3 180) (size 1.7272 7) (layers B.Cu B.Paste B.Mask)
      (net 13 GNDA))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 5A90426B)
    (at 51.57 128.28)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C101 (at -1.98 -1.74) (layer B.SilkS))
    (fp_text value 4700pF (at 0 -2.3) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 13 GNDA) (zone_connect 1) (thermal_gap 0.15))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C101-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 5A90425A)
    (at 53.1 130.58)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C102 (at -0.01 1.73) (layer B.SilkS))
    (fp_text value 2200pF (at 0 -2.3) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 13 GNDA) (zone_connect 1) (thermal_gap 0.15))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C101-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:KNOWLES-JZ500_Handsolder (layer B.Cu) (tedit 5A8ED46A)
    (at 77.98 123.22 270)
    (fp_text reference C103 (at 0 2.54 270) (layer B.SilkS))
    (fp_text value 12-60pF (at 0 -2.54 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.4 0 270) (size 1.9 1.5) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C103-Pad1)"))
    (pad 2 smd rect (at 2.4 0 270) (size 1.9 1.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C103-Pad2)"))
  )
  (module Capacitors_SMD:KNOWLES-JZ500_Handsolder (layer B.Cu) (tedit 5A90427B)
    (at 48.62 122.87 270)
    (fp_text reference C104 (at 0 0.07 360) (layer B.SilkS))
    (fp_text value 12-60pF (at 0 -2.54 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.4 0 270) (size 1.9 1.5) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C101-Pad2)"))
    (pad 2 smd rect (at 2.4 0 270) (size 1.9 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 GNDA) (zone_connect 1) (thermal_gap 0.15))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A8ED228)
    (at 72.5 78.85)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C503 (at 0 -1.64) (layer F.SilkS))
    (fp_text value 68pF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 13 GNDA))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(ANT501-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 5A8ED33D)
    (at 61.77 135.74)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C504 (at 0.04 1.64) (layer B.SilkS))
    (fp_text value 470nF (at 0 -2.3) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 19 PIN_Switch_1))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C504-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A8ED378)
    (at 59.74 134.56 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R101 (at 0.14 1.79 90) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 PIN_Switch_2))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R101-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_CTS_270X_Series (layer F.Cu) (tedit 5A8F76C2)
    (at 47.39 154.17 90)
    (descr "Potentiometer, Trimmer, Piher, PT15, Type V17.5, horizontal, Rev A, 02 Aug 2010,")
    (tags "Potentiometer, Trimmer, Piher, PT15, Type V17.5, horizontal, Rev A, 02 Aug 2010,")
    (fp_text reference RV101 (at -0.254 6.3119 90) (layer F.SilkS))
    (fp_text value 1K (at -0.0889 3.9624 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 2.49936 2.49936) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J106-Pad1)"))
    (pad 1 thru_hole circle (at 4.37 0 90) (size 2.49936 2.49936) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J105-Pad1)"))
    (pad 3 thru_hole rect (at -4.37 0 90) (size 2.49936 2.49936) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 13 GNDA) (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
  )
  (module Oddities:BN-2402_Core_2_windings_Vert_TH (layer F.Cu) (tedit 5A8ED25B)
    (at 72.64 83.51 270)
    (descr "Through hole toroid")
    (tags toroid)
    (fp_text reference T502 (at 0.01 4.32 270) (layer F.SilkS))
    (fp_text value "#24 / BN-61-2402" (at 0.3175 7.3914 270) (layer F.Fab))
    (fp_text user S1 (at 3.3528 1.6383 270) (layer F.SilkS))
    (fp_text user S1' (at 3.3274 -2.9337 270) (layer F.SilkS))
    (fp_text user P (at -3.048 1.6383 270) (layer F.SilkS))
    (fp_text user P' (at -2.9845 -2.6543 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1 -1.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(ANT501-Pad1)"))
    (pad 2 thru_hole oval (at -1 1.45 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GNDA))
    (pad 3 thru_hole oval (at 1 -1.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C108-Pad2)"))
    (pad 4 thru_hole oval (at 1 1.45 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06 locked (layer F.Cu) (tedit 5A91A4CE)
    (at 73.46 127.48 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J101 (at 1.22 15.31 180) (layer F.SilkS))
    (fp_text value "Plug-in Capacitors" (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C103-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C103-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C103-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C103-Pad2)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C103-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C103-Pad2)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C103-Pad1)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C103-Pad2)"))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C103-Pad1)"))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C103-Pad2)"))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C103-Pad1)"))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C103-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x06.wrl
      (at (xyz 0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:NP_Thru_Hole_0.5mm (layer F.Cu) (tedit 59E653AA)
    (at 43.78 143)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value NP_Thru_Hole_0.5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Oddities:FT-23_Core_3_windings_Horiz_TH (layer F.Cu) (tedit 5A9042B9)
    (at 50.23 124.02 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference T501 (at 0.2794 -7.1374 180) (layer F.SilkS))
    (fp_text value "Trifilar #24 / FT-23-43" (at 0.3175 7.3914 180) (layer F.Fab))
    (fp_text user S2 (at -0.4699 1.4224 180) (layer F.SilkS))
    (fp_text user S2' (at -7.6581 2.6543 180) (layer F.SilkS))
    (fp_text user S1 (at -0.6731 -1.1176 180) (layer F.SilkS))
    (fp_text user S1' (at -7.1755 -3.302 180) (layer F.SilkS))
    (fp_text user P (at -1.4478 0.0508 180) (layer F.SilkS))
    (fp_text user P' (at -7.7978 -0.1778 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -6.1849 -0.127 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C101-Pad2)"))
    (pad 2 thru_hole rect (at -2.8702 0.0508 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GNDA) (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
    (pad 3 thru_hole oval (at -5.5753 -2.4511 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(R101-Pad2)"))
    (pad 4 thru_hole oval (at -2.1209 -2.0066 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(T501-Pad4)"))
    (pad 5 thru_hole oval (at -5.9182 2.1463 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(T501-Pad4)"))
    (pad 6 thru_hole oval (at -2.1209 2.1082 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C101-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Oddities:FT-23_Core_2_windings_Horiz_TH (layer B.Cu) (tedit 5A919FB6)
    (at 62.75 123.66 90)
    (descr "Through hole toroid")
    (tags toroid)
    (fp_text reference T101 (at 0.56 0.04 180) (layer B.SilkS))
    (fp_text value "Bifilar #24 / FT-23-43" (at 0.3175 -7.3914 90) (layer B.Fab))
    (fp_text user S1 (at -0.8001 1.2954 90) (layer B.SilkS))
    (fp_text user S1' (at -7.2136 3.1242 90) (layer B.SilkS))
    (fp_text user P (at -1.4224 -0.1778 90) (layer B.SilkS))
    (fp_text user P' (at -7.6327 -0.0254 90) (layer B.SilkS))
    (pad 1 thru_hole rect (at -6.0325 -0.0762 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(R101-Pad2)"))
    (pad 2 thru_hole oval (at -3.0734 -0.2667 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(J105-Pad1)"))
    (pad 3 thru_hole oval (at -5.5372 2.3241 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(J105-Pad1)"))
    (pad 4 thru_hole oval (at -2.4765 1.8161 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 14 PIN_Switch_2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A933BB4)
    (at 57.95 152.4)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference GNDA (at -3.43 -0.8) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GNDA) (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A905B96)
    (at 85.55 160.57)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J104 (at 2.65 0.69) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J104-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A8F7670)
    (at 61.13 140.62)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J105 (at 3.14 0.5) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J105-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5A9336B1)
    (at 79.57 136.85)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P101 (at -1.81 -2.37) (layer F.SilkS))
    (fp_text value "Option 2 Conn." (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(JP103-Pad1)") (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 PIN_Switch_3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A905582)
    (at 65.45 132.28)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C105 (at -0.03 -1.63) (layer F.SilkS))
    (fp_text value 470nF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 PIN_Switch_2))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C105-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-3_Handsolder (layer F.Cu) (tedit 5A905556)
    (at 63.39 136.11)
    (fp_text reference D501 (at 0 2.54) (layer F.SilkS))
    (fp_text value PIN (at 0 -2.286) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.94996 1.19888) (size 0.8 1.00076) (layers F.Cu F.SilkS F.Mask)
      (net 2 "Net-(C504-Pad2)"))
    (pad 2 smd rect (at 0.94996 1.19888) (size 0.8 1.00076) (layers F.Cu F.SilkS F.Mask))
    (pad 3 smd rect (at 0 -1.19888) (size 0.8 1.00076) (layers F.Cu F.SilkS F.Mask)
      (net 15 "Net-(C106-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23-3_Handsolder (layer B.Cu) (tedit 5A905565)
    (at 66.81 135.21 180)
    (fp_text reference D502 (at 0 -2.54 180) (layer B.SilkS))
    (fp_text value PIN (at 0 2.286 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.94996 -1.19888 180) (size 0.8 1.00076) (layers B.Cu B.SilkS B.Mask)
      (net 20 GND))
    (pad 2 smd rect (at 0.94996 -1.19888 180) (size 0.8 1.00076) (layers B.Cu B.SilkS B.Mask))
    (pad 3 smd rect (at 0 1.19888 180) (size 0.8 1.00076) (layers B.Cu B.SilkS B.Mask)
      (net 11 "Net-(C105-Pad2)"))
  )
  (module Buttons_Switches_ThroughHole:NKK_AB11AH-HA_SPDT_MOM (layer F.Cu) (tedit 5A9058D8)
    (at 87.4 156.07 90)
    (descr "tactile switch SPDT right angle, 1825027-2")
    (tags "tactile switch SPDT angled 1825027-2")
    (fp_text reference SW101 (at 2.413 2.5908 90) (layer F.SilkS))
    (fp_text value SPDT (at 1.9685 -2.3495 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 5.08 0 90) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J108-Pad1)") (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
    (pad "" thru_hole circle (at 5.08 5.08 90) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J103-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J104-Pad1)"))
    (pad "" thru_hole circle (at 0 5.08 90) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_Tactile_SPST_Angled.wrl
      (at (xyz 0.09 0.1 0.1575))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 180))
    )
  )
  (module Buttons_Switches_ThroughHole:NKK_AB11AH-HA_SPDT_MOM (layer F.Cu) (tedit 5A905D22)
    (at 57.34 133.97 270)
    (descr "tactile switch SPDT right angle, 1825027-2")
    (tags "tactile switch SPDT angled 1825027-2")
    (fp_text reference SW501 (at 2.413 2.5908 270) (layer F.SilkS))
    (fp_text value Cardioid (at 1.9685 -2.3495 270) (layer F.Fab))
    (pad 3 thru_hole rect (at 5.08 0 270) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 GNDA) (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
    (pad "" thru_hole circle (at 5.08 5.08 270) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 PIN_Switch_2))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 PIN_Switch_1))
    (pad "" thru_hole circle (at 0 5.08 270) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_Tactile_SPST_Angled.wrl
      (at (xyz 0.09 0.1 0.1575))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A932F9B)
    (at 91.48 146.06)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference GNDA (at 2.02 1.96) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J108-Pad1)") (zone_connect 1) (thermal_width 1) (thermal_gap 0.15))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_5mm locked (layer F.Cu) (tedit 5A90BA5E)
    (at 48.84 136)
    (descr "Mounting hole, Befestigungsbohrung, 5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -6.49986) (layer F.SilkS) hide)
    (fp_text value MountingHole_5mm (at 0 7.00024) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm locked (layer F.Cu) (tedit 5A90BA2D)
    (at 97.7 146.85)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Inductors:Bourns_SRR0604_Series_Handsolder (layer F.Cu) (tedit 5A91ABAA)
    (at 69.86 137.02)
    (attr smd)
    (fp_text reference L504 (at 0.0127 0.2159) (layer F.SilkS))
    (fp_text value 150uH (at 0 -2.75) (layer F.Fab))
    (pad 1 smd rect (at -3.5 0) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C504-Pad2)"))
    (pad 2 smd rect (at 3.5 0) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 PIN_Switch_3))
  )
  (module Inductors:Bourns_SRR0604_Series_Handsolder (layer B.Cu) (tedit 5A91ABAA)
    (at 71.75 135.23 90)
    (attr smd)
    (fp_text reference L101 (at 0.0127 -0.2159 90) (layer B.SilkS))
    (fp_text value 150uH (at 0 2.75 90) (layer B.Fab))
    (pad 1 smd rect (at -3.5 0 90) (size 2.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 16 PIN_Switch_3))
    (pad 2 smd rect (at 3.5 0 90) (size 2.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C105-Pad2)"))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A942F61)
    (at 66.8 124.95 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C106 (at -1.16 1.61 270) (layer F.SilkS))
    (fp_text value 470nF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 PIN_Switch_2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C106-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A9336C8)
    (at 80.16 131.06 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C107 (at 0.19 1.75 270) (layer F.SilkS))
    (fp_text value 4700pF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 16 PIN_Switch_3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C107-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A942F40)
    (at 63.48 120.48 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C108 (at 0.11 1.65 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 13 GNDA))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C108-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 5A942FB1)
    (at 61.81 132.87 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C109 (at 0.99 1.6 180) (layer B.SilkS))
    (fp_text value 100pF (at 0 -2.3 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 13 GNDA) (zone_connect 1) (thermal_gap 0.15))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 19 PIN_Switch_1))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer B.Cu) (tedit 5A933605)
    (at 51.82 147.22 180)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (fp_text reference JP101 (at 0.08 1.96 180) (layer B.SilkS))
    (fp_text value Jumper_NO_Small (at 2.54 -3.81 180) (layer B.Fab))
    (pad 1 smd trapezoid (at -1.016 0) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J105-Pad1)"))
    (pad 2 smd trapezoid (at 1.016 0 180) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J106-Pad1)"))
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer B.Cu) (tedit 5A942FD8)
    (at 54.9 135.29 90)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (fp_text reference JP102 (at -3.6 0 90) (layer B.SilkS))
    (fp_text value Jumper_NO_Small (at 2.54 -3.81 90) (layer B.Fab))
    (pad 1 smd trapezoid (at -1.016 0 270) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers B.Cu B.Paste B.Mask)
      (net 14 PIN_Switch_2))
    (pad 2 smd trapezoid (at 1.016 0 90) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers B.Cu B.Paste B.Mask)
      (net 19 PIN_Switch_1))
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer F.Cu) (tedit 5A93367B)
    (at 85.26 138.42)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (fp_text reference JP103 (at -0.04 1.95) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 2.54 3.81) (layer F.Fab))
    (pad 1 smd trapezoid (at -1.016 0 180) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(JP103-Pad1)"))
    (pad 2 smd trapezoid (at 1.016 0) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 13 GNDA))
  )
  (module Wire_Connections_Bridges:Solder-Jumper-NO-SMD-Pad_Small (layer F.Cu) (tedit 5A9336DA)
    (at 85.22 130.62)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point, Square, SMD Pad, 1.5mm x 1.5mm,")
    (fp_text reference JP104 (at 0.05 -2.03) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 2.54 3.81) (layer F.Fab))
    (pad 1 smd trapezoid (at -1.016 0 180) (size 1.50114 1.50114) (rect_delta 0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 16 PIN_Switch_3))
    (pad 2 smd trapezoid (at 1.016 0) (size 1.524 1.524) (rect_delta 0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J106-Pad1)"))
  )
  (module Inductors:Bourns_SRR0604_Series_Handsolder (layer B.Cu) (tedit 5A91ABAA)
    (at 85.38 131.49 270)
    (attr smd)
    (fp_text reference L102 (at 0.0127 -0.2159 270) (layer B.SilkS))
    (fp_text value 150uH (at 0 2.75 270) (layer B.Fab))
    (pad 1 smd rect (at -3.5 0 270) (size 2.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C106-Pad2)"))
    (pad 2 smd rect (at 3.5 0 270) (size 2.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 20 GND))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A942F26)
    (at 59.89 126.3 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference L103 (at -0.04 1.66 270) (layer F.SilkS))
    (fp_text value 390nH (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C108-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 PIN_Switch_1))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Transformers_CHK:CX2045LNL (layer F.Cu) (tedit 5A93369A)
    (at 85.27 134.42 270)
    (descr http://productfinder.pulseeng.com/products/datasheets/CX2045LNL.pdf)
    (solder_mask_margin 0.1)
    (clearance 0.1)
    (fp_text reference T102 (at 0 -2.32 360) (layer F.SilkS))
    (fp_text value "1:2 Balun" (at 0.254 4.191 270) (layer F.Fab))
    (pad 1 smd rect (at 1.27 2 270) (size 0.77 2.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(JP103-Pad1)"))
    (pad 2 smd rect (at 0 2 270) (size 0.77 2.6) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 3 smd rect (at -1.27 2 270) (size 0.77 2.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C107-Pad2)"))
    (pad 5 smd rect (at 1.27 -2 270) (size 0.77 2.6) (layers F.Cu F.Paste F.Mask)
      (net 13 GNDA))
    (pad 4 smd rect (at -1.27 -2 270) (size 0.77 2.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J106-Pad1)"))
  )
  (gr_text Trace (at 71.89 145.16) (layer B.SilkS))
  (gr_text Trace (at 72.01 145.16) (layer F.SilkS))
  (gr_text Traces (at 55.86 145.19) (layer F.SilkS))
  (gr_text Traces (at 55.94 145.41) (layer B.SilkS))
  (gr_text J109 (at 82.52 136.86) (layer F.SilkS))
  (gr_text J107 (at 82.53 139.48) (layer F.SilkS))
  (gr_text "80m ARDF Antenna\nVersion X2 - Feb 2018\nThanks to W7PUA" (at 61.43 66.32) (layer B.SilkS))
  (gr_line (start 43.2 38.3) (end 43.2 163.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.4 38.3) (end 43.2 38.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.4 163.8) (end 101.4 38.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 43.2 163.8) (end 101.4 163.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name "Net-(C103-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69.6 113.55) (xy 69.6 128.75) (xy 72.12 128.75) (xy 72.12 110.64) (xy 69.6 110.64)
        (xy 69.6 113.58)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C103-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.71 128.8) (xy 72.36 128.8) (xy 72.36 110.66) (xy 74.71 110.66)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C103-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.71 128.8) (xy 72.36 128.8) (xy 72.36 110.66) (xy 74.71 110.66)
      )
    )
  )
  (zone (net 5) (net_name "Net-(C103-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69.6 113.55) (xy 69.6 128.75) (xy 72.12 128.75) (xy 72.12 110.64) (xy 69.6 110.64)
        (xy 69.6 113.58)
      )
    )
  )
  (zone (net 13) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.32 117.82) (xy 43.39 117.82) (xy 43.39 142.52) (xy 101.21 142.52) (xy 101.21 117.79)
        (xy 75.35 117.79) (xy 75.35 129.65) (xy 69.05 129.65) (xy 69.05 117.82) (xy 62.31 117.82)
      )
    )
  )
  (zone (net 13) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.32 117.82) (xy 43.39 117.82) (xy 43.39 142.52) (xy 101.21 142.52) (xy 101.21 117.79)
        (xy 75.35 117.79) (xy 75.35 129.65) (xy 69.05 129.65) (xy 69.05 117.82) (xy 62.31 117.82)
      )
    )
  )
  (zone (net 13) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43.47 143.79) (xy 43.47 163.53) (xy 59.74 163.53) (xy 59.74 143.71) (xy 43.47 143.71)
        (xy 43.47 143.8)
      )
    )
  )
  (zone (net 13) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43.47 143.79) (xy 43.47 163.53) (xy 59.74 163.53) (xy 59.74 143.71) (xy 43.47 143.71)
        (xy 43.47 143.8)
      )
    )
  )
  (zone (net 22) (net_name "Net-(JP103-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.91 143.78) (xy 60.91 163.5) (xy 82.36 163.5) (xy 82.36 143.62) (xy 60.91 143.62)
      )
    )
  )
  (zone (net 22) (net_name "Net-(JP103-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.91 143.78) (xy 60.91 163.5) (xy 82.36 163.5) (xy 82.36 143.62) (xy 60.91 143.62)
      )
    )
  )
  (zone (net 12) (net_name "Net-(J108-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.41 143.68) (xy 83.41 143.66) (xy 101.11 143.66) (xy 101.11 163.5) (xy 83.41 163.5)
        (xy 83.41 143.7) (xy 83.4 143.7)
      )
    )
  )
  (zone (net 12) (net_name "Net-(J108-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.41 143.68) (xy 83.41 143.66) (xy 101.11 143.66) (xy 101.11 163.5) (xy 83.41 163.5)
        (xy 83.41 143.7) (xy 83.4 143.7)
      )
    )
  )
)
