(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 59)
    (zones 0)
    (modules 3)
    (nets 22)
  )
  (page A4)
  (title_block
    (title Dediprog_2_UP)
    (date 2020-08-23)
    (rev v01)
    (comment 2 creativecommons.org/licenses/by/4.0)
    (comment 3 "License: CC BY 4.0")
    (comment 4 "Author: David Hendricks")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.381)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/sc/src/up_dediprog_adapter/dediprog2up_v2/gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /CLK)
  (net 3 /MISO)
  (net 4 /MOSI)
  (net 5 "Net-(GND1-Pad1)")
  (net 6 "Net-(J2-Pad1)")
  (net 7 "Net-(J2-Pad2)")
  (net 8 "Net-(J2-Pad11)")
  (net 9 "Net-(J2-Pad12)")
  (net 10 "Net-(J2-Pad13)")
  (net 11 "Net-(J2-Pad14)")
  (net 12 "Net-(J2-Pad15)")
  (net 13 "Net-(J2-Pad16)")
  (net 14 "Net-(J2-Pad17)")
  (net 15 "Net-(J2-Pad18)")
  (net 16 "Net-(J2-Pad19)")
  (net 17 "Net-(J2-Pad20)")
  (net 18 /VCC)
  (net 19 /#HOLD)
  (net 20 "Net-(J2-Pad7)")
  (net 21 /CS#)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net /#HOLD)
    (add_net /CLK)
    (add_net /CS#)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /VCC)
    (add_net GND)
    (add_net "Net-(GND1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad7)")
  )
  (net_class Narrow ""
    (clearance 0.254)
    (trace_width 0.1524)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 134.62 88.5444)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference J2 (at -2.256801 -1.494801) (layer F.SilkS))
    (fp_text value Conn_02x10_Odd_Even (at 1.27 25.19) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /CS#))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /VCC))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /MISO))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /#HOLD))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /CLK))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /MOSI))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad20)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x06_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 145.8976 97.9932 180)
    (descr "Through hole straight pin header, 2x06, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 1.27mm double row")
    (fp_text reference J1 (at -1.016 -1.4986) (layer F.SilkS))
    (fp_text value Conn_02x6_Odd_Even (at 0.635 8.045) (layer F.Fab))
    (fp_text user %R (at 0.635 3.175 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "Net-(GND1-Pad1)"))
    (pad 3 thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 1.27 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 /VCC))
    (pad 5 thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 /VCC))
    (pad 6 thru_hole oval (at 1.27 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 /CS#))
    (pad 7 thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /CLK))
    (pad 8 thru_hole oval (at 1.27 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 /MISO))
    (pad 9 thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 /VCC))
    (pad 10 thru_hole oval (at 1.27 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 0 6.35 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 /MOSI))
    (pad 12 thru_hole oval (at 1.27 6.35 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 19 /#HOLD))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x06_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module NetTie:NetTie-2_SMD_Pad0.5mm (layer B.Cu) (tedit 5A1CF6D3)
    (at 145.1864 99.8474)
    (descr "Net tie, 2 pin, 0.5mm square SMD pads")
    (tags "net tie")
    (attr virtual)
    (fp_text reference GND1 (at -1.524 0.0254) (layer B.SilkS))
    (fp_text value Net-Tie_2 (at 0.0254 0.762) (layer B.Fab))
    (pad 1 smd circle (at -0.5 0) (size 0.5 0.5) (layers B.Cu)
      (net 5 "Net-(GND1-Pad1)"))
    (pad 2 smd circle (at 0.5 0) (size 0.5 0.5) (layers B.Cu)
      (net 1 GND))
  )
  (gr_text V03 (at 147.3454 113.2332) (layer F.SilkS))
  (gr_text "NC   NC\nCS1  Vcc\nMISO /HOLD\nNC   CLK\nGND  MOSI\nNC   NC\nNC   NC\nNC   NC\nNC   NC\nNC   NC" (at 140.1572 108.712) (layer F.SilkS))
  (gr_text "/HOLD  MOSI\nGND VCC\nMISO  CLK\n/CS  NC\nVCC  GND\nGND  GND\n" (at 143.7386 87.8586) (layer F.SilkS))
  (gr_line (start 130.7846 115.4938) (end 130.7846 85.0646) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 150.7236 115.4938) (end 130.7846 115.4938) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 150.7236 85.0646) (end 150.7236 115.4938) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 130.7846 85.0646) (end 150.7236 85.0646) (layer Edge.Cuts) (width 0.0254))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.8887 115.9637) (xy 130.556 115.824) (xy 130.556 84.836) (xy 150.8633 84.9503)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.13 115.7986) (xy 130.556 115.824) (xy 130.556 84.836) (xy 151.13 84.8106)
      )
    )
  )
)
