(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 5)
    (zones 0)
    (modules 2)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 2.2)
    (pad_drill 1.6)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01000_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294E91)
    (at 118.5 60.01 270)
    (descr "Terminal Block 4Ucon ItemNo. 19963, 2 pins, pitch 3.5mm, size 7.7x7mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see http://www.4uconnector.com/online/object/4udrawing/19963.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 19963 pitch 3.5mm size 7.7x7mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J1 (at 1.75 -4.46 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.75 4.66 90) (layer F.Fab))
    (fp_text user %R (at 1.75 2.9 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5FD53FCD)
    (at 125.45 58.96)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 5.08) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 122.3 58.175) (end 124 57.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.9 58.175) (end 122.3 58.175) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.9 65.425) (end 114.9 58.175) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.3 65.425) (end 114.9 65.425) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.3 57.5) (end 127.3 65.425) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124 57.5) (end 127.3 57.5) (layer Edge.Cuts) (width 0.05))
)
