(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 238)
    (zones 0)
    (modules 40)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu power)
    (31 B.Cu power)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad1)")
  (net 2 "Net-(A1-Pad17)")
  (net 3 "Net-(A1-Pad2)")
  (net 4 "Net-(A1-Pad28)")
  (net 5 /ProbeA0/A0)
  (net 6 /ProbeA0/A1)
  (net 7 "Net-(A1-Pad5)")
  (net 8 /ProbeA2/A2)
  (net 9 "Net-(A1-Pad6)")
  (net 10 /ProbeA2/A3)
  (net 11 "Net-(A1-Pad7)")
  (net 12 /SDA)
  (net 13 "Net-(A1-Pad8)")
  (net 14 /SCL)
  (net 15 "Net-(A1-Pad9)")
  (net 16 /ProbeA4/A4)
  (net 17 "Net-(A1-Pad10)")
  (net 18 /ProbeA4/A5)
  (net 19 "Net-(A1-Pad11)")
  (net 20 "Net-(A1-Pad12)")
  (net 21 "Net-(A1-Pad13)")
  (net 22 "Net-(A1-Pad14)")
  (net 23 "Net-(A1-Pad15)")
  (net 24 "Net-(A1-Pad16)")
  (net 25 "Net-(D1-Pad1)")
  (net 26 "Net-(D2-Pad1)")
  (net 27 GND)
  (net 28 "Net-(J3-Pad1)")
  (net 29 "Net-(J4-Pad1)")
  (net 30 "Net-(J5-Pad1)")
  (net 31 "Net-(J7-Pad1)")
  (net 32 "Net-(J9-Pad1)")
  (net 33 "Net-(J10-Pad1)")
  (net 34 VDD)
  (net 35 /ProbeA0/Q1_5)
  (net 36 /ProbeA0/Q1_2)
  (net 37 /ProbeA4/Q2_2)
  (net 38 /ProbeA4/Q2_3)
  (net 39 /ProbeA2/Q3_5)
  (net 40 /ProbeA2/Q3_2)
  (net 41 "Net-(A1-Pad30)")
  (net 42 "Net-(J1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ProbeA0/A0)
    (add_net /ProbeA0/A1)
    (add_net /ProbeA0/Q1_2)
    (add_net /ProbeA0/Q1_5)
    (add_net /ProbeA2/A2)
    (add_net /ProbeA2/A3)
    (add_net /ProbeA2/Q3_2)
    (add_net /ProbeA2/Q3_5)
    (add_net /ProbeA4/A4)
    (add_net /ProbeA4/A5)
    (add_net /ProbeA4/Q2_2)
    (add_net /ProbeA4/Q2_3)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad30)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net VDD)
  )
  (module Diode_SMD:D_0805_2012Metric (layer F.Cu) (tedit 5F68FEF0)
    (at 120.65 80.01)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value DataReceive (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 VDD))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric (layer F.Cu) (tedit 5F68FEF0)
    (at 97.155 80.01)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value DataTransmit (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 VDD))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Graphics:farfetchd_small (layer B.Cu) (tedit 0)
    (at 118.3 86.9 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module Graphics:ferfetched_smalller (layer F.Cu) (tedit 0)
    (at 102.87 149.86)
    (fp_text reference G*** (at 0 0) (layer Dwgs.User) hide)
    (fp_text value LOGO (at 0.75 0) (layer Dwgs.User) hide)
  )
  (module MountingHole:MountingHole_2mm (layer F.Cu) (tedit 5B924920)
    (at 121.92 151.13)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2mm (layer F.Cu) (tedit 5B924920)
    (at 97.79 73.66)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2mm (layer F.Cu) (tedit 5B924920)
    (at 97.79 151.13)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2mm (layer F.Cu) (tedit 5B924920)
    (at 121.92 73.66)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module Leak_Components:SM04B-SRSS-TB_LFSN_ (layer F.Cu) (tedit 0)
    (at 113.03 72.39 180)
    (descr "SM04B-SRSS-TB(LFSN)")
    (tags Connector)
    (attr smd)
    (fp_text reference J1 (at 2.822 -1.556) (layer F.SilkS))
    (fp_text value SM04B-SRSS-TB_LF__SN_ (at 2.822 -1.556) (layer F.SilkS) hide)
    (fp_text user %R (at 2.822 -1.556) (layer F.Fab))
    (pad 6 smd rect (at 5.8 -0.786 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0.2 -0.786 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 4.5 -4.661 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /SCL))
    (pad 3 smd rect (at 3.5 -4.661 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /SDA))
    (pad 2 smd rect (at 2.5 -4.661 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at 1.5 -4.661 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 27 GND))
    (model SM04B-SRSS-TB_LF__SN_.stp
      (offset (xyz 2.999999954944458 4.179999765561417 -0.2899999872999835))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Module:Arduino_Nano (layer F.Cu) (tedit 58ACAF70)
    (at 122 132 180)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (fp_text reference A1 (at 2.6 -0.2) (layer F.SilkS))
    (fp_text value Arduino_Nano_v2.x (at 8.89 19.05 90) (layer F.Fab))
    (fp_text user %R (at 6.35 19.05 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 17 thru_hole oval (at 15.24 33.02 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad17)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad2)"))
    (pad 18 thru_hole oval (at 15.24 30.48 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 34 VDD))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad28)"))
    (pad 19 thru_hole oval (at 15.24 27.94 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 /ProbeA0/A0))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 GND))
    (pad 20 thru_hole oval (at 15.24 25.4 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 /ProbeA0/A1))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad5)"))
    (pad 21 thru_hole oval (at 15.24 22.86 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 /ProbeA2/A2))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad6)"))
    (pad 22 thru_hole oval (at 15.24 20.32 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 /ProbeA2/A3))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad7)"))
    (pad 23 thru_hole oval (at 15.24 17.78 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SDA))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad8)"))
    (pad 24 thru_hole oval (at 15.24 15.24 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 /SCL))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad9)"))
    (pad 25 thru_hole oval (at 15.24 12.7 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 /ProbeA4/A4))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad10)"))
    (pad 26 thru_hole oval (at 15.24 10.16 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 /ProbeA4/A5))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad11)"))
    (pad 27 thru_hole oval (at 15.24 7.62 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 34 VDD))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad12)"))
    (pad 28 thru_hole oval (at 15.24 5.08 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad28)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad13)"))
    (pad 29 thru_hole oval (at 15.24 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 GND))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad14)"))
    (pad 30 thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(A1-Pad30)"))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad15)"))
    (pad 16 thru_hole oval (at 15.24 35.56 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad16)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal (layer F.Cu) (tedit 5B783024)
    (at 100 103.1 270)
    (descr "Molex PicoBlade Connector System, 53048-0210, 2 Pins per row (http://www.molex.com/pdm_docs/sd/530480210_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade top entry")
    (fp_text reference J3 (at 0.62 -1.95 90) (layer F.SilkS))
    (fp_text value 53047-0210 (at 0.62 5.65 90) (layer F.Fab))
    (fp_text user %R (at 0.62 3.75 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.25 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 27 GND))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal (layer F.Cu) (tedit 5B783024)
    (at 100.1 90.4 270)
    (descr "Molex PicoBlade Connector System, 53048-0210, 2 Pins per row (http://www.molex.com/pdm_docs/sd/530480210_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade top entry")
    (fp_text reference J4 (at 0.62 -1.95 90) (layer F.SilkS))
    (fp_text value 53047-0210 (at 0.62 5.65 90) (layer F.Fab))
    (fp_text user %R (at 0.62 3.75 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.25 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 27 GND))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal (layer F.Cu) (tedit 5B783024)
    (at 101.9 141.3)
    (descr "Molex PicoBlade Connector System, 53048-0210, 2 Pins per row (http://www.molex.com/pdm_docs/sd/530480210_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade top entry")
    (fp_text reference J5 (at 0.62 -1.95) (layer F.SilkS))
    (fp_text value 53047-0210 (at 0.62 5.65) (layer F.Fab))
    (fp_text user %R (at 0.62 3.75) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 1.25 0) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 27 GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal (layer F.Cu) (tedit 5B783024)
    (at 119.6 140.9)
    (descr "Molex PicoBlade Connector System, 53048-0210, 2 Pins per row (http://www.molex.com/pdm_docs/sd/530480210_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade top entry")
    (fp_text reference J7 (at 0.62 -1.95) (layer F.SilkS))
    (fp_text value 53047-0210 (at 0.62 5.65) (layer F.Fab))
    (fp_text user %R (at 0.62 3.75) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.25 0) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 27 GND))
    (pad 1 thru_hole roundrect (at 0 0) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal (layer F.Cu) (tedit 5B783024)
    (at 100.8 129 270)
    (descr "Molex PicoBlade Connector System, 53048-0210, 2 Pins per row (http://www.molex.com/pdm_docs/sd/530480210_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade top entry")
    (fp_text reference J9 (at 0.62 -1.95 90) (layer F.SilkS))
    (fp_text value 53047-0210 (at 0.62 5.65 90) (layer F.Fab))
    (fp_text user %R (at 0.62 3.75 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(J9-Pad1)"))
    (pad 2 thru_hole oval (at 1.25 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 27 GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal (layer F.Cu) (tedit 5B783024)
    (at 100.524999 115.025001 270)
    (descr "Molex PicoBlade Connector System, 53048-0210, 2 Pins per row (http://www.molex.com/pdm_docs/sd/530480210_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade top entry")
    (fp_text reference J10 (at 0.62 -1.95 90) (layer F.SilkS))
    (fp_text value 53047-0210 (at 0.62 5.65 90) (layer F.Fab))
    (fp_text user %R (at 0.62 3.75 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(J10-Pad1)"))
    (pad 2 thru_hole oval (at 1.25 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 27 GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_PicoBlade_53048-0210_1x02_P1.25mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 5A02FF57)
    (at 100.3 98.8 180)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference Q1 (at 0 -2) (layer F.SilkS))
    (fp_text value Q_DUAL_PNP_PNP_E1B1C2E2B2C1 (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 VDD))
    (pad 3 smd rect (at -0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /ProbeA0/A1))
    (pad 5 smd rect (at 0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 /ProbeA0/Q1_5))
    (pad 2 smd rect (at -0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 /ProbeA0/Q1_2))
    (pad 4 smd rect (at 0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 VDD))
    (pad 6 smd rect (at 0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /ProbeA0/A0))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 5A02FF57)
    (at 111.5 144)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference Q2 (at 0 -2) (layer F.SilkS))
    (fp_text value Q_DUAL_PNP_PNP_E1B1C2E2B2C1 (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 6 smd rect (at 0.95 -0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 /ProbeA4/A4))
    (pad 4 smd rect (at 0.95 0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 VDD))
    (pad 2 smd rect (at -0.95 0) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 /ProbeA4/Q2_2))
    (pad 5 smd rect (at 0.95 0) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 /ProbeA4/Q2_3))
    (pad 3 smd rect (at -0.95 0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 /ProbeA4/A5))
    (pad 1 smd rect (at -0.95 -0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 VDD))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 5A02FF57)
    (at 97.8 124 180)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference Q3 (at 0 -2) (layer F.SilkS))
    (fp_text value Q_DUAL_PNP_PNP_E1B1C2E2B2C1 (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 VDD))
    (pad 3 smd rect (at -0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /ProbeA2/A3))
    (pad 5 smd rect (at 0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 /ProbeA2/Q3_5))
    (pad 2 smd rect (at -0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 /ProbeA2/Q3_2))
    (pad 4 smd rect (at 0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 VDD))
    (pad 6 smd rect (at 0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /ProbeA2/A2))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 97.3 83.4)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 350 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 25 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 7 "Net-(A1-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 120.8 84.1)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 350 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 9 "Net-(A1-Pad6)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 26 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 102.4 137)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 27k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 34 VDD))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 4 "Net-(A1-Pad28)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 99 95.2)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 28 "Net-(J3-Pad1)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 36 /ProbeA0/Q1_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 97.3 87 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 35 /ProbeA0/Q1_5))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 29 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 101.9 87)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 27K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 36 /ProbeA0/Q1_2))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 34 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 96 98.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 27K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 35 /ProbeA0/Q1_5))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 34 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 103.2 105.5875 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 27 GND))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 5 /ProbeA0/A0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 103.2 110.9 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 6 /ProbeA0/A1))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 27 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 96.8 140.5875 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 30 "Net-(J5-Pad1)"))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 37 /ProbeA4/Q2_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 114.8 138.7)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 31 "Net-(J7-Pad1)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 38 /ProbeA4/Q2_3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 96.8 145.7 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 27K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 37 /ProbeA4/Q2_2))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 34 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 108.3 138.8 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 27K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 34 VDD))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 38 /ProbeA4/Q2_3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 107.6 144 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 16 /ProbeA4/A4))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 27 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 115.7 143.9 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 18 /ProbeA4/A5))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 27 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 97.8875 134.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 40 /ProbeA2/Q3_2))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 32 "Net-(J9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 98.0875 108.3)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 33 "Net-(J10-Pad1)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 39 /ProbeA2/Q3_5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 97.7 120.4)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 27K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 40 /ProbeA2/Q3_2))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 34 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 98.0875 111.3)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 27K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 34 VDD))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 39 /ProbeA2/Q3_5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 102.2875 124.1)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 27 GND))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 8 /ProbeA2/A2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 102.2 120.4)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 10 /ProbeA2/A3))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 27 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 125.73 71.12) (end 127 153.67) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.98 71.12) (end 125.73 71.12) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.98 153.67) (end 93.98 71.12) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127 153.67) (end 93.98 153.67) (layer Edge.Cuts) (width 0.1))
  (gr_text "Trent Moca\nLeak Detection\nScion 2022" (at 106.68 149.86) (layer F.SilkS))
  (dimension 12.6 (width 0.15) (layer Dwgs.User)
    (gr_text "12.600 mm" (at 135.8 142.3 270) (layer Dwgs.User))
    (feature1 (pts (xy 117.5 148.6) (xy 135.086421 148.6)))
    (feature2 (pts (xy 117.5 136) (xy 135.086421 136)))
    (crossbar (pts (xy 134.5 136) (xy 134.5 148.6)))
    (arrow1a (pts (xy 134.5 148.6) (xy 133.913579 147.473496)))
    (arrow1b (pts (xy 134.5 148.6) (xy 135.086421 147.473496)))
    (arrow2a (pts (xy 134.5 136) (xy 133.913579 137.126504)))
    (arrow2b (pts (xy 134.5 136) (xy 135.086421 137.126504)))
  )
  (gr_text "Trent Moca\nLeak Detection Board\nScion 2022" (at 113.2 84.1) (layer B.SilkS))
  (gr_text USB (at 114.7 97.2) (layer Dwgs.User))
  (dimension 15.420081 (width 0.15) (layer Dwgs.User)
    (gr_text "15.420 mm" (at 111.330198 73.677718 359.8142167) (layer Dwgs.User))
    (feature1 (pts (xy 119 86.1) (xy 119.037885 74.416294)))
    (feature2 (pts (xy 103.58 86.05) (xy 103.617885 74.366294)))
    (crossbar (pts (xy 103.615983 74.952711) (xy 119.035983 75.002711)))
    (arrow1a (pts (xy 119.035983 75.002711) (xy 117.907584 75.585476)))
    (arrow1b (pts (xy 119.035983 75.002711) (xy 117.911387 74.412641)))
    (arrow2a (pts (xy 103.615983 74.952711) (xy 104.740579 75.542781)))
    (arrow2b (pts (xy 103.615983 74.952711) (xy 104.744382 74.369946)))
  )
  (dimension 12.6 (width 0.15) (layer Dwgs.User)
    (gr_text "12.600 mm" (at 117.5 83.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 114.5 89.8) (xy 116.786421 89.8)))
    (feature2 (pts (xy 114.5 77.2) (xy 116.786421 77.2)))
    (crossbar (pts (xy 116.2 77.2) (xy 116.2 89.8)))
    (arrow1a (pts (xy 116.2 89.8) (xy 115.613579 88.673496)))
    (arrow1b (pts (xy 116.2 89.8) (xy 116.786421 88.673496)))
    (arrow2a (pts (xy 116.2 77.2) (xy 115.613579 78.326504)))
    (arrow2b (pts (xy 116.2 77.2) (xy 116.786421 78.326504)))
  )
  (dimension 7.5 (width 0.15) (layer Dwgs.User)
    (gr_text "7.500 mm" (at 86.3 97.35 90) (layer Dwgs.User))
    (feature1 (pts (xy 98.4 93.6) (xy 87.013579 93.6)))
    (feature2 (pts (xy 98.4 101.1) (xy 87.013579 101.1)))
    (crossbar (pts (xy 87.6 101.1) (xy 87.6 93.6)))
    (arrow1a (pts (xy 87.6 93.6) (xy 88.186421 94.726504)))
    (arrow1b (pts (xy 87.6 93.6) (xy 87.013579 94.726504)))
    (arrow2a (pts (xy 87.6 101.1) (xy 88.186421 99.973496)))
    (arrow2b (pts (xy 87.6 101.1) (xy 87.013579 99.973496)))
  )
  (dimension 6.7 (width 0.15) (layer Dwgs.User)
    (gr_text "6.700 mm" (at 86.3 109.65 90) (layer Dwgs.User))
    (feature1 (pts (xy 99.5 106.3) (xy 87.013579 106.3)))
    (feature2 (pts (xy 99.5 113) (xy 87.013579 113)))
    (crossbar (pts (xy 87.6 113) (xy 87.6 106.3)))
    (arrow1a (pts (xy 87.6 106.3) (xy 88.186421 107.426504)))
    (arrow1b (pts (xy 87.6 106.3) (xy 87.013579 107.426504)))
    (arrow2a (pts (xy 87.6 113) (xy 88.186421 111.873496)))
    (arrow2b (pts (xy 87.6 113) (xy 87.013579 111.873496)))
  )
  (dimension 8.7 (width 0.15) (layer Dwgs.User)
    (gr_text "8.700 mm" (at 87.2 122.65 90) (layer Dwgs.User))
    (feature1 (pts (xy 99.8 118.3) (xy 87.913579 118.3)))
    (feature2 (pts (xy 99.8 127) (xy 87.913579 127)))
    (crossbar (pts (xy 88.5 127) (xy 88.5 118.3)))
    (arrow1a (pts (xy 88.5 118.3) (xy 89.086421 119.426504)))
    (arrow1b (pts (xy 88.5 118.3) (xy 87.913579 119.426504)))
    (arrow2a (pts (xy 88.5 127) (xy 89.086421 125.873496)))
    (arrow2b (pts (xy 88.5 127) (xy 87.913579 125.873496)))
  )
  (dimension 7.45 (width 0.15) (layer Dwgs.User)
    (gr_text "7.450 mm" (at 87.4 136.025 90) (layer Dwgs.User))
    (feature1 (pts (xy 99.9 132.3) (xy 88.113579 132.3)))
    (feature2 (pts (xy 99.9 139.75) (xy 88.113579 139.75)))
    (crossbar (pts (xy 88.7 139.75) (xy 88.7 132.3)))
    (arrow1a (pts (xy 88.7 132.3) (xy 89.286421 133.426504)))
    (arrow1b (pts (xy 88.7 132.3) (xy 88.113579 133.426504)))
    (arrow2a (pts (xy 88.7 139.75) (xy 89.286421 138.623496)))
    (arrow2b (pts (xy 88.7 139.75) (xy 88.113579 138.623496)))
  )
  (dimension 12.300102 (width 0.15) (layer Dwgs.User)
    (gr_text "12.300 mm" (at 111.481701 153.673255 0.2329083899) (layer Dwgs.User))
    (feature1 (pts (xy 105.3 145.9) (xy 105.3288 152.984682)))
    (feature2 (pts (xy 117.6 145.85) (xy 117.6288 152.934682)))
    (crossbar (pts (xy 117.626416 152.348266) (xy 105.326416 152.398266)))
    (arrow1a (pts (xy 105.326416 152.398266) (xy 106.450527 151.807271)))
    (arrow1b (pts (xy 105.326416 152.398266) (xy 106.455294 152.980103)))
    (arrow2a (pts (xy 117.626416 152.348266) (xy 116.497538 151.766429)))
    (arrow2b (pts (xy 117.626416 152.348266) (xy 116.502305 152.939261)))
  )
  (dimension 71.5 (width 0.15) (layer Dwgs.User)
    (gr_text "71.500 mm" (at 150 112.95 90) (layer Dwgs.User))
    (feature1 (pts (xy 125.7 77.2) (xy 149.286421 77.2)))
    (feature2 (pts (xy 125.7 148.7) (xy 149.286421 148.7)))
    (crossbar (pts (xy 148.7 148.7) (xy 148.7 77.2)))
    (arrow1a (pts (xy 148.7 77.2) (xy 149.286421 78.326504)))
    (arrow1b (pts (xy 148.7 77.2) (xy 148.113579 78.326504)))
    (arrow2a (pts (xy 148.7 148.7) (xy 149.286421 147.573496)))
    (arrow2b (pts (xy 148.7 148.7) (xy 148.113579 147.573496)))
  )
  (dimension 32.5 (width 0.15) (layer Dwgs.User)
    (gr_text "32.500 mm" (at 109.35 166.4) (layer Dwgs.User))
    (feature1 (pts (xy 125.6 148.9) (xy 125.6 165.686421)))
    (feature2 (pts (xy 93.1 148.9) (xy 93.1 165.686421)))
    (crossbar (pts (xy 93.1 165.1) (xy 125.6 165.1)))
    (arrow1a (pts (xy 125.6 165.1) (xy 124.473496 165.686421)))
    (arrow1b (pts (xy 125.6 165.1) (xy 124.473496 164.513579)))
    (arrow2a (pts (xy 93.1 165.1) (xy 94.226504 165.686421)))
    (arrow2b (pts (xy 93.1 165.1) (xy 94.226504 164.513579)))
  )
  (zone (net 27) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127 153.67) (xy 93.98 153.67) (xy 93.98 71.12) (xy 125.73 71.12)
      )
    )
  )
  (zone (net 27) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127 153.67) (xy 93.98 153.67) (xy 93.98 71.12) (xy 125.73 71.12)
      )
    )
  )
)
