(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 2)
    (zones 0)
    (modules 4)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.3)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 150 100)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./Gerber"))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 "Net-(BT1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(BT1-Pad2)")
  )
  (module Karrots-library:@karrots (layer F.Cu) (tedit 5D5225F8)
    (at 143.25 108.1)
    (descr "@karrots signature")
    (tags "@karrots signature")
    (attr virtual)
    (fp_text reference Ref** (at 0 0) (layer F.SilkS) hide)
    (fp_text value @karrots (at 0 0) (layer F.SilkS) hide)
  )
  (module TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded (layer F.Cu) (tedit 5A0F774F)
    (at 129.3 112.85)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (fp_text reference TP1 (at 1.1 2.3) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 1 -2.1) (layer F.Fab))
    (fp_text user %R (at 1.1 2.3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded (layer F.Cu) (tedit 5A0F774F)
    (at 159.45 112.85)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (fp_text reference TP2 (at 1.1 2.3) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 1 -2.1) (layer F.Fab))
    (fp_text user %R (at 1.1 2.3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Karrots-library:JKK_CR2032 (layer F.Cu) (tedit 5F0544BA)
    (at 146.45 112.9)
    (fp_text reference BT1 (at 0 1.4) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 -11.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (fp_text user - (at 7.874 -1.524) (layer F.SilkS))
    (fp_text user + (at -14.35 -1.15) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.808 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad2)"))
    (pad 1 thru_hole circle (at -12.192 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
  )
  (gr_arc (start 130.3 120.5) (end 129.3 120.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 130.3 105.5) (end 130.3 104.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.049999 110.100001) (end 159.3 110.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.060681 115.566304) (end 159.3 115.55) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 146.45 113) (end 153.299999 121.499999) (angle -37.53879023) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 146.4 112.85) (end 157.049999 110.100001) (angle -34.8) (layer Edge.Cuts) (width 0.15))
  (gr_text "@Karrots\nCR2032-1/2AA Adapter\nV2" (at 142.3 117.6) (layer B.SilkS))
  (gr_line (start 130.3 121.5) (end 153.299999 121.499999) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.3 105.5) (end 129.3 120.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.575777 104.513742) (end 130.3 104.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.3 115.55) (end 159.3 110.1) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.4 123.55) (xy 126.4 122.55) (xy 127.3 102.95) (xy 127.8 102.95) (xy 162.6 101.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.2 124.25) (xy 126.25 123.4) (xy 126.45 122.95) (xy 127.35 102.7) (xy 130.05 102.75)
        (xy 163.25 102.2)
      )
    )
  )
)
