(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 144)
    (no_connects 0)
    (area 86.259999 41.809999 204.570001 132.180001)
    (thickness 1.6)
    (drawings 4)
    (tracks 629)
    (zones 0)
    (modules 46)
    (nets 72)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.8 0.8)
    (pad_drill 0.4)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 +3V3)
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D3-Pad1)")
  (net 5 "Net-(D4-Pad1)")
  (net 6 "Net-(D5-Pad1)")
  (net 7 "Net-(D6-Pad1)")
  (net 8 "Net-(D7-Pad1)")
  (net 9 "Net-(D8-Pad1)")
  (net 10 "Net-(D9-Pad1)")
  (net 11 "Net-(D10-Pad1)")
  (net 12 "Net-(D11-Pad1)")
  (net 13 "Net-(D12-Pad1)")
  (net 14 GND)
  (net 15 /3V)
  (net 16 /P3.7)
  (net 17 /P3.6)
  (net 18 /P3.5)
  (net 19 /P3.4)
  (net 20 /P3.3)
  (net 21 /P3.2)
  (net 22 /P3.1)
  (net 23 /P3.0)
  (net 24 /P5.5)
  (net 25 /P5.6)
  (net 26 /P5.7)
  (net 27 "Net-(DS1-Pad3)")
  (net 28 /P1.0)
  (net 29 /P1.1)
  (net 30 /P1.2)
  (net 31 /P1.3)
  (net 32 /P1.4)
  (net 33 /P1.5)
  (net 34 /P1.6)
  (net 35 /P1.7)
  (net 36 /P2.0)
  (net 37 /P2.1)
  (net 38 /P2.2)
  (net 39 /P2.3)
  (net 40 /P2.4)
  (net 41 /P2.5)
  (net 42 /P2.6)
  (net 43 /P2.7)
  (net 44 /SN74_C)
  (net 45 /SN74_D)
  (net 46 /SN74_E)
  (net 47 /SN74_F)
  (net 48 "Net-(J5-Pad5)")
  (net 49 /P8.0)
  (net 50 /P8.1)
  (net 51 /P8.2)
  (net 52 /P8.3)
  (net 53 "Net-(J8-Pad7)")
  (net 54 "Net-(R1-Pad2)")
  (net 55 "Net-(R2-Pad2)")
  (net 56 "Net-(R3-Pad2)")
  (net 57 "Net-(R4-Pad2)")
  (net 58 "Net-(R5-Pad2)")
  (net 59 "Net-(R6-Pad2)")
  (net 60 "Net-(R7-Pad2)")
  (net 61 "Net-(R8-Pad2)")
  (net 62 "Net-(R9-Pad2)")
  (net 63 "Net-(R10-Pad2)")
  (net 64 "Net-(R11-Pad2)")
  (net 65 "Net-(R12-Pad2)")
  (net 66 /24d_enc_GND)
  (net 67 /12d_enc_GND)
  (net 68 "Net-(SW13-Pad1)")
  (net 69 "Net-(SW13-Pad2)")
  (net 70 "Net-(SW13-Pad7)")
  (net 71 "Net-(SW13-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /P1.0)
    (add_net /P1.1)
    (add_net /P1.2)
    (add_net /P1.3)
    (add_net /P1.4)
    (add_net /P1.5)
    (add_net /P1.6)
    (add_net /P1.7)
    (add_net /P2.0)
    (add_net /P2.1)
    (add_net /P2.2)
    (add_net /P2.3)
    (add_net /P2.4)
    (add_net /P2.5)
    (add_net /P2.6)
    (add_net /P2.7)
    (add_net /P3.0)
    (add_net /P3.1)
    (add_net /P3.2)
    (add_net /P3.3)
    (add_net /P3.4)
    (add_net /P3.5)
    (add_net /P3.6)
    (add_net /P3.7)
    (add_net /P5.5)
    (add_net /P5.6)
    (add_net /P5.7)
    (add_net /P8.0)
    (add_net /P8.1)
    (add_net /P8.2)
    (add_net /P8.3)
    (add_net /SN74_C)
    (add_net /SN74_D)
    (add_net /SN74_E)
    (add_net /SN74_F)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(DS1-Pad3)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J8-Pad7)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(SW13-Pad1)")
    (add_net "Net-(SW13-Pad2)")
    (add_net "Net-(SW13-Pad7)")
    (add_net "Net-(SW13-Pad8)")
  )
  (net_class PWR ""
    (clearance 0.254)
    (trace_width 0.381)
    (via_dia 1.016)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /12d_enc_GND)
    (add_net /24d_enc_GND)
    (add_net /3V)
    (add_net GND)
  )
  (module "Front Panel Proto:PEC16-with_SW" (layer F.Cu) (tedit 58D89A6C)
    (at 147.32 100.33)
    (fp_text reference SW7 (at 8.89 -8.89) (layer F.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 8.89 -7.62) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 /P2.5))
    (pad 1 thru_hole circle (at 0 -5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 /P2.4))
    (pad 3 thru_hole circle (at 0 5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 /24d_enc_GND))
    (pad 4 thru_hole circle (at 17.5 -2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 /P1.2))
    (pad 5 thru_hole circle (at 17.5 2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 /24d_enc_GND))
  )
  (module "Front Panel Proto:NHD-0420H1Z-FL-GBW-33V3" (layer F.Cu) (tedit 58D89B96)
    (at 101.6 59.69)
    (fp_text reference DS1 (at 43.18 29.21) (layer F.SilkS))
    (fp_text value LCD-4x20 (at 68.58 22.86) (layer F.Fab))
    (pad 16 thru_hole circle (at 75 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 15 thru_hole circle (at 75 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 /3V))
    (pad 14 thru_hole circle (at 75 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 /P3.7))
    (pad 13 thru_hole circle (at 75 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 /P3.6))
    (pad 12 thru_hole circle (at 75 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 /P3.5))
    (pad 11 thru_hole circle (at 75 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 /P3.4))
    (pad 10 thru_hole circle (at 75 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 /P3.3))
    (pad 9 thru_hole circle (at 75 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 /P3.2))
    (pad 9 thru_hole circle (at 75 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 /P3.2))
    (pad 10 thru_hole circle (at 75 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 /P3.3))
    (pad 11 thru_hole circle (at 75 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 /P3.4))
    (pad 12 thru_hole circle (at 75 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 /P3.5))
    (pad 13 thru_hole circle (at 75 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 /P3.6))
    (pad 14 thru_hole circle (at 75 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 /P3.7))
    (pad 15 thru_hole circle (at 75 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 /3V))
    (pad 16 thru_hole circle (at 75 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 /P3.1))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 /P3.0))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 /P5.5))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 /P5.6))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 /P5.7))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(DS1-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(DS1-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 /P5.7))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 /P5.6))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 /P5.5))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 /P3.0))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 /P3.1))
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer B.Cu) (tedit 58D89911)
    (at 129.54 55.88 270)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 2.39 270) (layer B.SilkS))
    (fp_text value SN74LVC14APWR (at 3.81 -7.62 540) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /P3.0))
    (pad 8 thru_hole oval (at 7.62 -15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /P3.3))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(R1-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 -12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(R4-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /P3.1))
    (pad 10 thru_hole oval (at 7.62 -10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /P3.4))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(R2-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(R5-Pad2)"))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /P3.2))
    (pad 12 thru_hole oval (at 7.62 -5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /P3.5))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(R3-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 -2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(R6-Pad2)"))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 14 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D8999C)
    (at 92.71 46.99 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D8999F)
    (at 92.71 55.88 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D899A2)
    (at 92.71 64.77 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D899A6)
    (at 92.71 73.66 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D899A8)
    (at 92.71 82.55 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D899AC)
    (at 92.71 91.44 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D899AF)
    (at 92.71 100.33 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D7 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D899B9)
    (at 92.71 109.22 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D8 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D8-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D899C2)
    (at 200.025 100.33 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D9 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D9-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D899C6)
    (at 200.025 109.22 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D10 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D10-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D899D5)
    (at 200.025 118.11 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D11 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(D11-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58D899CA)
    (at 200.025 127 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D12 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(D12-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58D89B56)
    (at 196.85 66.04 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J1 (at -2.54 8.89 270) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 2.54 8.89 270) (layer F.Fab))
    (fp_text user %R (at -2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /P1.0))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /P1.1))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /P1.2))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /P1.3))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /P1.4))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /P1.5))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /P1.6))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /P1.7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58D89B17)
    (at 148.59 45.72 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J2 (at -2.54 8.89 180) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 2.54 8.89 180) (layer F.Fab))
    (fp_text user %R (at -2.54 17.78 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /P2.0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /P2.1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /P2.2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /P2.3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /P2.4))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /P2.5))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /P2.6))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /P2.7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58D89B1A)
    (at 125.73 45.72 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J3 (at -2.54 8.89 180) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 2.54 8.89 180) (layer F.Fab))
    (fp_text user %R (at -2.54 17.78 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /P3.0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /P3.1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /P3.2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /P3.3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /P3.4))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /P3.5))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /P3.6))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /P3.7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58D89B1F)
    (at 120.65 45.72 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J5 (at 2.54 8.89 360) (layer F.SilkS))
    (fp_text value CONN_01X08 (at -2.54 8.89 360) (layer F.Fab))
    (fp_text user %R (at 2.54 0 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /SN74_C))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /SN74_D))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /SN74_E))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /SN74_F))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /P5.5))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /P5.6))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /P5.7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58D89B13)
    (at 189.23 45.72 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J8 (at 2.54 8.89 360) (layer F.SilkS))
    (fp_text value CONN_01X08 (at -2.54 8.89 360) (layer F.Fab))
    (fp_text user %R (at 2.54 0 540) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /P8.0))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /P8.1))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /P8.2))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /P8.3))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /3V))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J8-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D89970)
    (at 106.68 53.34)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 6.35 -2.54) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(R1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D89973)
    (at 106.68 58.42)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 -2.54) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(R2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D89976)
    (at 106.68 63.5)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R3 (at 6.35 -2.54) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(R3-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D8997A)
    (at 106.68 68.58)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R4 (at 6.35 -2.54) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D4-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(R4-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D8997F)
    (at 106.68 73.66)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R5 (at 6.35 -2.54) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(R5-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D89983)
    (at 106.68 79.375)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R6 (at 6.35 -2.54) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(R6-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D89986)
    (at 106.68 85.09)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R7 (at 6.35 -2.54) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D7-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(R7-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D89947)
    (at 130.175 68.58)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R8 (at 6.35 -2.54) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D8-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(R8-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D8994B)
    (at 130.175 73.66)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R9 (at 6.35 -2.54) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D9-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(R9-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D8994E)
    (at 130.175 79.375)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R10 (at 6.35 -2.54) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(D10-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R10-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D89953)
    (at 130.175 85.09)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R11 (at 6.35 -2.54) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D11-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(R11-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 58D89B7E)
    (at 163.83 68.58 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R12 (at 6.35 2.66 180) (layer B.SilkS))
    (fp_text value 100 (at 6.35 0 180) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D12-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(R12-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Bourns_3339P_Horizontal (layer B.Cu) (tedit 58D89453)
    (at 100.965 52.07)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK09Y11/RK09Y11L0001.html")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single")
    (fp_text reference RV1 (at -3.175 7.62) (layer B.SilkS))
    (fp_text value POT_TRIM (at 0 -2.52) (layer B.Fab))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.26 1.26) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 1.26 1.26) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 "Net-(DS1-Pad3)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.26 1.26) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Bourns_3339P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 58134C96)
    (at 182.88 78.74)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 /P1.4))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 /P1.4))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 58134C96)
    (at 194.31 78.74)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW2 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 /P1.5))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 /P1.5))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 58134C96)
    (at 182.88 66.04)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW3 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 /P1.6))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 /P1.6))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 58134C96)
    (at 182.88 53.34)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW4 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 /P1.7))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 /P1.7))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Front Panel Proto:PEC16-with_SW" (layer F.Cu) (tedit 58D89A72)
    (at 101.6 100.33)
    (fp_text reference SW5 (at 8.89 -8.89) (layer F.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 8.89 -7.62) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 /P2.1))
    (pad 1 thru_hole circle (at 0 -5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 /P2.0))
    (pad 3 thru_hole circle (at 0 5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 /24d_enc_GND))
    (pad 4 thru_hole circle (at 17.5 -2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 /P1.0))
    (pad 5 thru_hole circle (at 17.5 2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 /24d_enc_GND))
  )
  (module "Front Panel Proto:PEC16-with_SW" (layer F.Cu) (tedit 58D89A6F)
    (at 124.46 100.33)
    (fp_text reference SW6 (at 8.89 -8.89) (layer F.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 8.89 -7.62) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 /P2.3))
    (pad 1 thru_hole circle (at 0 -5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 /P2.2))
    (pad 3 thru_hole circle (at 0 5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 /24d_enc_GND))
    (pad 4 thru_hole circle (at 17.5 -2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 /P1.1))
    (pad 5 thru_hole circle (at 17.5 2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 /24d_enc_GND))
  )
  (module "Front Panel Proto:PEC16-with_SW" (layer F.Cu) (tedit 58D89A68)
    (at 170.18 100.33)
    (fp_text reference SW8 (at 8.89 -8.89) (layer F.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 8.89 -7.62) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 /P2.7))
    (pad 1 thru_hole circle (at 0 -5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 /P2.6))
    (pad 3 thru_hole circle (at 0 5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 /24d_enc_GND))
    (pad 4 thru_hole circle (at 17.5 -2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 /P1.3))
    (pad 5 thru_hole circle (at 17.5 2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 /24d_enc_GND))
  )
  (module "Front Panel Proto:PEC16-with_SW" (layer F.Cu) (tedit 58D89A76)
    (at 101.6 121.92)
    (fp_text reference SW9 (at 8.89 -8.89) (layer F.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 8.89 -7.62) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 /P2.1))
    (pad 1 thru_hole circle (at 0 -5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 /P2.0))
    (pad 3 thru_hole circle (at 0 5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 /12d_enc_GND))
    (pad 4 thru_hole circle (at 17.5 -2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 /P1.0))
    (pad 5 thru_hole circle (at 17.5 2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 /12d_enc_GND))
  )
  (module "Front Panel Proto:PEC16-with_SW" (layer F.Cu) (tedit 58D89AA4)
    (at 124.46 121.92)
    (fp_text reference SW10 (at 8.89 -8.89) (layer F.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 8.89 -7.62) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 /P2.3))
    (pad 1 thru_hole circle (at 0 -5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 /P2.2))
    (pad 3 thru_hole circle (at 0 5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 /12d_enc_GND))
    (pad 4 thru_hole circle (at 17.5 -2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 /P1.1))
    (pad 5 thru_hole circle (at 17.5 2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 /12d_enc_GND))
  )
  (module "Front Panel Proto:PEC16-with_SW" (layer F.Cu) (tedit 58D89AA5)
    (at 147.32 121.92)
    (fp_text reference SW11 (at 8.89 -8.89) (layer F.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 8.89 -7.62) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 /P2.5))
    (pad 1 thru_hole circle (at 0 -5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 /P2.4))
    (pad 3 thru_hole circle (at 0 5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 /12d_enc_GND))
    (pad 4 thru_hole circle (at 17.5 -2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 /P1.2))
    (pad 5 thru_hole circle (at 17.5 2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 /12d_enc_GND))
  )
  (module "Front Panel Proto:PEC16-with_SW" (layer F.Cu) (tedit 58D89AA8)
    (at 170.18 121.92)
    (fp_text reference SW12 (at 8.89 -8.89) (layer F.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 8.89 -7.62) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 /P2.7))
    (pad 1 thru_hole circle (at 0 -5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 /P2.6))
    (pad 3 thru_hole circle (at 0 5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 /12d_enc_GND))
    (pad 4 thru_hole circle (at 17.5 -2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 /P1.3))
    (pad 5 thru_hole circle (at 17.5 2.5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 /12d_enc_GND))
  )
  (module "Front Panel Proto:C&K-BD04" (layer B.Cu) (tedit 58D89B77)
    (at 161.29 80.645 90)
    (fp_text reference SW13 (at 3.81 -10.16 90) (layer B.SilkS))
    (fp_text value SW_DIP_x04 (at 3.81 2.54 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 68 "Net-(SW13-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 69 "Net-(SW13-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 /24d_enc_GND))
    (pad 4 thru_hole circle (at 0 -7.62 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 /12d_enc_GND))
    (pad 5 thru_hole circle (at 7.62 -7.62 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 6 thru_hole circle (at 7.62 -5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 7 thru_hole circle (at 7.62 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 70 "Net-(SW13-Pad7)"))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 71 "Net-(SW13-Pad8)"))
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer B.Cu) (tedit 58D89904)
    (at 149.86 55.88 270)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 2.39 270) (layer B.SilkS))
    (fp_text value SN74LVC14APWR (at 3.81 -7.62 540) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /P3.6))
    (pad 8 thru_hole oval (at 7.62 -15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /SN74_D))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(R7-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 -12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R10-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /P3.7))
    (pad 10 thru_hole oval (at 7.62 -10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /SN74_E))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(R8-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(R11-Pad2)"))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /SN74_C))
    (pad 12 thru_hole oval (at 7.62 -5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /SN74_F))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(R9-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 -2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(R12-Pad2)"))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 14 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 86.36 132.08) (end 86.36 41.275) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.47 132.08) (end 86.36 132.08) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.47 41.275) (end 204.47 132.08) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.36 41.275) (end 204.47 41.275) (layer Edge.Cuts) (width 0.15))
  (zone (net 14) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.44 45.085) (xy 201.93 45.72) (xy 201.93 100.33) (xy 194.31 100.33) (xy 104.14 100.33)
        (xy 91.44 100.33)
      )
    )
  )
  (zone (net 14) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.31 80.645) (xy 201.93 80.645) (xy 201.93 100.33) (xy 194.31 100.33)
      )
    )
  )
)
