(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 152.4 101.6)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(H1-Pad1)")
  (net 3 "Net-(H6-Pad1)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J1-Pad2)")
  (net 6 "Net-(R1-Pad2)")
  (net 7 "Net-(U1-Pad3)")
  (net 8 "unconnected-(U1-Pad5)")
  (net 9 "unconnected-(U1-Pad6)")
  (net 10 "GND")
  (net 11 "GND1")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 181.864 97.79)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Jumper" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.936 101.626 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.11 99.822)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "Net-(H6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 193.04 76.2)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.136 103.378)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -0.026 2.032) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "Net-(H1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 104.14 124.46)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 193.04 124.46)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 168.402 106.68)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 1.778) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 10 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 111.252 105.918 180)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -2.9) (layer "F.SilkS"))
    (fp_text value "Vce+" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle (at 0 0 180) (size 3.8 3.8) (layers "B.Cu" "B.Mask")
      (net 2 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.6 2.6) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 180) (size 3.8 3.8) (layers "F.Cu" "F.Mask")
      (net 2 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 111.252 96.52)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -2.9) (layer "F.SilkS"))
    (fp_text value "Vce-" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers *.Cu *.Mask)
      (net 3 "Net-(H6-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(H6-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "B.Cu" "B.Mask")
      (net 3 "Net-(H6-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 104.14 76.2)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "_es_Uncommon:AMP_AD202KY" (layer "F.Cu")
    (tedit 62E17ED2)
    (at 128.905 102.87)
    (property "MPN" "AD202KY")
    (property "OC_FARNELL" "unknown")
    (property "OC_NEWARK" "05F6719")
    (property "PACKAGE" "SIP-10")
    (property "SUPPLIER" "Analog Devices")
    (property "Sheetfile" "Model 37 HV Vce Interface Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -1.905 -6.35) (layer "F.SilkS"))
    (fp_text value "AD202KY" (at 43.815 -6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 "Net-(R1-Pad2)") (pinfunction "+IN") (pintype "input"))
    (pad "2" thru_hole circle locked (at 1.27 -2.54) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 11 "GND1") (pinfunction "IN/VISO_COM") (pintype "input"))
    (pad "3" thru_hole circle locked (at 2.54 0) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad3)") (pinfunction "-IN") (pintype "input"))
    (pad "4" thru_hole circle locked (at 3.81 -2.54) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad3)") (pinfunction "IN_FDBK") (pintype "output"))
    (pad "5" thru_hole circle locked (at 5.08 0) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 "unconnected-(U1-Pad5)") (pinfunction "-VISO_OUT") (pintype "output+no_connect"))
    (pad "6" thru_hole circle locked (at 6.35 -2.54) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "unconnected-(U1-Pad6)") (pinfunction "+VISO_OUT") (pintype "output+no_connect"))
    (pad "31" thru_hole circle locked (at 38.1 0) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pinfunction "+V") (pintype "power_in"))
    (pad "32" thru_hole circle locked (at 39.37 -2.54) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "COM") (pintype "power_in"))
    (pad "37" thru_hole circle locked (at 45.72 0) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)") (pinfunction "OUT_LO") (pintype "output"))
    (pad "38" thru_hole circle locked (at 46.99 -2.54) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)") (pinfunction "OUT_HI") (pintype "output"))
  )
  (gr_arc (start 193.04 71.12) (mid 196.632102 72.607898) (end 198.12 76.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 104.14 129.54) (end 193.04 129.54) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 187.96 109.22) (mid 186.163949 108.476051) (end 185.42 106.68) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 187.96 93.98) (end 193.04 93.98) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 187.96 109.22) (end 195.58 109.22) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 193.04 71.12) (end 104.14 71.12) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 99.06 76.2) (mid 100.547898 72.607898) (end 104.14 71.12) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 185.42 96.52) (end 185.42 106.68) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 195.58 109.22) (mid 197.376051 109.963949) (end 198.12 111.76) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 198.12 88.9) (mid 196.632102 92.492102) (end 193.04 93.98) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 198.12 124.46) (mid 196.632102 128.052102) (end 193.04 129.54) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 104.14 129.54) (mid 100.547898 128.052102) (end 99.06 124.46) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 198.12 88.9) (end 198.12 76.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.06 76.2) (end 99.06 124.46) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 198.12 111.76) (end 198.12 124.46) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 185.42 96.52) (mid 186.163949 94.723949) (end 187.96 93.98) (layer "Edge.Cuts") (width 0.1))
  (gr_text "Model 37 HV Vce Interface Board, v1\n14 Sept. 2012, E. Stiers" (at 152.4 121.92) (layer "F.SilkS"))
  (gr_text "Vce+" (at 106.934 105.918) (layer "F.SilkS"))
  (gr_text "Vce-" (at 106.934 96.52) (layer "F.SilkS"))
  (zone (net 10) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 7.62))
    (polygon
      (pts
        (xy 200.66 132.08)
        (xy 162.56 132.08)
        (xy 162.56 68.58)
        (xy 200.66 68.58)
      )
    )
  )
  (zone (net 11) (net_name "GND1") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 7.62))
    (polygon
      (pts
        (xy 139.7 132.08)
        (xy 96.52 132.08)
        (xy 96.52 68.58)
        (xy 139.7 68.58)
      )
    )
  )
)
