(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 103)
    (no_connects 0)
    (area 98.896099 65.558599 198.106101 144.448601)
    (thickness 1.6)
    (drawings 37)
    (tracks 284)
    (zones 0)
    (modules 46)
    (nets 33)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.048 1.524)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 DGND)
  (net 2 N$37)
  (net 3 N$40)
  (net 4 LCD_D5)
  (net 5 LCD_D7)
  (net 6 LCD_D4)
  (net 7 LCD_D6)
  (net 8 +5V)
  (net 9 N$3)
  (net 10 N$5)
  (net 11 N$6)
  (net 12 N$7)
  (net 13 N$9)
  (net 14 N$10)
  (net 15 N$17)
  (net 16 N$2)
  (net 17 N$11)
  (net 18 N$13)
  (net 19 DDS_RESET)
  (net 20 DDS_DATA)
  (net 21 DDS_UPDATE)
  (net 22 N$1)
  (net 23 DDS_CLOCK)
  (net 24 V_REV)
  (net 25 V_FWD)
  (net 26 N$12)
  (net 27 BAND_SEL)
  (net 28 LCD_RS)
  (net 29 LCD_E)
  (net 30 MODE_SEL)
  (net 31 TONE)
  (net 32 AUX)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net AUX)
    (add_net BAND_SEL)
    (add_net DDS_CLOCK)
    (add_net DDS_DATA)
    (add_net DDS_RESET)
    (add_net DDS_UPDATE)
    (add_net DGND)
    (add_net LCD_D4)
    (add_net LCD_D5)
    (add_net LCD_D6)
    (add_net LCD_D7)
    (add_net LCD_E)
    (add_net LCD_RS)
    (add_net MODE_SEL)
    (add_net N$1)
    (add_net N$10)
    (add_net N$11)
    (add_net N$12)
    (add_net N$13)
    (add_net N$17)
    (add_net N$2)
    (add_net N$3)
    (add_net N$37)
    (add_net N$40)
    (add_net N$5)
    (add_net N$6)
    (add_net N$7)
    (add_net N$9)
    (add_net TONE)
    (add_net V_FWD)
    (add_net V_REV)
  )
  (module "" (layer Top) (tedit 0)
    (at 193.5861 141.8336)
    (fp_text reference @HOLE0 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
  )
  (module "" (layer Top) (tedit 0)
    (at 101.5111 68.1736)
    (fp_text reference @HOLE1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
  )
  (module "" (layer Top) (tedit 0)
    (at 193.5861 68.1736)
    (fp_text reference @HOLE2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
  )
  (module "" (layer Top) (tedit 0)
    (at 101.5111 141.8336)
    (fp_text reference @HOLE3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
  )
  (module E1,8-4 (layer Top) (tedit 0)
    (at 183.4261 104.84485)
    (descr "<b>ELECTROLYTIC CAPACITOR</b><p>\ngrid 1.8 mm, diameter 4 mm")
    (fp_text reference C4 (at 2.159 -0.762) (layer F.SilkS))
    (fp_text value 10uf (at 2.159 1.778) (layer F.SilkS))
    (pad - thru_hole circle (at 0.889 0) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad + thru_hole circle (at -0.889 0) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 8 +5V))
  )
  (module DC_COAXIAL_JACK (layer Top) (tedit 0)
    (at 185.6486 77.0636 270)
    (fp_text reference J1 (at -11.1125 -5.08 450) (layer F.SilkS))
    (fp_text value DC_JACK (at -11.1125 6.35 270) (layer F.SilkS))
    (pad 2 thru_hole oval (at -0.9525 4.8 270) (size 4.3688 2.1844) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.9525 0) (size 4.3688 2.1844) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 3 thru_hole oval (at 2.0475 0) (size 4.3688 2.1844) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 N$1))
    (pad 4 thru_hole circle (at -0.9688 1.905) (size 2.1844 2.1844) (drill 1.1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -0.9688 -3.175) (size 2.1844 2.1844) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module E1,8-4 (layer Top) (tedit 0)
    (at 188.1886 105.0036)
    (descr "<b>ELECTROLYTIC CAPACITOR</b><p>\ngrid 1.8 mm, diameter 4 mm")
    (fp_text reference C5 (at 2.159 -0.762) (layer F.SilkS))
    (fp_text value 10uf (at 2.159 1.778) (layer F.SilkS))
    (pad - thru_hole circle (at 0.889 0) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad + thru_hole circle (at -0.889 0) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 22 N$1))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 143.1036 116.59235 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R13 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 10 (at -2.2606 0.635 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 N$37))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 +5V))
  )
  (module OP_AMP_8_PIN (layer Top) (tedit 0)
    (at 146.2786 99.6061 270)
    (fp_text reference U3 (at -5.2578 2.54 360) (layer F.SilkS))
    (fp_text value 6002_OP_AMP (at 7.239 2.54 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.81 3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 V_REV))
    (pad 2 thru_hole oval (at -1.27 3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 N$17))
    (pad 3 thru_hole oval (at 1.27 3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 N$11))
    (pad 4 thru_hole oval (at 3.81 3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 5 thru_hole oval (at 3.81 -3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 N$10))
    (pad 6 thru_hole oval (at 1.27 -3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 N$13))
    (pad 7 thru_hole oval (at -1.27 -3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 V_FWD))
    (pad 8 thru_hole oval (at -3.81 -3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 +5V))
  )
  (module E1,8-4 (layer Top) (tedit 0)
    (at 110.7186 82.61985 180)
    (descr "<b>ELECTROLYTIC CAPACITOR</b><p>\ngrid 1.8 mm, diameter 4 mm")
    (fp_text reference C3 (at 2.159 -0.762 360) (layer F.SilkS))
    (fp_text value 1uf (at 2.159 1.778 360) (layer F.SilkS))
    (pad - thru_hole circle (at 0.889 0 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 10 N$5))
    (pad + thru_hole circle (at -0.889 0 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 9 N$3))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 101.5111 78.9686 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R1 (at -3.048 -1.524 90) (layer F.SilkS))
    (fp_text value 49R9 (at -2.2606 0.635 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 N$5))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 N$7))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 115.1636 91.9861 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R3 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 49R9 (at -2.2606 0.635 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 N$6))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 N$5))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 115.32235 99.76485 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R4 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 49R9 (at -2.2606 0.635 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 N$6))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 101.1936 97.7011 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R2 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 10k (at -2.2606 0.635 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 N$10))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 N$9))
  )
  (module DO35-7 (layer Top) (tedit 0)
    (at 108.1786 89.60485)
    (descr "<B>DIODE</B><p>\ndiameter 2 mm, horizontal, grid 7.62 mm")
    (fp_text reference D1 (at -2.286 -1.27) (layer F.SilkS))
    (fp_text value AA143 (at -2.286 2.667) (layer F.SilkS))
    (pad C thru_hole oval (at -3.81 0) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 N$9))
    (pad A thru_hole oval (at 3.81 0) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 N$6))
  )
  (module C025-025X050 (layer Top) (tedit 0)
    (at 102.7811 87.06485 180)
    (descr "<b>CAPACITOR</b><p>\ngrid 2.5 mm, outline 2.5 x 5 mm")
    (fp_text reference C2 (at -2.286 -1.524 360) (layer F.SilkS))
    (fp_text value 0.1 (at -2.286 2.794 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 N$7))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 N$9))
  )
  (module C025-025X050 (layer Top) (tedit 0)
    (at 135.4836 105.0036 180)
    (descr "<b>CAPACITOR</b><p>\ngrid 2.5 mm, outline 2.5 x 5 mm")
    (fp_text reference C1 (at -2.286 -1.524 360) (layer F.SilkS))
    (fp_text value 0.01 (at -2.286 2.794 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 N$10))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 DGND))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 101.1936 111.9886 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R12 (at -3.048 -1.524 90) (layer F.SilkS))
    (fp_text value 100k (at -2.2606 0.635 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 N$10))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 133.2611 95.1611)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R5 (at -3.048 -1.524) (layer F.SilkS))
    (fp_text value 33k (at -2.2606 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 N$17))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 V_REV))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 133.2611 99.6061 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R6 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 649 (at -2.2606 0.635 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 N$17))
  )
  (module C025-025X050 (layer Top) (tedit 0)
    (at 155.4861 95.9231)
    (descr "<b>CAPACITOR</b><p>\ngrid 2.5 mm, outline 2.5 x 5 mm")
    (fp_text reference C8 (at -2.286 -1.524) (layer F.SilkS))
    (fp_text value 0.01 (at -2.286 2.794) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 DGND))
  )
  (module DO35-7 (layer Top) (tedit 0)
    (at 108.1786 94.2086)
    (descr "<B>DIODE</B><p>\ndiameter 2 mm, horizontal, grid 7.62 mm")
    (fp_text reference D2 (at -2.286 -1.27) (layer F.SilkS))
    (fp_text value AA143 (at -2.286 2.667) (layer F.SilkS))
    (pad C thru_hole oval (at -3.81 0) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 N$2))
    (pad A thru_hole oval (at 3.81 0) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 N$6))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 109.4486 104.0511 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R7 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 10k (at -2.2606 0.635 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 N$11))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 N$2))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 122.4661 104.0511 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R8 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 100k (at -2.2606 0.635 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 N$11))
  )
  (module C025-025X050 (layer Top) (tedit 0)
    (at 124.0536 96.58985 90)
    (descr "<b>CAPACITOR</b><p>\ngrid 2.5 mm, outline 2.5 x 5 mm")
    (fp_text reference C7 (at -2.286 -1.524 360) (layer F.SilkS))
    (fp_text value 0.01 (at -2.286 2.794 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 N$11))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 DGND))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 158.6611 100.8761 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R9 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 33k (at -2.2606 0.635 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 N$13))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 V_FWD))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 158.6611 104.6861 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R10 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 649 (at -2.2606 0.635 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 N$13))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 DGND))
  )
  (module B3F-10XX (layer Top) (tedit 0)
    (at 191.9986 111.3536)
    (descr "<b>OMRON SWITCH</b>")
    (fp_text reference S1 (at -3.048 -3.683 90) (layer F.SilkS))
    (fp_text value RESET (at -3.048 5.08) (layer F.SilkS))
    (fp_text user 1 (at -4.318 -1.651) (layer Dwgs.User))
    (fp_text user 2 (at 3.556 -1.524) (layer Dwgs.User))
    (fp_text user 3 (at -4.572 2.794) (layer Dwgs.User))
    (fp_text user 4 (at 3.556 2.794) (layer Dwgs.User))
    (pad 1 thru_hole oval (at -3.2512 -2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 3 thru_hole oval (at -3.2512 2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 N$12))
    (pad 2 thru_hole oval (at 3.2512 -2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 4 thru_hole oval (at 3.2512 2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 N$12))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 173.2661 125.0061 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R16 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 10k (at -2.2606 0.635 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 MODE_SEL))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 +5V))
  )
  (module C025-025X050 (layer Top) (tedit 0)
    (at 105.6386 99.44735)
    (descr "<b>CAPACITOR</b><p>\ngrid 2.5 mm, outline 2.5 x 5 mm")
    (fp_text reference C6 (at -2.286 -1.524) (layer F.SilkS))
    (fp_text value 0.1 (at -2.286 2.794) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 N$2))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 DGND))
  )
  (module DDS_DIL (layer Top) (tedit 0)
    (at 130.7211 83.0961 90)
    (fp_text reference U2 (at 1.27 22.86 360) (layer F.SilkS))
    (fp_text value AD9850_MOD (at 0 0 90) (layer F.SilkS))
    (pad P$1 thru_hole rect (at -6.35 -6.35 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad P$2 thru_hole circle (at -6.35 -3.81 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad P$3 thru_hole circle (at -6.35 -1.27 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad P$4 thru_hole circle (at -6.35 1.27 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad P$5 thru_hole circle (at -6.35 3.81 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad P$6 thru_hole circle (at -6.35 6.35 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad P$7 thru_hole circle (at -6.35 8.89 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad P$8 thru_hole circle (at -6.35 11.43 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad P$9 thru_hole circle (at -6.35 13.97 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad P$10 thru_hole circle (at -6.35 16.51 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad P$11 thru_hole circle (at 13.97 16.51 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad P$12 thru_hole circle (at 13.97 13.97 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 DDS_CLOCK))
    (pad P$13 thru_hole circle (at 13.97 11.43 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 DDS_UPDATE))
    (pad P$14 thru_hole circle (at 13.97 8.89 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 DDS_DATA))
    (pad P$15 thru_hole circle (at 13.97 6.35 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 DDS_RESET))
    (pad P$16 thru_hole circle (at 13.97 3.81 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad P$17 thru_hole circle (at 13.97 1.27 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad P$18 thru_hole circle (at 13.97 -1.27 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
    (pad P$19 thru_hole circle (at 13.97 -3.81 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 N$3))
    (pad P$20 thru_hole circle (at 13.97 -6.35 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module ARDUINO_PRO_MICRO (layer Top) (tedit 0)
    (at 162.4711 68.4911)
    (fp_text reference U1 (at 5.08 6.985 90) (layer F.SilkS))
    (fp_text value ARDUINO_PRO_MICRO (at 3.81 32.385 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 DDS_RESET))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 DDS_DATA))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 DDS_UPDATE))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 DDS_CLOCK))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 TONE))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 AUX))
    (pad 11 thru_hole circle (at 0 25.4) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 LCD_RS))
    (pad 12 thru_hole circle (at 0 27.94) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 LCD_E))
    (pad 13 thru_hole circle (at 15.24 27.94) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 LCD_D7))
    (pad 14 thru_hole circle (at 15.24 25.4) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 LCD_D6))
    (pad 15 thru_hole circle (at 15.24 22.86) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 LCD_D5))
    (pad 16 thru_hole circle (at 15.24 20.32) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 LCD_D4))
    (pad 17 thru_hole circle (at 15.24 17.78) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 V_FWD))
    (pad 18 thru_hole circle (at 15.24 15.24) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 V_REV))
    (pad 19 thru_hole circle (at 15.24 12.7) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 MODE_SEL))
    (pad 20 thru_hole circle (at 15.24 10.16) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 BAND_SEL))
    (pad 21 thru_hole circle (at 15.24 7.62) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 22 thru_hole circle (at 15.24 5.08) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 N$12))
    (pad 23 thru_hole circle (at 15.24 2.54) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 24 thru_hole circle (at 15.24 0) (size 1.6764 1.6764) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module B3F-10XX (layer Top) (tedit 586024A5)
    (at 191.9986 131.6736)
    (descr "<b>OMRON SWITCH</b>")
    (fp_text reference S3 (at -3.048 -3.683 90) (layer F.SilkS))
    (fp_text value BAND (at -3.048 5.08) (layer F.SilkS))
    (fp_text user 1 (at -4.318 -1.651) (layer Dwgs.User))
    (fp_text user 2 (at 3.556 -1.524) (layer Dwgs.User))
    (fp_text user 3 (at -4.572 2.794) (layer Dwgs.User))
    (fp_text user 4 (at 3.556 2.794) (layer Dwgs.User))
    (pad 1 thru_hole oval (at -3.2512 -2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 3 thru_hole oval (at -3.2512 2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 BAND_SEL))
    (pad 2 thru_hole oval (at 3.2512 -2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 4 thru_hole oval (at 3.2512 2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 BAND_SEL))
  )
  (module B3F-10XX (layer Top) (tedit 0)
    (at 191.9986 121.5136)
    (descr "<b>OMRON SWITCH</b>")
    (fp_text reference S2 (at -3.048 -3.683 90) (layer F.SilkS))
    (fp_text value MODE (at -3.048 5.08) (layer F.SilkS))
    (fp_text user 1 (at -4.318 -1.651) (layer Dwgs.User))
    (fp_text user 2 (at 3.556 -1.524) (layer Dwgs.User))
    (fp_text user 3 (at -4.572 2.794) (layer Dwgs.User))
    (fp_text user 4 (at 3.556 2.794) (layer Dwgs.User))
    (pad 1 thru_hole oval (at -3.2512 -2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 3 thru_hole oval (at -3.2512 2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 MODE_SEL))
    (pad 2 thru_hole oval (at 3.2512 -2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 4 thru_hole oval (at 3.2512 2.2606) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 MODE_SEL))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 181.8386 125.0061 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R17 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 10k (at -2.2606 0.635 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 BAND_SEL))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 +5V))
  )
  (module LCD_2X16 (layer Top) (tedit 0)
    (at 144.6911 117.7036)
    (fp_text reference LCD1 (at 15.24 -6.985) (layer F.SilkS))
    (fp_text value LCD_2_16 (at 26.035 -6.985) (layer F.SilkS))
    (pad 1 thru_hole circle (at -32 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 2 thru_hole circle (at -29.46 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 3 thru_hole circle (at -26.92 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 3 N$40))
    (pad 4 thru_hole circle (at -24.38 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 28 LCD_RS))
    (pad 5 thru_hole circle (at -21.84 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 6 thru_hole circle (at -19.3 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 29 LCD_E))
    (pad 7 thru_hole circle (at -16.76 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 8 thru_hole circle (at -14.22 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 9 thru_hole circle (at -11.68 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 10 thru_hole circle (at -9.14 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 11 thru_hole circle (at -6.6 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 6 LCD_D4))
    (pad 12 thru_hole circle (at -4.06 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 4 LCD_D5))
    (pad 13 thru_hole circle (at -1.52 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 7 LCD_D6))
    (pad 14 thru_hole circle (at 1.02 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 5 LCD_D7))
    (pad 15 thru_hole circle (at 3.56 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 2 N$37))
    (pad 16 thru_hole circle (at 6.1 -7.88) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad "" np_thru_hole circle (at -37.5 23.12) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
    (pad "" np_thru_hole circle (at 37.5 23.12) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
    (pad "" np_thru_hole circle (at -37.5 -7.88) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
    (pad "" np_thru_hole circle (at 37.5 -7.88) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
  )
  (module BNC-SMALL (layer Top) (tedit 0)
    (at 113.8936 77.0636 90)
    (fp_text reference CON1 (at 0 0 90) (layer F.SilkS))
    (fp_text value "" (at 0 0 90) (layer F.SilkS))
    (pad G1 thru_hole circle (at 0 -6.598919 90) (size 4.064 4.064) (drill 2.2606) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad G4 thru_hole circle (at 6.598919 -6.598919 90) (size 4.064 4.064) (drill 2.2606) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad G2 thru_hole circle (at 0 0 90) (size 4.064 4.064) (drill 2.2606) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad G3 thru_hole circle (at 6.598919 0 90) (size 4.064 4.064) (drill 2.2606) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad CENT thru_hole circle (at 3.299459 -3.299459 90) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 157.7086 116.59235 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R14 (at -3.048 -1.524 360) (layer F.SilkS))
    (fp_text value 10k (at -2.2606 0.635 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 N$40))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 +5V))
  )
  (module 0207%2f10 (layer Top) (tedit 0)
    (at 176.7586 116.59235)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R15 (at -3.048 -1.524) (layer F.SilkS))
    (fp_text value 649 (at -2.2606 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 N$40))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 DGND))
  )
  (module CS-2016-LOGO-15MM (layer Top) (tedit 0)
    (at 112.6236 144.21485)
    (fp_text reference U$1 (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
  )
  (module CS-2016-LOGO-15MM (layer Bottom) (tedit 0)
    (at 132.6261 143.89735 180)
    (fp_text reference U$2 (at 0 0 180) (layer B.SilkS))
    (fp_text value "" (at 0 0 180) (layer B.SilkS))
  )
  (module 3362U (layer Top) (tedit 0)
    (at 170.56735 106.11485)
    (fp_text reference R18 (at -1.27 -6.35 90) (layer F.SilkS))
    (fp_text value "" (at -1.778 3.302) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 -2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 N$40))
    (pad 3 thru_hole circle (at 5.08 -2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 +5V))
  )
  (module SOLDER_PAD_35_HOLE (layer Top) (tedit 0)
    (at 156.91485 70.0786)
    (fp_text reference P1 (at 1.5875 0.635) (layer F.SilkS))
    (fp_text value SOLDER_PAD_35_HOLE (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 31 TONE))
  )
  (module SOLDER_PAD_35_HOLE (layer Top) (tedit 0)
    (at 154.69235 74.04735)
    (fp_text reference P2 (at 1.5875 0.635) (layer F.SilkS))
    (fp_text value SOLDER_PAD_35_HOLE (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 32 AUX))
  )
  (module SOLDER_PAD_35_HOLE (layer Top) (tedit 0)
    (at 152.46985 70.0786)
    (fp_text reference P3 (at 1.5875 0.635) (layer F.SilkS))
    (fp_text value SOLDER_PAD_35_HOLE (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 DGND))
  )
  (module SWITCHING_REGULATOR (layer Top) (tedit 0)
    (at 185.17235 100.71735)
    (fp_text reference U5 (at 0 0) (layer F.SilkS))
    (fp_text value SWITCHING_REGULATOR (at 0 0) (layer F.SilkS))
    (pad OUT thru_hole circle (at -2.54 0) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad GND thru_hole circle (at 0 0) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad IN thru_hole circle (at 2.54 0) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 N$1))
  )
  (gr_line (start 100.2411 144.3736) (end 196.7611 144.3736) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.7611 65.6336) (end 100.2411 65.6336) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.9711 66.9036) (end 98.9711 143.1036) (layer Edge.Cuts) (width 0.15))
  (gr_text "DDS Module" (at 131.70535 74.61885) (layer F.SilkS))
  (gr_line (start 198.0311 143.1036) (end 198.0311 66.9036) (layer Edge.Cuts) (width 0.15))
  (gr_text "Antenna Analyser" (at 197.0151 85.1281 90) (layer F.SilkS))
  (gr_text K6BEZ (at 195.1101 83.5406 90) (layer F.SilkS))
  (gr_text OPAMP (at 146.9136 102.93985 90) (layer F.SilkS))
  (gr_text "DESIGNED WITH" (at 113.698856 119.608697) (layer F.SilkS))
  (gr_text "EAGLE PCB" (at 107.666356 124.847447) (layer F.SilkS))
  (gr_text "DESIGNED WITH" (at 131.392094 119.132447) (layer B.SilkS))
  (gr_text "EAGLE PCB" (at 137.265844 124.688697) (layer B.SilkS))
  (gr_text WWW.HAMRADIO360.COM (at 164.816356 140.246197) (layer B.SilkS))
  (gr_arc (start 100.2411 66.9036) (end 98.9711 66.9036) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100.2411 143.1036) (end 100.2411 144.3736) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 196.7611 66.9036) (end 196.7611 65.6336) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 196.7611 143.1036) (end 198.0311 143.1036) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text WWW.HAMRADIO360.COM (at 138.781356 140.404947) (layer F.SilkS))
  (gr_text Workbench (at 142.908856 137.229947) (layer F.SilkS))
  (gr_text "PCB Version 7" (at 160.91535 142.4051) (layer B.SilkS))
  (gr_text Workbench (at 163.228856 137.706197) (layer B.SilkS))
  (gr_text Tone (at 158.81985 66.9036 180) (layer F.SilkS))
  (gr_text GND (at 154.37485 66.9036 180) (layer F.SilkS))
  (gr_text Aux (at 156.27985 75.95235 180) (layer F.SilkS))
  (gr_text In (at 188.66485 96.58985) (layer F.SilkS))
  (gr_text Out (at 184.3786 96.58985) (layer F.SilkS))
  (gr_text GND (at 150.0886 66.9036 180) (layer B.SilkS))
  (gr_text Tone (at 154.8511 66.9036 180) (layer B.SilkS))
  (gr_text Aux (at 153.10485 75.95235 180) (layer B.SilkS))
  (gr_text Voltage (at 184.53735 94.8436 90) (layer F.SilkS))
  (gr_text Regulator (at 187.07735 95.00235 90) (layer F.SilkS))
  (zone (net 1) (net_name DGND) (layer Bottom) (hatch none 0.508)
    (priority 6)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 99.822 143.51) (xy 197.104 143.51) (xy 197.104 66.294) (xy 99.822 66.294)
      )
    )
  )
  (zone (net 1) (net_name DGND) (layer Top) (hatch none 0.508)
    (priority 6)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 99.822 143.51) (xy 197.104 143.51) (xy 197.104 66.294) (xy 99.822 66.294)
      )
    )
  )
)
