(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 11)
    (zones 0)
    (modules 6)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 "Net-(BT1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(BT1-Pad2)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 147.32 78.74 90)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference BT1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value 9V (at 1.27 2.33 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 135.128 76.708 180)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U1 (at 2.54 -4.27) (layer F.SilkS))
    (fp_text value LM7805_TO220 (at 2.54 2.5) (layer F.SilkS))
    (fp_text user %R (at 2.54 -4.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:WEMOS_D1_mini_light (layer F.Cu) (tedit 5BBFB1CE)
    (at 124.535001 89.765001)
    (descr "16-pin module, column spacing 22.86 mm (900 mils), https://wiki.wemos.cc/products:d1:d1_mini, https://c1.staticflickr.com/1/734/31400410271_f278b087db_z.jpg")
    (tags "ESP8266 WiFi microcontroller")
    (fp_text reference U2 (at 3.226999 12.342999) (layer F.SilkS))
    (fp_text value WeMos_D1_mini (at 11.7 0) (layer F.SilkS))
    (fp_text user "KEEP OUT" (at 11.43 -6.35) (layer Cmts.User))
    (fp_text user "No copper" (at 11.43 -3.81) (layer Cmts.User))
    (pad 2 thru_hole oval (at 0 2.54) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 22.86 17.78) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 10 thru_hole oval (at 22.86 15.24) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad2)"))
    (pad 11 thru_hole oval (at 22.86 12.7) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 22.86 10.16) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 22.86 7.62) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 22.86 5.08) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 22.86 2.54) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 22.86 0) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Module.3dshapes/WEMOS_D1_mini_light.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (offset (xyz 0 0 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (offset (xyz 22.86 0 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (offset (xyz 22.86 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 140.97 80.01 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.5 -2.5 90) (layer F.SilkS))
    (fp_text value 0.33uF (at 2.5 2.5 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 123.444 80.01 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 2.5 -2.5 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.5 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_5W_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 131.064 95.25)
    (descr "Diode, 5W series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif")
    (tags "Diode 5W series Axial Horizontal pin pitch 10.16mm  length 8.9mm diameter 3.7mm")
    (fp_text reference D1 (at 5.08 -2.97) (layer F.SilkS))
    (fp_text value 1N4001 (at 5.08 2.97) (layer F.SilkS))
    (fp_text user %R (at 5.7475 0) (layer F.Fab))
    (fp_text user K (at 0 -2.4) (layer F.Fab))
    (fp_text user K (at 0 -2.4) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_5W_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "usb connector in front" (at 135.89 113.792) (layer F.SilkS))
  (gr_text "wifi antenna in back" (at 134.62 84.074) (layer F.SilkS))
  (gr_text 5V (at 145.034 107.442) (layer F.SilkS))
  (gr_text - (at 149.352 75.692 90) (layer F.SilkS))
  (gr_text + (at 149.606 78.994) (layer F.SilkS))
  (gr_line (start 151.13 72.39) (end 119.38 72.39) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.13 118.11) (end 151.13 72.39) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.38 118.11) (end 151.13 118.11) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.38 116.84) (end 119.38 118.11) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.38 72.39) (end 119.38 116.84) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name "Net-(BT1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.86 116.84) (xy 120.65 116.84) (xy 120.65 73.66) (xy 149.86 73.66)
      )
    )
  )
)
