(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~66~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 335)
    (tracks 1467)
    (zones 0)
    (modules 128)
    (nets 134)
  )
  (page A4)
  (title_block
    (title iCEBreaker)
    (rev V1.0a)
    (company 1BitSquared)
    (comment 1 "(C) 2018 Piotr Esden-Tempski <piotr@1bitsquared.com>")
    (comment 2 "(C) 2018 1BitSquared <info@1bitsquared.com>")
    (comment 3 "License: CC-BY-SA 4.0")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (trace_clearance 0.15)
    (zone_clearance 0.15)
    (zone_45_only yes)
    (trace_min 0.149)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.5 0.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 55.1 47.5)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 /~LEDG)
  (net 2 /xFIFO_~WR)
  (net 3 +3V3)
  (net 4 /iCE_SS_B)
  (net 5 +1V2)
  (net 6 /xFIFO_WKUP)
  (net 7 /~BUTTON)
  (net 8 /~LEDR)
  (net 9 /xFIFO_~RD)
  (net 10 /xFIFO_~RXF)
  (net 11 /P2_4)
  (net 12 /P2_9)
  (net 13 /xFIFO_D7)
  (net 14 /xFIFO_D6)
  (net 15 /P2_3)
  (net 16 /P2_8)
  (net 17 /xFIFO_D5)
  (net 18 /xFIFO_D4)
  (net 19 /P2_2)
  (net 20 /P2_7)
  (net 21 /xFIFO_D3)
  (net 22 /xFIFO_D2)
  (net 23 /P2_1)
  (net 24 /xFIFO_~TXE)
  (net 25 /P2_10)
  (net 26 GND)
  (net 27 "Net-(R6-Pad1)")
  (net 28 "Net-(R2-Pad1)")
  (net 29 "Net-(R7-Pad2)")
  (net 30 /FTDI_CLK)
  (net 31 "Net-(C3-Pad1)")
  (net 32 +5V)
  (net 33 "Net-(C11-Pad1)")
  (net 34 /iCE_SCK)
  (net 35 "Net-(U4-Pad3)")
  (net 36 "Net-(C12-Pad1)")
  (net 37 "Net-(R8-Pad1)")
  (net 38 "Net-(C13-Pad1)")
  (net 39 +1V8)
  (net 40 "Net-(R9-Pad1)")
  (net 41 "Net-(U4-Pad19)")
  (net 42 "Net-(U4-Pad22)")
  (net 43 /iCE_CDONE)
  (net 44 /iCE_CRESET)
  (net 45 "Net-(U4-Pad26)")
  (net 46 "Net-(U4-Pad27)")
  (net 47 "Net-(U4-Pad28)")
  (net 48 "Net-(U4-Pad29)")
  (net 49 "Net-(U4-Pad30)")
  (net 50 "Net-(U4-Pad32)")
  (net 51 "Net-(U4-Pad33)")
  (net 52 "Net-(U4-Pad34)")
  (net 53 "Net-(U4-Pad36)")
  (net 54 "Net-(U4-Pad57)")
  (net 55 "Net-(U4-Pad58)")
  (net 56 "Net-(U4-Pad59)")
  (net 57 "Net-(U4-Pad60)")
  (net 58 /P1B9)
  (net 59 /P1B10)
  (net 60 /P1B4)
  (net 61 /P1A1)
  (net 62 /P1A7)
  (net 63 /P1A2)
  (net 64 /P1A8)
  (net 65 /P1A3)
  (net 66 /P1A9)
  (net 67 /P1A4)
  (net 68 /P1A10)
  (net 69 /~LED_RED)
  (net 70 /~LED_GRN)
  (net 71 /~LED_BLU)
  (net 72 /P1B1)
  (net 73 /P1B7)
  (net 74 /P1B2)
  (net 75 /P1B8)
  (net 76 /P1B3)
  (net 77 "Net-(D6-PadA)")
  (net 78 "Net-(D9-PadA)")
  (net 79 "Net-(D7-PadA)")
  (net 80 "Net-(D10-PadA)")
  (net 81 /shield)
  (net 82 "Net-(D8-PadA)")
  (net 83 "Net-(D1-PadA)")
  (net 84 "Net-(D4-PadA)")
  (net 85 "Net-(D5-PadA)")
  (net 86 "Net-(P1-Pad4)")
  (net 87 "Net-(C35-Pad1)")
  (net 88 "Net-(R2-Pad5)")
  (net 89 "Net-(R2-Pad3)")
  (net 90 "Net-(C39-Pad1)")
  (net 91 "Net-(U7-Pad2)")
  (net 92 /P1A1x)
  (net 93 /P1A7x)
  (net 94 /P1A2x)
  (net 95 /P1A8x)
  (net 96 /P2_4x)
  (net 97 /P2_3x)
  (net 98 /P2_2x)
  (net 99 /P2_1x)
  (net 100 /P1B7x)
  (net 101 /P1B8x)
  (net 102 /P1B9x)
  (net 103 /P1B10x)
  (net 104 /P2_10x)
  (net 105 /P2_9x)
  (net 106 /P2_8x)
  (net 107 /P2_7x)
  (net 108 /P1B1x)
  (net 109 /P1B2x)
  (net 110 /P1B3x)
  (net 111 /P1B4x)
  (net 112 /P1A10x)
  (net 113 /P1A4x)
  (net 114 /P1A9x)
  (net 115 /P1A3x)
  (net 116 /USB_DP)
  (net 117 /USB_DM)
  (net 118 /Tx_TTL|FIFO_D1)
  (net 119 /Rx_TTL|FIFO_D0)
  (net 120 /FLASH_MISO|IO1)
  (net 121 /FLASH_MOSI|IO0)
  (net 122 /FLASH_~WP~|IO2)
  (net 123 /FLASH_~HLD~|~RST~|IO3)
  (net 124 /FLASH_CS)
  (net 125 /xFIFO_D1)
  (net 126 /xFIFO_D0)
  (net 127 /VCCIO_2)
  (net 128 /VCCIO_0|1)
  (net 129 /VCCPLL)
  (net 130 /VCORE)
  (net 131 /xiCE_CRESET)
  (net 132 /iCE_SO)
  (net 133 /iCE_SI)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.15)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V2)
    (add_net +1V8)
    (add_net +3V3)
    (add_net +5V)
    (add_net /FLASH_CS)
    (add_net /FLASH_MISO|IO1)
    (add_net /FLASH_MOSI|IO0)
    (add_net /FLASH_~HLD~|~RST~|IO3)
    (add_net /FLASH_~WP~|IO2)
    (add_net /FTDI_CLK)
    (add_net /P1A1)
    (add_net /P1A10)
    (add_net /P1A10x)
    (add_net /P1A1x)
    (add_net /P1A2)
    (add_net /P1A2x)
    (add_net /P1A3)
    (add_net /P1A3x)
    (add_net /P1A4)
    (add_net /P1A4x)
    (add_net /P1A7)
    (add_net /P1A7x)
    (add_net /P1A8)
    (add_net /P1A8x)
    (add_net /P1A9)
    (add_net /P1A9x)
    (add_net /P1B1)
    (add_net /P1B10)
    (add_net /P1B10x)
    (add_net /P1B1x)
    (add_net /P1B2)
    (add_net /P1B2x)
    (add_net /P1B3)
    (add_net /P1B3x)
    (add_net /P1B4)
    (add_net /P1B4x)
    (add_net /P1B7)
    (add_net /P1B7x)
    (add_net /P1B8)
    (add_net /P1B8x)
    (add_net /P1B9)
    (add_net /P1B9x)
    (add_net /P2_1)
    (add_net /P2_10)
    (add_net /P2_10x)
    (add_net /P2_1x)
    (add_net /P2_2)
    (add_net /P2_2x)
    (add_net /P2_3)
    (add_net /P2_3x)
    (add_net /P2_4)
    (add_net /P2_4x)
    (add_net /P2_7)
    (add_net /P2_7x)
    (add_net /P2_8)
    (add_net /P2_8x)
    (add_net /P2_9)
    (add_net /P2_9x)
    (add_net /Rx_TTL|FIFO_D0)
    (add_net /Tx_TTL|FIFO_D1)
    (add_net /USB_DM)
    (add_net /USB_DP)
    (add_net /VCCIO_0|1)
    (add_net /VCCIO_2)
    (add_net /VCCPLL)
    (add_net /VCORE)
    (add_net /iCE_CDONE)
    (add_net /iCE_CRESET)
    (add_net /iCE_SCK)
    (add_net /iCE_SI)
    (add_net /iCE_SO)
    (add_net /iCE_SS_B)
    (add_net /shield)
    (add_net /xFIFO_D0)
    (add_net /xFIFO_D1)
    (add_net /xFIFO_D2)
    (add_net /xFIFO_D3)
    (add_net /xFIFO_D4)
    (add_net /xFIFO_D5)
    (add_net /xFIFO_D6)
    (add_net /xFIFO_D7)
    (add_net /xFIFO_WKUP)
    (add_net /xFIFO_~RD)
    (add_net /xFIFO_~RXF)
    (add_net /xFIFO_~TXE)
    (add_net /xFIFO_~WR)
    (add_net /xiCE_CRESET)
    (add_net /~BUTTON)
    (add_net /~LEDG)
    (add_net /~LEDR)
    (add_net /~LED_BLU)
    (add_net /~LED_GRN)
    (add_net /~LED_RED)
    (add_net GND)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C35-Pad1)")
    (add_net "Net-(C39-Pad1)")
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(D10-PadA)")
    (add_net "Net-(D4-PadA)")
    (add_net "Net-(D5-PadA)")
    (add_net "Net-(D6-PadA)")
    (add_net "Net-(D7-PadA)")
    (add_net "Net-(D8-PadA)")
    (add_net "Net-(D9-PadA)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R2-Pad3)")
    (add_net "Net-(R2-Pad5)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U4-Pad19)")
    (add_net "Net-(U4-Pad22)")
    (add_net "Net-(U4-Pad26)")
    (add_net "Net-(U4-Pad27)")
    (add_net "Net-(U4-Pad28)")
    (add_net "Net-(U4-Pad29)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad30)")
    (add_net "Net-(U4-Pad32)")
    (add_net "Net-(U4-Pad33)")
    (add_net "Net-(U4-Pad34)")
    (add_net "Net-(U4-Pad36)")
    (add_net "Net-(U4-Pad57)")
    (add_net "Net-(U4-Pad58)")
    (add_net "Net-(U4-Pad59)")
    (add_net "Net-(U4-Pad60)")
    (add_net "Net-(U7-Pad2)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x07 locked (layer F.Cu) (tedit 5B9C47C7)
    (at 55.1 64.01 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J20 (at -4.29 -0.1 180) (layer F.Fab))
    (fp_text value Flash (at -2.89 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 124 /FLASH_CS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /iCE_SCK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 121 /FLASH_MOSI|IO0))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 120 /FLASH_MISO|IO1))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 122 /FLASH_~WP~|IO2))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 123 /FLASH_~HLD~|~RST~|IO3))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07.wrl
      (offset (xyz 0 -7.619999885559082 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 locked (layer F.Cu) (tedit 5B9C47A2)
    (at 42.4 64.01 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J25 (at -4.29 0 180) (layer F.Fab))
    (fp_text value "RGB Led" (at -2.99 -0.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 /~LED_GRN))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 69 /~LED_RED))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 +1V2))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 71 /~LED_BLU))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 +5V))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (offset (xyz 1.269999980926514 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x01_P2.54mm_Vertical (layer F.Cu) (tedit 5B9C4738)
    (at 70.34 56.39 270)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference J28 (at 0.01 -0.96 90) (layer F.Fab))
    (fp_text value CRESET (at 1.31 0.94 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /iCE_CRESET))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x01_P2.54mm_VerticalX.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 locked (layer F.Cu) (tedit 5B9C42DF)
    (at 75.42 58.93)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J27 (at -0.02 0.87) (layer F.Fab))
    (fp_text value "5V AUX" (at 1.38 -0.83) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 locked (layer F.Cu) (tedit 5B9C4257)
    (at 55.1 33.53 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J26 (at 6.13 1.5 90) (layer F.Fab))
    (fp_text value "5V AUX" (at 7.62 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 +5V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06 locked (layer F.Cu) (tedit 5B9C423A)
    (at 86.85 53.85 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J24 (at 0.05 -0.05 270) (layer F.Fab))
    (fp_text value PMOD (at 2.65 6.35 270) (layer F.Fab))
    (pad 6 thru_hole circle (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 12 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 5 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (pad 11 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (pad 4 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 96 /P2_4x))
    (pad 10 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 104 /P2_10x))
    (pad 3 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 97 /P2_3x))
    (pad 9 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 105 /P2_9x))
    (pad 2 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 98 /P2_2x))
    (pad 8 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 106 /P2_8x))
    (pad 1 thru_hole rect (at 0 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 99 /P2_1x))
    (pad 7 thru_hole oval (at 2.54 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 107 /P2_7x))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x06.wrl
      (offset (xyz 1.269999980926514 -6.349999904632568 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06 locked (layer F.Cu) (tedit 5B9C41F7)
    (at 75.42 53.85 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference J23 (at -0.15 3.48 90) (layer F.Fab))
    (fp_text value PMOD (at 6.45 0.68 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 12 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 5 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (pad 11 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (pad 4 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 96 /P2_4x))
    (pad 10 thru_hole oval (at 5.08 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 104 /P2_10x))
    (pad 3 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 97 /P2_3x))
    (pad 9 thru_hole oval (at 7.62 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 105 /P2_9x))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 98 /P2_2x))
    (pad 8 thru_hole oval (at 10.16 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 106 /P2_8x))
    (pad 1 thru_hole rect (at 12.7 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 99 /P2_1x))
    (pad 7 thru_hole oval (at 12.7 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 107 /P2_7x))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x06.wrl
      (offset (xyz 6.349999904632568 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_2x06 locked (layer F.Cu) (tedit 5B9C3E90)
    (at 72.88 33.53 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference J22 (at 0.08 2.93 180) (layer F.Fab))
    (fp_text value PMOD (at 5.98 0.03 180) (layer F.Fab))
    (pad 7 thru_hole oval (at 12.7 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 100 /P1B7x))
    (pad 1 thru_hole rect (at 12.7 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 108 /P1B1x))
    (pad 8 thru_hole oval (at 10.16 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 101 /P1B8x))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 109 /P1B2x))
    (pad 9 thru_hole oval (at 7.62 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 102 /P1B9x))
    (pad 3 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 110 /P1B3x))
    (pad 10 thru_hole oval (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 103 /P1B10x))
    (pad 4 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 111 /P1B4x))
    (pad 11 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (pad 5 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (pad 12 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 6 thru_hole circle (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model dis${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_2x06 locked (layer F.Cu) (tedit 5B9C3E10)
    (at 50.02 33.53 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference J21 (at 0.02 2.93 180) (layer F.Fab))
    (fp_text value PMOD (at 6.32 0.03 180) (layer F.Fab))
    (pad 6 thru_hole circle (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 12 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 5 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (pad 11 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 GND))
    (pad 4 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 113 /P1A4x))
    (pad 10 thru_hole oval (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 112 /P1A10x))
    (pad 3 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 115 /P1A3x))
    (pad 9 thru_hole oval (at 7.62 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 114 /P1A9x))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 94 /P1A2x))
    (pad 8 thru_hole oval (at 10.16 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 95 /P1A8x))
    (pad 1 thru_hole rect (at 12.7 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 92 /P1A1x))
    (pad 7 thru_hole oval (at 12.7 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 93 /P1A7x))
    (model dis${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Horizontal.step
      (offset (xyz 6.35 -1.27 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 5B8B7ED4)
    (at 58.9 53 225)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R26 (at 0.070711 -0.070711 225) (layer F.Fab))
    (fp_text value 2k2 (at -1.838478 0 225) (layer F.Fab))
    (pad 1 smd roundrect (at -0.499999 0 225) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /iCE_CRESET))
    (pad 2 smd roundrect (at 0.499999 0 225) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 /xiCE_CRESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 5B8B7ED4)
    (at 50.5 47.2)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R25 (at 0 0) (layer F.Fab))
    (fp_text value 10k (at 1.9 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /xFIFO_D3))
    (pad 2 smd roundrect (at 0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_jumpers:J_NC_0603_15 (layer B.Cu) (tedit 5B909785)
    (at 53.8 52.85)
    (descr "Jumper Normally Closed SMD 0603, 0.15mm connection, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J1 (at 0 1.1) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 126 /xFIFO_D0))
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 119 /Rx_TTL|FIFO_D0))
  )
  (module pkl_jumpers:J_NC_0603_15 (layer B.Cu) (tedit 5B909785)
    (at 51.4 52.85)
    (descr "Jumper Normally Closed SMD 0603, 0.15mm connection, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J2 (at 0 1.1) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab))
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 118 /Tx_TTL|FIFO_D1))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 125 /xFIFO_D1))
  )
  (module pkl_jumpers:J_NC_0603_15 (layer B.Cu) (tedit 5B909785)
    (at 63 59.1 180)
    (descr "Jumper Normally Closed SMD 0603, 0.15mm connection, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J16 (at 0 1.1 180) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.575 0 180) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 133 /iCE_SI))
    (pad 2 smd roundrect (at 0.575 0 180) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 120 /FLASH_MISO|IO1))
  )
  (module pkl_jumpers:J_NC_0603_15 (layer B.Cu) (tedit 5B909785)
    (at 63 57.6)
    (descr "Jumper Normally Closed SMD 0603, 0.15mm connection, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J18 (at 0 1.1) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab))
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 /iCE_SS_B))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 124 /FLASH_CS))
  )
  (module pkl_jumpers:J_NC_0603_15 (layer B.Cu) (tedit 5B909785)
    (at 63 60.2 180)
    (descr "Jumper Normally Closed SMD 0603, 0.15mm connection, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J15 (at 0 1.1 180) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.575 0 180) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 121 /FLASH_MOSI|IO0))
    (pad 2 smd roundrect (at 0.575 0 180) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 132 /iCE_SO))
  )
  (module pkl_jumpers:J_NC_0603_30 (layer B.Cu) (tedit 5B90984B)
    (at 55.25 45.3 135)
    (descr "Jumper Normally Closed SMD 0603, 0.30mm connection, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J17 (at 0 1.1 135) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2 135) (layer B.Fab))
    (pad 1 smd roundrect (at -0.574999 0 135) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 /VCCIO_2))
    (pad 2 smd roundrect (at 0.574999 0 135) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
  )
  (module pkl_jumpers:J_NC_0603_30 (layer B.Cu) (tedit 5B90984B)
    (at 65.1 40.3 45)
    (descr "Jumper Normally Closed SMD 0603, 0.30mm connection, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J19 (at 0 1.1 45) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2 45) (layer B.Fab))
    (pad 2 smd roundrect (at 0.574999 0 45) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.574999 0 45) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 128 /VCCIO_0|1))
  )
  (module pkl_jumpers:J_NC_0603_30 (layer B.Cu) (tedit 5B90984B)
    (at 55.4 56 180)
    (descr "Jumper Normally Closed SMD 0603, 0.30mm connection, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J14 (at 0 1.1 180) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.575 0 180) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 +1V2))
    (pad 1 smd roundrect (at -0.575 0 180) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 130 /VCORE))
  )
  (module pkl_jumpers:J_0603 (layer B.Cu) (tedit 5B90967F)
    (at 51.4 43.35)
    (descr "Jumper SMD 0603, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J12 (at 0 0.05) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 /~LEDG))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /xFIFO_~WR))
  )
  (module pkl_jumpers:J_0603 (layer B.Cu) (tedit 5B90967F)
    (at 51.4 44.8)
    (descr "Jumper SMD 0603, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J10 (at 0 0) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /P2_1))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 /xFIFO_~TXE))
  )
  (module pkl_jumpers:J_0603 (layer B.Cu) (tedit 5B90967F)
    (at 53.8 51.2)
    (descr "Jumper SMD 0603, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J3 (at 0 0) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 /P2_10))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /xFIFO_D2))
  )
  (module pkl_jumpers:J_0603 (layer B.Cu) (tedit 5B90967F)
    (at 51.4 51.2)
    (descr "Jumper SMD 0603, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J4 (at 0 0) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 /P2_4))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /xFIFO_D3))
  )
  (module pkl_jumpers:J_0603 (layer B.Cu) (tedit 5B90967F)
    (at 53.8 49.55)
    (descr "Jumper SMD 0603, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J5 (at 0 0.05) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 /P2_9))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 /xFIFO_D4))
  )
  (module pkl_jumpers:J_0603 (layer B.Cu) (tedit 5B90967F)
    (at 51.4 49.55)
    (descr "Jumper SMD 0603, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J6 (at 0 0.05) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /P2_3))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 /xFIFO_D5))
  )
  (module pkl_jumpers:J_0603 (layer B.Cu) (tedit 5B90967F)
    (at 53.8 47.9)
    (descr "Jumper SMD 0603, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J7 (at 0 0) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 /P2_8))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 /xFIFO_D6))
  )
  (module pkl_jumpers:J_0603 (layer B.Cu) (tedit 5B90967F)
    (at 51.4 47.9)
    (descr "Jumper SMD 0603, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J8 (at 0 0) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 /P2_2))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 /xFIFO_D7))
  )
  (module pkl_jumpers:J_0603 (layer B.Cu) (tedit 5B90967F)
    (at 51.4 46.25)
    (descr "Jumper SMD 0603, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J9 (at 0 0.05) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 /P2_7))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 /xFIFO_~RXF))
  )
  (module pkl_jumpers:J_0603 (layer B.Cu) (tedit 5B90967F)
    (at 51.4 54.5)
    (descr "Jumper SMD 0603, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J11 (at 0 0) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 /~LEDR))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 /xFIFO_~RD))
  )
  (module pkl_jumpers:J_0603 (layer B.Cu) (tedit 5B90967F)
    (at 53.8 54.5)
    (descr "Jumper SMD 0603, reflow soldering")
    (tags "jumper 0603")
    (attr smd)
    (fp_text reference J13 (at 0 0) (layer B.Fab))
    (fp_text value Jumper (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 /~BUTTON))
    (pad 1 smd roundrect (at -0.575 0) (size 0.95 0.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 /xFIFO_WKUP))
  )
  (module pkl_logos:1b2_Logo_SilkS_5mm locked (layer B.Cu) (tedit 5A7CF31B)
    (at 42.2 47.2 180)
    (fp_text reference REF** (at 0 -4 180) (layer B.Fab) hide)
    (fp_text value 1b2_Logo_SilkS_5mm (at 0 4 180) (layer B.Fab) hide)
  )
  (module pkl_dipol:R_Array_Convex_4x0402 (layer F.Cu) (tedit 5AEF8AD8)
    (at 57.105546 43.866206 135)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R23 (at -0.027818 0.019974 45) (layer F.Fab))
    (fp_text value 33E (at -1.398833 -0.063173 45) (layer F.Fab))
    (pad 8 smd roundrect (at 0.5 0.85 135) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 /P1A10x))
    (pad 6 smd roundrect (at 0.5 0.25 135) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 113 /P1A4x))
    (pad 4 smd roundrect (at 0.5 -0.25 135) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 114 /P1A9x))
    (pad 2 smd roundrect (at 0.5 -0.85 135) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 115 /P1A3x))
    (pad 7 smd roundrect (at -0.5 0.85 135) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 /P1A10))
    (pad 1 smd roundrect (at -0.5 -0.85 135) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /P1A3))
    (pad 5 smd roundrect (at -0.5 0.25 135) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /P1A4))
    (pad 3 smd roundrect (at -0.5 -0.25 135) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /P1A9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_Array_Convex_4x0402 (layer F.Cu) (tedit 5AEF8AD8)
    (at 62.2 39.3 90)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R24 (at 0 0) (layer F.Fab))
    (fp_text value 33E (at 1.35 0) (layer F.Fab))
    (pad 8 smd roundrect (at 0.5 0.85 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 /P1B10x))
    (pad 6 smd roundrect (at 0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 /P1B4x))
    (pad 4 smd roundrect (at 0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 /P1B9x))
    (pad 2 smd roundrect (at 0.5 -0.85 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 110 /P1B3x))
    (pad 7 smd roundrect (at -0.5 0.85 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /P1B10))
    (pad 1 smd roundrect (at -0.5 -0.85 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 /P1B3))
    (pad 5 smd roundrect (at -0.5 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /P1B4))
    (pad 3 smd roundrect (at -0.5 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /P1B9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_Array_Convex_4x0402 (layer F.Cu) (tedit 5AEF8AD8)
    (at 67 52.6 315)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R22 (at 0 0 225) (layer F.Fab))
    (fp_text value 33E (at 1.449569 0.035355 225) (layer F.Fab))
    (pad 8 smd roundrect (at 0.5 0.85 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 /P2_10x))
    (pad 6 smd roundrect (at 0.5 0.25 315) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /P2_4x))
    (pad 4 smd roundrect (at 0.5 -0.25 315) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 /P2_9x))
    (pad 2 smd roundrect (at 0.5 -0.85 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /P2_3x))
    (pad 7 smd roundrect (at -0.5 0.85 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /P2_10))
    (pad 1 smd roundrect (at -0.5 -0.85 315) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /P2_3))
    (pad 5 smd roundrect (at -0.5 0.25 315) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /P2_4))
    (pad 3 smd roundrect (at -0.5 -0.25 315) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /P2_9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_Array_Convex_4x0402 (layer F.Cu) (tedit 5AEF8AD8)
    (at 40.1 38.1 180)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R2 (at 0 0 90) (layer F.Fab))
    (fp_text value 10k (at 0 1.7) (layer F.Fab))
    (pad 3 smd roundrect (at -0.5 -0.25 180) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(R2-Pad3)"))
    (pad 5 smd roundrect (at -0.5 0.25 180) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(R2-Pad5)"))
    (pad 1 smd roundrect (at -0.5 -0.85 180) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R2-Pad1)"))
    (pad 7 smd roundrect (at -0.5 0.85 180) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 -0.85 180) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 4 smd roundrect (at 0.5 -0.25 180) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 6 smd roundrect (at 0.5 0.25 180) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 8 smd roundrect (at 0.5 0.85 180) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_Array_Convex_4x0402 (layer F.Cu) (tedit 5AEF8AD8)
    (at 59.6 41.2 135)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R21 (at 0 0 45) (layer F.Fab))
    (fp_text value 33E (at 1.484924 0.070711 225) (layer F.Fab))
    (pad 8 smd roundrect (at 0.5 0.85 135) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 /P1B8x))
    (pad 6 smd roundrect (at 0.5 0.25 135) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 /P1B2x))
    (pad 4 smd roundrect (at 0.5 -0.25 135) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 /P1B7x))
    (pad 2 smd roundrect (at 0.5 -0.85 135) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 /P1B1x))
    (pad 7 smd roundrect (at -0.5 0.85 135) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /P1B8))
    (pad 1 smd roundrect (at -0.5 -0.85 135) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 /P1B1))
    (pad 5 smd roundrect (at -0.5 0.25 135) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 /P1B2))
    (pad 3 smd roundrect (at -0.5 -0.25 135) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 /P1B7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_Array_Convex_4x0402 (layer F.Cu) (tedit 5AEF8AD8)
    (at 70.4 46.9)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R4 (at 0 0 -90) (layer F.Fab))
    (fp_text value 33E (at 1.4 -0.1 -90) (layer F.Fab))
    (pad 8 smd roundrect (at 0.5 0.85) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 /P2_8x))
    (pad 6 smd roundrect (at 0.5 0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /P2_2x))
    (pad 4 smd roundrect (at 0.5 -0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 /P2_7x))
    (pad 2 smd roundrect (at 0.5 -0.85) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /P2_1x))
    (pad 7 smd roundrect (at -0.5 0.85) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /P2_8))
    (pad 1 smd roundrect (at -0.5 -0.85) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /P2_1))
    (pad 5 smd roundrect (at -0.5 0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /P2_2))
    (pad 3 smd roundrect (at -0.5 -0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /P2_7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_Array_Convex_4x0402 (layer F.Cu) (tedit 5AEF8AD8)
    (at 55 49 225)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R20 (at 0 0 135) (layer F.Fab))
    (fp_text value 33E (at 1.555635 0 315) (layer F.Fab))
    (pad 8 smd roundrect (at 0.5 0.85 225) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 /P1A8x))
    (pad 6 smd roundrect (at 0.5 0.25 225) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /P1A2x))
    (pad 4 smd roundrect (at 0.5 -0.25 225) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 /P1A7x))
    (pad 2 smd roundrect (at 0.5 -0.85 225) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 /P1A1x))
    (pad 7 smd roundrect (at -0.5 0.85 225) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /P1A8))
    (pad 1 smd roundrect (at -0.5 -0.85 225) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /P1A1))
    (pad 5 smd roundrect (at -0.5 0.25 225) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /P1A2))
    (pad 3 smd roundrect (at -0.5 -0.25 225) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /P1A7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_Array_Convex_4x0402 (layer F.Cu) (tedit 5AEF8AD8)
    (at 62.9 55.1 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R11 (at 0 0 180) (layer F.Fab))
    (fp_text value 10k (at 0 1.8 90) (layer F.Fab))
    (pad 8 smd roundrect (at 0.5 0.85 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 /FLASH_~WP~|IO2))
    (pad 6 smd roundrect (at 0.5 0.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 /FLASH_CS))
    (pad 4 smd roundrect (at 0.5 -0.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /iCE_SCK))
    (pad 2 smd roundrect (at 0.5 -0.85 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 123 /FLASH_~HLD~|~RST~|IO3))
    (pad 7 smd roundrect (at -0.5 0.85 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.5 -0.85 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 5 smd roundrect (at -0.5 0.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 3 smd roundrect (at -0.5 -0.25 270) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_Array_Convex_4x0402 (layer F.Cu) (tedit 5AEF8AD8)
    (at 95.4 50.5)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R16 (at 0 0 -90) (layer F.Fab))
    (fp_text value 10k (at 0 1.8 -180) (layer F.Fab))
    (pad 3 smd roundrect (at -0.5 -0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /P2_4x))
    (pad 5 smd roundrect (at -0.5 0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 /P2_10x))
    (pad 1 smd roundrect (at -0.5 -0.85) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 /P2_9x))
    (pad 7 smd roundrect (at -0.5 0.85) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 -0.85) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 4 smd roundrect (at 0.5 -0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 6 smd roundrect (at 0.5 0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 8 smd roundrect (at 0.5 0.85) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_Array_Convex_4x0402 (layer F.Cu) (tedit 5AEF8AD8)
    (at 89.4 44.5 180)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R17 (at 0 0 90) (layer F.Fab))
    (fp_text value 330E (at 0 1.75 180) (layer F.Fab))
    (pad 8 smd roundrect (at 0.5 0.85 180) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /P2_1x))
    (pad 6 smd roundrect (at 0.5 0.25 180) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /P2_2x))
    (pad 4 smd roundrect (at 0.5 -0.25 180) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 /P2_8x))
    (pad 2 smd roundrect (at 0.5 -0.85 180) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /P2_3x))
    (pad 7 smd roundrect (at -0.5 0.85 180) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(D6-PadA)"))
    (pad 1 smd roundrect (at -0.5 -0.85 180) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(D9-PadA)"))
    (pad 5 smd roundrect (at -0.5 0.25 180) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(D10-PadA)"))
    (pad 3 smd roundrect (at -0.5 -0.25 180) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(D7-PadA)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_pads:PAD_SMD_1x2.65 (layer B.Cu) (tedit 5AA4E193)
    (at 31.84 51.31)
    (fp_text reference P5 (at 0 -2.5) (layer B.Fab) hide)
    (fp_text value UP (at 0 2.2) (layer B.Fab) hide)
    (pad 1 smd roundrect (at 0 0) (size 2.65 1) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
  )
  (module pkl_pads:PAD_SMD_1x2.65 (layer B.Cu) (tedit 5AA4E18B)
    (at 31.84 43.69)
    (fp_text reference P2 (at 0 -2.5) (layer B.Fab) hide)
    (fp_text value UP (at 0 2.2) (layer B.Fab) hide)
    (pad 1 smd roundrect (at 0 0) (size 2.65 1) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
  )
  (module pkl_pads:PAD_SMD_1x2.65 (layer B.Cu) (tedit 5AA4E183)
    (at 31.84 46.23)
    (fp_text reference P3 (at 0 -2.5) (layer B.Fab) hide)
    (fp_text value UP (at 0 2.2) (layer B.Fab) hide)
    (pad 1 smd roundrect (at 0 0) (size 2.65 1) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 117 /USB_DM))
  )
  (module pkl_pads:PAD_SMD_1x2.65 (layer B.Cu) (tedit 5AA4E17D)
    (at 31.84 48.77)
    (fp_text reference P4 (at 0 -2.5) (layer B.Fab) hide)
    (fp_text value UP (at 0 2.2) (layer B.Fab) hide)
    (pad 1 smd roundrect (at 0 0) (size 2.65 1) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 116 /USB_DP))
  )
  (module pkl_dipol:C_0603 (layer F.Cu) (tedit 552C8666)
    (at 46.85 40.4 90)
    (descr "Capacitor SMD 0603, reflow soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 1.8 0.25 270) (layer F.Fab))
    (fp_text value 4u7 (at 0 -0.05 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.75 0 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 +1V8))
    (pad 2 smd roundrect (at 0.75 0 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0603 (layer F.Cu) (tedit 552C8666)
    (at 37.2 45 180)
    (descr "Capacitor SMD 0603, reflow soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 0 180) (layer F.Fab))
    (fp_text value 4u7 (at -2.1 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.75 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.75 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0603 (layer F.Cu) (tedit 552C8666)
    (at 37.2 48 180)
    (descr "Capacitor SMD 0603, reflow soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 0 180) (layer F.Fab))
    (fp_text value 4u7 (at -2.1 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.75 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(C13-Pad1)"))
    (pad 2 smd roundrect (at 0.75 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_housings_sot:SOT-23-5 (layer F.Cu) (tedit 5A97B700)
    (at 37 39.45 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U7 (at 0 0 180) (layer F.Fab))
    (fp_text value 12MHz (at 2.15 -0.05) (layer F.Fab))
    (pad 1 smd roundrect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 2 smd roundrect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(U7-Pad2)"))
    (pad 3 smd roundrect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R7-Pad2)"))
    (pad 4 smd roundrect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 5 smd roundrect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /FTDI_CLK))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module pkl_buttons_switches:SW_SPST_KMR2 (layer F.Cu) (tedit 5A60E855)
    (at 99.4 54.4)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW4 (at 0 0) (layer F.Fab))
    (fp_text value TACT (at 5.6 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.05 -0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 /P2_10x))
    (pad 2 smd roundrect (at -2.05 0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at 2.05 -0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 /P2_10x))
    (pad 2 smd roundrect (at 2.05 0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ../../lib/pkl/packages3d/pkl_buttons_switches.3dshapes/KMR211GLFS.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module pkl_buttons_switches:SW_SPST_KMR2 (layer F.Cu) (tedit 5A60E84A)
    (at 99.4 47.5)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW3 (at 0 0.1) (layer F.Fab))
    (fp_text value TACT (at 5.6 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.05 0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at 2.05 -0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /P2_4x))
    (pad 2 smd roundrect (at -2.05 0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -2.05 -0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /P2_4x))
    (model ../../lib/pkl/packages3d/pkl_buttons_switches.3dshapes/KMR211GLFS.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module pkl_buttons_switches:SW_SPST_KMR2 (layer F.Cu) (tedit 5A60E83C)
    (at 99.4 40.7)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW2 (at 0 0) (layer F.Fab))
    (fp_text value TACT (at 5.6 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.05 0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at 2.05 -0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 /P2_9x))
    (pad 2 smd roundrect (at -2.05 0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -2.05 -0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 /P2_9x))
    (model ../../lib/pkl/packages3d/pkl_buttons_switches.3dshapes/KMR211GLFS.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module pkl_housings_soic:SOIC-8_5.3x5.3mm_Pitch1.27mm (layer F.Cu) (tedit 5A5FEA0C)
    (at 63 58.9)
    (descr "8-Lead Plastic Small Outline (SN) - Wide, 5.20 mm Body [SOIC]")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at 0 -0.6) (layer F.Fab))
    (fp_text value W25Q (at 0 1.5) (layer F.Fab))
    (pad 1 smd roundrect (at -3.4 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 /FLASH_CS))
    (pad 2 smd roundrect (at -3.4 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 120 /FLASH_MISO|IO1))
    (pad 3 smd roundrect (at -3.4 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 /FLASH_~WP~|IO2))
    (pad 4 smd roundrect (at -3.4 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 5 smd roundrect (at 3.4 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 121 /FLASH_MOSI|IO0))
    (pad 6 smd roundrect (at 3.4 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /iCE_SCK))
    (pad 7 smd roundrect (at 3.4 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 123 /FLASH_~HLD~|~RST~|IO3))
    (pad 8 smd roundrect (at 3.4 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIJ-8_5.3x5.3mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 40.4 58.8 270)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C39 (at 0 0 270) (layer F.Fab))
    (fp_text value 1u (at 0 1.2 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 "Net-(C39-Pad1)"))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 40.4 56.9 270)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0.1 0 270) (layer F.Fab))
    (fp_text value 10k (at 0 1.2 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 "Net-(C39-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 57.5 51.6 225)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C36 (at 0 0 225) (layer F.Fab))
    (fp_text value 1u (at -1.555635 0 225) (layer F.Fab))
    (pad 2 smd roundrect (at 0.499999 0 225) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.499999 0 225) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /VCORE))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 56.8 50.9 225)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C37 (at 0 0 225) (layer F.Fab))
    (fp_text value 100n (at -2.192031 0.070711 225) (layer F.Fab))
    (pad 1 smd roundrect (at -0.499999 0 225) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /VCORE))
    (pad 2 smd roundrect (at 0.499999 0 225) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 56.125001 50.2322 225)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C38 (at -0.00509 0.040447 225) (layer F.Fab))
    (fp_text value 10n (at -1.843568 0.040447 225) (layer F.Fab))
    (pad 2 smd roundrect (at 0.499999 0 225) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.499999 0 225) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /VCORE))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3-5mm locked (layer F.Cu) (tedit 5A58B8B3)
    (at 92 55)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.Fab) hide)
    (fp_text value MH3 (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm locked (layer F.Cu) (tedit 5A58B8B3)
    (at 92 40)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.Fab) hide)
    (fp_text value MH3 (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm locked (layer F.Cu) (tedit 5A58B8B3)
    (at 77 32)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.Fab) hide)
    (fp_text value MH3 (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module pkl_buttons_switches:SW_SPST_KMR2 (layer F.Cu) (tedit 5A5A3EC4)
    (at 31.9 55.8 270)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW1 (at 0 0 270) (layer F.Fab))
    (fp_text value TACT (at 0 2.55 270) (layer F.Fab))
    (pad 1 smd roundrect (at -2.05 -0.8) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /~BUTTON))
    (pad 2 smd roundrect (at -2.05 0.8) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at 2.05 -0.8) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /~BUTTON))
    (pad 2 smd roundrect (at 2.05 0.8) (size 0.9 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ../../lib/pkl/packages3d/pkl_buttons_switches.3dshapes/KMR211GLFS.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3-5mm locked (layer F.Cu) (tedit 5A58B8B3)
    (at 33 63)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.Fab) hide)
    (fp_text value MH3 (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm locked (layer F.Cu) (tedit 5A58B8B3)
    (at 77 63)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.Fab) hide)
    (fp_text value MH3 (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3-5mm locked (layer F.Cu) (tedit 5A58B8B3)
    (at 33 32)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.Fab) hide)
    (fp_text value MH3 (at 0 5.00126) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 58.2 52.3 45)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R19 (at 0 0 45) (layer F.Fab))
    (fp_text value 10k (at 1.838478 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /iCE_CRESET))
    (pad 1 smd roundrect (at -0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 70.6 49.1 315)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C35 (at 0 0 315) (layer F.Fab))
    (fp_text value DNP (at 0.565685 -0.989949 315) (layer F.Fab))
    (pad 2 smd roundrect (at 0.499999 0 315) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.499999 0 315) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(C35-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_connectors:Connector_USB_Micro_B_SMD locked (layer F.Cu) (tedit 5A77A473)
    (at 31.5 47.5 180)
    (fp_text reference P1 (at 4 0 270) (layer F.Fab))
    (fp_text value pkl_USB_OTG (at 2.1 -0.1 270) (layer F.Fab) hide)
    (pad GND smd roundrect (at 0 1.2 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /shield))
    (pad GND smd roundrect (at 0 -1.2 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /shield))
    (pad GND smd roundrect (at 0 -3.8 270) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /shield))
    (pad GND smd roundrect (at 0 3.8 270) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /shield))
    (pad GND smd roundrect (at -2.55 -3.1 270) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /shield))
    (pad GND smd roundrect (at -2.55 3.1 270) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /shield))
    (pad 1 smd roundrect (at -2.675 1.3 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
    (pad 2 smd roundrect (at -2.675 0.65 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 117 /USB_DM))
    (pad 3 smd roundrect (at -2.675 0 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 116 /USB_DP))
    (pad 4 smd roundrect (at -2.675 -0.65 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(P1-Pad4)"))
    (pad 5 smd roundrect (at -2.675 -1.3 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.step
      (offset (xyz -1.2 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 65.8 41 45)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C23 (at -0.070711 0.070711 45) (layer F.Fab))
    (fp_text value 1u (at 1.555635 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /VCORE))
    (pad 2 smd roundrect (at 0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 5A7CF196)
    (at 37.2 41.75)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at -0.1 0) (layer F.Fab))
    (fp_text value 100n (at 2 0.05 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 44.4 59.2 180)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0.1 0 180) (layer F.Fab))
    (fp_text value 10n (at -1.9 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 5A77A4E4)
    (at 45.1 38.5 90)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 0 90) (layer F.Fab))
    (fp_text value 100n (at 0.3 0.9 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 5A7CF0FD)
    (at 47.7 53.6 270)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C19 (at 0 0 270) (layer F.Fab))
    (fp_text value 100n (at 1.4 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 66.5 41.7 45)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C25 (at 0 0 45) (layer F.Fab))
    (fp_text value 100n (at 2.192031 -0.070711 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /VCORE))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 69.7 44.9 45)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C26 (at 0 0 45) (layer F.Fab))
    (fp_text value 100n (at 2.262742 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 /VCCPLL))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 56.1 46.2 315)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C27 (at -1.979899 0 315) (layer F.Fab))
    (fp_text value 100n (at 0.070711 1.06066 315) (layer F.Fab))
    (pad 1 smd roundrect (at -0.499999 0 315) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 2 smd roundrect (at 0.499999 0 315) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 /VCCIO_2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 67.2 42.4 45)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C28 (at 0 0 45) (layer F.Fab))
    (fp_text value 10n (at 1.909188 -0.070711 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /VCORE))
    (pad 2 smd roundrect (at 0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 68.9 50.8 135)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C29 (at 0 0 135) (layer F.Fab))
    (fp_text value 100n (at -2.192031 -0.070711 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.499999 0 135) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.499999 0 135) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 68.2 51.5 315)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C31 (at 0 0 315) (layer F.Fab))
    (fp_text value 100n (at 2.192031 0.070711 315) (layer F.Fab))
    (pad 2 smd roundrect (at 0.499999 0 315) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.499999 0 315) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 /VCCIO_0|1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 65.1 40.3 45)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C30 (at 0 0 45) (layer F.Fab))
    (fp_text value 100n (at 2.192031 -0.070711 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 /VCCIO_0|1))
    (pad 2 smd roundrect (at 0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 50.5 49.2)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at 0 0) (layer F.Fab))
    (fp_text value 100n (at 0.2 1) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 +1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 48.1 40.4 90)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0 0 90) (layer F.Fab))
    (fp_text value 100n (at 2.2 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 +1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 52.6 59.1 180)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at -1.9 -0.1 180) (layer F.Fab))
    (fp_text value 10n (at 0 -0.1 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C11-Pad1)"))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 37.2 43.75 180)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0 0 180) (layer F.Fab))
    (fp_text value 100n (at -2.2 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 37.2 49.25 180)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 0 -0.1 180) (layer F.Fab))
    (fp_text value 100n (at -2.2 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(C13-Pad1)"))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 37.2 51.25 180)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 0 0 180) (layer F.Fab))
    (fp_text value 100n (at -2.2 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 +1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 5A7CF187)
    (at 40.1 40.4 90)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C17 (at 0 0 270) (layer F.Fab))
    (fp_text value 100n (at 0 -0.9 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 +1V8))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 41.7 53.6 270)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C18 (at 0 0 270) (layer F.Fab))
    (fp_text value 100n (at 0 0.9 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 50.5 46.2)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C20 (at 0 0) (layer F.Fab))
    (fp_text value 100n (at 2.2 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 5A77A51A)
    (at 45.1 40.4 90)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C21 (at 0 0 90) (layer F.Fab))
    (fp_text value 100n (at -1.4 0.1 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0402 (layer F.Cu) (tedit 552C58AA)
    (at 65.9 55.5 180)
    (descr "Capacitor SMD 0402, reflow soldering")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C22 (at 0 0 180) (layer F.Fab))
    (fp_text value 100n (at -0.1 0.9 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0603 (layer F.Cu) (tedit 552C8666)
    (at 68.9 43.8 45)
    (descr "Capacitor SMD 0603, reflow soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at 0 0 45) (layer F.Fab))
    (fp_text value 10u (at 2.12132 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.75 0 45) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 /VCCPLL))
    (pad 2 smd roundrect (at 0.75 0 45) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0603 (layer F.Cu) (tedit 552C8666)
    (at 44.4 54.7 180)
    (descr "Capacitor SMD 0603, reflow soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 0 180) (layer F.Fab))
    (fp_text value 4u7 (at 0 1.2 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.75 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0603 (layer F.Cu) (tedit 5A7CF0DF)
    (at 41.7 57.1 270)
    (descr "Capacitor SMD 0603, reflow soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 0 270) (layer F.Fab))
    (fp_text value 4u7 (at 1.6 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0603 (layer F.Cu) (tedit 552C8666)
    (at 48.7 35.75 90)
    (descr "Capacitor SMD 0603, reflow soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C32 (at 0 0 90) (layer F.Fab))
    (fp_text value DNP (at 2.2 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.75 0 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 2 smd roundrect (at 0.75 0 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0603 (layer F.Cu) (tedit 552C8666)
    (at 71.6 35.75 90)
    (descr "Capacitor SMD 0603, reflow soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C33 (at 0 0 90) (layer F.Fab))
    (fp_text value DNP (at 2.2 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.75 0 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.75 0 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0603 (layer F.Cu) (tedit 5A7CF0EC)
    (at 50 57.1 270)
    (descr "Capacitor SMD 0603, reflow soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 0 270) (layer F.Fab))
    (fp_text value 4u7 (at 1.6 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
    (pad 2 smd roundrect (at 0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0603 (layer F.Cu) (tedit 552C8666)
    (at 52.6 54.6 180)
    (descr "Capacitor SMD 0603, reflow soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 0 180) (layer F.Fab))
    (fp_text value 4u7 (at 0 1.2 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.75 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.75 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:C_0603 (layer F.Cu) (tedit 552C8666)
    (at 73.2 52.6)
    (descr "Capacitor SMD 0603, reflow soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at 0 0) (layer F.Fab))
    (fp_text value DNP (at 2.2 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.75 0) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 2 smd roundrect (at 0.75 0) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:D_0603 (layer F.Cu) (tedit 5568E1FC)
    (at 37 56.6 180)
    (descr "Diode SMD 0603, reflow soldering")
    (tags "diode led 0603")
    (attr smd)
    (fp_text reference D5 (at 0 0) (layer F.Fab))
    (fp_text value RED (at 2.1 0 180) (layer F.Fab))
    (pad C smd roundrect (at -0.75 0) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /~LEDR))
    (pad A smd roundrect (at 0.75 0) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(D5-PadA)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:D_0603 (layer F.Cu) (tedit 5568E1FC)
    (at 92.4 50.5 180)
    (descr "Diode SMD 0603, reflow soldering")
    (tags "diode led 0603")
    (attr smd)
    (fp_text reference D9 (at 0 0 180) (layer F.Fab))
    (fp_text value GRN (at 0 -1.3 180) (layer F.Fab))
    (pad C smd roundrect (at -0.75 0) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad A smd roundrect (at 0.75 0) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(D9-PadA)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:D_0603 (layer F.Cu) (tedit 5568E1FC)
    (at 92.4 47.5 90)
    (descr "Diode SMD 0603, reflow soldering")
    (tags "diode led 0603")
    (attr smd)
    (fp_text reference D8 (at 0 0 90) (layer F.Fab))
    (fp_text value RED (at 0 -1.2 90) (layer F.Fab))
    (pad C smd roundrect (at -0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad A smd roundrect (at 0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(D8-PadA)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:D_0603 (layer F.Cu) (tedit 5568E1FC)
    (at 92.4 44.5 180)
    (descr "Diode SMD 0603, reflow soldering")
    (tags "diode led 0603")
    (attr smd)
    (fp_text reference D7 (at 0 0 180) (layer F.Fab))
    (fp_text value GRN (at 0 -1.2 180) (layer F.Fab))
    (pad C smd roundrect (at -0.75 0) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad A smd roundrect (at 0.75 0) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(D7-PadA)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:D_0603 (layer F.Cu) (tedit 5568E1FC)
    (at 89.4 47.5 90)
    (descr "Diode SMD 0603, reflow soldering")
    (tags "diode led 0603")
    (attr smd)
    (fp_text reference D6 (at 0 0 270) (layer F.Fab))
    (fp_text value GRN (at -1.7 0.2 180) (layer F.Fab))
    (pad A smd roundrect (at 0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(D6-PadA)"))
    (pad C smd roundrect (at -0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:D_0603 (layer F.Cu) (tedit 5568E1FC)
    (at 37 55 180)
    (descr "Diode SMD 0603, reflow soldering")
    (tags "diode led 0603")
    (attr smd)
    (fp_text reference D4 (at 0 0) (layer F.Fab))
    (fp_text value GRN (at 2.2 0 180) (layer F.Fab))
    (pad A smd roundrect (at 0.75 0) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(D4-PadA)"))
    (pad C smd roundrect (at -0.75 0) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /~LEDG))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:D_0603 (layer F.Cu) (tedit 5A7CF141)
    (at 56.7 58.25 90)
    (descr "Diode SMD 0603, reflow soldering")
    (tags "diode led 0603")
    (attr smd)
    (fp_text reference D3 (at -0.05 0 90) (layer F.Fab))
    (fp_text value BLU (at -1.65 0 180) (layer F.Fab))
    (pad C smd roundrect (at -0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad A smd roundrect (at 0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /iCE_CDONE))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:D_0603 (layer F.Cu) (tedit 5568E1FC)
    (at 69.9 50.1 315)
    (descr "Diode SMD 0603, reflow soldering")
    (tags "diode led 0603")
    (attr smd)
    (fp_text reference D2 (at 0 0 315) (layer F.Fab))
    (fp_text value CDBU0520 (at 1.697056 -1.838478 45) (layer F.Fab))
    (pad C smd roundrect (at -0.75 0 135) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(C35-Pad1)"))
    (pad A smd roundrect (at 0.75 0 135) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:D_0603 (layer F.Cu) (tedit 5568E1FC)
    (at 31.6 40.3 270)
    (descr "Diode SMD 0603, reflow soldering")
    (tags "diode led 0603")
    (attr smd)
    (fp_text reference D1 (at 0 0 270) (layer F.Fab))
    (fp_text value GRN (at -2.3 -0.1 270) (layer F.Fab))
    (pad C smd roundrect (at -0.75 0 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad A smd roundrect (at 0.75 0 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(D1-PadA)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:D_0603 (layer F.Cu) (tedit 5568E1FC)
    (at 95.4 47.5 90)
    (descr "Diode SMD 0603, reflow soldering")
    (tags "diode led 0603")
    (attr smd)
    (fp_text reference D10 (at 0 0 90) (layer F.Fab))
    (fp_text value GRN (at 1.6 0.1 180) (layer F.Fab))
    (pad C smd roundrect (at -0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad A smd roundrect (at 0.75 0 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(D10-PadA)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:L_0402 (layer F.Cu) (tedit 552C745C)
    (at 37.2 42.75)
    (descr "Inductor SMD 0402, reflow soldering")
    (tags "inductor 0402")
    (attr smd)
    (fp_text reference L2 (at -0.1 0) (layer F.Fab))
    (fp_text value 600 (at 1.9 0.05) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C12-Pad1)"))
    (pad 1 smd roundrect (at -0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:L_0402 (layer F.Cu) (tedit 552C745C)
    (at 37.2 50.25)
    (descr "Inductor SMD 0402, reflow soldering")
    (tags "inductor 0402")
    (attr smd)
    (fp_text reference L1 (at 0 0) (layer F.Fab))
    (fp_text value 600 (at 1.9 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 34.9 40.3 90)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 0 90) (layer F.Fab))
    (fp_text value 10k (at 1.8 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 37 58)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at 0 0) (layer F.Fab))
    (fp_text value 330E (at -2.2 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(D5-PadA)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 37 53.5)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R14 (at 0 0) (layer F.Fab))
    (fp_text value 330E (at 2.2 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(D4-PadA)"))
    (pad 2 smd roundrect (at 0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 31.9 59.1)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at 0 0) (layer F.Fab))
    (fp_text value 10k (at 0 1.2) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /~BUTTON))
    (pad 2 smd roundrect (at 0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 58 57.95 90)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at 0 0 90) (layer F.Fab))
    (fp_text value 2k2 (at -1.85 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /iCE_CDONE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 67.9 43.1 45)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 0 0 45) (layer F.Fab))
    (fp_text value 100E (at 2.12132 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /VCORE))
    (pad 1 smd roundrect (at -0.499999 0 45) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 /VCCPLL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 37.2 52.25 180)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at 0 0 180) (layer F.Fab))
    (fp_text value 10k (at -1.9 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(R9-Pad1)"))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 37.2 46.25 180)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 0 0 180) (layer F.Fab))
    (fp_text value 12k (at -1.9 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 42.7 37)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 0) (layer F.Fab))
    (fp_text value 2k2 (at 1.9 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(R6-Pad1)"))
    (pad 2 smd roundrect (at 0.5 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(R2-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 32.9 40.3 270)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 0 270) (layer F.Fab))
    (fp_text value 330E (at -2.3 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(D1-PadA)"))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 93.9 47.5 90)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at 0 0.1 90) (layer F.Fab))
    (fp_text value 330E (at 2.2 0.3 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 /P2_7x))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(D8-PadA)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_dipol:R_0402 (layer F.Cu) (tedit 552C709B)
    (at 33.9 40.3 270)
    (descr "Resistor SMD 0402, reflow soldering")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 0 270) (layer F.Fab))
    (fp_text value 1M (at -1.7 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /shield))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_housings_dfn_qfn:QFN-48-1EP_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 5A7CF2E7)
    (at 62.2 47.5 135)
    (descr "UK Package; 48-Lead Plastic QFN (7mm x 7mm); (see Linear Technology QFN_48_05-08-1704.pdf)")
    (tags "QFN 0.5")
    (solder_mask_margin 0.075)
    (attr smd)
    (fp_text reference U6 (at 0 0 180) (layer F.Fab))
    (fp_text value ICE5LP4K-SG48 (at -0.777817 -0.777817 180) (layer F.Fab))
    (pad 1 smd oval (at 2.75 -3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 127 /VCCIO_2))
    (pad 2 smd oval (at 2.25 -3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 63 /P1A2))
    (pad 3 smd oval (at 1.75 -3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 62 /P1A7))
    (pad 4 smd oval (at 1.25 -3.400001 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 /P1A1))
    (pad 5 smd oval (at 0.75 -3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 130 /VCORE))
    (pad 6 smd oval (at 0.25 -3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 119 /Rx_TTL|FIFO_D0))
    (pad 7 smd oval (at -0.25 -3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /iCE_CDONE))
    (pad 8 smd oval (at -0.75 -3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 /iCE_CRESET))
    (pad 9 smd oval (at -1.25 -3.400001 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 118 /Tx_TTL|FIFO_D1))
    (pad 10 smd oval (at -1.75 -3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /~BUTTON))
    (pad 11 smd oval (at -2.25 -3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /~LEDR))
    (pad 12 smd oval (at -2.75 -3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 122 /FLASH_~WP~|IO2))
    (pad 13 smd oval (at -3.4 -2.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 123 /FLASH_~HLD~|~RST~|IO3))
    (pad 14 smd oval (at -3.4 -2.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 132 /iCE_SO))
    (pad 15 smd oval (at -3.4 -1.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 /iCE_SCK))
    (pad 16 smd oval (at -3.400001 -1.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /iCE_SS_B))
    (pad 17 smd oval (at -3.4 -0.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 133 /iCE_SI))
    (pad 18 smd oval (at -3.4 -0.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /P2_10))
    (pad 19 smd oval (at -3.4 0.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /P2_4))
    (pad 20 smd oval (at -3.4 0.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /P2_9))
    (pad 21 smd oval (at -3.400001 1.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /P2_3))
    (pad 22 smd oval (at -3.4 1.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 128 /VCCIO_0|1))
    (pad 23 smd oval (at -3.4 2.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /P2_8))
    (pad 24 smd oval (at -3.4 2.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(C35-Pad1)"))
    (pad 25 smd oval (at -2.75 3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /P2_2))
    (pad 26 smd oval (at -2.25 3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /P2_7))
    (pad 27 smd oval (at -1.75 3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /P2_1))
    (pad 28 smd oval (at -1.25 3.400001 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 /P1B10))
    (pad 29 smd oval (at -0.75 3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 129 /VCCPLL))
    (pad 30 smd oval (at -0.25 3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 130 /VCORE))
    (pad 31 smd oval (at 0.25 3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 60 /P1B4))
    (pad 32 smd oval (at 0.75 3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 /P1B9))
    (pad 33 smd oval (at 1.25 3.400001 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 128 /VCCIO_0|1))
    (pad 34 smd oval (at 1.75 3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 76 /P1B3))
    (pad 35 smd oval (at 2.25 3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /FTDI_CLK))
    (pad 36 smd oval (at 2.75 3.4 45) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 /P1B8))
    (pad 37 smd oval (at 3.4 2.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /~LEDG))
    (pad 38 smd oval (at 3.4 2.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 /P1B2))
    (pad 39 smd oval (at 3.4 1.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 69 /~LED_RED))
    (pad 40 smd oval (at 3.400001 1.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 70 /~LED_GRN))
    (pad 41 smd oval (at 3.4 0.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 71 /~LED_BLU))
    (pad 42 smd oval (at 3.4 0.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 73 /P1B7))
    (pad 43 smd oval (at 3.4 -0.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 /P1B1))
    (pad 44 smd oval (at 3.4 -0.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 68 /P1A10))
    (pad 45 smd oval (at 3.400001 -1.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 67 /P1A4))
    (pad 46 smd oval (at 3.4 -1.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 66 /P1A9))
    (pad 47 smd oval (at 3.4 -2.25 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 65 /P1A3))
    (pad 48 smd oval (at 3.4 -2.75 135) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 64 /P1A8))
    (pad 49 smd rect (at -2.1 2.1 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.7 2.1 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.7 2.1 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 2.1 2.1 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -2.1 0.7 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.7 0.7 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.7 0.7 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 2.1 0.7 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -2.1 -0.7 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.7 -0.7 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.7 -0.7 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 2.1 -0.7 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -2.1 -2.1 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.7 -2.1 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.7 -2.1 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 2.1 -2.1 45) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 thru_hole circle (at 0 0 45) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 26 GND) (zone_connect 2))
    (pad 49 thru_hole circle (at 1.399999 0 45) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 26 GND) (zone_connect 2))
    (pad 49 thru_hole circle (at 1.4 1.4 45) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 26 GND) (zone_connect 2))
    (pad 49 thru_hole circle (at 0 1.399999 45) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 26 GND) (zone_connect 2))
    (pad 49 thru_hole circle (at -1.4 1.4 45) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 26 GND) (zone_connect 2))
    (pad 49 thru_hole circle (at -1.399999 0 45) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 26 GND) (zone_connect 2))
    (pad 49 thru_hole circle (at -1.4 -1.4 45) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 26 GND) (zone_connect 2))
    (pad 49 thru_hole circle (at 0 -1.399999 45) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 26 GND) (zone_connect 2))
    (pad 49 thru_hole circle (at 1.4 -1.4 45) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 26 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_housings_dfn_qfn:QFN-64-4.45mm1EP_9x9mm_Pitch0.5mm (layer F.Cu) (tedit 5A666374)
    (at 44.35 47.5)
    (descr "FTDI FT2232HQ Footprint Spec")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U4 (at 0 0) (layer F.Fab))
    (fp_text value FT2232H (at 0 1.3) (layer F.Fab))
    (pad 1 smd oval (at -4.575 -3.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 2 smd oval (at -4.575 -3.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 /FTDI_CLK))
    (pad 3 smd oval (at -4.575 -2.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U4-Pad3)"))
    (pad 4 smd oval (at -4.575 -2.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C12-Pad1)"))
    (pad 5 smd oval (at -4.575 -1.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 6 smd oval (at -4.575 -1.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R8-Pad1)"))
    (pad 7 smd oval (at -4.575 -0.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 117 /USB_DM))
    (pad 8 smd oval (at -4.575 -0.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 116 /USB_DP))
    (pad 9 smd oval (at -4.575 0.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C13-Pad1)"))
    (pad 10 smd oval (at -4.575 0.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 11 smd oval (at -4.575 1.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 12 smd oval (at -4.575 1.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 +1V8))
    (pad 13 smd oval (at -4.575 2.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 14 smd oval (at -4.575 2.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R9-Pad1)"))
    (pad 15 smd oval (at -4.575 3.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 16 smd oval (at -4.575 3.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 /iCE_SCK))
    (pad 17 smd oval (at -3.75 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 121 /FLASH_MOSI|IO0))
    (pad 18 smd oval (at -3.25 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 120 /FLASH_MISO|IO1))
    (pad 19 smd oval (at -2.75 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U4-Pad19)"))
    (pad 20 smd oval (at -2.25 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 21 smd oval (at -1.75 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /iCE_SS_B))
    (pad 22 smd oval (at -1.25 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U4-Pad22)"))
    (pad 23 smd oval (at -0.75 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 /iCE_CDONE))
    (pad 24 smd oval (at -0.25 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 131 /xiCE_CRESET))
    (pad 25 smd oval (at 0.25 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 26 smd oval (at 0.75 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U4-Pad26)"))
    (pad 27 smd oval (at 1.25 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U4-Pad27)"))
    (pad 28 smd oval (at 1.75 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U4-Pad28)"))
    (pad 29 smd oval (at 2.25 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U4-Pad29)"))
    (pad 30 smd oval (at 2.75 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U4-Pad30)"))
    (pad 31 smd oval (at 3.25 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 32 smd oval (at 3.75 4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U4-Pad32)"))
    (pad 33 smd oval (at 4.575 3.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U4-Pad33)"))
    (pad 34 smd oval (at 4.575 3.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U4-Pad34)"))
    (pad 35 smd oval (at 4.575 2.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 36 smd oval (at 4.575 2.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U4-Pad36)"))
    (pad 37 smd oval (at 4.575 1.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 +1V8))
    (pad 38 smd oval (at 4.575 1.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 126 /xFIFO_D0))
    (pad 39 smd oval (at 4.575 0.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 125 /xFIFO_D1))
    (pad 40 smd oval (at 4.575 0.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /xFIFO_D2))
    (pad 41 smd oval (at 4.575 -0.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /xFIFO_D3))
    (pad 42 smd oval (at 4.575 -0.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 43 smd oval (at 4.575 -1.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /xFIFO_D4))
    (pad 44 smd oval (at 4.575 -1.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /xFIFO_D5))
    (pad 45 smd oval (at 4.575 -2.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /xFIFO_D6))
    (pad 46 smd oval (at 4.575 -2.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /xFIFO_D7))
    (pad 47 smd oval (at 4.575 -3.25) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 48 smd oval (at 4.575 -3.75) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /xFIFO_~RXF))
    (pad 49 smd oval (at 3.75 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 +1V8))
    (pad 50 smd oval (at 3.25 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 51 smd oval (at 2.75 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 52 smd oval (at 2.25 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 /xFIFO_~TXE))
    (pad 53 smd oval (at 1.75 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /xFIFO_~RD))
    (pad 54 smd oval (at 1.25 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /xFIFO_~WR))
    (pad 55 smd oval (at 0.75 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /xFIFO_WKUP))
    (pad 56 smd oval (at 0.25 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 57 smd oval (at -0.25 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U4-Pad57)"))
    (pad 58 smd oval (at -0.75 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U4-Pad58)"))
    (pad 59 smd oval (at -1.25 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U4-Pad59)"))
    (pad 60 smd oval (at -1.75 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U4-Pad60)"))
    (pad 61 smd oval (at -2.25 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R6-Pad1)"))
    (pad 62 smd oval (at -2.75 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R2-Pad1)"))
    (pad 63 smd oval (at -3.25 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(R2-Pad3)"))
    (pad 64 smd oval (at -3.75 -4.575 90) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 +1V8))
    (pad 65 smd rect (at 1.1125 -1.1125) (size 2.225 2.225) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -1.1125 -1.1125) (size 2.225 2.225) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 1.1125 1.1125) (size 2.225 2.225) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -1.1125 1.1125) (size 2.225 2.225) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (solder_paste_margin_ratio -0.2))
    (pad 65 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 26 GND))
    (pad 65 thru_hole circle (at -1.9 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 26 GND))
    (pad 65 thru_hole circle (at -1.9 -1.9) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 26 GND))
    (pad 65 thru_hole circle (at 1.9 -1.9) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 26 GND))
    (pad 65 thru_hole circle (at 0 -1.9) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 26 GND))
    (pad 65 thru_hole circle (at 1.9 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 26 GND))
    (pad 65 thru_hole circle (at 1.9 1.9) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 26 GND))
    (pad 65 thru_hole circle (at 0 1.9) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 26 GND))
    (pad 65 thru_hole circle (at -1.9 1.9) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 26 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-64-1EP_9x9mm_P0.5mm_EP7.35x7.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_housings_sot:SOT-23-5 (layer F.Cu) (tedit 5A53FC6B)
    (at 52.6 57 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 0 -0.8 180) (layer F.Fab))
    (fp_text value 1V2 (at 0 0.6 180) (layer F.Fab))
    (pad 1 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
    (pad 2 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 3 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
    (pad 4 smd roundrect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C11-Pad1)"))
    (pad 5 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +1V2))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module pkl_housings_sot:SOT-23-5 (layer F.Cu) (tedit 5A53FC59)
    (at 44.4 57.1 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0 -0.9 180) (layer F.Fab))
    (fp_text value 3.3V (at 0 0.5 180) (layer F.Fab))
    (pad 5 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 4 smd roundrect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(C3-Pad1)"))
    (pad 3 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 "Net-(C39-Pad1)"))
    (pad 2 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 1 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module pkl_housings_sot:SOT-23-6 (layer F.Cu) (tedit 5A77A4C9)
    (at 42.7 39.3 90)
    (descr "6-pin SOT23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 0 180) (layer F.Fab))
    (fp_text value 93C46B-SOT-23-6 (at -0.6 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(R2-Pad5)"))
    (pad 2 smd roundrect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 3 smd roundrect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(R6-Pad1)"))
    (pad 4 smd roundrect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R2-Pad1)"))
    (pad 6 smd roundrect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 5 smd roundrect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(R2-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1v2 (at 46.21 62.74) (layer F.SilkS))
  (gr_text B (at 46.21 60.835) (layer F.SilkS))
  (gr_text G (at 43.67 63.121) (layer F.SilkS))
  (gr_text R (at 43.67 60.835) (layer F.SilkS))
  (gr_text 5v0 (at 51.925 63.375) (layer F.SilkS))
  (gr_text 3v3 (at 52.052 60.835) (layer F.SilkS))
  (gr_text ~CS (at 55.1 62.359) (layer F.SilkS))
  (gr_text "GND\nGND" (at 47.5 58.8) (layer B.SilkS))
  (gr_text SCK (at 57.64 62.359) (layer F.SilkS))
  (gr_text IO0 (at 60.18 62.359) (layer F.SilkS))
  (gr_text IO1 (at 62.72 62.359) (layer F.SilkS))
  (gr_text IO2 (at 65.26 62.359) (layer F.SilkS))
  (gr_text IO3 (at 67.8 62.359) (layer F.SilkS))
  (gr_text GND (at 70.34 62.359) (layer F.SilkS))
  (gr_text CRESET (at 68.181 57.66 270) (layer B.SilkS))
  (gr_text GND (at 89.136 51.31) (layer B.SilkS))
  (gr_text 3v3 (at 89.009 53.85) (layer B.SilkS))
  (gr_text 3v3 (at 89.009 53.85) (layer F.SilkS))
  (gr_text GND (at 89.136 51.31) (layer F.SilkS))
  (gr_text 1 (at 86.85 39.626 270) (layer F.SilkS))
  (gr_text 7 (at 84.31 39.626 270) (layer F.SilkS))
  (gr_text 6 (at 86.85 55.5 270) (layer F.SilkS))
  (gr_text 12 (at 84.31 56.009 270) (layer F.SilkS))
  (gr_text CRESET (at 68.181 57.66 270) (layer F.SilkS))
  (gr_text 6 (at 75.42 55.628 270) (layer B.SilkS))
  (gr_text 12 (at 77.96 56.009 270) (layer B.SilkS))
  (gr_text 6 (at 75.42 55.628 270) (layer F.SilkS))
  (gr_text 12 (at 77.96 56.009 270) (layer F.SilkS))
  (gr_text GND (at 47.353 35.689 270) (layer F.SilkS))
  (gr_text 3v3 (at 50.147 35.55 270) (layer F.SilkS))
  (gr_text GND (at 70.213 35.689 270) (layer F.SilkS))
  (gr_text 3v3 (at 73.007 35.55 270) (layer F.SilkS))
  (gr_text GND (at 73.261 51.183) (layer F.SilkS))
  (gr_text 3v3 (at 73.388 53.977) (layer F.SilkS))
  (gr_text 12 (at 84.31 56.009 270) (layer B.SilkS))
  (gr_text 6 (at 86.85 55.5 270) (layer B.SilkS))
  (gr_text 7 (at 84.31 39.626 270) (layer B.SilkS))
  (gr_text 1 (at 86.85 39.626 270) (layer B.SilkS))
  (gr_text 1 (at 75.42 39.372 270) (layer F.SilkS))
  (gr_text 7 (at 77.96 39.372 270) (layer F.SilkS))
  (gr_text 12 (at 74.785 29.974) (layer F.SilkS))
  (gr_text 6 (at 74.658 33.53) (layer F.SilkS))
  (gr_text 12 (at 52.179 30.99) (layer F.SilkS))
  (gr_text 6 (at 51.798 33.53) (layer F.SilkS))
  (gr_text 1 (at 58.402 33.53) (layer F.SilkS))
  (gr_text 7 (at 58.402 30.99) (layer F.SilkS))
  (gr_text 1 (at 35.542 33.53) (layer F.SilkS))
  (gr_text 7 (at 35.542 30.99) (layer F.SilkS))
  (gr_text 3v3 (at 73.388 53.85) (layer B.SilkS))
  (gr_text GND (at 73.261 51.31) (layer B.SilkS))
  (gr_text 3v3 (at 50.02 35.562 270) (layer B.SilkS))
  (gr_text GND (at 47.48 35.689 90) (layer B.SilkS))
  (gr_text 7 (at 77.96 39.372 270) (layer B.SilkS))
  (gr_text 1 (at 75.42 39.372 270) (layer B.SilkS))
  (gr_text 3v3 (at 72.88 35.562 270) (layer B.SilkS))
  (gr_text GND (at 70.213 35.689 90) (layer B.SilkS))
  (gr_text 12 (at 74.785 29.974) (layer B.SilkS))
  (gr_text 1 (at 58.402 33.53) (layer B.SilkS))
  (gr_text 7 (at 58.402 30.99) (layer B.SilkS))
  (gr_text 6 (at 74.658 33.53) (layer B.SilkS))
  (gr_text 7 (at 35.55 31) (layer B.SilkS))
  (gr_text 12 (at 52.179 30.99) (layer B.SilkS))
  (gr_text 6 (at 51.798 33.53) (layer B.SilkS))
  (gr_text 1 (at 35.55 33.55) (layer B.SilkS))
  (gr_text "1B2 (C) 2018\nCC-BY-SA 4.0\n" (at 35.15 58.25 315) (layer B.SilkS))
  (gr_text GND (at 34.4 51.3) (layer B.SilkS))
  (gr_text DP (at 34.25 48.75) (layer B.SilkS))
  (gr_text DM (at 34.25 46.2) (layer B.SilkS))
  (gr_text 5V (at 34.25 43.75) (layer B.SilkS))
  (gr_text "RED\nGRN" (at 42.4 58.8) (layer B.SilkS))
  (gr_text "BLU\n1V2" (at 44.95 58.8) (layer B.SilkS))
  (gr_text "3v3\n5v" (at 50.1 58.8) (layer B.SilkS))
  (gr_text ~CS (at 55.1 62.105) (layer B.SilkS))
  (gr_text SCK (at 57.64 62.105) (layer B.SilkS))
  (gr_text IO0 (at 60.18 62.105) (layer B.SilkS))
  (gr_text IO1 (at 62.72 62.105) (layer B.SilkS))
  (gr_text IO2 (at 65.26 62.105) (layer B.SilkS))
  (gr_text IO3 (at 67.8 62.105) (layer B.SilkS))
  (gr_text GND (at 70.34 62.105) (layer B.SilkS))
  (gr_text "(C) 2018\n1Bitsquared" (at 52.7 42.4) (layer F.SilkS))
  (gr_text 1Bitsquared (at 42.1 51) (layer B.SilkS))
  (gr_text CDONE (at 56.7 56.7) (layer F.SilkS))
  (gr_text UBUTTON (at 34.2 55.8 270) (layer F.SilkS))
  (gr_text R (at 39.1 56.6) (layer F.SilkS))
  (gr_text G (at 39.1 55) (layer F.SilkS))
  (gr_text L5 (at 92.4 49.3) (layer F.SilkS))
  (gr_text L4 (at 92.3 43.3) (layer F.SilkS))
  (gr_text L3 (at 95.4 45.8) (layer F.SilkS))
  (gr_text L2 (at 89.4 49.3) (layer F.SilkS))
  (gr_text L1 (at 92.4 45.8) (layer F.SilkS))
  (gr_text "Button 3" (at 99.4 51.9) (layer F.SilkS))
  (gr_text "Button 2" (at 99.4 45) (layer F.SilkS))
  (gr_text "Button 1" (at 99.4 38.1) (layer F.SilkS))
  (gr_text V1.0a (at 97.2 47.5 270) (layer B.SilkS))
  (gr_text iCEBreaker (at 99.5 47.6 270) (layer B.SilkS))
  (gr_text PMOD (at 85.58 38.356) (layer F.SilkS))
  (gr_text PMOD (at 85.58 38.356) (layer B.SilkS))
  (gr_text +5V (at 73.134 58.93 270) (layer F.SilkS))
  (gr_text RGBLED (at 40.241 62.74 270) (layer F.SilkS))
  (gr_text FLASH (at 72.753 63.502 270) (layer F.SilkS))
  (gr_text PMOD2 (at 72.88 44.96 270) (layer F.SilkS))
  (gr_text PMOD1B (at 63.99 35.816) (layer F.SilkS))
  (gr_text +5V (at 55.1 35.816) (layer F.SilkS))
  (gr_text PMOD1A (at 41.13 35.816) (layer F.SilkS))
  (gr_text V1.0a (at 55.8 39.9) (layer B.SilkS))
  (gr_text iCEBreaker (at 53.7 37.9) (layer B.SilkS))
  (gr_text +5V (at 55.1 35.816) (layer B.SilkS))
  (gr_text +5V (at 73.134 58.93 270) (layer B.SilkS))
  (gr_text FLASH (at 60.2 57.1) (layer B.SilkS))
  (gr_text FPGA (at 60.2 58.2) (layer B.SilkS))
  (gr_text FPGA (at 60.2 60.4) (layer B.SilkS))
  (gr_text FLASH (at 60.2 59.3) (layer B.SilkS))
  (gr_text FLASH (at 72.8 63.5 270) (layer B.SilkS))
  (gr_text RGBLED (at 40.241 62.74 270) (layer B.SilkS))
  (gr_text PMOD2 (at 72.88 44.96 270) (layer B.SilkS))
  (gr_text PMOD1B (at 63.99 35.816) (layer B.SilkS))
  (gr_text PMOD1A (at 41.13 35.816) (layer B.SilkS))
  (gr_text VPLL (at 70.2 42.5 315) (layer F.SilkS))
  (gr_text VCORE (at 51.6 56.1) (layer B.SilkS))
  (gr_text VCCIO2 (at 55.3 43.4 315) (layer B.SilkS))
  (gr_text VCCIO0&1 (at 67.165 40.388 45) (layer B.SilkS))
  (gr_text "Jump for FTDI FIFO" (at 49.1 47.8 270) (layer B.SilkS))
  (gr_text PWR (at 31.6 37.4 270) (layer F.SilkS))
  (gr_line (start 80 45.5) (end 80 49.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82 45.5) (end 82 49.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 81 49.5) (end 80 49.5) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 81 45.5) (end 82 45.5) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82 38.2) (end 82 42) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 83 38.2) (end 83 37.2) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 81 42) (end 80 42) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82 56.8) (end 82 53) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 83 56.8) (end 82 56.8) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 81 53) (end 82 53) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_text V1.0a (at 52.1 39.9) (layer F.SilkS))
  (gr_text iCEBreaker (at 52.2 37.9) (layer F.SilkS))
  (gr_arc (start 32 64) (end 30 64) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 32 31) (end 32 29) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 78 31) (end 80 31) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102 56.8) (end 102 57.8) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102 38.2) (end 103 38.2) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 78 64) (end 78 66) (angle -90) (layer Edge.Cuts) (width 0.15))
  (dimension 37 (width 0.3) (layer Dwgs.User)
    (gr_text "37.000 mm" (at 22.750001 47.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 30 66) (xy 21.400001 66)))
    (feature2 (pts (xy 30 29) (xy 21.400001 29)))
    (crossbar (pts (xy 24.100001 29) (xy 24.100001 66)))
    (arrow1a (pts (xy 24.100001 66) (xy 23.51358 64.873496)))
    (arrow1b (pts (xy 24.100001 66) (xy 24.686422 64.873496)))
    (arrow2a (pts (xy 24.100001 29) (xy 23.51358 30.126504)))
    (arrow2b (pts (xy 24.100001 29) (xy 24.686422 30.126504)))
  )
  (gr_line (start 80 42) (end 80 31) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102 37.2) (end 83 37.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83 57.8) (end 102 57.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80 64) (end 80 53) (layer Edge.Cuts) (width 0.15))
  (dimension 20.6 (width 0.3) (layer Dwgs.User)
    (gr_text "0.8 in" (at 111.127689 47.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 102.977689 57.8) (xy 112.477689 57.8)))
    (feature2 (pts (xy 102.977689 37.2) (xy 112.477689 37.2)))
    (crossbar (pts (xy 109.777689 37.2) (xy 109.777689 57.8)))
    (arrow1a (pts (xy 109.777689 57.8) (xy 109.191268 56.673496)))
    (arrow1b (pts (xy 109.777689 57.8) (xy 110.36411 56.673496)))
    (arrow2a (pts (xy 109.777689 37.2) (xy 109.191268 38.326504)))
    (arrow2b (pts (xy 109.777689 37.2) (xy 110.36411 38.326504)))
  )
  (dimension 50 (width 0.3) (layer Dwgs.User)
    (gr_text "50.000 mm" (at 55 19.25) (layer Dwgs.User))
    (feature1 (pts (xy 80 30) (xy 80 17.9)))
    (feature2 (pts (xy 30 30) (xy 30 17.9)))
    (crossbar (pts (xy 30 20.6) (xy 80 20.6)))
    (arrow1a (pts (xy 80 20.6) (xy 78.873496 21.186421)))
    (arrow1b (pts (xy 80 20.6) (xy 78.873496 20.013579)))
    (arrow2a (pts (xy 30 20.6) (xy 31.126504 21.186421)))
    (arrow2b (pts (xy 30 20.6) (xy 31.126504 20.013579)))
  )
  (dimension 73 (width 0.3) (layer Dwgs.User)
    (gr_text "73.000 mm" (at 66.5 16.15) (layer Dwgs.User))
    (feature1 (pts (xy 103 30) (xy 103 14.8)))
    (feature2 (pts (xy 30 30) (xy 30 14.8)))
    (crossbar (pts (xy 30 17.5) (xy 103 17.5)))
    (arrow1a (pts (xy 103 17.5) (xy 101.873496 18.086421)))
    (arrow1b (pts (xy 103 17.5) (xy 101.873496 16.913579)))
    (arrow2a (pts (xy 30 17.5) (xy 31.126504 18.086421)))
    (arrow2b (pts (xy 30 17.5) (xy 31.126504 16.913579)))
  )
  (gr_line (start 30 64) (end 30 31) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78 66) (end 32 66) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103 38.2) (end 103 56.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 32 29) (end 78 29) (layer Edge.Cuts) (width 0.15))
  (zone (net 26) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 30 29) (xy 80 29) (xy 80 66) (xy 30 66)
      )
    )
  )
  (zone (net 26) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 82 57.8) (xy 82 37.2) (xy 103 37.2) (xy 103 57.8)
      )
    )
  )
  (zone (net 26) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 82 57.8) (xy 82 37.2) (xy 103 37.2) (xy 103 57.8)
      )
    )
  )
  (zone (net 26) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 30 29) (xy 80 29) (xy 80 66) (xy 30 66)
      )
    )
  )
  (zone (net 26) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 30 29) (xy 80 29) (xy 80 66) (xy 30 66)
      )
    )
  )
  (zone (net 26) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 82 57.8) (xy 82 37.2) (xy 103 37.2) (xy 103 57.8)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 30 29) (xy 80 29) (xy 80 66) (xy 30 66)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 82 57.8) (xy 82 37.2) (xy 103 37.2) (xy 103 57.8)
      )
    )
  )
  (zone (net 81) (net_name /shield) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 30 52.7) (xy 35.3 52.7) (xy 35.3 42.2) (xy 30 42.2)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 44.7 56.6) (xy 46.3 56.6) (xy 46.3 54.2) (xy 44.7 54.2)
      )
    )
  )
)
