(kicad_pcb (version 3) (host pcbnew "(2013-may-18)-stable")
  (general
    (links 51)
    (no_connects 0)
    (area 173.307912 136.5468 220.550001 158.800001)
    (thickness 1.6)
    (drawings 44)
    (tracks 150)
    (zones 0)
    (modules 21)
    (nets 14)
  )
  (page A3)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user hide)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1778)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (trace_clearance 0.2032)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.1)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.3302)
    (via_min_size 0.889)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 8 8)
    (pad_drill 4)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFDF)
    (pcbplotparams
      (layerselection 284196865)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /tmp/solenoid-driver/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 +9V)
  (net 3 /+5V_Gated)
  (net 4 /SW)
  (net 5 GND)
  (net 6 N-0000012)
  (net 7 N-0000013)
  (net 8 N-000002)
  (net 9 N-000005)
  (net 10 N-000006)
  (net 11 N-000007)
  (net 12 N-000008)
  (net 13 N-000009)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net +5V)
    (add_net +9V)
    (add_net /+5V_Gated)
    (add_net /SW)
    (add_net GND)
    (add_net N-0000012)
    (add_net N-0000013)
    (add_net N-000002)
    (add_net N-000005)
    (add_net N-000006)
    (add_net N-000007)
    (add_net N-000008)
    (add_net N-000009)
  )
  (module SOT23_6 (layer F.Cu) (tedit 53E819FF)
    (at 212.5 148.5 90)
    (fp_text reference U1 (at 1.63 -0.02 180) (layer F.SilkS))
    (fp_text value MIC2009A-1 (at -1.9 0 180) (layer F.SilkS))
    (pad 6 smd rect (at -0.9525 -1.27 90) (size 0.70104 1.00076)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /+5V_Gated)
    )
    (pad 5 smd rect (at 0 -1.27 90) (size 0.70104 1.00076)
      (layers F.Cu F.Paste F.Mask)
      (net 8 N-000002)
    )
    (pad 4 smd rect (at 0.9525 -1.27 90) (size 0.70104 1.00076)
      (layers F.Cu F.Paste F.Mask)
      (net 6 N-0000012)
    )
    (pad 3 smd rect (at 0.9525 1.27 90) (size 0.70104 1.00076)
      (layers F.Cu F.Paste F.Mask)
      (net 11 N-000007)
    )
    (pad 2 smd rect (at 0 1.27 90) (size 0.70104 1.00076)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (pad 1 smd rect (at -0.9525 1.27 90) (size 0.70104 1.00076)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +5V)
    )
    (model smd/SOT23_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-5 (layer F.Cu) (tedit 53E819DC)
    (at 201.3 152.5 270)
    (attr smd)
    (fp_text reference U3 (at -1 2.43 360) (layer F.SilkS))
    (fp_text value MIC2250-2 (at 1.93 -0.03 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 1.27 270) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /SW)
    )
    (pad 3 smd rect (at 0.9525 1.27 270) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 7 N-0000013)
    )
    (pad 5 smd rect (at -0.9525 -1.27 270) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /+5V_Gated)
    )
    (pad 2 smd rect (at 0 1.27 270) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (pad 4 smd rect (at 0.9525 -1.27 270) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 6 N-0000012)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module so-16 (layer F.Cu) (tedit 5340D383)
    (at 180.5 154.5)
    (descr SO-16)
    (attr smd)
    (fp_text reference U2 (at -4.25 -4.25) (layer F.SilkS))
    (fp_text value ULN2003 (at 0 1.016) (layer F.SilkS))
    (pad 1 smd rect (at -4.445 2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000005)
    )
    (pad 2 smd rect (at -3.175 2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000005)
    )
    (pad 3 smd rect (at -1.905 2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000005)
    )
    (pad 4 smd rect (at -0.635 2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000005)
    )
    (pad 5 smd rect (at 0.635 2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000005)
    )
    (pad 6 smd rect (at 1.905 2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000005)
    )
    (pad 7 smd rect (at 3.175 2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000005)
    )
    (pad 8 smd rect (at 4.445 2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (pad 9 smd rect (at 4.445 -2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +9V)
    )
    (pad 10 smd rect (at 3.175 -2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 10 N-000006)
    )
    (pad 11 smd rect (at 1.905 -2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 10 N-000006)
    )
    (pad 12 smd rect (at 0.635 -2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 10 N-000006)
    )
    (pad 13 smd rect (at -0.635 -2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 10 N-000006)
    )
    (pad 14 smd rect (at -1.905 -2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 10 N-000006)
    )
    (pad 15 smd rect (at -3.175 -2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 10 N-000006)
    )
    (pad 16 smd rect (at -4.445 -2.794) (size 0.635 1.27)
      (layers F.Cu F.Paste F.Mask)
      (net 12 N-000008)
    )
    (model smd/smd_dil/so-16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1210 (layer F.Cu) (tedit 5340D3F6)
    (at 194 152.5)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference C5 (at -2.7 0.8 90) (layer F.SilkS))
    (fp_text value 22uF (at 0.15 -0.05 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.524 0) (size 1.27 2.54)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +9V)
    )
    (pad 2 smd rect (at 1.524 0) (size 1.27 2.54)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.2 0.17))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1210 (layer F.Cu) (tedit 5340D6FD)
    (at 205.5 153.5 270)
    (tags "CMS SM")
    (attr smd)
    (fp_text reference C3 (at -1.75 -2.25 360) (layer F.SilkS))
    (fp_text value 22uF (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.524 0 270) (size 1.27 2.54)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /+5V_Gated)
    )
    (pad 2 smd rect (at 1.524 0 270) (size 1.27 2.54)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.2 0.17))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 5340D4D2)
    (at 216.5 143.25 180)
    (attr smd)
    (fp_text reference R2 (at -2.05 0 270) (layer F.SilkS))
    (fp_text value 100K (at -0.05 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +5V)
    )
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 6 N-0000012)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 5340D406)
    (at 198.5 155.5)
    (attr smd)
    (fp_text reference R5 (at 2 0 90) (layer F.SilkS))
    (fp_text value 16K (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 7 N-0000013)
    )
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 5340D3FF)
    (at 195 155.5)
    (attr smd)
    (fp_text reference R4 (at -1.9 0 90) (layer F.SilkS))
    (fp_text value 100K (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +9V)
    )
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 7 N-0000013)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 536DB93A)
    (at 218 148.5 90)
    (attr smd)
    (fp_text reference C1 (at -2 0 180) (layer F.SilkS))
    (fp_text value 1uF (at -0.1 0.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +5V)
    )
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 5340D4CC)
    (at 212.5 145.5 180)
    (attr smd)
    (fp_text reference R1 (at 2 0 270) (layer F.SilkS))
    (fp_text value 470 (at 0 0.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 8 N-000002)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 5340D38E)
    (at 187 156.2 270)
    (attr smd)
    (fp_text reference C4 (at -1.95 0 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.05 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +9V)
    )
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 536DB937)
    (at 216 148.5 90)
    (attr smd)
    (fp_text reference C2 (at -2 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.1 -0.4 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +5V)
    )
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 5340D3A9)
    (at 189.75 140.75 270)
    (attr smd)
    (fp_text reference R3 (at 2.25 0.5 270) (layer F.SilkS))
    (fp_text value 470 (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 13 N-000009)
    )
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +9V)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pin_array_3x2 (layer F.Cu) (tedit 5340D4A0)
    (at 214.75 153.5)
    (descr "Double rangee de contacts 2 x 4 pins")
    (tags CONN)
    (fp_text reference P1 (at -4.95 -1.8) (layer F.SilkS))
    (fp_text value CONN_3X2 (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V)
    )
    (pad 2 thru_hole circle (at -2.54 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 11 N-000007)
    )
    (pad 3 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 4 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 9 N-000005)
    )
    (pad 5 thru_hole circle (at 2.54 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 6 thru_hole circle (at 2.54 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 5 GND)
    )
    (model pin_array/pins_array_3x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_2X1 (layer F.Cu) (tedit 5340D380)
    (at 180.5 148.75 180)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (fp_text reference P3 (at 3.5 0.75 180) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +9V)
    )
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 10 N-000006)
    )
    (model pin_array/pins_array_2x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module c_elec_6.3x7.7 (layer F.Cu) (tedit 53E8185F)
    (at 186.75 146 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (fp_text reference C6 (at 4 1.5 360) (layer F.SilkS))
    (fp_text value 220uF (at -0.05 0.15 360) (layer F.SilkS))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +9V)
    )
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (model smd/capacitors/c_elec_6_3x7_7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module INDUCTOR_12.8x12.8 (layer F.Cu) (tedit 5340D40D)
    (at 201.2 144.2 180)
    (fp_text reference L1 (at 7.3 5.6 180) (layer F.SilkS))
    (fp_text value 22uH (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -5.05 0 180) (size 3.1 5.6)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /+5V_Gated)
    )
    (pad 2 smd rect (at 5.05 0 180) (size 3.1 5.6)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /SW)
    )
  )
  (module 1pin (layer F.Cu) (tedit 536DB824)
    (at 178.5 140.75)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P4 (at 0 -3.048) (layer F.SilkS))
    (fp_text value "Chassis GND" (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 8 8) (drill 4)
      (layers *.Cu *.Mask F.SilkS)
      (net 5 GND)
      (zone_connect 2)
    )
  )
  (module SM0805 (layer F.Cu) (tedit 536DB924)
    (at 216.5 145.5)
    (attr smd)
    (fp_text reference R6 (at 2 0 90) (layer F.SilkS))
    (fp_text value 100K (at 0.1 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 11 N-000007)
    )
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 5 GND)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED-0603 (layer F.Cu) (tedit 4E16AFB4)
    (at 187 139.75 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.016 180) (layer F.SilkS))
    (fp_text value Actuating (at 0 1.016 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756)
      (layers F.Cu F.Paste F.Mask)
      (net 13 N-000009)
    )
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756)
      (layers F.Cu F.Paste F.Mask)
      (net 12 N-000008)
    )
  )
  (module DO214AC_SMA (layer F.Cu) (tedit 53E8181D)
    (at 192.5 146.75 270)
    (fp_text reference D1 (at -3.75 0 360) (layer F.SilkS))
    (fp_text value B220A (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.7)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /SW)
    )
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.7)
      (layers F.Cu F.Paste F.Mask)
      (net 2 +9V)
    )
  )
  (gr_line (start 220.5 155.5) (end 220.5 137.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 217.25 158.75) (end 175.25 158.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 175.25 140.75) (end 175.25 158.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.5 137.5) (end 220.5 137.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 217.25 155.5) (end 220.5 155.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 178.5 140.75) (end 175.25 140.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "Tom Wong-Cornall" (at 183.25 148.75) (layer B.SilkS))
  (gr_text "Rev3 20140811" (at 183.25 147.5) (layer B.SilkS))
  (gr_text "Beamspring USB Solenoid Driver" (at 183.25 146.25) (layer B.SilkS))
  (gr_text "Tom Wong-Cornall" (at 220.16 139.645) (layer F.SilkS))
  (gr_text "Rev3 20140811" (at 220.16 139.02) (layer F.SilkS))
  (gr_text "Beamspring USB Solenoid Driver" (at 220.16 138.395) (layer F.SilkS))
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.381))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 175.25 137.5) (xy 220.5 137.5) (xy 220.5 158.75) (xy 175.25 158.75)
      )
    )
  )
  (zone (net 4) (net_name /SW) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.381))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 201 151.75) (xy 199.25 151.75) (xy 194.5 147) (xy 191.25 147) (xy 191.25 141)
        (xy 201 141)
      )
    )
  )
  (zone (net 2) (net_name +9V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.381))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 194.75 156.25) (xy 187.5 156.25) (xy 184.25 153) (xy 184.25 150.75) (xy 181.25 150.75)
        (xy 180.5 150) (xy 180.5 147.5) (xy 181.25 146.75) (xy 187.75 146.75) (xy 188.5 147.5)
        (xy 193.5 147.5) (xy 193.5 154) (xy 194 154.5) (xy 194.75 154.5)
      )
    )
  )
  (zone (net 3) (net_name /+5V_Gated) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.381))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 201.5 151.75) (xy 201.5 141) (xy 209.75 141) (xy 210.5 141.75) (xy 210.5 148.5)
        (xy 211 149) (xy 211.75 149) (xy 211.75 150) (xy 209 152.75) (xy 201.5 152.75)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.381))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 220.5 158.75) (xy 175.25 158.75) (xy 175.25 151.25) (xy 183.75 151.25) (xy 183.75 153.25)
        (xy 187.25 156.75) (xy 195.25 156.75) (xy 195.25 154) (xy 194.25 154) (xy 194 153.75)
        (xy 194 147.5) (xy 198.75 152.25) (xy 201 152.25) (xy 201 153.25) (xy 209.25 153.25)
        (xy 212.25 150.25) (xy 212.25 148.5) (xy 211.25 148.5) (xy 211 148.25) (xy 211 141.5)
        (xy 210 140.5) (xy 190.75 140.5) (xy 190.75 147) (xy 188.75 147) (xy 188 146.25)
        (xy 181 146.25) (xy 180 147.25) (xy 180 150.25) (xy 180.5 150.75) (xy 175.25 150.75)
        (xy 175.25 137.5) (xy 211 137.5) (xy 220.5 137.5) (xy 220.5 158.75)
      )
    )
  )
)
