(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "Net-(J1-Pin_2)")
  (net 3 "Net-(J1-Pin_3)")
  (net 4 "Net-(J1-Pin_4)")
  (net 5 "Net-(D1-K)")
  (net 6 "Net-(J2-Pin_4)")
  (net 7 "Net-(D2-K)")
  (net 8 "Net-(J2-Pin_2)")
  (net 9 "Net-(J2-Pin_5)")
  (net 10 "Net-(J2-Pin_3)")
  (net 11 "Net-(J2-Pin_1)")
  (net 12 "Net-(H13-Pad1)")
  (net 13 "GND")
  (net 14 "VC3_p")
  (net 15 "VC1_n")
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 71.755 107.477875)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J2-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 123.2154 67.945)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H13" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "Heater Pwr" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(H13-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 12 "Net-(H13-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 12 "Net-(H13-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 133.3754 67.945)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H3" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "TS2" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 77.4954 142.1638)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H8" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "VC3_p" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 14 "VC3_p") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 14 "VC3_p") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 14 "VC3_p") (pinfunction "1") (pintype "input"))
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 75.96 82.077875 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 71.755 110.652875)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J2-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 120.6754 142.1638)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H9" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "TS3_1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J2-Pin_2)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 8 "Net-(J2-Pin_2)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 8 "Net-(J2-Pin_2)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO14580_Pad" (layer "F.Cu")
    (at 67.056 80.2132)
    (descr "Mounting Hole 2.7mm, M2.5, ISO14580")
    (tags "mounting hole 2.7mm m2.5 iso14580")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H14" (at 0 -3.25) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO14580_Pad" (layer "F.Cu")
    (at 159.0548 67.056)
    (descr "Mounting Hole 2.7mm, M2.5, ISO14580")
    (tags "mounting hole 2.7mm m2.5 iso14580")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H15" (at -0.3048 3.429) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 82.5754 142.1638)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H10" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "DP_SW_NC" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J2-Pin_5)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(J2-Pin_5)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 9 "Net-(J2-Pin_5)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 125.7554 142.1638)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H12" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "TS3_0" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J2-Pin_1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 11 "Net-(J2-Pin_1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 11 "Net-(J2-Pin_1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 87.63 111.287875)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D2-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "VC1_n") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 92.7354 142.1638)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H11" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "DP_SW_Comm" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J2-Pin_3)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(J2-Pin_3)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 10 "Net-(J2-Pin_3)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 79.7325 82.077875)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 2.8175 0) (layer "F.SilkS"))
    (fp_text value "806" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D1-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 118.1354 67.945)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H1" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "Payload Pwr" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 1 "VCC") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 1 "VCC") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 107.95 71.12 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pin_3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 148.6154 67.945)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H6" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "VC1_n" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 15 "VC1_n") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 15 "VC1_n") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 15 "VC1_n") (pinfunction "1") (pintype "input"))
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 87.6554 142.1638)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H7" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "VC1_p_VC2_n" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J2-Pin_4)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 6 "Net-(J2-Pin_4)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 6 "Net-(J2-Pin_4)") (pinfunction "1") (pintype "input"))
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 83.285 111.287875 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "VC3_p") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 103.505 71.12 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pin_4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 143.5354 67.945)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H5" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "GND" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 13 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 13 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 13 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 128.2954 67.945)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H2" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "VC2_p_VC3_n" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "1") (pintype "input"))
  )
  (footprint "TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-6_1x06_P2.54mm_Horizontal" (layer "F.Cu")
    (at 75 115.917875 -90)
    (descr "Terminal Block TE 282834-6, 6 pins, pitch 2.54mm, size 15.7x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-6 pitch 2.54mm size 15.7x6.5mm^2 drill 1.1mm pad 2.1mm")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J2" (at 6.35 -4.37 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x06" (at 6.35 4.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J2-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J2-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J2-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J2-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.16 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J2-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 12.7 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 14 "VC3_p") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-6_1x06_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-6_1x06_P2.54mm_Horizontal" (layer "F.Cu")
    (at 75 88.417875 -90)
    (descr "Terminal Block TE 282834-6, 6 pins, pitch 2.54mm, size 15.7x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-6 pitch 2.54mm size 15.7x6.5mm^2 drill 1.1mm pad 2.1mm")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J1" (at 6.35 -4.37 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x06" (at 6.35 4.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J1-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.16 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 13 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 12.7 0 270) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 15 "VC1_n") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-6_1x06_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO14580_Pad" (layer "F.Cu")
    (at 67.056 143.0528)
    (descr "Mounting Hole 2.7mm, M2.5, ISO14580")
    (tags "mounting hole 2.7mm m2.5 iso14580")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H17" (at 0 -3.25) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO14580_Pad" (layer "F.Cu")
    (at 159.0548 143.0528)
    (descr "Mounting Hole 2.7mm, M2.5, ISO14580")
    (tags "mounting hole 2.7mm m2.5 iso14580")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H16" (at 0 -3.25) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_3149_Swage_pin" (layer "F.Cu")
    (at 138.4554 67.945)
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H4" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "TS1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.0922) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J1-Pin_4)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 4 "Net-(J1-Pin_4)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 4 "Net-(J1-Pin_4)") (pinfunction "1") (pintype "input"))
  )
  (footprint "TestPoint:TestPoint_Pad_3.0x3.0mm" (layer "F.Cu")
    (at 95.25 74.93)
    (descr "SMD rectangular pad as test Point, square 3.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "battery_breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -2.398) (layer "F.SilkS"))
    (fp_text value "HeaterPwr" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.4) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 3 3) (layers "F.Cu" "F.Mask")
      (net 12 "Net-(H13-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (gr_poly
    (pts
      (xy 63.5 63.5)
      (xy 63.5 146.60894)
      (xy 162.610945 146.608583)
      (xy 162.611734 63.5)
    )
    (fill none) (layer "Edge.Cuts"))
  (gr_text "TS2" (at 82 94.142875) (layer "F.SilkS"))
  (gr_text "VC1_n" (at 82 101.762875) (layer "F.SilkS"))
  (gr_text "VC3_p" (at 82 129.067875) (layer "F.SilkS"))
  (gr_text "GND\n" (at 82 99.222875) (layer "F.SilkS"))
  (gr_text "Payload_Pwr" (at 74.295 79.375) (layer "F.SilkS"))
  (gr_text "TS3_1" (at 82 118.907875) (layer "F.SilkS"))
  (gr_text "Battery_Pwr" (at 77.47 110.017875) (layer "F.SilkS"))
  (gr_text "PayloadPwr" (at 82 89.062875) (layer "F.SilkS"))
  (gr_text "VC1_p_VC2_n" (at 82 123.987875) (layer "F.SilkS"))
  (gr_text "Battery Breakout Board" (at 67.945 66.675) (layer "F.SilkS"))
  (gr_text "TS3_0" (at 82 116.367875) (layer "F.SilkS"))
  (gr_text "VC2_p_VC3_n" (at 82 91.602875) (layer "F.SilkS"))
  (gr_text "DP_SW_Comm" (at 82 121.447875) (layer "F.SilkS"))
  (gr_text "202401017 v1.0" (at 67.945 68.58) (layer "F.SilkS"))
  (gr_text "TS1" (at 82 96.682875) (layer "F.SilkS"))
  (gr_text "DP_SW_NC\n" (at 82 126.527875) (layer "F.SilkS"))
  (gr_text "HeaterPwr" (at 91.44 78.105) (layer "F.SilkS"))
  (zone (net 13) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 63.5 63.5)
        (xy 63.5 146.685)
        (xy 162.56 146.685)
        (xy 162.56 63.5)
      )
    )
  )
  (zone (net 13) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 63.5 63.5)
        (xy 63.5 146.685)
        (xy 162.56 146.685)
        (xy 162.56 63.5)
      )
    )
  )
)
