(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 35)
    (tracks 186)
    (zones 0)
    (modules 22)
    (nets 16)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.4 5.4)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /RST)
  (net 2 /GC_4)
  (net 3 /GC_3)
  (net 4 /GC_2)
  (net 5 /GC_1)
  (net 6 /USB_D+)
  (net 7 /USB_D-)
  (net 8 /BT_D-)
  (net 9 /BT_D+)
  (net 10 /AUDIO_RIGHT)
  (net 11 /AUDIO_LEFT)
  (net 12 /VIDEO_PR)
  (net 13 /VIDEO_PB)
  (net 14 /VIDEO_Y)
  (net 15 GND)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net /AUDIO_LEFT)
    (add_net /AUDIO_RIGHT)
    (add_net /BT_D+)
    (add_net /BT_D-)
    (add_net /GC_1)
    (add_net /GC_2)
    (add_net /GC_3)
    (add_net /GC_4)
    (add_net /RST)
    (add_net /USB_D+)
    (add_net /USB_D-)
    (add_net /VIDEO_PB)
    (add_net /VIDEO_PR)
    (add_net /VIDEO_Y)
    (add_net GND)
  )
  (module project-footprints:controller (layer Top) (tedit 0)
    (at 58.35 72.15)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module project-footprints:controller (layer Top) (tedit 0)
    (at 40.75 77.2)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module project-footprints:bluetooth (layer Top) (tedit 0)
    (at 44.3 77.2)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module project-footprints:reset (layer Top) (tedit 0)
    (at 42.65 77.2)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module project-footprints:reset (layer Top) (tedit 0)
    (at 64.05 76.4)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module project-footprints:bluetooth (layer Top) (tedit 0)
    (at 66.4 73.85)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module project-footprints:usb (layer Top) (tedit 0)
    (at 66.45 76.25)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module project-footprints:usb (layer Top) (tedit 0)
    (at 51.55 77.2)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module project-footprints:audio (layer Top) (tedit 0)
    (at 29.5 77.2)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module project-footprints:video (layer Top) (tedit 0)
    (at 21.4 77.3)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO14580_Pad (layer Top) (tedit 56D1B4CB)
    (at 69.421 74.55 270)
    (descr "Mounting Hole 2.7mm, M2.5, ISO14580")
    (tags "mounting hole 2.7mm m2.5 iso14580")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.25 90) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.25 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 4.5 4.5) (drill 2.7) (layers *.Cu *.Mask)
      (net 15 GND))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO14580_Pad (layer Top) (tedit 56D1B4CB)
    (at 11.02 74.55 270)
    (descr "Mounting Hole 2.7mm, M2.5, ISO14580")
    (tags "mounting hole 2.7mm m2.5 iso14580")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.25 90) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.25 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 4.5 4.5) (drill 2.7) (layers *.Cu *.Mask)
      (net 15 GND))
  )
  (module Connector_JST:JST_SH_BM07B-SRSS-TB_1x07-1MP_P1.00mm_Vertical (layer Top) (tedit 5B78AD88)
    (at 42.55 74.25 180)
    (descr "JST SH series connector, BM07B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH side entry")
    (attr smd)
    (fp_text reference J1 (at 0 -3.3) (layer F.SilkS) hide)
    (fp_text value Peripherals (at 0 -2.6) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -0.25) (layer F.Fab))
    (pad 1 smd roundrect (at -3 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /BT_D-))
    (pad 2 smd roundrect (at -2 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /BT_D+))
    (pad 3 smd roundrect (at -1 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /RST))
    (pad 4 smd roundrect (at 0 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /GC_1))
    (pad 5 smd roundrect (at 1 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /GC_2))
    (pad 6 smd roundrect (at 2 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /GC_3))
    (pad 7 smd roundrect (at 3 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /GC_4))
    (pad MP smd roundrect (at -4.3 -1.2 180) (size 1.2 1.8) (layers Top F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at 4.3 -1.2 180) (size 1.2 1.8) (layers Top F.Paste F.Mask) (roundrect_rratio 0.208333))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_BM07B-SRSS-TB_1x07-1MP_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SH_BM02B-SRSS-TB_1x02-1MP_P1.00mm_Vertical (layer Top) (tedit 5B78AD87)
    (at 51.55 74.25 180)
    (descr "JST SH series connector, BM02B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH side entry")
    (attr smd)
    (fp_text reference J10 (at 0 -3.3) (layer F.SilkS) hide)
    (fp_text value USB (at 1.3 -2.85) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -0.25) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /USB_D+))
    (pad 2 smd roundrect (at 0.5 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /USB_D-))
    (pad MP smd roundrect (at -1.8 -1.2 180) (size 1.2 1.8) (layers Top F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at 1.8 -1.2 180) (size 1.2 1.8) (layers Top F.Paste F.Mask) (roundrect_rratio 0.208333))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_BM02B-SRSS-TB_1x02-1MP_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical (layer Top) (tedit 5B78AD87)
    (at 21.45 74.25 180)
    (descr "JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH side entry")
    (attr smd)
    (fp_text reference J3 (at 0 -3.3) (layer F.SilkS) hide)
    (fp_text value Video (at 0 -2.65) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -0.25) (layer F.Fab))
    (pad 1 smd roundrect (at -1.5 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 GND))
    (pad 2 smd roundrect (at -0.5 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /VIDEO_PR))
    (pad 3 smd roundrect (at 0.5 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /VIDEO_PB))
    (pad 4 smd roundrect (at 1.5 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /VIDEO_Y))
    (pad MP smd roundrect (at -2.8 -1.2 180) (size 1.2 1.8) (layers Top F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at 2.8 -1.2 180) (size 1.2 1.8) (layers Top F.Paste F.Mask) (roundrect_rratio 0.208333))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SH_BM03B-SRSS-TB_1x03-1MP_P1.00mm_Vertical (layer Top) (tedit 5B78AD87)
    (at 29.45 74.25 180)
    (descr "JST SH series connector, BM03B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH side entry")
    (attr smd)
    (fp_text reference J2 (at 0 -3.3) (layer F.SilkS) hide)
    (fp_text value Audio (at 0.05 -2.6) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -0.25) (layer F.Fab))
    (pad 1 smd roundrect (at -1 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 GND))
    (pad 2 smd roundrect (at 0 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /AUDIO_RIGHT))
    (pad 3 smd roundrect (at 1 1.325 180) (size 0.6 1.55) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /AUDIO_LEFT))
    (pad MP smd roundrect (at -2.3 -1.2 180) (size 1.2 1.8) (layers Top F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at 2.3 -1.2 180) (size 1.2 1.8) (layers Top F.Paste F.Mask) (roundrect_rratio 0.208333))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_BM03B-SRSS-TB_1x03-1MP_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module project-footprints:TestPoint_Pad_2.0x1.0mm (layer Top) (tedit 5ECFF6F6)
    (at 64.05 78.1 90)
    (fp_text reference J6 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value RST (at -0.1 -1.7 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0 90) (size 1 1) (layers Top F.Paste F.Mask)
      (net 1 /RST))
  )
  (module project-footprints:TestPoint_2Pads_2.0x1.0mm (layer Top) (tedit 5ECFF524)
    (at 35.25 78.1 90)
    (fp_text reference J8 (at 0 0.5 270) (layer F.SilkS) hide)
    (fp_text value Audio (at -1.4 -5.3 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -0.7 90) (size 1 1) (layers Top F.Paste F.Mask)
      (net 11 /AUDIO_LEFT))
    (pad 2 smd rect (at 0 0.7 90) (size 1 1) (layers Top F.Paste F.Mask)
      (net 10 /AUDIO_RIGHT))
  )
  (module project-footprints:TestPoint_3Pads_2.0x1.0mm (layer Top) (tedit 5ECFF4C1)
    (at 14.7 78.1 90)
    (fp_text reference J9 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value Video (at 0.15 4.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -1.4 90) (size 1 1) (layers Top F.Paste F.Mask)
      (net 14 /VIDEO_Y))
    (pad 2 smd rect (at 0 0 90) (size 1 1) (layers Top F.Paste F.Mask)
      (net 13 /VIDEO_PB))
    (pad 3 smd rect (at 0 1.4 90) (size 1 1) (layers Top F.Paste F.Mask)
      (net 12 /VIDEO_PR))
  )
  (module project-footprints:TestPoint_2Pads_2.0x1.0mm (layer Top) (tedit 5ECF0077)
    (at 66.45 78.1 90)
    (fp_text reference J4 (at 1.9 0.05) (layer F.SilkS) hide)
    (fp_text value USB (at -0.05 -2.4) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0 0.7 90) (size 1 1) (layers Top F.Paste F.Mask)
      (net 6 /USB_D+))
    (pad 1 smd rect (at 0 -0.7 90) (size 1 1) (layers Top F.Paste F.Mask)
      (net 7 /USB_D-))
  )
  (module project-footprints:TestPoint_4Pads_2.0x1.0mm (layer Top) (tedit 5ECF011B)
    (at 61.95 71.75 270)
    (fp_text reference J5 (at -2.1 0.4 270) (layer Top) hide)
    (fp_text value GC (at 0.05 3.575) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0 0.7 270) (size 1 1) (layers Top F.Paste F.Mask)
      (net 3 /GC_3))
    (pad 2 smd rect (at 0 -0.7 270) (size 1 1) (layers Top F.Paste F.Mask)
      (net 5 /GC_1))
    (pad 1 smd rect (at 0 -2.1 270) (size 1 1) (layers Top F.Paste F.Mask)
      (net 4 /GC_2))
    (pad 4 smd rect (at 0 2.1 270) (size 1 1) (layers Top F.Paste F.Mask)
      (net 2 /GC_4))
  )
  (module project-footprints:TestPoint_2Pads_2.0x1.0mm (layer Top) (tedit 5ECF00E3)
    (at 66.45 71.75 270)
    (fp_text reference J7 (at 0 0.5 270) (layer F.SilkS) hide)
    (fp_text value BT (at 0.05 -1.9) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0 0.7 270) (size 1 1) (layers Top F.Paste F.Mask)
      (net 9 /BT_D+))
    (pad 1 smd rect (at 0 -0.7 270) (size 1 1) (layers Top F.Paste F.Mask)
      (net 8 /BT_D-))
  )
  (gr_arc (start 62.1 74.2) (end 63.1 74.2) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 62.1 74.9) (end 62.1 75.9) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 57.6 74.9) (end 56.6 74.9) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 57.6 74.2) (end 57.6 73.2) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 12.75 73.070027) (end 12.75 71.25) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 10.929973 76.779973) (end 10.929973 73.070027) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 12.75 76.779973) (end 10.929973 76.779973) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 69.420027 73.070027) (end 69.420027 76.78) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 67.6 73.070027) (end 69.420027 73.070027) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 67.6 76.78) (end 67.6 78.600027) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 57.6 73.2) (end 62.1 73.2) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 56.6 74.9) (end 56.6 74.2) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 62.1 75.9) (end 57.6 75.9) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 63.1 74.2) (end 63.1 74.9) (layer Edge.Cuts) (width 0.02))
  (gr_text v3.0 (at 14.6 73.15) (layer F.SilkS))
  (gr_text @loopj (at 14.6 71.95) (layer F.SilkS))
  (gr_text Pr (at 16.1 77.1) (layer F.SilkS))
  (gr_text Pb (at 14.7 77.1) (layer F.SilkS))
  (gr_text Y (at 13.25 77.1) (layer F.SilkS))
  (gr_text R (at 35.95 77.05) (layer F.SilkS))
  (gr_text L (at 34.5 77.05) (layer F.SilkS))
  (gr_text 4 (at 59.85 72.85) (layer F.SilkS))
  (gr_text 3 (at 61.25 72.8) (layer F.SilkS))
  (gr_text 2 (at 64.1 72.8) (layer F.SilkS))
  (gr_text 1 (at 62.7 72.8) (layer F.SilkS))
  (gr_text 2 (at 65.75 72.8) (layer F.SilkS))
  (gr_text 1 (at 67.15 72.75) (layer F.SilkS))
  (gr_text "\n-" (at 65.75 77.8 180) (layer F.SilkS))
  (gr_text + (at 67.15 77.2 180) (layer F.SilkS))
  (gr_line (start 12.75 78.6) (end 67.6 78.600027) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 67.604973 71.25) (end 12.75 71.25) (layer Edge.Cuts) (width 0.02))
  (zone (net 15) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69.35 78.6) (xy 11.025 78.6) (xy 11.025 71.25) (xy 69.35 71.25)
      )
    )
  )
)
