(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 129)
    (zones 0)
    (modules 20)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.71 3.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 98 115)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 VCC)
  (net 4 "Net-(C1-Pad2)")
  (net 5 "Net-(C2-Pad1)")
  (net 6 "Net-(C2-Pad2)")
  (net 7 "Net-(C3-Pad1)")
  (net 8 "Net-(R1-Pad2)")
  (net 9 "Net-(R2-Pad2)")
  (net 10 "Net-(R3-Pad1)")
  (net 11 "Net-(R4-Pad1)")
  (net 12 "Net-(D1-Pad2)")
  (net 13 "Net-(D1-Pad1)")
  (net 14 "Net-(D2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net VCC)
  )
  (module piezo:DDA0008B (layer F.Cu) (tedit 5F25C320)
    (at 121.5 132)
    (descr "Powerpad SOIC")
    (tags DDA0008B)
    (attr smd)
    (fp_text reference U1 (at 0 3.705 180) (layer F.SilkS))
    (fp_text value LME49724 (at -5.08 0 90) (layer F.Fab))
    (pad 9 smd rect (at 0 0) (size 2.71 3.4) (layers B.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 0 0) (size 2.71 3.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.7 -1.905 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R3-Pad1)"))
    (pad 5 smd rect (at -2.7 -1.905 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R4-Pad1)"))
    (pad 3 smd rect (at 2.7 -0.635 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 6 smd rect (at -2.7 -0.635 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.7 0.635 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C3-Pad1)"))
    (pad 7 smd rect (at -2.7 0.635 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 1 smd rect (at 2.7 1.905 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 8 smd rect (at -2.7 1.905 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D2-Pad2)"))
  )
  (module Capacitor_SMD:CP_Elec_5x5.9 (layer F.Cu) (tedit 5BCA39CF)
    (at 132.8 136 180)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic B6, 5.0x5.9mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C1 (at 0 -3.7) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 4 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_5x5.9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_RJ:RJ14_Connfly_DS1133-S4_Horizontal (layer F.Cu) (tedit 5E73C846)
    (at 142.5 130.5 270)
    (descr "RJ14 connector 6P4C Horizontal http://www.connfly.com/userfiles/image/UpLoadFile/File/2012/10/26/DS1133.pdf")
    (tags "RJ14 connector 6P4C Connfly DS1133")
    (fp_text reference J5 (at 1 -5 270) (layer F.SilkS))
    (fp_text value RJ14 (at 0.81 6.35 270) (layer F.Fab))
    (fp_text user %R (at 1.03 -5.22 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at -4.47 -2.3 90) (size 2.3 2.3) (drill 2.3) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 1.02 2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 2.04 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad1)"))
    (pad "" np_thru_hole circle (at 7.53 -2.3 90) (size 2.3 2.3) (drill 2.3) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 3.06 2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ14_Connfly_DS1133-S4_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 145.5 119)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference J1 (at 0 -2.9) (layer F.SilkS))
    (fp_text value "conn to ground" (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 145.5 145.5)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference J2 (at 0 -2.9) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 102 119)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference J3 (at 0 -2.9) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 102 145.5)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference J4 (at 0 -2.9) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:CP_Elec_5x5.9 (layer F.Cu) (tedit 5BCA39CF)
    (at 132.8 128 180)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic B6, 5.0x5.9mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C2 (at 0 -3.7) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 5 "Net-(C2-Pad1)"))
    (pad 2 smd roundrect (at 2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 6 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_5x5.9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_5x5.9 (layer F.Cu) (tedit 5BCA39CF)
    (at 137.2 143.5)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic B6, 5.0x5.9mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C3 (at 0 -3.7) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 7 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_5x5.9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_5x5.9 (layer F.Cu) (tedit 5BCA39CF)
    (at 114 132.3 90)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic B6, 5.0x5.9mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C4 (at 0 -3.7 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 3.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.2 0 90) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 3 VCC))
    (pad 2 smd roundrect (at 2.2 0 90) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_5x5.9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_5x5.9 (layer F.Cu) (tedit 5BCA39CF)
    (at 138.8 121)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic B6, 5.0x5.9mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C5 (at 0 -3.7) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_5x5.9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1806_4516Metric_Pad1.57x1.80mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 115.5 139 180)
    (descr "Resistor SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 100 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.0875 0 180) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 8 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -2.0875 0 180) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 12 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1806_4516Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1806_4516Metric_Pad1.57x1.80mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 115.412 124.5 180)
    (descr "Resistor SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 100 (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.0875 0 180) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 14 "Net-(D2-Pad2)"))
    (pad 2 smd roundrect (at 2.0875 0 180) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 9 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1806_4516Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1806_4516Metric_Pad1.57x1.80mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 122.588 139 180)
    (descr "Resistor SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 10K (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.0875 0 180) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 12 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -2.0875 0 180) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 10 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1806_4516Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1806_4516Metric_Pad1.57x1.80mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 122.588 124.5 180)
    (descr "Resistor SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 10K (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.0875 0 180) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 11 "Net-(R4-Pad1)"))
    (pad 2 smd roundrect (at 2.0875 0 180) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 14 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1806_4516Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1806_4516Metric_Pad1.57x1.80mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 127.5 135.088 90)
    (descr "Resistor SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.85 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.0875 0 90) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 10 "Net-(R3-Pad1)"))
    (pad 1 smd roundrect (at -2.0875 0 90) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 4 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1806_4516Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1806_4516Metric_Pad1.57x1.80mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 127.5 128.412 90)
    (descr "Resistor SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.85 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.0875 0 90) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 6 "Net-(C2-Pad2)"))
    (pad 2 smd roundrect (at 2.0875 0 90) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 11 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1806_4516Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock:TerminalBlock_Altech_AK300-2_P5.00mm (layer F.Cu) (tedit 59FF0306)
    (at 104.5 134.5 90)
    (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
    (tags "Altech AK300 terminal block pitch 5.0mm")
    (fp_text reference X1 (at -1.92 -6.99 90) (layer F.SilkS))
    (fp_text value Piezo (at 2.78 7.75 90) (layer F.Fab))
    (fp_text user %R (at 2.5 -2 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 5 0 90) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_Altech_AK300-2_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P5.08mm_Vertical_KathodeUp (layer F.Cu) (tedit 5AE50CD5)
    (at 104.5 139)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 5.08mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 2.54 -2.326371) (layer F.SilkS))
    (fp_text value "1N5225B 3V" (at 2.54 2.326371) (layer F.Fab))
    (fp_text user K (at 1.5 0.8) (layer F.SilkS))
    (fp_text user K (at 1.5 0.8) (layer F.Fab))
    (fp_text user %R (at 2.54 -2.326371) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P5.08mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P5.08mm_Vertical_KathodeUp (layer F.Cu) (tedit 5AE50CD5)
    (at 104.5 124.5)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 5.08mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 2.54 -2.326371) (layer F.SilkS))
    (fp_text value "1N5225B 3V" (at 2.54 2.326371) (layer F.Fab))
    (fp_text user %R (at 2.54 -2.326371) (layer F.Fab))
    (fp_text user K (at 1.5 0.8) (layer F.Fab))
    (fp_text user K (at 1.5 0.8) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P5.08mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 4 (width 0.15) (layer Dwgs.User)
    (gr_text "4,000 mm" (at 147.5 123.3) (layer Dwgs.User))
    (feature1 (pts (xy 149.5 119) (xy 149.5 122.586421)))
    (feature2 (pts (xy 145.5 119) (xy 145.5 122.586421)))
    (crossbar (pts (xy 145.5 122) (xy 149.5 122)))
    (arrow1a (pts (xy 149.5 122) (xy 148.373496 122.586421)))
    (arrow1b (pts (xy 149.5 122) (xy 148.373496 121.413579)))
    (arrow2a (pts (xy 145.5 122) (xy 146.626504 122.586421)))
    (arrow2b (pts (xy 145.5 122) (xy 146.626504 121.413579)))
  )
  (dimension 4 (width 0.15) (layer Dwgs.User)
    (gr_text "4,000 mm" (at 141.2 117 90) (layer Dwgs.User))
    (feature1 (pts (xy 145.5 115) (xy 141.913579 115)))
    (feature2 (pts (xy 145.5 119) (xy 141.913579 119)))
    (crossbar (pts (xy 142.5 119) (xy 142.5 115)))
    (arrow1a (pts (xy 142.5 115) (xy 143.086421 116.126504)))
    (arrow1b (pts (xy 142.5 115) (xy 141.913579 116.126504)))
    (arrow2a (pts (xy 142.5 119) (xy 143.086421 117.873496)))
    (arrow2b (pts (xy 142.5 119) (xy 141.913579 117.873496)))
  )
  (dimension 4 (width 0.15) (layer Dwgs.User)
    (gr_text "4,000 mm" (at 100 123.8) (layer Dwgs.User))
    (feature1 (pts (xy 98 119) (xy 98 123.086421)))
    (feature2 (pts (xy 102 119) (xy 102 123.086421)))
    (crossbar (pts (xy 102 122.5) (xy 98 122.5)))
    (arrow1a (pts (xy 98 122.5) (xy 99.126504 121.913579)))
    (arrow1b (pts (xy 98 122.5) (xy 99.126504 123.086421)))
    (arrow2a (pts (xy 102 122.5) (xy 100.873496 121.913579)))
    (arrow2b (pts (xy 102 122.5) (xy 100.873496 123.086421)))
  )
  (dimension 4 (width 0.15) (layer Dwgs.User)
    (gr_text "4,000 mm" (at 106.3 117 90) (layer Dwgs.User))
    (feature1 (pts (xy 102 115) (xy 105.586421 115)))
    (feature2 (pts (xy 102 119) (xy 105.586421 119)))
    (crossbar (pts (xy 105 119) (xy 105 115)))
    (arrow1a (pts (xy 105 115) (xy 105.586421 116.126504)))
    (arrow1b (pts (xy 105 115) (xy 104.413579 116.126504)))
    (arrow2a (pts (xy 105 119) (xy 105.586421 117.873496)))
    (arrow2b (pts (xy 105 119) (xy 104.413579 117.873496)))
  )
  (dimension 4 (width 0.15) (layer Dwgs.User)
    (gr_text "4,000 mm" (at 100 141.2) (layer Dwgs.User))
    (feature1 (pts (xy 98 145.5) (xy 98 141.913579)))
    (feature2 (pts (xy 102 145.5) (xy 102 141.913579)))
    (crossbar (pts (xy 102 142.5) (xy 98 142.5)))
    (arrow1a (pts (xy 98 142.5) (xy 99.126504 141.913579)))
    (arrow1b (pts (xy 98 142.5) (xy 99.126504 143.086421)))
    (arrow2a (pts (xy 102 142.5) (xy 100.873496 141.913579)))
    (arrow2b (pts (xy 102 142.5) (xy 100.873496 143.086421)))
  )
  (dimension 4 (width 0.15) (layer Dwgs.User)
    (gr_text "4,000 mm" (at 106.8 147.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 102 149.5) (xy 106.086421 149.5)))
    (feature2 (pts (xy 102 145.5) (xy 106.086421 145.5)))
    (crossbar (pts (xy 105.5 145.5) (xy 105.5 149.5)))
    (arrow1a (pts (xy 105.5 149.5) (xy 104.913579 148.373496)))
    (arrow1b (pts (xy 105.5 149.5) (xy 106.086421 148.373496)))
    (arrow2a (pts (xy 105.5 145.5) (xy 104.913579 146.626504)))
    (arrow2b (pts (xy 105.5 145.5) (xy 106.086421 146.626504)))
  )
  (dimension 34.5 (width 0.15) (layer Dwgs.User)
    (gr_text "34,500 mm" (at 90.7 132.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 98 149.5) (xy 91.413579 149.5)))
    (feature2 (pts (xy 98 115) (xy 91.413579 115)))
    (crossbar (pts (xy 92 115) (xy 92 149.5)))
    (arrow1a (pts (xy 92 149.5) (xy 91.413579 148.373496)))
    (arrow1b (pts (xy 92 149.5) (xy 92.586421 148.373496)))
    (arrow2a (pts (xy 92 115) (xy 91.413579 116.126504)))
    (arrow2b (pts (xy 92 115) (xy 92.586421 116.126504)))
  )
  (dimension 51.5 (width 0.15) (layer Dwgs.User)
    (gr_text "51,500 mm" (at 123.75 109.2) (layer Dwgs.User))
    (feature1 (pts (xy 98 115) (xy 98 109.913579)))
    (feature2 (pts (xy 149.5 115) (xy 149.5 109.913579)))
    (crossbar (pts (xy 149.5 110.5) (xy 98 110.5)))
    (arrow1a (pts (xy 98 110.5) (xy 99.126504 109.913579)))
    (arrow1b (pts (xy 98 110.5) (xy 99.126504 111.086421)))
    (arrow2a (pts (xy 149.5 110.5) (xy 148.373496 109.913579)))
    (arrow2b (pts (xy 149.5 110.5) (xy 148.373496 111.086421)))
  )
  (dimension 34.5 (width 0.15) (layer Dwgs.User)
    (gr_text "34,500 mm" (at 155.8 132.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 149.5 149.5) (xy 155.086421 149.5)))
    (feature2 (pts (xy 149.5 115) (xy 155.086421 115)))
    (crossbar (pts (xy 154.5 115) (xy 154.5 149.5)))
    (arrow1a (pts (xy 154.5 149.5) (xy 153.913579 148.373496)))
    (arrow1b (pts (xy 154.5 149.5) (xy 155.086421 148.373496)))
    (arrow2a (pts (xy 154.5 115) (xy 153.913579 116.126504)))
    (arrow2b (pts (xy 154.5 115) (xy 155.086421 116.126504)))
  )
  (target plus (at 98 115) (size 5) (width 0.1) (layer Edge.Cuts))
  (gr_line (start 149.5 149.5) (end 149.5 115) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98 149.5) (end 149.5 149.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98 149.5) (end 98 115) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.5 115) (end 98 115) (layer Edge.Cuts) (width 0.1))
  (dimension 4 (width 0.15) (layer Dwgs.User)
    (gr_text "4,000 mm" (at 147.5 140.7) (layer Dwgs.User))
    (feature1 (pts (xy 149.5 145) (xy 149.5 141.413579)))
    (feature2 (pts (xy 145.5 145) (xy 145.5 141.413579)))
    (crossbar (pts (xy 145.5 142) (xy 149.5 142)))
    (arrow1a (pts (xy 149.5 142) (xy 148.373496 142.586421)))
    (arrow1b (pts (xy 149.5 142) (xy 148.373496 141.413579)))
    (arrow2a (pts (xy 145.5 142) (xy 146.626504 142.586421)))
    (arrow2b (pts (xy 145.5 142) (xy 146.626504 141.413579)))
  )
  (gr_text "Amplifier for piezo electric crystal" (at 121.5 118.5) (layer B.SilkS))
  (gr_text "Amplifier for piezo electric crystal" (at 123 148.5) (layer F.SilkS))
  (gr_text PIEZO (at 100 132 90) (layer B.SilkS))
  (gr_text PIEZO (at 100 132 90) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.5 149.5) (xy 98 149.5) (xy 98 115) (xy 149.5 115)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.5 149.5) (xy 98 149.5) (xy 98 115) (xy 149.5 115)
      )
    )
  )
)
