(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 14)
    (no_connects 0)
    (area 102.599 75.69488 176.890287 116.575001)
    (thickness 1.6)
    (drawings 19)
    (tracks 53)
    (zones 0)
    (modules 21)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.006)
    (trace_clearance 0.006)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.027)
    (via_drill 0.013)
    (via_min_size 0.027)
    (via_min_drill 0.013)
    (uvia_size 0.03)
    (uvia_drill 0.02)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.4 3.4)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 127.5 88)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01020_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(T1-Pad5)")
  (net 4 "Net-(T2-Pad5)")
  (net 5 "Net-(P1-Pad1)")
  (net 6 "Net-(P2-Pad1)")
  (net 7 "Net-(P3-Pad1)")
  (net 8 "Net-(P4-Pad1)")
  (net 9 "Net-(P5-Pad1)")
  (net 10 "Net-(P6-Pad1)")
  (net 11 "Net-(D2-Pad2)")
  (net 12 "Net-(D3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.006)
    (trace_width 0.006)
    (via_dia 0.027)
    (via_drill 0.013)
    (uvia_dia 0.03)
    (uvia_drill 0.02)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(T1-Pad5)")
    (add_net "Net-(T2-Pad5)")
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 573C88FD)
    (at 153.75 99.25 225)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D1 (at 5.43052 2.53746 225) (layer F.SilkS) hide)
    (fp_text value D (at 4.41452 -3.55854 225) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16052 -0.00254 45) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 45) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 573C88F7)
    (at 139.75 106.5 135)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D2 (at 5.43052 2.53746 135) (layer F.SilkS) hide)
    (fp_text value D (at 4.41452 -3.55854 135) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16052 -0.00254 315) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 315) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 573C8913)
    (at 147.25 83.5 315)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D3 (at 5.43052 2.53746 315) (layer F.SilkS) hide)
    (fp_text value D (at 4.41452 -3.55854 315) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16052 -0.00254 135) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 135) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D3-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 573C8904)
    (at 132.5 90.75 45)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D4 (at 5.43052 2.53746 45) (layer F.SilkS) hide)
    (fp_text value D (at 4.41452 -3.55854 45) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16052 -0.00254 225) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D3-Pad1)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 225) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D2-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 573C87AC)
    (at 156.5 85.5)
    (fp_text reference P1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 573C8799)
    (at 152 80.5)
    (fp_text reference P2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P2-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 573C87DB)
    (at 146.5 112.5)
    (fp_text reference P3 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P3-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 573C87D5)
    (at 140.4 112.4)
    (fp_text reference P4 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P4-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 573C878B)
    (at 130 86)
    (fp_text reference P5 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P5-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 573C8785)
    (at 134.5 81)
    (fp_text reference P6 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P6-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 573C8776)
    (at 167 85)
    (fp_text reference "" (at 0 -3.81) (layer F.SilkS))
    (fp_text value SolderWirePad_single_1mmDrill (at -1.905 3.175) (layer F.Fab) hide)
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 573C87BA)
    (at 167 105.5)
    (fp_text reference "" (at 0 -3.81) (layer F.SilkS))
    (fp_text value SolderWirePad_single_1mmDrill (at -1.905 3.175) (layer F.Fab) hide)
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 573C877D)
    (at 119 85.5)
    (fp_text reference "" (at -16.32 -5.05) (layer F.SilkS))
    (fp_text value SolderWirePad_single_1mmDrill (at -1.905 3.175) (layer F.Fab) hide)
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 573C87C7)
    (at 119 105.5)
    (fp_text reference "" (at 0 -3.81) (layer F.SilkS))
    (fp_text value SolderWirePad_single_1mmDrill (at -1.905 3.175) (layer F.Fab) hide)
  )
  (module ringmod:alien5 (layer F.Cu) (tedit 0)
    (at 143.22 95.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 573C87CD)
    (at 128.516 104.51)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 573C87C2)
    (at 157.726 104.51)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 573C87A0)
    (at 143.248 80.126)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module OPENHARDWARE:OSHWLOGO0.3IN (layer B.Cu) (tedit 0)
    (at 147.14 88.39 180)
    (descr "OSHW LOGO")
    (tags "Open Source Hardware Logo")
    (fp_text reference G*** (at 0 -7.27964 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 7.27964 180) (layer B.SilkS) hide)
  )
  (module ringmod:trafo-xicon-42TM (layer F.Cu) (tedit 58691B97)
    (at 167.2 95.4 270)
    (descr "XICON ULTRA-MINI AUDIO TRANSFORMER 42TM SERIES")
    (tags "XICON ULTRA-MINI AUDIO TRANSFORMER 42TM SERIES")
    (attr virtual)
    (fp_text reference T1 (at -0.4 0.2 360) (layer F.SilkS))
    (fp_text value audio_transformer (at 0.508 -4.318 270) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at -9.98474 -0.01524 270) (size 3.4 3.4) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 9.98474 0.00508 270) (size 3.4 3.4) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -3.556 6.35 270) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 12 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 0 6.35 270) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 7 "Net-(P3-Pad1)"))
    (pad 3 thru_hole circle (at 3.556 6.35 270) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (pad 4 thru_hole circle (at 3.556 -6.35 270) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 5 "Net-(P1-Pad1)"))
    (pad 5 thru_hole circle (at 0 -6.35 270) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 3 "Net-(T1-Pad5)"))
    (pad 6 thru_hole circle (at -3.556 -6.35 270) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 6 "Net-(P2-Pad1)"))
  )
  (module ringmod:trafo-xicon-42TM (layer F.Cu) (tedit 58691BB5)
    (at 119.2 95.6 90)
    (descr "XICON ULTRA-MINI AUDIO TRANSFORMER 42TM SERIES")
    (tags "XICON ULTRA-MINI AUDIO TRANSFORMER 42TM SERIES")
    (attr virtual)
    (fp_text reference T2 (at -0.4 0.2 180) (layer F.SilkS))
    (fp_text value audio_transformer (at 0.508 -4.318 90) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at -9.98474 -0.01524 90) (size 3.4 3.4) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 9.98474 0.00508 90) (size 3.4 3.4) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -3.556 6.35 90) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 0 6.35 90) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 8 "Net-(P4-Pad1)"))
    (pad 3 thru_hole circle (at 3.556 6.35 90) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 11 "Net-(D2-Pad2)"))
    (pad 4 thru_hole circle (at 3.556 -6.35 90) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 10 "Net-(P6-Pad1)"))
    (pad 5 thru_hole circle (at 0 -6.35 90) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 4 "Net-(T2-Pad5)"))
    (pad 6 thru_hole circle (at -3.556 -6.35 90) (size 1.29794 1.29794) (drill 0.6985) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 9 "Net-(P5-Pad1)"))
  )
  (gr_text OUT (at 156.55 82.23) (layer F.SilkS))
  (gr_text "X IN" (at 130.06 82.77) (layer F.SilkS))
  (gr_text "Y IN" (at 143.51 109.09) (layer F.SilkS))
  (gr_text 11:11 (at 158.742 78.602) (layer F.SilkS))
  (gr_text 4096 (at 127.5 78.856) (layer F.SilkS))
  (gr_line (start 163.06 76.57) (end 161.79 76.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.506 89.016) (end 163.06 76.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.944 76.57) (end 162.044 76.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.498 89.016) (end 123.944 76.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.5 102) (end 161 116.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "adapted by\nmisterbonnie\nfrom" (at 127.41 110.98) (layer F.SilkS))
  (gr_text "RING\nMODULATOR\n" (at 156.456 110.606) (layer F.SilkS))
  (gr_text https://www.asciipr0n.com/4096/ringmod/ (at 143.48 115.25) (layer F.SilkS))
  (gr_line (start 111 102) (end 125.5 116.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111 89.5) (end 111 102) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.5 89) (end 111 89.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161 116.5) (end 125.5 116.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.5 89) (end 175.5 102) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.5 116.5) (end 159 116.5) (angle 90) (layer Edge.Cuts) (width 0.15))
)
