(kicad_pcb (version 20171130) (host pcbnew 5.1.4)
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 518)
    (zones 0)
    (modules 43)
    (nets 54)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.153)
    (trace_clearance 0.1)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.153)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.7)
    (via_min_drill 0.35)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (aux_axis_origin 0 0)
    (grid_origin 153.67 121.8674)
    (visible_elements FEFFFEFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "grb/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad13)")
  (net 2 "Net-(J1-Pad11)")
  (net 3 "Net-(J1-Pad14)")
  (net 4 "Net-(J1-Pad10)")
  (net 5 "Net-(J1-Pad15)")
  (net 6 "Net-(J1-Pad9)")
  (net 7 "Net-(J1-Pad16)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad17)")
  (net 10 "Net-(J1-Pad7)")
  (net 11 "Net-(J1-Pad6)")
  (net 12 "Net-(J1-Pad5)")
  (net 13 "Net-(J1-Pad4)")
  (net 14 "Net-(J1-Pad3)")
  (net 15 "Net-(J1-Pad2)")
  (net 16 "Net-(J1-Pad1)")
  (net 17 GND)
  (net 18 "Net-(C1-Pad1)")
  (net 19 +5V)
  (net 20 "Net-(C3-Pad2)")
  (net 21 /RESET)
  (net 22 "Net-(C5-Pad1)")
  (net 23 "Net-(C8-Pad1)")
  (net 24 "Net-(C9-Pad1)")
  (net 25 "Net-(D1-Pad1)")
  (net 26 "Net-(D2-Pad1)")
  (net 27 "Net-(D3-Pad2)")
  (net 28 /EOI)
  (net 29 /SCK)
  (net 30 /DAV)
  (net 31 "Net-(R1-Pad1)")
  (net 32 "Net-(R2-Pad1)")
  (net 33 "Net-(R4-Pad1)")
  (net 34 /RX)
  (net 35 "Net-(R5-Pad1)")
  (net 36 /TX)
  (net 37 /DIO1)
  (net 38 /DIO2)
  (net 39 /DIO3)
  (net 40 /DIO4)
  (net 41 /NRFD)
  (net 42 /NDAC)
  (net 43 /IFC)
  (net 44 /SRQ)
  (net 45 /ATN)
  (net 46 /DIO5)
  (net 47 /DIO6)
  (net 48 /DIO7)
  (net 49 /DIO8)
  (net 50 /REN)
  (net 51 "Net-(F1-Pad1)")
  (net 52 /USB_D-)
  (net 53 /USB_D+)
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.153)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ATN)
    (add_net /DAV)
    (add_net /DIO1)
    (add_net /DIO2)
    (add_net /DIO3)
    (add_net /DIO4)
    (add_net /DIO5)
    (add_net /DIO6)
    (add_net /DIO7)
    (add_net /DIO8)
    (add_net /EOI)
    (add_net /IFC)
    (add_net /NDAC)
    (add_net /NRFD)
    (add_net /REN)
    (add_net /RESET)
    (add_net /RX)
    (add_net /SCK)
    (add_net /SRQ)
    (add_net /TX)
    (add_net /USB_D+)
    (add_net /USB_D-)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
  )
  (net_class pwr ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (module hbib:112-024-113R001 locked (layer F.Cu) (tedit 5D93A170)
    (at 153.67 100.33)
    (descr "Connector GPIB")
    (fp_text reference J1 (at -14.055 0 90) (layer F.SilkS) hide)
    (fp_text value Conn_02x12_Top_Bottom (at 0.35772 -5.36894) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at -23.85 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 23.85 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -11.91456 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 13 thru_hole oval (at 11.86772 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad13)"))
    (pad 11 thru_hole oval (at -9.75456 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad11)"))
    (pad 14 thru_hole oval (at 9.70772 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad14)"))
    (pad 10 thru_hole oval (at -7.59456 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad10)"))
    (pad 15 thru_hole oval (at 7.54772 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad15)"))
    (pad 9 thru_hole oval (at -5.43456 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad9)"))
    (pad 16 thru_hole oval (at 5.38772 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad16)"))
    (pad 8 thru_hole oval (at -3.27456 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 17 thru_hole oval (at 3.22772 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad17)"))
    (pad 7 thru_hole oval (at -1.11456 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad7)"))
    (pad 18 thru_hole oval (at 1.06772 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 6 thru_hole oval (at 1.04544 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad6)"))
    (pad 19 thru_hole oval (at -1.09228 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 5 thru_hole oval (at 3.20544 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad 20 thru_hole oval (at -3.25228 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 4 thru_hole oval (at 5.36544 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (pad 21 thru_hole oval (at -5.41228 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 3 thru_hole oval (at 7.52544 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 22 thru_hole oval (at -7.57228 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 2 thru_hole oval (at 9.68544 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 23 thru_hole oval (at -9.73228 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 1 thru_hole oval (at 11.84544 2.145) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad1)"))
    (pad 24 thru_hole oval (at -11.89228 -2.15894) (size 1.35 2) (drill 0.9) (layers *.Cu *.Mask))
  )
  (module hbib:OSHW-Logo_7.5x8mm_Mask (layer F.Cu) (tedit 5D9270B1)
    (at 175.4378 115.4412)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_7.5x8mm_Mask (at 0.75 0) (layer F.Fab) hide)
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 58CC9A48)
    (at 141 113 270)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at 0 -6.05 90) (layer F.SilkS) hide)
    (fp_text value ATmega328P-AU (at 0 6.05 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -4.25 -2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 /REN))
    (pad 2 smd rect (at -4.25 -2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 /DIO7))
    (pad 3 smd rect (at -4.25 -1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 4 smd rect (at -4.25 -0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 5 smd rect (at -4.25 0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 6 smd rect (at -4.25 1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 7 smd rect (at -4.25 2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C9-Pad1)"))
    (pad 8 smd rect (at -4.25 2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C8-Pad1)"))
    (pad 9 smd rect (at -2.8 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 /DIO8))
    (pad 10 smd rect (at -2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -1.2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 /ATN))
    (pad 12 smd rect (at -0.4 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 /IFC))
    (pad 13 smd rect (at 0.4 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 /NDAC))
    (pad 14 smd rect (at 1.2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 /NRFD))
    (pad 15 smd rect (at 2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 /DAV))
    (pad 16 smd rect (at 2.8 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /EOI))
    (pad 17 smd rect (at 4.25 2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 /SCK))
    (pad 18 smd rect (at 4.25 2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 19 smd rect (at 4.25 1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 4.25 0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C5-Pad1)"))
    (pad 21 smd rect (at 4.25 -0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 22 smd rect (at 4.25 -1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 4.25 -2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 /DIO1))
    (pad 24 smd rect (at 4.25 -2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 /DIO2))
    (pad 25 smd rect (at 2.8 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 /DIO3))
    (pad 26 smd rect (at 2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /DIO4))
    (pad 27 smd rect (at 1.2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 /DIO5))
    (pad 28 smd rect (at 0.4 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 /DIO6))
    (pad 29 smd rect (at -0.4 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /RESET))
    (pad 30 smd rect (at -1.2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R4-Pad1)"))
    (pad 31 smd rect (at -2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R5-Pad1)"))
    (pad 32 smd rect (at -2.8 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 /SRQ))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_B3U-1000P (layer F.Cu) (tedit 58724258)
    (at 128.579 112.209 270)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -2.5 90) (layer F.SilkS) hide)
    (fp_text value SW_Push (at 0.6287 3.2427 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -2.5 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.7 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 2 smd rect (at 1.7 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /RESET))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3U-1000P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 152.3915 107.764 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference F1 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value MF-FSMF050X-2 (at 0 1.5 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_3225-4pin_3.2x2.5mm_HandSoldering (layer F.Cu) (tedit 58CD2E9C)
    (at 132 107 180)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, hand-soldering, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at 0 -3.05) (layer F.SilkS) hide)
    (fp_text value "TSX-3225 16.0000MF09Z-AC0" (at 0 3.05) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.45 1.15 180) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.45 1.15 180) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.45 -1.15 180) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C8-Pad1)"))
    (pad 4 smd rect (at -1.45 -1.15 180) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_3225-4pin_3.2x2.5mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 144.8985 105.4145 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R22 (at 0 -1.35 90) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 /REN))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad17)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 133.532 110.558 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R21 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 /DIO8))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad16)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 143.8825 105.4145 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R20 (at 0 -1.35 90) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /DIO7))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad15)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 147.3115 107.8275 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R19 (at 0 -1.35 90) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 /DIO6))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad14)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 148.518 107.8275 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at 0 -1.35 90) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 /DIO5))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad13)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 133.532 111.7645)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R17 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad11)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 /ATN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 146.105 105.4145 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at 0 -1.35 90) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad10)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 /SRQ))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 133.532 112.971)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad9)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 /IFC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 133.532 114.1775)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R14 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /NDAC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 133.532 115.384)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad7)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /NRFD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 133.532 116.5905)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad6)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /DAV))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 133.532 117.797)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /EOI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 149.7245 107.8275 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 0 -1.35 90) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /DIO4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 150.931 107.8275 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at 0 -1.35 90) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /DIO3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 144.8985 119.067 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /DIO2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 142.168 119.067 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /DIO1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 140.8726 105.351 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 -1.35 90) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /SCK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 164.1898 107.256)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /TX))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 164.1644 105.9606)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /RX))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 133.532 119.2956)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /RESET))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 169.473 104.6144 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 169.4658 105.8844 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 -1.35) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm locked (layer F.Cu) (tedit 59650532)
    (at 138.8618 102.4872 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_02x03_Odd_Even (at -16.0232 10.2933) (layer F.SilkS) hide)
    (fp_text user %R (at 0.8424 7.9565 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /EOI))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 +5V))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /DAV))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 57FE9357)
    (at 142.2188 105.5542 90)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -1.2 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.4 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 57FE9357)
    (at 167.441 104.6652 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.2) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.4) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 57FE9357)
    (at 167.4156 105.8844 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.2) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.4) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 136.072 105.3256)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.27) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.27) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 136.072 106.8242)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.27) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.27) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 138.6374 105.5796 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0 -1.27 90) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 1.27 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.27 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 139.3105 119.067)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.27) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.27) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 154.9188 108.9832)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 1.27) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.27) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 131.5508 119.2956 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.27) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.27) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 21 /RESET))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 166.9076 107.6116 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.27) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.27) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 163.4786 118.4574)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.27) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.27) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:USB_Mini-B locked (layer F.Cu) (tedit 5543E571)
    (at 153.67 114.73 90)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (attr smd)
    (fp_text reference J2 (at -0.65 6.9 90) (layer F.SilkS) hide)
    (fp_text value USB_B_Mini (at -0.65 -7.1 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.8 -1.6 90) (size 2.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 2.8 -0.8 90) (size 2.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 52 /USB_D-))
    (pad 3 smd rect (at 2.8 0 90) (size 2.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 53 /USB_D+))
    (pad 4 smd rect (at 2.8 0.8 90) (size 2.3 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 2.8 1.6 90) (size 2.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 6 smd rect (at 2.7 -4.45 90) (size 2.5 2) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 6 smd rect (at -2.8 -4.45 90) (size 2.5 2) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 6 smd rect (at 2.7 4.45 90) (size 2.5 2) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 6 smd rect (at -2.8 4.45 90) (size 2.5 2) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad "" np_thru_hole circle (at 0.2 -2.2 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.2 2.2 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 154.995 107.4084)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value 4u7 (at 0 1.75) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.5) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 166 113 270)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -6.25 90) (layer F.SilkS) hide)
    (fp_text value FT232RL (at 0 6.25 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3.6 -4.225 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 /RX))
    (pad 2 smd rect (at -3.6 -3.575 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C3-Pad2)"))
    (pad 3 smd rect (at -3.6 -2.925 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -3.6 -2.275 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 5 smd rect (at -3.6 -1.625 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 /TX))
    (pad 6 smd rect (at -3.6 -0.975 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -3.6 -0.325 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 8 smd rect (at -3.6 0.325 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -3.6 0.975 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -3.6 1.625 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -3.6 2.275 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -3.6 2.925 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -3.6 3.575 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -3.6 4.225 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 3.6 4.225 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 /USB_D+))
    (pad 16 smd rect (at 3.6 3.575 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 /USB_D-))
    (pad 17 smd rect (at 3.6 2.925 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C1-Pad1)"))
    (pad 18 smd rect (at 3.6 2.275 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 19 smd rect (at 3.6 1.625 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 3.6 0.975 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 21 smd rect (at 3.6 0.325 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 22 smd rect (at 3.6 -0.325 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R2-Pad1)"))
    (pad 23 smd rect (at 3.6 -0.975 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R1-Pad1)"))
    (pad 24 smd rect (at 3.6 -1.625 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 3.6 -2.275 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 26 smd rect (at 3.6 -2.925 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 3.6 -3.575 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 3.6 -4.225 270) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "yet another\nArduino GPIB\ninterface V0.1" (at 175.8061 108.4181) (layer F.Mask))
  (dimension 31.9786 (width 0.15) (layer Dwgs.User)
    (gr_text "31.979 mm" (at 190.5554 105.6749 270) (layer Dwgs.User))
    (feature1 (pts (xy 176.9237 121.6642) (xy 189.841821 121.6642)))
    (feature2 (pts (xy 176.9237 89.6856) (xy 189.841821 89.6856)))
    (crossbar (pts (xy 189.2554 89.6856) (xy 189.2554 121.6642)))
    (arrow1a (pts (xy 189.2554 121.6642) (xy 188.668979 120.537696)))
    (arrow1b (pts (xy 189.2554 121.6642) (xy 189.841821 120.537696)))
    (arrow2a (pts (xy 189.2554 89.6856) (xy 188.668979 90.812104)))
    (arrow2b (pts (xy 189.2554 89.6856) (xy 189.841821 90.812104)))
  )
  (gr_arc (start 177.681499 118.4892) (end 177.684499 121.7277) (angle -89.9469238) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.02 121.095) (end 160.655 121.095) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 147.32 121.095) (end 147.32 120.46) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.684499 121.7277) (end 161.29 121.7277) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.02 120.46) (end 147.32 120.46) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.29 121.095) (end 160.655 121.095) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.05 121.095) (end 146.05 121.73) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.42 91.73) (end 128.42 89.73) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 178.92 91.73) (end 180.92 91.73) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 129.67 118.48) (end 126.42 118.48) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.42 89.73) (end 178.92 89.73) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.67 121.73) (end 146.05 121.73) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.42 91.73) (end 126.42 118.48) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.92 91.73) (end 180.92 118.4892) (layer Edge.Cuts) (width 0.15))
  (dimension 54.5 (width 0.15) (layer Dwgs.User)
    (gr_text "54.500 mm" (at 153.67 83.7) (layer Dwgs.User))
    (feature1 (pts (xy 180.92 89.73) (xy 180.92 84.413579)))
    (feature2 (pts (xy 126.42 89.73) (xy 126.42 84.413579)))
    (crossbar (pts (xy 126.42 85) (xy 180.92 85)))
    (arrow1a (pts (xy 180.92 85) (xy 179.793496 85.586421)))
    (arrow1b (pts (xy 180.92 85) (xy 179.793496 84.413579)))
    (arrow2a (pts (xy 126.42 85) (xy 127.546504 85.586421)))
    (arrow2b (pts (xy 126.42 85) (xy 127.546504 84.413579)))
  )
  (zone (net 17) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 181.5973 88.8982) (xy 125.6157 89.0252) (xy 125.2601 122.7056) (xy 182.3847 121.9944) (xy 181.8005 93.4448)
      )
    )
  )
  (zone (net 17) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 182.0672 88.7839) (xy 182.0926 91.7557) (xy 182.245 123.8105) (xy 124.9934 123.5946) (xy 124.8283 88.2251)
      )
    )
  )
)
