(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (title "Beetje 32U4 Blok")
    (date "2018-08-10")
    (rev "0.0")
    (company "www.MakersBox.us")
    (comment 1 "648.ken@gmail.com")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/D4")
  (net 3 "Net-(C6-Pad2)")
  (net 4 "/D13")
  (net 5 "/D12")
  (net 6 "/D10")
  (net 7 "/D9")
  (net 8 "/D7")
  (net 9 "/A0")
  (net 10 "/A3")
  (net 11 "/A5")
  (net 12 "/SCK")
  (net 13 "/MOSI")
  (net 14 "/MISO")
  (net 15 "/D5")
  (net 16 "Net-(C11-Pad2)")
  (net 17 "/~{RESET}")
  (net 18 "/D+")
  (net 19 "/D-")
  (net 20 "Net-(D2-Pad1)")
  (net 21 "+3V3")
  (net 22 "VBUS")
  (net 23 "Net-(R2-Pad1)")
  (net 24 "/D2")
  (net 25 "unconnected-(J1-Pad4)")
  (net 26 "/SCL")
  (net 27 "/SDA")
  (net 28 "unconnected-(P1-Pad1)")
  (net 29 "/D11")
  (net 30 "/A1")
  (net 31 "/A2")
  (net 32 "/A4")
  (net 33 "unconnected-(P2-Pad1)")
  (net 34 "unconnected-(P3-Pad1)")
  (net 35 "unconnected-(P4-Pad1)")
  (net 36 "unconnected-(P5-Pad1)")
  (net 37 "unconnected-(P6-Pad1)")
  (net 38 "Net-(R1-Pad1)")
  (net 39 "Net-(R4-Pad1)")
  (net 40 "Net-(R10-Pad1)")
  (net 41 "Net-(R12-Pad1)")
  (net 42 "/AREF")
  (net 43 "+5V")
  (net 44 "Net-(R15-Pad1)")
  (net 45 "/SWCLK")
  (net 46 "/DOTSTAR_CLK")
  (net 47 "/DOTSTAR_DATA")
  (net 48 "unconnected-(RGB1-Pad5)")
  (net 49 "/01")
  (net 50 "/02")
  (net 51 "/03")
  (net 52 "/04")
  (net 53 "/05")
  (net 54 "/06")
  (net 55 "/07")
  (net 56 "/08")
  (net 57 "/09")
  (net 58 "/10")
  (net 59 "/11")
  (net 60 "/12")
  (net 61 "/13")
  (net 62 "/14")
  (net 63 "/15")
  (net 64 "/16")
  (net 65 "/24")
  (net 66 "/23")
  (net 67 "/22")
  (net 68 "/21")
  (net 69 "/20")
  (net 70 "/19")
  (net 71 "/18")
  (net 72 "/17")
  (net 73 "unconnected-(RGB1-Pad6)")
  (net 74 "/D3")
  (net 75 "unconnected-(U1-Pad5)")
  (net 76 "unconnected-(U1-Pad6)")
  (net 77 "unconnected-(U1-Pad8)")
  (net 78 "unconnected-(U2-Pad4)")
  (net 79 "/25")
  (net 80 "/26")
  (net 81 "/27")
  (net 82 "/28")
  (net 83 "/29")
  (net 84 "/30")
  (net 85 "/31")
  (net 86 "/32")
  (net 87 "/40")
  (net 88 "/39")
  (net 89 "/38")
  (net 90 "/37")
  (net 91 "/36")
  (net 92 "/35")
  (net 93 "/34")
  (net 94 "/33")
  (net 95 "unconnected-(U3-Pad5)")
  (net 96 "unconnected-(U3-Pad6)")
  (net 97 "unconnected-(U3-Pad8)")
  (net 98 "unconnected-(U4-Pad5)")
  (net 99 "unconnected-(U4-Pad6)")
  (net 100 "unconnected-(U4-Pad8)")
  (net 101 "unconnected-(U5-Pad39)")
  (net 102 "Net-(L1-Pad2)")
  (net 103 "unconnected-(U9-Pad5)")
  (net 104 "unconnected-(U6-Pad5)")
  (net 105 "unconnected-(U6-Pad6)")
  (net 106 "unconnected-(U6-Pad8)")
  (net 107 "/QSPI_CS")
  (net 108 "/QSPI_DATA_0")
  (net 109 "/QSPI_SCK")
  (net 110 "/QSPI_DATA_1")
  (net 111 "/QSPI_DATA_2")
  (net 112 "/QSPI_DATA_3")
  (net 113 "/RX_D0")
  (net 114 "/TX_D1")
  (net 115 "unconnected-(U9-Pad6)")
  (net 116 "unconnected-(U9-Pad8)")
  (net 117 "/SWDIO")
  (net 118 "Net-(R9-Pad2)")
  (net 119 "Net-(D11-Pad1)")
  (net 120 "Net-(D13-Pad1)")
  (net 121 "unconnected-(J4-Pad1)")
  (net 122 "unconnected-(J4-Pad2)")
  (net 123 "Net-(U7-Pad1)")
  (net 124 "Net-(U7-Pad2)")
  (footprint "footprints:LED_0603" (layer "F.Cu")
    (tedit 636FBDBF)
    (at 109.95 87)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 2.032 0) (layer "F.SilkS") hide)
    (fp_text value "PWR" (at 0.032 1.392 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -0.8 0 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 0.8 0 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KIPRJMOD}/3D/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603" (layer "F.Cu")
    (tedit 636FBDBF)
    (at 168.364 124.46 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D13" (at 2.032 0 180) (layer "F.SilkS") hide)
    (fp_text value "D13" (at 3.01 0 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "Net-(D13-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/D13") (pinfunction "A") (pintype "passive"))
    (model "${KIPRJMOD}/3D/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:USB_Micro-B_Molex-105017-0001" locked (layer "F.Cu")
    (tedit 636FBEAD)
    (at 109.22 100.33 -90)
    (descr "http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf")
    (tags "Micro-USB SMD Typ-B")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 0 -1.016 -90) (layer "F.Fab"))
    (fp_text value "USB" (at 0 -3.81 -90) (layer "F.SilkS"))
    (fp_text user "PCB Edge" (at 0 1.8 -90) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.3 -2.35 270) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "+5V") (pinfunction "VBUS") (pintype "power_in"))
    (pad "2" smd rect locked (at -0.65 -2.35 270) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/D-") (pinfunction "D-") (pintype "passive"))
    (pad "3" smd rect locked (at 0 -2.35 270) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/D+") (pinfunction "D+") (pintype "passive"))
    (pad "4" smd rect locked (at 0.65 -2.35 270) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "unconnected-(J1-Pad4)") (pinfunction "ID") (pintype "passive"))
    (pad "5" smd rect locked (at 1.3 -2.35 270) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole oval locked (at -3.5 0.35 90) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect locked (at 2.9 0.35 270) (size 1.2 1.9) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect locked (at 1 0.35 270) (size 1.5 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.5 -2.35 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect locked (at -2.9 0.35 270) (size 1.2 1.9) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect locked (at -1 0.35 270) (size 1.5 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 3.5 0.35 270) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole circle locked (at -2.5 -2.35 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KIPRJMOD}/3D/USB_micro_105017-0001.stp"
      (offset (xyz 0 0 1.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "footprints:M3mount" (layer "F.Cu")
    (tedit 636FC1C2)
    (at 110.49 80.01)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at 0 -3.3) (layer "F.SilkS") hide)
    (fp_text value "M3" (at 0.1 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 28 "unconnected-(P1-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "footprints:M25standoff" (layer "F.Cu")
    (tedit 636FF644)
    (at 168 87.75)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P5" (at 0 -5.08) (layer "F.SilkS") hide)
    (fp_text value "Standoff" (at 0 5.08) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 6 6) (drill 3.7) (layers *.Cu *.Mask)
      (net 36 "unconnected-(P5-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/3D/standoff9774027151R (rev1).stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3D/M2_5X6MM.step"
      (offset (xyz 0 0 6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603" (layer "F.Cu")
    (tedit 636FBDBF)
    (at 168.402 122.428 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D11" (at 2.032 0 180) (layer "F.SilkS") hide)
    (fp_text value "D11" (at 3.048 0 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "Net-(D11-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/D11") (pinfunction "A") (pintype "passive"))
    (model "${KIPRJMOD}/3D/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:M3mount" (layer "F.Cu")
    (tedit 636FC1C2)
    (at 167.64 80.01)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P2" (at 0 -3.3) (layer "F.SilkS") hide)
    (fp_text value "M3" (at 0.1 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 33 "unconnected-(P2-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "footprints:M3mount" (layer "F.Cu")
    (tedit 636FC1C2)
    (at 167.64 131)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P4" (at 0 -3.3) (layer "F.SilkS") hide)
    (fp_text value "M3" (at 0.1 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 35 "unconnected-(P4-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "footprints:M25standoff" (layer "F.Cu")
    (tedit 636FF644)
    (at 168 110)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P6" (at 0 -5.08) (layer "F.SilkS") hide)
    (fp_text value "Standoff" (at 0 5.08) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 6 6) (drill 3.7) (layers *.Cu *.Mask)
      (net 37 "unconnected-(P6-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/3D/standoff9774027151R (rev1).stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3D/M2_5X6MM.step"
      (offset (xyz 0 0 6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 110 85.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "1K" (at 2.014 0 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 163.068 104.21 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "1K" (at 2.159 -0.057) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "Net-(D13-Pad1)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 163.068 102.305 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "1K" (at 2.159 -0.057) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "Net-(D11-Pad1)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0805_HandSoldering" (layer "F.Cu")
    (tedit 636FC06B)
    (at 109.22 92.376 -90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at -0.14 -1.784 -90) (layer "F.Fab"))
    (fp_text value "Polyfuse" (at 0 1.778 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.35 0 270) (size 1.5 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "+5V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.35 0 270) (size 1.5 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3D/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SAMTEC_MEC8-113-TOP-BOTTOM" locked (layer "F.Cu")
    (tedit 63786631)
    (at 119 110 90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X2" (at -9.38 0.126 180) (layer "F.SilkS"))
    (fp_text value "MEC8-113" (at 8.21 6.135 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad "1" smd rect locked (at -6.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/21") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect locked (at -5.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/22") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect locked (at -4.8 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/23") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect locked (at -4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/24") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect locked (at -3.2 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/25") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect locked (at -2.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/26") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect locked (at 1.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/27") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect locked (at 2.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/28") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect locked (at 3.2 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/29") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect locked (at 4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "/30") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect locked (at 4.8 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/A1") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect locked (at 5.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/A3") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect locked (at 6.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "VBUS") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect locked (at -6.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/31") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect locked (at -5.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "/32") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect locked (at -4.8 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "/33") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect locked (at -4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "/34") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect locked (at -3.2 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "/35") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect locked (at -2.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "/36") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect locked (at 1.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "/37") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect locked (at 2.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/38") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect locked (at 3.2 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/39") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect locked (at 4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/40") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect locked (at 4.8 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/SCL") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect locked (at 5.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/SDA") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect locked (at 6.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_26") (pintype "passive"))
    (model "${KIPRJMOD}/3D/mec8-113-02-l-d-ra1.stp"
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 143.625 120.015 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at -2.032 0) (layer "Dwgs.User"))
    (fp_text value "4K7" (at 2.286 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/SDA") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:MEC8-113-CARD_2outline" locked (layer "F.Cu")
    (tedit 637EA855)
    (at 116.459 120 90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "CardOutline2" (at 4.375 -1.25 90) (layer "F.Fab"))
    (fp_text value "SYM_Arrow_Large" (at 10.9 -1 90) (layer "F.Fab"))
  )
  (footprint "footprints:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm" (layer "F.Cu")
    (tedit 63CC3BF1)
    (at 132 118 180)
    (descr "QFN, 20 Pin (https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U9" (at 3.222 -0.0084 180) (layer "F.SilkS"))
    (fp_text value "MCP23008" (at 0 3.3 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.675 0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 -0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 -0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "1" smd roundrect (at -1.95 -1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "A2") (pintype "input"))
    (pad "2" smd roundrect (at -1.95 -0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A1") (pintype "input"))
    (pad "3" smd roundrect (at -1.95 0 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A0") (pintype "input"))
    (pad "4" smd roundrect (at -1.95 0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(R15-Pad1)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "5" smd roundrect (at -1.95 1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "unconnected-(U9-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at -1 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "unconnected-(U9-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -0.5 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/D7") (pinfunction "INT") (pintype "output"))
    (pad "8" smd roundrect (at 0 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "unconnected-(U9-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd roundrect (at 0.5 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "/40") (pinfunction "GP0") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 1 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/39") (pinfunction "GP1") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 1.95 1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/38") (pinfunction "GP2") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 1.95 0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "/37") (pinfunction "GP3") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 1.95 0 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "/36") (pinfunction "GP4") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.95 -0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "/35") (pinfunction "GP5") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 1.95 -1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "/34") (pinfunction "GP6") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 1 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "/33") (pinfunction "GP7") (pintype "bidirectional"))
    (pad "17" smd rect (at 0 0 180) (size 2.7 2.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "17" smd roundrect (at 0.5 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "18" smd roundrect (at 0 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "19" smd roundrect (at -0.5 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "20" smd roundrect (at -1 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm" (layer "F.Cu")
    (tedit 63CC3BF1)
    (at 132 82 180)
    (descr "QFN, 20 Pin (https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 3.222 0.085 180) (layer "F.SilkS"))
    (fp_text value "MCP23008" (at 0 3.3 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "" smd roundrect (at 0.675 0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 -0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 -0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "1" smd roundrect (at -1.95 -1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A2") (pintype "input"))
    (pad "2" smd roundrect (at -1.95 -0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A1") (pintype "input"))
    (pad "3" smd roundrect (at -1.95 0 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "A0") (pintype "input"))
    (pad "4" smd roundrect (at -1.95 0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(R4-Pad1)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "5" smd roundrect (at -1.95 1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "unconnected-(U3-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at -1 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "unconnected-(U3-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -0.5 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/MOSI") (pinfunction "INT") (pintype "output"))
    (pad "8" smd roundrect (at 0 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "unconnected-(U3-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd roundrect (at 0.5 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/16") (pinfunction "GP0") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 1 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/15") (pinfunction "GP1") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 1.95 1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/14") (pinfunction "GP2") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 1.95 0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/13") (pinfunction "GP3") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 1.95 0 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/12") (pinfunction "GP4") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.95 -0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/11") (pinfunction "GP5") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 1.95 -1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/10") (pinfunction "GP6") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 1 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/09") (pinfunction "GP7") (pintype "bidirectional"))
    (pad "17" smd rect (at 0 0 180) (size 2.7 2.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "17" smd roundrect (at 0.5 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "18" smd roundrect (at 0 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "19" smd roundrect (at -0.5 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "20" smd roundrect (at -1 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm" (layer "F.Cu")
    (tedit 63CC3BF1)
    (at 132 100 180)
    (descr "QFN, 20 Pin (https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 4.2126 -0.9142 180) (layer "F.SilkS"))
    (fp_text value "MCP23008" (at 0 3.3 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.675 0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 -0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 -0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "1" smd roundrect (at -1.95 -1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A2") (pintype "input"))
    (pad "2" smd roundrect (at -1.95 -0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "A1") (pintype "input"))
    (pad "3" smd roundrect (at -1.95 0 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A0") (pintype "input"))
    (pad "4" smd roundrect (at -1.95 0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(R10-Pad1)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "5" smd roundrect (at -1.95 1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "unconnected-(U4-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at -1 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "unconnected-(U4-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -0.5 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/MISO") (pinfunction "INT") (pintype "output"))
    (pad "8" smd roundrect (at 0 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "unconnected-(U4-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd roundrect (at 0.5 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/24") (pinfunction "GP0") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 1 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/23") (pinfunction "GP1") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 1.95 1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/22") (pinfunction "GP2") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 1.95 0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "/21") (pinfunction "GP3") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 1.95 0 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "/20") (pinfunction "GP4") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.95 -0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/19") (pinfunction "GP5") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 1.95 -1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/18") (pinfunction "GP6") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 1 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "/17") (pinfunction "GP7") (pintype "bidirectional"))
    (pad "17" smd roundrect (at 0.5 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "17" smd rect (at 0 0 180) (size 2.7 2.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "18" smd roundrect (at 0 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "19" smd roundrect (at -0.5 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "20" smd roundrect (at -1 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm" (layer "F.Cu")
    (tedit 63CC3BF1)
    (at 132 109 180)
    (descr "QFN, 20 Pin (https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at 3.222 -0.093 180) (layer "F.SilkS"))
    (fp_text value "MCP23008" (at 0 3.3 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.675 -0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 -0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "1" smd roundrect (at -1.95 -1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A2") (pintype "input"))
    (pad "2" smd roundrect (at -1.95 -0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "A1") (pintype "input"))
    (pad "3" smd roundrect (at -1.95 0 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "A0") (pintype "input"))
    (pad "4" smd roundrect (at -1.95 0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(R12-Pad1)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "5" smd roundrect (at -1.95 1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "unconnected-(U6-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at -1 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "unconnected-(U6-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -0.5 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/D9") (pinfunction "INT") (pintype "output"))
    (pad "8" smd roundrect (at 0 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "unconnected-(U6-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd roundrect (at 0.5 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "/32") (pinfunction "GP0") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 1 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/31") (pinfunction "GP1") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 1.95 1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "/30") (pinfunction "GP2") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 1.95 0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/29") (pinfunction "GP3") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 1.95 0 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/28") (pinfunction "GP4") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.95 -0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "/27") (pinfunction "GP5") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 1.95 -1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "/26") (pinfunction "GP6") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 1 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "/25") (pinfunction "GP7") (pintype "bidirectional"))
    (pad "17" smd rect (at 0 0 180) (size 2.7 2.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "17" smd roundrect (at 0.5 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "18" smd roundrect (at 0 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "19" smd roundrect (at -0.5 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "20" smd roundrect (at -1 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm" (layer "F.Cu")
    (tedit 63CC3BF1)
    (at 132 91 180)
    (descr "QFN, 20 Pin (https://www.silabs.com/documents/public/data-sheets/Si5351-B.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 3.222 -0.0082 180) (layer "F.SilkS"))
    (fp_text value "MCP23008" (at 0 3.3 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.675 -0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 -0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at 0.675 0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "" smd roundrect (at -0.675 0.675 180) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.229358))
    (pad "1" smd roundrect (at -1.95 -1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A2") (pintype "input"))
    (pad "2" smd roundrect (at -1.95 -0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A1") (pintype "input"))
    (pad "3" smd roundrect (at -1.95 0 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A0") (pintype "input"))
    (pad "4" smd roundrect (at -1.95 0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R1-Pad1)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "5" smd roundrect (at -1.95 1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "unconnected-(U1-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at -1 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "unconnected-(U1-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -0.5 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/SCK") (pinfunction "INT") (pintype "output"))
    (pad "8" smd roundrect (at 0 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "unconnected-(U1-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd roundrect (at 0.5 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/08") (pinfunction "GP0") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 1 1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/07") (pinfunction "GP1") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 1.95 1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/06") (pinfunction "GP2") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 1.95 0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/05") (pinfunction "GP3") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 1.95 0 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/04") (pinfunction "GP4") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.95 -0.5 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/03") (pinfunction "GP5") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 1.95 -1 180) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/02") (pinfunction "GP6") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 1 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/01") (pinfunction "GP7") (pintype "bidirectional"))
    (pad "17" smd rect (at 0 0 180) (size 2.7 2.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "17" smd roundrect (at 0.5 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "18" smd roundrect (at 0 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "19" smd roundrect (at -0.5 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "20" smd roundrect (at -1 -1.95 180) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SAMTEC_MEC8-113-TOP-BOTTOM" locked (layer "F.Cu")
    (tedit 63786631)
    (at 119 87.75 90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X1" (at -9.278 0.126 180) (layer "F.SilkS"))
    (fp_text value "MEC8-113" (at 8.21 6.135 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad "1" smd rect locked (at -6.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/01") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect locked (at -5.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect locked (at -4.8 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect locked (at -4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect locked (at -3.2 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/05") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect locked (at -2.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/06") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect locked (at 1.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/07") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect locked (at 2.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/08") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect locked (at 3.2 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/09") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect locked (at 4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/10") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect locked (at 4.8 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/A0") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect locked (at 5.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/A2") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect locked (at 6.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "VBUS") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect locked (at -6.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/11") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect locked (at -5.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/12") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect locked (at -4.8 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/13") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect locked (at -4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/14") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect locked (at -3.2 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/15") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect locked (at -2.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/16") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect locked (at 1.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/17") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect locked (at 2.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/18") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect locked (at 3.2 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/19") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect locked (at 4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/20") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect locked (at 4.8 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/SCL") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect locked (at 5.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/SDA") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect locked (at 6.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_26") (pintype "passive"))
    (model "${KIPRJMOD}/3D/mec8-113-02-l-d-ra1.stp"
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "footprints:MEC8-113-CARD_2outline" locked (layer "F.Cu")
    (tedit 637EA855)
    (at 116.5 97.75 90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "CardOutline1" (at 4.375 -1.25 90) (layer "F.Fab"))
    (fp_text value "SYM_Arrow_Large" (at 10.9 -1 90) (layer "F.Fab"))
  )
  (footprint "footprints:SW_TS10-63-26-BE-250-SMT-TR" (layer "F.Cu")
    (tedit 63700F76)
    (at 169.4 100.3 90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW3" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "RESET" (at 6.32 1.034 270) (layer "F.SilkS"))
    (pad "1" smd rect (at -3.25 0 90) (size 1.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "Net-(R9-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 3.25 0 90) (size 1.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/3D/434121025816_Wurth_tactile.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 143.625 118.11 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at -2.032 0) (layer "Dwgs.User"))
    (fp_text value "4K7" (at 2.286 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/SCL") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:M3mount" (layer "F.Cu")
    (tedit 636FC1C2)
    (at 110.49 131)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P3" (at 0 -3.3) (layer "F.SilkS") hide)
    (fp_text value "M3" (at 0.1 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 34 "unconnected-(P3-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "footprints:SW_TS10-63-26-BE-250-SMT-TR" (layer "F.Cu")
    (tedit 63700F76)
    (at 116.3 129 -90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 0 0 -90) (layer "F.SilkS"))
    (fp_text value "D4" (at 5.112 -0.2298) (layer "F.SilkS"))
    (pad "1" smd rect (at -3.25 0 270) (size 1.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/D4") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 3.25 0 270) (size 1.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/3D/434121025816_Wurth_tactile.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:I2C_OLED_DISP" (layer "F.Cu")
    (tedit 63CC6AF2)
    (at 156.3 123.7)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.Fab"))
    (fp_text value "I2C" (at -0.022 9.294) (layer "F.SilkS"))
    (fp_text user "I2C OLED DISPLAY" (at -18 4 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/SCL") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/SDA") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KIPRJMOD}/3D/OLED_0.91_128x32.stp"
      (offset (xyz -17.5 -3.75 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "footprints:SW_TS10-63-26-BE-250-SMT-TR" (layer "F.Cu")
    (tedit 63700F76)
    (at 162 129 -90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 0 0 -90) (layer "F.SilkS"))
    (fp_text value "D3" (at 5.112 -0.2298) (layer "F.SilkS"))
    (pad "1" smd rect (at -3.25 0 270) (size 1.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/D3") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 3.25 0 270) (size 1.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/3D/434121025816_Wurth_tactile.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 143.51 100.838)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP5" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "D1" (at -1.016 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 114 "/TX_D1") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 136.144 92.214 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -2 0 90) (layer "F.Fab"))
    (fp_text value "0.1uF" (at -0.496 1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 156.21 98.044)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "D2" (at 1 0) (layer "F.SilkS"))
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 24 "/D2") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 142.24 82.284 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 1.905 0 270) (layer "Dwgs.User"))
    (fp_text value "0" (at 0.0134 -1.1176 270) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "VBUS") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "+5V") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 155.714 83.185 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "10K" (at -2.147 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "Net-(U7-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 152.194 116.332 90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.06 90) (layer "F.Fab"))
    (fp_text value "SWD" (at 0 9.096 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "/SWCLK") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "/SWDIO") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 110.5 117.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "100K" (at 3.038 0.102 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 136.144 101.358 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -2 0 90) (layer "F.Fab"))
    (fp_text value "0.1uF" (at -0.496 1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 152.388 85.598 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at -2 0 180) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 4.56 -1.27 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 180) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 180) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 149.098 112.1664)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 2.032 -0.254) (layer "F.Fab"))
    (fp_text value "100nF" (at -3.048 0.0254) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/~{RESET}") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:L_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 149.9405 110.5154)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L1" (at 2.4595 0.1016) (layer "F.Fab"))
    (fp_text value "10uH" (at -3.4815 -0.0254) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0625 0) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C11-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0625 0) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "Net-(L1-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 143.51 98.044)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "D5" (at -1.016 0) (layer "F.SilkS"))
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 15 "/D5") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 163.08 97.79)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "1K" (at -2.286 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/SWCLK") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 110.5 120.75 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.4 -90) (layer "F.Fab"))
    (fp_text value "AP2127K" (at 0 2.4 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C6-Pad2)") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(R2-Pad1)") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "unconnected-(U2-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 143.51 96.52)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP6" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "3V3" (at -1.27 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 21 "+3V3") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 136.144 89.408 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "10K" (at -0.254 -1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 136.144 110.248 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -2 0 90) (layer "F.Fab"))
    (fp_text value "0.1uF" (at -0.496 1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 148.987 108.839 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at -2 0 180) (layer "F.Fab"))
    (fp_text value "4.7uF" (at 2.9624 0.0254 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 180) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 180) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(C11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0805" (layer "F.Cu")
    (tedit 636FC0BD)
    (at 110.5 124 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.5) (layer "F.Fab"))
    (fp_text value "10uF" (at 0 -1.73) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd rect (at -1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 143.51 99.568)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP4" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "D0" (at -1.016 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 113 "/RX_D0") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:1x4spacer" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 123 123.7)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "SPACER" (at 0 4 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 121 "unconnected-(J4-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 122 "unconnected-(J4-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOP-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 153.7558 93.3064)
    (descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOP SO")
    (property "Footprint_1" "")
    (property "MPN" "GD25Q16CTIGR")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "GD25x16")
    (attr smd)
    (fp_text reference "U8" (at 0 0) (layer "F.Fab"))
    (fp_text value "GD25x16" (at 0 3.4) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "/QSPI_CS") (pinfunction "SSEL") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "/QSPI_DATA_1") (pinfunction "MISO") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "/QSPI_DATA_2") (pinfunction "WP#/IO2") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "bidirectional"))
    (pad "5" smd roundrect (at 2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "/QSPI_DATA_0") (pinfunction "MOSI") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "/QSPI_SCK") (pinfunction "SCK") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "/QSPI_DATA_3") (pinfunction "HOLD#/IO3") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VCC") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 113.538 120.384 -90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at -2 0 -90) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 3.06 -1.27 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 150.114 81.28 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U7" (at 0 0 180) (layer "F.Fab"))
    (fp_text value "INA219AxD" (at 0 3.4 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "Net-(U7-Pad1)") (pinfunction "A1") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(U7-Pad2)") (pinfunction "A0") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "5" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VS") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "VBUS") (pinfunction "IN-") (pintype "input"))
    (pad "8" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "+5V") (pinfunction "IN+") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 136.144 83.324 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -2 0 90) (layer "F.Fab"))
    (fp_text value "0.1uF" (at -0.496 1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 143.51 95.25)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP7" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "GND" (at -1.27 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:C_0805" (layer "F.Cu")
    (tedit 636FC0BD)
    (at 110.5 115)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.5) (layer "F.Fab"))
    (fp_text value "10uF" (at 0.244 -1.462) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd rect (at -1 0) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 1 0) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 153.7342 89.5096)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "100K" (at -2.6296 0.0254 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "/QSPI_CS") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 136.144 116.574 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "10K" (at -0.75 -1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(R15-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 136.144 119.392 -90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -2 0 -90) (layer "F.Fab"))
    (fp_text value "0.1uF" (at -0.266 -1.27 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 147.828 85.598)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at -2 0) (layer "F.Fab"))
    (fp_text value "1uF" (at 4.572 1.27) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 136.144 98.564 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "10K" (at -1.028 -1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(R10-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm" (layer "F.Cu")
    (tedit 5DC5F6A5)
    (at 150.5204 103.2002 180)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at 0 -4.82) (layer "F.Fab"))
    (fp_text value "ATSAMD51G" (at -0.1016 5.1562) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "1" smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/MOSI") (pinfunction "PA00") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/SCK") (pinfunction "PA01") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/A0") (pinfunction "PA02") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/AREF") (pinfunction "PA03") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GNDANA") (pintype "power_in"))
    (pad "6" smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VDDANA") (pintype "power_in"))
    (pad "7" smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/A2") (pinfunction "PB08") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/A3") (pinfunction "PB09") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/A4") (pinfunction "PA04") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/A1") (pinfunction "PA05") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/A5") (pinfunction "PA06") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/D2") (pinfunction "PA07") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "/QSPI_DATA_0") (pinfunction "PA08") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "/QSPI_DATA_1") (pinfunction "PA09") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "/QSPI_DATA_2") (pinfunction "PA10") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "/QSPI_DATA_3") (pinfunction "PA11") (pintype "bidirectional"))
    (pad "17" smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "18" smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "19" smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "/QSPI_SCK") (pinfunction "PB10") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "/QSPI_CS") (pinfunction "PB11") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/SDA") (pinfunction "PA12") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/SCL") (pinfunction "PA13") (pintype "bidirectional"))
    (pad "23" smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/D4") (pinfunction "PA14") (pintype "bidirectional"))
    (pad "24" smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/D5") (pinfunction "PA15") (pintype "bidirectional"))
    (pad "25" smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "/RX_D0") (pinfunction "PA16") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "/TX_D1") (pinfunction "PA17") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/D7") (pinfunction "PA18") (pintype "bidirectional"))
    (pad "28" smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/D9") (pinfunction "PA19") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/D10") (pinfunction "PA20") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/D11") (pinfunction "PA21") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/D13") (pinfunction "PA22") (pintype "bidirectional"))
    (pad "32" smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/D12") (pinfunction "PA23") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/D-") (pinfunction "PA24") (pintype "bidirectional"))
    (pad "34" smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/D+") (pinfunction "PA25") (pintype "bidirectional"))
    (pad "35" smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "36" smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "37" smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "/D3") (pinfunction "PB22") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/MISO") (pinfunction "PB23") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "unconnected-(U5-Pad39)") (pinfunction "PA27") (pintype "bidirectional+no_connect"))
    (pad "40" smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/~{RESET}") (pinfunction "~{RESET}") (pintype "input"))
    (pad "41" smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C11-Pad2)") (pinfunction "VDDCORE") (pintype "power_in"))
    (pad "42" smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "43" smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "Net-(L1-Pad2)") (pinfunction "VSW") (pintype "power_out"))
    (pad "44" smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "45" smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/SWCLK") (pinfunction "PA30") (pintype "bidirectional"))
    (pad "46" smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "/SWDIO") (pinfunction "PA31") (pintype "bidirectional"))
    (pad "47" smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/DOTSTAR_CLK") (pinfunction "PB02") (pintype "bidirectional"))
    (pad "48" smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/DOTSTAR_DATA") (pinfunction "PB03") (pintype "bidirectional"))
    (pad "49" smd rect (at 0 0 180) (size 5.15 5.15) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "EP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 136.144 80.53 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "10K" (at -0.52 -1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 163.03 100.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "330" (at -2.552 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/~{RESET}") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "Net-(R9-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 113.5 123.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at -2 0 90) (layer "F.Fab"))
    (fp_text value "1uF" (at 3.358 1.308 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_2512_6332Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.24 82.296 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 -2.62 90) (layer "F.Fab"))
    (fp_text value "0.1" (at 0 2.62 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.9625 0 90) (size 1.225 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 22 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 2.9625 0 90) (size 1.225 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 43 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 156.21 104.001 -90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at -2 0 90) (layer "F.Fab"))
    (fp_text value "1uF" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/AREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 156.21 99.568)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "A5" (at 1 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 11 "/A5") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 155.702 81.661 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "10K" (at -2.159 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "Net-(U7-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Jumper" (layer "F.Cu")
    (tedit 5B6DD72B)
    (at 155.706 85.852)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "A0" (at 2.028 0) (layer "F.SilkS"))
    (fp_text value "Jumper" (at 0 1.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.2) (layer "F.Fab"))
    (pad "1" smd rect (at -0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "Net-(U7-Pad1)") (pinfunction "A") (pintype "passive") (clearance 0.1))
    (pad "2" smd rect (at 0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pinfunction "B") (pintype "passive") (clearance 0.1))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 136.144 107.43 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "10K" (at -0.496 -1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(R12-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Jumper" (layer "F.Cu")
    (tedit 5B6DD72B)
    (at 155.706 84.709)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "A1" (at 2.028 0) (layer "F.SilkS"))
    (fp_text value "Jumper" (at 0 1.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.2) (layer "F.Fab"))
    (pad "1" smd rect (at -0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "Net-(U7-Pad2)") (pinfunction "A") (pintype "passive") (clearance 0.1))
    (pad "2" smd rect (at 0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pinfunction "B") (pintype "passive") (clearance 0.1))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SK9822_ADA" (layer "F.Cu")
    (tedit 0)
    (at 110 109.75 -90)
    (tags "2343 ")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RGB1" (at 0 0 unlocked) (layer "F.SilkS"))
    (fp_text value "DOTSTAR" (at -3.959 -0.109 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -2.6416 -3.390701 -90) (layer "F.SilkS"))
    (fp_text user "*" (at -1.8796 -2.641401 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.3876 -1.599999 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/DOTSTAR_CLK") (pinfunction "SDI") (pintype "input"))
    (pad "2" smd rect (at -2.3876 0 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/DOTSTAR_DATA") (pinfunction "CKI") (pintype "input"))
    (pad "3" smd rect (at -2.3876 1.599999 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "4" smd rect (at 2.3876 1.599999 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd rect (at 2.3876 0 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "unconnected-(RGB1-Pad5)") (pinfunction "CKO") (pintype "output+no_connect"))
    (pad "6" smd rect (at 2.3876 -1.599999 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "unconnected-(RGB1-Pad6)") (pinfunction "SDO") (pintype "output+no_connect"))
  )
  (footprint "footprints:AR_logo_18mm" (layer "B.Cu")
    (tedit 63780F59)
    (at 148 110 180)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "ARlogo1" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "SYM_Arrow_Large" (at 0.75 0) (layer "Dwgs.User"))
  )
  (footprint "footprints:Snake" (layer "B.Cu")
    (tedit 0)
    (at 139.446 94.742 180)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SnakeBack1" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "SYM_Arrow_Large" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (gr_line (start 110.49 135) (end 167.64 135) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 167.64 76.2) (end 110.49 76.2) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 171.45 80.01) (end 171.45 123.19) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 106.68 123.19) (end 106.68 131.19) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 171.45 123.19) (end 171.45 131.19) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 106.68 123.19) (end 106.68 80.01) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 167.64 76.2) (mid 170.334077 77.315923) (end 171.45 80.01) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 110.49 135) (mid 107.795923 133.884077) (end 106.68 131.19) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 106.68 80.01) (mid 107.795923 77.315923) (end 110.49 76.2) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 171.45 131.19) (mid 170.334077 133.884077) (end 167.64 135) (layer "Edge.Cuts") (width 0.15))
  (gr_text "Killroy was here!" (at 123.698 142.113) (layer "B.Cu"))
  (gr_text "Rapid Prototyping Board" (at 138.176 104.394) (layer "B.SilkS"))
  (gr_text "Agilityrobotics.com" (at 135 109) (layer "B.SilkS"))
  (gr_text "Rev 2.0\nOct 2023" (at 121 131.572) (layer "B.SilkS"))
  (gr_text "I2C 0x20 = MCP23X08 U1\nI2C 0x21 = MCP23X08 U3\nI2C 0x22 = MCP23X08 U4\nI2C 0x23 = MCP23X08 U6\nI2C 0x24 = MCP23X08 U9\nI2C 0x3C = SSD1306 OLED\nI2C 0x40 = INA219A\nI2C 0x50 = EEPROM \n" (at 148.336 119.634) (layer "B.SilkS"))
  (gr_text "M3" (at 163.7 83.95) (layer "F.SilkS"))
  (gr_text "M2.5" (at 164.5158 92.8116) (layer "F.SilkS"))
  (gr_text "3V3\n\nSWCLK\n\nSWDIO\n\nGND" (at 155.194 117.602 90) (layer "F.SilkS"))
  (gr_text "Rapid Prototyping\nBoard" (at 191.262 97.028) (layer "F.SilkS"))
  (gr_text "SDA SCL VCC GND" (at 159.1 128.2 90) (layer "F.SilkS"))
  (gr_text "500mA" (at 111 92.71 90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 110.49 135) (xy 110.49 76.2))
    (height -12.49)
    (gr_text "58.8000 mm" (at 96.85 105.6 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 171.45 131.19) (xy 106.68 131.19))
    (height -7.81)
    (gr_text "64.7700 mm" (at 139.065 137.85) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 134.6 86.4) (xy 134.6 83.6))
    (height 2.4)
    (gr_text "2.8000 mm" (at 135.85 85 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.26 137.16)
        (xy 101.6 137.16)
        (xy 101.6 73.66)
        (xy 175.26 73.66)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.72 139.7)
        (xy 104.14 139.7)
        (xy 104.14 76.2)
        (xy 172.72 76.2)
      )
    )
  )
)
