(kicad_pcb (version 20171130) (host pcbnew 5.1.9+dfsg1-1~bpo10+1)
  (general
    (thickness 1.6)
    (drawings 69)
    (tracks 17057)
    (zones 0)
    (modules 258)
    (nets 297)
  )
  (page A4)
  (title_block
    (title ULX4M-LS)
    (date 2021-11-08)
    (rev v0.0.2)
    (company "Intergalaktik d.o.o.")
  )
  (layers
    (0 F.Cu signal)
    (1 GND1.Cu power)
    (2 In2signal.Cu signal)
    (3 POWER.Cu power)
    (4 GND2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.127)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.127)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.419)
    (via_drill 0.2)
    (via_min_size 0.419)
    (via_min_drill 0.2)
    (user_via 0.42 0.2)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.1)
    (pad_size 0.35 0.35)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance -0.05)
    (aux_axis_origin 94.1 112.22)
    (grid_origin 94.1 112.22)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x012fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plot/ulx4m/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 /power/FB1)
  (net 4 +2V5)
  (net 5 /power/FB3)
  (net 6 /power/FB2)
  (net 7 /flash/FLASH_nWP)
  (net 8 /flash/FLASH_nHOLD)
  (net 9 /flash/FLASH_MOSI)
  (net 10 /flash/FLASH_MISO)
  (net 11 /flash/FLASH_SCK)
  (net 12 /flash/FLASH_nCS)
  (net 13 /flash/FPGA_PROGRAMN)
  (net 14 /flash/FPGA_DONE)
  (net 15 /flash/FPGA_INITN)
  (net 16 LED0)
  (net 17 LED1)
  (net 18 LED2)
  (net 19 LED3)
  (net 20 CLK_25MHz)
  (net 21 USB_FPGA_D+)
  (net 22 /blinkey/ALED0)
  (net 23 /blinkey/ALED1)
  (net 24 /blinkey/ALED2)
  (net 25 /blinkey/ALED3)
  (net 26 USB_FPGA_D-)
  (net 27 /power/P3V3)
  (net 28 /power/P2V5)
  (net 29 /power/L1)
  (net 30 /power/L3)
  (net 31 /power/L2)
  (net 32 /power/P1V1)
  (net 33 GN0)
  (net 34 GP3)
  (net 35 2V5_3V3)
  (net 36 HDMI0_TX2_P)
  (net 37 FPDI_D2+)
  (net 38 FPDI_D2-)
  (net 39 HDMI0_TX2_N)
  (net 40 HDMI0_TX1_P)
  (net 41 FPDI_D1+)
  (net 42 FPDI_D1-)
  (net 43 HDMI0_TX1_N)
  (net 44 HDMI0_TX0_P)
  (net 45 FPDI_D0+)
  (net 46 FPDI_D0-)
  (net 47 HDMI0_TX0_N)
  (net 48 HDMI0_CLK_P)
  (net 49 FPDI_CLK+)
  (net 50 FPDI_CLK-)
  (net 51 HDMI0_CLK_N)
  (net 52 CM4_1.8V)
  (net 53 CM4_3.3V)
  (net 54 USB_N)
  (net 55 USB_P)
  (net 56 HDMI1_HOTPLUG)
  (net 57 HDMI1_SDA)
  (net 58 HDMI1_TX2_P)
  (net 59 HDMI1_SCL)
  (net 60 HDMI1_TX2_N)
  (net 61 HDMI1_CEC)
  (net 62 HDMI1_TX1_P)
  (net 63 HDMI1_TX1_N)
  (net 64 HDMI1_TX0_P)
  (net 65 HDMI1_TX0_N)
  (net 66 HDMI1_CLK_P)
  (net 67 HDMI1_CLK_N)
  (net 68 USB_FPGA_PULL_D-)
  (net 69 GN3)
  (net 70 GP5)
  (net 71 USB_FPGA_PULL_D+)
  (net 72 GP0)
  (net 73 GN5)
  (net 74 GN4)
  (net 75 GP4)
  (net 76 HDMI0_CEC)
  (net 77 HDMI0_HOTPLUG)
  (net 78 HDMI0_SDA)
  (net 79 HDMI0_SCL)
  (net 80 PCIe_CLK_P)
  (net 81 PCIe_CLK_N)
  (net 82 PCIe_RX_P)
  (net 83 PCIe_RX_N)
  (net 84 PCIe_TX_P)
  (net 85 PCIe_TX_N)
  (net 86 /serdes/S_2_P)
  (net 87 /serdes/S_3_P)
  (net 88 /serdes/S_6_P)
  (net 89 /serdes/S_7_P)
  (net 90 /serdes/CLK_0_P)
  (net 91 /serdes/S_0_P)
  (net 92 /serdes/S_1_P)
  (net 93 /serdes/CLK_1_P)
  (net 94 /serdes/S_4_P)
  (net 95 /serdes/S_5_P)
  (net 96 /serdes/CLK_0_N)
  (net 97 /serdes/S_0_N)
  (net 98 /serdes/S_1_N)
  (net 99 /serdes/CLK_1_N)
  (net 100 /serdes/S_4_N)
  (net 101 /serdes/S_5_N)
  (net 102 /serdes/S_2_N)
  (net 103 /serdes/S_3_N)
  (net 104 /serdes/S_6_N)
  (net 105 /serdes/S_7_N)
  (net 106 GPIO12)
  (net 107 GPIO16)
  (net 108 GPIO20)
  (net 109 GPIO21)
  (net 110 PCIe_CLK_nREQ)
  (net 111 PCIe_nRST)
  (net 112 CAM0_D0_N)
  (net 113 CAM0_D0_P)
  (net 114 CAM0_D1_N)
  (net 115 CAM0_D1_P)
  (net 116 CAM0_C_N)
  (net 117 CAM0_C_P)
  (net 118 DSI0_D0_N)
  (net 119 DSI0_D0_P)
  (net 120 DSI0_D1_N)
  (net 121 DSI0_D1_P)
  (net 122 DSI0_C_N)
  (net 123 DSI0_C_P)
  (net 124 SD_PWR_ON)
  (net 125 GPIO9)
  (net 126 ETH_0P)
  (net 127 ETH_2P)
  (net 128 ETH_0N)
  (net 129 ETH_2N)
  (net 130 ETH_1N)
  (net 131 ETH_3N)
  (net 132 ETH_1P)
  (net 133 ETH_3P)
  (net 134 US2_ID)
  (net 135 BTN1)
  (net 136 BTN2)
  (net 137 GPIO2)
  (net 138 GPIO3)
  (net 139 GPIO14)
  (net 140 GPIO4)
  (net 141 GPIO15)
  (net 142 GPIO18)
  (net 143 GPIO23)
  (net 144 GPIO24)
  (net 145 GPIO25)
  (net 146 GPIO8)
  (net 147 GPIO7)
  (net 148 GPIO6)
  (net 149 GPIO13)
  (net 150 GPIO19)
  (net 151 GPIO26)
  (net 152 DSI1_D0_N)
  (net 153 DSI1_D0_P)
  (net 154 DSI1_D1_N)
  (net 155 DSI1_D1_P)
  (net 156 DSI1_C_N)
  (net 157 DSI1_C_P)
  (net 158 DSI1_D2_N)
  (net 159 DSI1_D3_N)
  (net 160 DSI1_D2_P)
  (net 161 DSI1_D3_P)
  (net 162 GPIO27)
  (net 163 CAM1_D0_N)
  (net 164 CAM1_D0_P)
  (net 165 CAM1_D1_N)
  (net 166 CAM1_D1_P)
  (net 167 CAM1_C_N)
  (net 168 CAM1_C_P)
  (net 169 "Net-(R22-Pad2)")
  (net 170 "Net-(R23-Pad2)")
  (net 171 "Net-(R24-Pad2)")
  (net 172 "Net-(R25-Pad2)")
  (net 173 "Net-(R26-Pad2)")
  (net 174 "Net-(R34-Pad1)")
  (net 175 "Net-(R35-Pad1)")
  (net 176 "Net-(R36-Pad1)")
  (net 177 "Net-(R37-Pad1)")
  (net 178 "Net-(R38-Pad1)")
  (net 179 "Net-(RC1-Pad1)")
  (net 180 DDR3_A8)
  (net 181 DDR3_A14)
  (net 182 DDR3_A13)
  (net 183 DDR3_RESET)
  (net 184 VCC1V35)
  (net 185 DDR3_A6)
  (net 186 DDR3_A11)
  (net 187 DDR3_A9)
  (net 188 DDR3_A7)
  (net 189 DDR3_A4)
  (net 190 DDR3_A1)
  (net 191 DDR3_A2)
  (net 192 DDR3_A5)
  (net 193 DDR3_BA1)
  (net 194 DDR3_A12)
  (net 195 DDR3_A0)
  (net 196 DDR3_A3)
  (net 197 DDR3_VREF)
  (net 198 DDR3_A15)
  (net 199 DDR3_BA2)
  (net 200 DDR3_BA0)
  (net 201 "Net-(R81-Pad1)")
  (net 202 DDR3_A10)
  (net 203 DDR3_WE)
  (net 204 DDR3_CS)
  (net 205 DDR3_CKE)
  (net 206 DDR3_CLK-)
  (net 207 DDR3_CAS)
  (net 208 DDR3_ODT)
  (net 209 DDR3_CLK+)
  (net 210 DDR3_RAS)
  (net 211 DDR3_DQ5)
  (net 212 DDR3_DQ7)
  (net 213 DDR3_DQ4)
  (net 214 DDR3_DQS0-)
  (net 215 DDR3_DQ6)
  (net 216 DDR3_DQ3)
  (net 217 DDR3_DQ1)
  (net 218 DDR3_DQS0+)
  (net 219 DDR3_DQ2)
  (net 220 DDR3_DM0)
  (net 221 DDR3_DQ0)
  (net 222 DDR3_DQ8)
  (net 223 DDR3_DM1)
  (net 224 DDR3_DQ10)
  (net 225 DDR3_DQS1+)
  (net 226 DDR3_DQ9)
  (net 227 DDR3_DQ11)
  (net 228 DDR3_DQS1-)
  (net 229 DDR3_DQ12)
  (net 230 DDR3_DQ15)
  (net 231 DDR3_DQ13)
  (net 232 "Net-(C94-Pad2)")
  (net 233 /power/P1V35)
  (net 234 /power/FB4)
  (net 235 /power/L4)
  (net 236 DDR3_DQ14)
  (net 237 Camera_GPIO)
  (net 238 SDA0)
  (net 239 SCL0)
  (net 240 GPIO17)
  (net 241 GPIO22)
  (net 242 GPIO10)
  (net 243 GPIO11)
  (net 244 ID_SD)
  (net 245 ID_SC)
  (net 246 GPIO5)
  (net 247 /blinkey/ALED4)
  (net 248 /blinkey/ALED5)
  (net 249 /blinkey/ALED6)
  (net 250 /blinkey/ALED7)
  (net 251 "Net-(D10-Pad1)")
  (net 252 "Net-(D11-Pad2)")
  (net 253 "Net-(D12-Pad1)")
  (net 254 "Net-(D13-Pad2)")
  (net 255 LED4)
  (net 256 LED5)
  (net 257 LED6)
  (net 258 LED7)
  (net 259 BTN3)
  (net 260 "Net-(BTN1-Pad1)")
  (net 261 /gpio/CAM0_D0_LP)
  (net 262 ETH_nLED1)
  (net 263 ETH_nLED2)
  (net 264 VCC1V2)
  (net 265 ETH_~RESET)
  (net 266 "Net-(C109-Pad1)")
  (net 267 /ethernet/AVDDL)
  (net 268 /ethernet/AVDDL_PLL)
  (net 269 RGMII_RXD0)
  (net 270 RGMII_RXD1)
  (net 271 RGMII_RXD2)
  (net 272 RGMII_RXD3)
  (net 273 RGMII_RX_DV)
  (net 274 RGMII_RX_CLK)
  (net 275 RGMII_REF_CLK)
  (net 276 ETH_MDIO)
  (net 277 ETH_INT_N)
  (net 278 /ethernet/ETH_LED1)
  (net 279 /ethernet/ETH_LED2)
  (net 280 "Net-(R65-Pad2)")
  (net 281 RGMII_TX_EN)
  (net 282 ETH_MDC)
  (net 283 RGMII_TXD0)
  (net 284 RGMII_TXD1)
  (net 285 RGMII_TXD2)
  (net 286 RGMII_TXD3)
  (net 287 RGMII_TX_CLK)
  (net 288 /ethernet/PHY_CLK)
  (net 289 "Net-(R70-Pad2)")
  (net 290 SW1)
  (net 291 SW2)
  (net 292 "Net-(TP_E9-Pad1)")
  (net 293 "Net-(TP_E8-Pad1)")
  (net 294 "Net-(TP_D8-Pad1)")
  (net 295 "Net-(TP_C16-Pad1)")
  (net 296 "Net-(TP_D16-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.3)
    (via_dia 0.419)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.127)
    (diff_pair_gap 0.127)
    (add_net +2V5)
    (add_net +5V)
    (add_net /blinkey/ALED0)
    (add_net /blinkey/ALED1)
    (add_net /blinkey/ALED2)
    (add_net /blinkey/ALED3)
    (add_net /blinkey/ALED4)
    (add_net /blinkey/ALED5)
    (add_net /blinkey/ALED6)
    (add_net /blinkey/ALED7)
    (add_net /ethernet/AVDDL)
    (add_net /ethernet/AVDDL_PLL)
    (add_net /ethernet/ETH_LED1)
    (add_net /ethernet/ETH_LED2)
    (add_net /ethernet/PHY_CLK)
    (add_net /flash/FLASH_MISO)
    (add_net /flash/FLASH_MOSI)
    (add_net /flash/FLASH_SCK)
    (add_net /flash/FLASH_nCS)
    (add_net /flash/FLASH_nHOLD)
    (add_net /flash/FLASH_nWP)
    (add_net /flash/FPGA_DONE)
    (add_net /flash/FPGA_INITN)
    (add_net /flash/FPGA_PROGRAMN)
    (add_net /gpio/CAM0_D0_LP)
    (add_net /power/FB1)
    (add_net /power/FB2)
    (add_net /power/FB3)
    (add_net /power/FB4)
    (add_net /power/L1)
    (add_net /power/L2)
    (add_net /power/L3)
    (add_net /power/L4)
    (add_net /power/P1V1)
    (add_net /power/P1V35)
    (add_net /power/P2V5)
    (add_net /power/P3V3)
    (add_net /serdes/CLK_0_N)
    (add_net /serdes/CLK_0_P)
    (add_net /serdes/CLK_1_N)
    (add_net /serdes/CLK_1_P)
    (add_net /serdes/S_0_N)
    (add_net /serdes/S_0_P)
    (add_net /serdes/S_1_N)
    (add_net /serdes/S_1_P)
    (add_net /serdes/S_2_N)
    (add_net /serdes/S_2_P)
    (add_net /serdes/S_3_N)
    (add_net /serdes/S_3_P)
    (add_net /serdes/S_4_N)
    (add_net /serdes/S_4_P)
    (add_net /serdes/S_5_N)
    (add_net /serdes/S_5_P)
    (add_net /serdes/S_6_N)
    (add_net /serdes/S_6_P)
    (add_net /serdes/S_7_N)
    (add_net /serdes/S_7_P)
    (add_net 2V5_3V3)
    (add_net BTN1)
    (add_net BTN2)
    (add_net BTN3)
    (add_net CAM0_C_N)
    (add_net CAM0_C_P)
    (add_net CAM0_D0_N)
    (add_net CAM0_D0_P)
    (add_net CAM0_D1_N)
    (add_net CAM0_D1_P)
    (add_net CAM1_C_N)
    (add_net CAM1_C_P)
    (add_net CAM1_D0_N)
    (add_net CAM1_D0_P)
    (add_net CAM1_D1_N)
    (add_net CAM1_D1_P)
    (add_net CLK_25MHz)
    (add_net CM4_1.8V)
    (add_net CM4_3.3V)
    (add_net Camera_GPIO)
    (add_net DDR3_A0)
    (add_net DDR3_A1)
    (add_net DDR3_A10)
    (add_net DDR3_A11)
    (add_net DDR3_A12)
    (add_net DDR3_A13)
    (add_net DDR3_A14)
    (add_net DDR3_A15)
    (add_net DDR3_A2)
    (add_net DDR3_A3)
    (add_net DDR3_A4)
    (add_net DDR3_A5)
    (add_net DDR3_A6)
    (add_net DDR3_A7)
    (add_net DDR3_A8)
    (add_net DDR3_A9)
    (add_net DDR3_BA0)
    (add_net DDR3_BA1)
    (add_net DDR3_BA2)
    (add_net DDR3_CAS)
    (add_net DDR3_CKE)
    (add_net DDR3_CLK+)
    (add_net DDR3_CLK-)
    (add_net DDR3_CS)
    (add_net DDR3_DM0)
    (add_net DDR3_DM1)
    (add_net DDR3_DQ0)
    (add_net DDR3_DQ1)
    (add_net DDR3_DQ10)
    (add_net DDR3_DQ11)
    (add_net DDR3_DQ12)
    (add_net DDR3_DQ13)
    (add_net DDR3_DQ14)
    (add_net DDR3_DQ15)
    (add_net DDR3_DQ2)
    (add_net DDR3_DQ3)
    (add_net DDR3_DQ4)
    (add_net DDR3_DQ5)
    (add_net DDR3_DQ6)
    (add_net DDR3_DQ7)
    (add_net DDR3_DQ8)
    (add_net DDR3_DQ9)
    (add_net DDR3_DQS0+)
    (add_net DDR3_DQS0-)
    (add_net DDR3_DQS1+)
    (add_net DDR3_DQS1-)
    (add_net DDR3_ODT)
    (add_net DDR3_RAS)
    (add_net DDR3_RESET)
    (add_net DDR3_VREF)
    (add_net DDR3_WE)
    (add_net DSI0_C_N)
    (add_net DSI0_C_P)
    (add_net DSI0_D0_N)
    (add_net DSI0_D0_P)
    (add_net DSI0_D1_N)
    (add_net DSI0_D1_P)
    (add_net DSI1_C_N)
    (add_net DSI1_C_P)
    (add_net DSI1_D0_N)
    (add_net DSI1_D0_P)
    (add_net DSI1_D1_N)
    (add_net DSI1_D1_P)
    (add_net DSI1_D2_N)
    (add_net DSI1_D2_P)
    (add_net DSI1_D3_N)
    (add_net DSI1_D3_P)
    (add_net ETH_0N)
    (add_net ETH_0P)
    (add_net ETH_1N)
    (add_net ETH_1P)
    (add_net ETH_2N)
    (add_net ETH_2P)
    (add_net ETH_3N)
    (add_net ETH_3P)
    (add_net ETH_INT_N)
    (add_net ETH_MDC)
    (add_net ETH_MDIO)
    (add_net ETH_nLED1)
    (add_net ETH_nLED2)
    (add_net ETH_~RESET)
    (add_net FPDI_CLK+)
    (add_net FPDI_CLK-)
    (add_net FPDI_D0+)
    (add_net FPDI_D0-)
    (add_net FPDI_D1+)
    (add_net FPDI_D1-)
    (add_net FPDI_D2+)
    (add_net FPDI_D2-)
    (add_net GN0)
    (add_net GN3)
    (add_net GN4)
    (add_net GN5)
    (add_net GND)
    (add_net GP0)
    (add_net GP3)
    (add_net GP4)
    (add_net GP5)
    (add_net GPIO10)
    (add_net GPIO11)
    (add_net GPIO12)
    (add_net GPIO13)
    (add_net GPIO14)
    (add_net GPIO15)
    (add_net GPIO16)
    (add_net GPIO17)
    (add_net GPIO18)
    (add_net GPIO19)
    (add_net GPIO2)
    (add_net GPIO20)
    (add_net GPIO21)
    (add_net GPIO22)
    (add_net GPIO23)
    (add_net GPIO24)
    (add_net GPIO25)
    (add_net GPIO26)
    (add_net GPIO27)
    (add_net GPIO3)
    (add_net GPIO4)
    (add_net GPIO5)
    (add_net GPIO6)
    (add_net GPIO7)
    (add_net GPIO8)
    (add_net GPIO9)
    (add_net HDMI0_CEC)
    (add_net HDMI0_CLK_N)
    (add_net HDMI0_CLK_P)
    (add_net HDMI0_HOTPLUG)
    (add_net HDMI0_SCL)
    (add_net HDMI0_SDA)
    (add_net HDMI0_TX0_N)
    (add_net HDMI0_TX0_P)
    (add_net HDMI0_TX1_N)
    (add_net HDMI0_TX1_P)
    (add_net HDMI0_TX2_N)
    (add_net HDMI0_TX2_P)
    (add_net HDMI1_CEC)
    (add_net HDMI1_CLK_N)
    (add_net HDMI1_CLK_P)
    (add_net HDMI1_HOTPLUG)
    (add_net HDMI1_SCL)
    (add_net HDMI1_SDA)
    (add_net HDMI1_TX0_N)
    (add_net HDMI1_TX0_P)
    (add_net HDMI1_TX1_N)
    (add_net HDMI1_TX1_P)
    (add_net HDMI1_TX2_N)
    (add_net HDMI1_TX2_P)
    (add_net ID_SC)
    (add_net ID_SD)
    (add_net LED0)
    (add_net LED1)
    (add_net LED2)
    (add_net LED3)
    (add_net LED4)
    (add_net LED5)
    (add_net LED6)
    (add_net LED7)
    (add_net "Net-(BTN1-Pad1)")
    (add_net "Net-(C109-Pad1)")
    (add_net "Net-(C94-Pad2)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(R22-Pad2)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R34-Pad1)")
    (add_net "Net-(R35-Pad1)")
    (add_net "Net-(R36-Pad1)")
    (add_net "Net-(R37-Pad1)")
    (add_net "Net-(R38-Pad1)")
    (add_net "Net-(R65-Pad2)")
    (add_net "Net-(R70-Pad2)")
    (add_net "Net-(R81-Pad1)")
    (add_net "Net-(RC1-Pad1)")
    (add_net "Net-(TP_C16-Pad1)")
    (add_net "Net-(TP_D16-Pad1)")
    (add_net "Net-(TP_D8-Pad1)")
    (add_net "Net-(TP_E8-Pad1)")
    (add_net "Net-(TP_E9-Pad1)")
    (add_net PCIe_CLK_N)
    (add_net PCIe_CLK_P)
    (add_net PCIe_CLK_nREQ)
    (add_net PCIe_RX_N)
    (add_net PCIe_RX_P)
    (add_net PCIe_TX_N)
    (add_net PCIe_TX_P)
    (add_net PCIe_nRST)
    (add_net RGMII_REF_CLK)
    (add_net RGMII_RXD0)
    (add_net RGMII_RXD1)
    (add_net RGMII_RXD2)
    (add_net RGMII_RXD3)
    (add_net RGMII_RX_CLK)
    (add_net RGMII_RX_DV)
    (add_net RGMII_TXD0)
    (add_net RGMII_TXD1)
    (add_net RGMII_TXD2)
    (add_net RGMII_TXD3)
    (add_net RGMII_TX_CLK)
    (add_net RGMII_TX_EN)
    (add_net SCL0)
    (add_net SDA0)
    (add_net SD_PWR_ON)
    (add_net SW1)
    (add_net SW2)
    (add_net US2_ID)
    (add_net USB_FPGA_D+)
    (add_net USB_FPGA_D-)
    (add_net USB_FPGA_PULL_D+)
    (add_net USB_FPGA_PULL_D-)
    (add_net USB_N)
    (add_net USB_P)
    (add_net VCC1V2)
    (add_net VCC1V35)
  )
  (net_class BGA ""
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.419)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.127)
    (diff_pair_gap 0.127)
  )
  (net_class Medium ""
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.419)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.127)
    (diff_pair_gap 0.127)
  )
  (module ecp5-dc-scm:Testpoint_smd_1mm (layer B.Cu) (tedit 5E4A935B)
    (at 115.8 90.1492)
    (attr virtual)
    (fp_text reference TP_E8 (at -1.72 0.0008) (layer B.SilkS))
    (fp_text value E8 (at 0 0.5) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0.0508) (size 1 1) (layers B.Cu B.Mask)
      (net 293 "Net-(TP_E8-Pad1)"))
  )
  (module ecp5-dc-scm:Testpoint_smd_1mm (layer B.Cu) (tedit 5E4A935B)
    (at 115.85 88.64)
    (attr virtual)
    (fp_text reference TP_D8 (at -1.72 0.03) (layer B.SilkS))
    (fp_text value D8 (at 0 0.5) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0.0508) (size 1 1) (layers B.Cu B.Mask)
      (net 294 "Net-(TP_D8-Pad1)"))
  )
  (module AS4C256M16D3:BGA-96_9.0x13.0mm_Layout2x3x16_P0.8mm (layer F.Cu) (tedit 61F3D2A1)
    (at 138.57 90.21 90)
    (descr "BGA-96, http://www.mouser.com/ds/2/198/43-46TR16640B-81280BL-706483.pdf")
    (tags BGA-96)
    (attr smd)
    (fp_text reference U2 (at -3.51 -7.26 90) (layer F.SilkS))
    (fp_text value AS4C256M16D3 (at 0.09 6.32 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad T9 smd circle (at 3.2 6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad T8 smd circle (at 2.4 6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 180 DDR3_A8))
    (pad T7 smd circle (at 1.6 6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 181 DDR3_A14))
    (pad T3 smd circle (at -1.6 6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 182 DDR3_A13))
    (pad T2 smd circle (at -2.4 6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 183 DDR3_RESET))
    (pad T1 smd circle (at -3.2 6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad R9 smd circle (at 3.2 5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad R8 smd circle (at 2.4 5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 185 DDR3_A6))
    (pad R7 smd circle (at 1.6 5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 186 DDR3_A11))
    (pad R3 smd circle (at -1.6 5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 187 DDR3_A9))
    (pad R2 smd circle (at -2.4 5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 188 DDR3_A7))
    (pad R1 smd circle (at -3.2 5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad P9 smd circle (at 3.2 4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P8 smd circle (at 2.4 4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 189 DDR3_A4))
    (pad P7 smd circle (at 1.6 4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 190 DDR3_A1))
    (pad P3 smd circle (at -1.6 4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 191 DDR3_A2))
    (pad P2 smd circle (at -2.4 4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 192 DDR3_A5))
    (pad P1 smd circle (at -3.2 4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad N9 smd circle (at 3.2 3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad N8 smd circle (at 2.4 3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 193 DDR3_BA1))
    (pad N7 smd circle (at 1.6 3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 194 DDR3_A12))
    (pad N3 smd circle (at -1.6 3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 195 DDR3_A0))
    (pad N2 smd circle (at -2.4 3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 196 DDR3_A3))
    (pad N1 smd circle (at -3.2 3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad M9 smd circle (at 3.2 2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad M8 smd circle (at 2.4 2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 197 DDR3_VREF))
    (pad M7 smd circle (at 1.6 2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 198 DDR3_A15))
    (pad M3 smd circle (at -1.6 2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 199 DDR3_BA2))
    (pad M2 smd circle (at -2.4 2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 200 DDR3_BA0))
    (pad M1 smd circle (at -3.2 2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad L9 smd circle (at 3.2 2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad L8 smd circle (at 2.4 2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(R81-Pad1)"))
    (pad L7 smd circle (at 1.6 2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 202 DDR3_A10))
    (pad L3 smd circle (at -1.6 2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 203 DDR3_WE))
    (pad L2 smd circle (at -2.4 2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 204 DDR3_CS))
    (pad L1 smd circle (at -3.2 2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad K9 smd circle (at 3.2 1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 205 DDR3_CKE))
    (pad K8 smd circle (at 2.4 1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad K7 smd circle (at 1.6 1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 206 DDR3_CLK-))
    (pad K3 smd circle (at -1.6 1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 207 DDR3_CAS))
    (pad K2 smd circle (at -2.4 1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad K1 smd circle (at -3.2 1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 208 DDR3_ODT))
    (pad J9 smd circle (at 3.2 0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad J8 smd circle (at 2.4 0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad J7 smd circle (at 1.6 0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 209 DDR3_CLK+))
    (pad J3 smd circle (at -1.6 0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 210 DDR3_RAS))
    (pad J2 smd circle (at -2.4 0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad J1 smd circle (at -3.2 0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask))
    (pad H9 smd circle (at 3.2 -0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad H8 smd circle (at 2.4 -0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 211 DDR3_DQ5))
    (pad H7 smd circle (at 1.6 -0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 212 DDR3_DQ7))
    (pad H3 smd circle (at -1.6 -0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 213 DDR3_DQ4))
    (pad H2 smd circle (at -2.4 -0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad H1 smd circle (at -3.2 -0.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 197 DDR3_VREF))
    (pad G9 smd circle (at 3.2 -1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad G8 smd circle (at 2.4 -1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad G7 smd circle (at 1.6 -1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad G3 smd circle (at -1.6 -1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 214 DDR3_DQS0-))
    (pad G2 smd circle (at -2.4 -1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 215 DDR3_DQ6))
    (pad G1 smd circle (at -3.2 -1.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad F9 smd circle (at 3.2 -2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad F8 smd circle (at 2.4 -2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 216 DDR3_DQ3))
    (pad F7 smd circle (at 1.6 -2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 217 DDR3_DQ1))
    (pad F3 smd circle (at -1.6 -2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 218 DDR3_DQS0+))
    (pad F2 smd circle (at -2.4 -2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 219 DDR3_DQ2))
    (pad F1 smd circle (at -3.2 -2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad E9 smd circle (at 3.2 -2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad E8 smd circle (at 2.4 -2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E7 smd circle (at 1.6 -2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 220 DDR3_DM0))
    (pad E3 smd circle (at -1.6 -2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 221 DDR3_DQ0))
    (pad E2 smd circle (at -2.4 -2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E1 smd circle (at -3.2 -2.8 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad D9 smd circle (at 3.2 -3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad D8 smd circle (at 2.4 -3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad D7 smd circle (at 1.6 -3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 222 DDR3_DQ8))
    (pad D3 smd circle (at -1.6 -3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 223 DDR3_DM1))
    (pad D2 smd circle (at -2.4 -3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad D1 smd circle (at -3.2 -3.6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C9 smd circle (at 3.2 -4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad C8 smd circle (at 2.4 -4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 224 DDR3_DQ10))
    (pad C7 smd circle (at 1.6 -4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 225 DDR3_DQS1+))
    (pad C3 smd circle (at -1.6 -4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 226 DDR3_DQ9))
    (pad C2 smd circle (at -2.4 -4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 227 DDR3_DQ11))
    (pad C1 smd circle (at -3.2 -4.4 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad B9 smd circle (at 3.2 -5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B8 smd circle (at 2.4 -5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 236 DDR3_DQ14))
    (pad B7 smd circle (at 1.6 -5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 228 DDR3_DQS1-))
    (pad B3 smd circle (at -1.6 -5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B2 smd circle (at -2.4 -5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad B1 smd circle (at -3.2 -5.2 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd circle (at 3.2 -6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A8 smd circle (at 2.4 -6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (pad A7 smd circle (at 1.6 -6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 229 DDR3_DQ12))
    (pad A3 smd circle (at -1.6 -6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 230 DDR3_DQ15))
    (pad A2 smd circle (at -2.4 -6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 231 DDR3_DQ13))
    (pad A1 smd circle (at -3.2 -6 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35))
    (model ${KISYS3DMOD}/Package_BGA.3dshapes/BGA-96_9.0x13.0mm_Layout2x3x16_P0.8mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_2x03_P1.00mm_Vertical_SMD (layer F.Cu) (tedit 61F7E6E5)
    (at 102 107.66 135)
    (descr "surface-mounted straight pin header, 2x03, 1.00mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 1.00mm double row")
    (attr smd)
    (fp_text reference J3 (at 0.106066 -1.110158 135) (layer F.SilkS) hide)
    (fp_text value JTAG (at 0.021213 2.38295 135) (layer F.SilkS))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd rect (at -1.65 -1 135) (size 2 0.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.65 -1 135) (size 2 0.5) (layers F.Cu F.Mask)
      (net 53 CM4_3.3V))
    (pad 3 smd rect (at -1.65 0 135) (size 2 0.5) (layers F.Cu F.Mask)
      (net 106 GPIO12))
    (pad 4 smd rect (at 1.65 0 135) (size 2 0.5) (layers F.Cu F.Mask)
      (net 108 GPIO20))
    (pad 5 smd rect (at -1.65 1 135) (size 2 0.5) (layers F.Cu F.Mask)
      (net 109 GPIO21))
    (pad 6 smd rect (at 1.65 1 135) (size 2 0.5) (layers F.Cu F.Mask)
      (net 107 GPIO16))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 61F7E650)
    (at 148.17 98.41)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J4 (at 0.01 9.08) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0.87 8.41) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 /serdes/S_5_P))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 /serdes/S_5_N))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 /serdes/S_7_P))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 /serdes/S_7_N))
  )
  (module Button_Switch_SMD:SW_DIP_SPSTx02_Slide_Copal_CVS-02xB_W5.9mm_P1mm (layer F.Cu) (tedit 5A4E1407)
    (at 139.16 81.52 180)
    (descr "SMD 2x-dip-switch SPST Copal_CVS-02xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)")
    (tags "SMD DIP Switch SPST Slide 5.9mm 232mil")
    (attr smd)
    (fp_text reference SW1 (at 0.01 -2.42) (layer F.SilkS))
    (fp_text value SW_DIP_x02 (at 0.07 2.06) (layer F.Fab))
    (fp_text user on (at 0.2 -1.125) (layer F.Fab))
    (fp_text user %R (at 1.675 0 90) (layer F.Fab))
    (pad 5 smd rect (at 2.15 1.5 180) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.15 1.5 180) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 2.15 -1.5 180) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.15 -1.5 180) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.95 -0.5 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 290 SW1))
    (pad 2 smd rect (at -2.95 0.5 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 289 "Net-(R70-Pad2)"))
    (pad 3 smd rect (at 2.95 0.5 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 291 SW2))
    (pad 1 smd rect (at -2.95 -0.5 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 289 "Net-(R70-Pad2)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_DIP_SPSTx02_Slide_Copal_CVS-02xB_W5.9mm_P1mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 142.5 76.76 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R70 (at 1.69 -0.02 90) (layer F.SilkS))
    (fp_text value 130 (at -0.02 0.38 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 289 "Net-(R70-Pad2)"))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lfe5bg381:BGA-381_pitch0.8mm_dia0.4mm (layer F.Cu) (tedit 5F7B3DD0)
    (at 117.21 94.25)
    (attr smd)
    (fp_text reference U1 (at -8.13 -9.44) (layer F.SilkS))
    (fp_text value LFE5U-85F-6BG381C (at -0.25 8.1) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.98) (layer F.Fab))
    (pad Y19 smd circle (at 6.8 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 93 /serdes/CLK_1_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y17 smd circle (at 5.2 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 101 /serdes/S_5_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y16 smd circle (at 4.4 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 95 /serdes/S_5_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y15 smd circle (at 3.6 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 100 /serdes/S_4_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y14 smd circle (at 2.8 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 94 /serdes/S_4_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y12 smd circle (at 1.2 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 96 /serdes/CLK_0_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y11 smd circle (at 0.4 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 90 /serdes/CLK_0_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y8 smd circle (at -2 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 98 /serdes/S_1_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y7 smd circle (at -2.8 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 92 /serdes/S_1_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y6 smd circle (at -3.6 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 97 /serdes/S_0_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y5 smd circle (at -4.4 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 91 /serdes/S_0_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y3 smd circle (at -6 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 /flash/FPGA_DONE) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad Y2 smd circle (at -6.8 7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /flash/FLASH_nWP) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W20 smd circle (at 7.6 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 99 /serdes/CLK_1_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W19 smd circle (at 6.8 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W18 smd circle (at 6 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 105 /serdes/S_7_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W17 smd circle (at 5.2 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 89 /serdes/S_7_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W16 smd circle (at 4.4 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W15 smd circle (at 3.6 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W14 smd circle (at 2.8 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 104 /serdes/S_6_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W13 smd circle (at 2 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 88 /serdes/S_6_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W12 smd circle (at 1.2 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W11 smd circle (at 0.4 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W10 smd circle (at -0.4 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W9 smd circle (at -1.2 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 103 /serdes/S_3_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W8 smd circle (at -2 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 87 /serdes/S_3_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W7 smd circle (at -2.8 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W6 smd circle (at -3.6 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W5 smd circle (at -4.4 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 102 /serdes/S_2_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W4 smd circle (at -5.2 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 86 /serdes/S_2_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W3 smd circle (at -6 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 /flash/FPGA_PROGRAMN) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W2 smd circle (at -6.8 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /flash/FLASH_MOSI) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad W1 smd circle (at -7.6 6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /flash/FLASH_nHOLD) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V20 smd circle (at 7.6 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V19 smd circle (at 6.8 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V18 smd circle (at 6 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V17 smd circle (at 5.2 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V16 smd circle (at 4.4 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V15 smd circle (at 3.6 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V14 smd circle (at 2.8 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V13 smd circle (at 2 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V12 smd circle (at 1.2 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V11 smd circle (at 0.4 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V10 smd circle (at -0.4 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V9 smd circle (at -1.2 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V8 smd circle (at -2 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V7 smd circle (at -2.8 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V6 smd circle (at -3.6 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V5 smd circle (at -4.4 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V4 smd circle (at -5.2 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 107 GPIO16) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V3 smd circle (at -6 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 /flash/FPGA_INITN) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V2 smd circle (at -6.8 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /flash/FLASH_MISO) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad V1 smd circle (at -7.6 6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 151 GPIO26) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U20 smd circle (at 7.6 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 182 DDR3_A13) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U19 smd circle (at 6.8 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 187 DDR3_A9) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U18 smd circle (at 6 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U17 smd circle (at 5.2 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 185 DDR3_A6) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U16 smd circle (at 4.4 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 223 DDR3_DM1) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U15 smd circle (at 3.6 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U14 smd circle (at 2.8 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U13 smd circle (at 2 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U12 smd circle (at 1.2 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U11 smd circle (at 0.4 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U10 smd circle (at -0.4 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U9 smd circle (at -1.2 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U8 smd circle (at -2 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U7 smd circle (at -2.8 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U6 smd circle (at -3.6 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U5 smd circle (at -4.4 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 109 GPIO21) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U4 smd circle (at -5.2 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U3 smd circle (at -6 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /flash/FLASH_SCK) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U2 smd circle (at -6.8 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad U1 smd circle (at -7.6 5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 150 GPIO19) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T20 smd circle (at 7.6 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 192 DDR3_A5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T19 smd circle (at 6.8 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 208 DDR3_ODT) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T18 smd circle (at 6 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 183 DDR3_RESET) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T17 smd circle (at 5.2 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 188 DDR3_A7) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T16 smd circle (at 4.4 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T15 smd circle (at 3.6 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T14 smd circle (at 2.8 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T13 smd circle (at 2 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T12 smd circle (at 1.2 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T11 smd circle (at 0.4 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T10 smd circle (at -0.4 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T9 smd circle (at -1.2 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T8 smd circle (at -2 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T7 smd circle (at -2.8 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T6 smd circle (at -3.6 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T5 smd circle (at -4.4 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 108 GPIO20) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T4 smd circle (at -5.2 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T3 smd circle (at -6 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T2 smd circle (at -6.8 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad T1 smd circle (at -7.6 4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 149 GPIO13) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad R20 smd circle (at 7.6 3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 210 DDR3_RAS) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad R19 smd circle (at 6.8 3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad R18 smd circle (at 6 3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad R17 smd circle (at 5.2 3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 221 DDR3_DQ0) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad R16 smd circle (at 4.4 3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 219 DDR3_DQ2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad R5 smd circle (at -4.4 3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 106 GPIO12) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad R4 smd circle (at -5.2 3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad R3 smd circle (at -6 3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad R2 smd circle (at -6.8 3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /flash/FLASH_nCS) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad R1 smd circle (at -7.6 3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 148 GPIO6) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P20 smd circle (at 7.6 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 199 DDR3_BA2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P19 smd circle (at 6.8 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 200 DDR3_BA0) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P18 smd circle (at 6 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 198 DDR3_A15) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P17 smd circle (at 5.2 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 194 DDR3_A12) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P16 smd circle (at 4.4 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 197 DDR3_VREF) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P15 smd circle (at 3.6 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P14 smd circle (at 2.8 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P13 smd circle (at 2 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P12 smd circle (at 1.2 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P11 smd circle (at 0.4 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P10 smd circle (at -0.4 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P9 smd circle (at -1.2 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P8 smd circle (at -2 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P7 smd circle (at -2.8 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P6 smd circle (at -3.6 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P5 smd circle (at -4.4 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 145 GPIO25) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P4 smd circle (at -5.2 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 146 GPIO8) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P3 smd circle (at -6 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 147 GPIO7) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P2 smd circle (at -6.8 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 139 GPIO14) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad P1 smd circle (at -7.6 2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 162 GPIO27) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N20 smd circle (at 7.6 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 181 DDR3_A14) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N19 smd circle (at 6.8 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 205 DDR3_CKE) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N18 smd circle (at 6 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 215 DDR3_DQ6) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N17 smd circle (at 5.2 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 212 DDR3_DQ7) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N16 smd circle (at 4.4 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 218 DDR3_DQS0+) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N15 smd circle (at 3.6 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N14 smd circle (at 2.8 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N13 smd circle (at 2 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N12 smd circle (at 1.2 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N11 smd circle (at 0.4 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N10 smd circle (at -0.4 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N9 smd circle (at -1.2 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N8 smd circle (at -2 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N7 smd circle (at -2.8 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N6 smd circle (at -3.6 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N5 smd circle (at -4.4 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 142 GPIO18) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N4 smd circle (at -5.2 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 143 GPIO23) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N3 smd circle (at -6 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 144 GPIO24) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N2 smd circle (at -6.8 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 243 GPIO11) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad N1 smd circle (at -7.6 2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 246 GPIO5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M20 smd circle (at 7.6 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 206 DDR3_CLK-) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M19 smd circle (at 6.8 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 211 DDR3_DQ5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M18 smd circle (at 6 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 213 DDR3_DQ4) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M17 smd circle (at 5.2 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 214 DDR3_DQS0-) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M16 smd circle (at 4.4 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M15 smd circle (at 3.6 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M14 smd circle (at 2.8 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M13 smd circle (at 2 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M12 smd circle (at 1.2 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M11 smd circle (at 0.4 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M10 smd circle (at -0.4 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M9 smd circle (at -1.2 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M8 smd circle (at -2 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M7 smd circle (at -2.8 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M6 smd circle (at -3.6 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M5 smd circle (at -4.4 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M4 smd circle (at -5.2 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M3 smd circle (at -6 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 241 GPIO22) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M2 smd circle (at -6.8 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad M1 smd circle (at -7.6 1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 277 ETH_INT_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L20 smd circle (at 7.6 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 209 DDR3_CLK+) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L19 smd circle (at 6.8 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 217 DDR3_DQ1) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L18 smd circle (at 6 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L17 smd circle (at 5.2 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 190 DDR3_A1) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L16 smd circle (at 4.4 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 216 DDR3_DQ3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L15 smd circle (at 3.6 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L14 smd circle (at 2.8 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L13 smd circle (at 2 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L12 smd circle (at 1.2 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L11 smd circle (at 0.4 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L10 smd circle (at -0.4 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L9 smd circle (at -1.2 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L8 smd circle (at -2 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L7 smd circle (at -2.8 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L6 smd circle (at -3.6 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L5 smd circle (at -4.4 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 125 GPIO9) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L4 smd circle (at -5.2 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 285 RGMII_TXD2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L3 smd circle (at -6 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 286 RGMII_TXD3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L2 smd circle (at -6.8 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 272 RGMII_RXD3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad L1 smd circle (at -7.6 0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 271 RGMII_RXD2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K20 smd circle (at 7.6 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 50 FPDI_CLK-) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K19 smd circle (at 6.8 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 231 DDR3_DQ13) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K18 smd circle (at 6 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K17 smd circle (at 5.2 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K16 smd circle (at 4.4 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K15 smd circle (at 3.6 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K14 smd circle (at 2.8 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K13 smd circle (at 2 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K12 smd circle (at 1.2 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K11 smd circle (at 0.4 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K10 smd circle (at -0.4 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K9 smd circle (at -1.2 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K8 smd circle (at -2 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K7 smd circle (at -2.8 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K6 smd circle (at -3.6 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K5 smd circle (at -4.4 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 283 RGMII_TXD0) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K4 smd circle (at -5.2 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 242 GPIO10) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K3 smd circle (at -6 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 281 RGMII_TX_EN) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K2 smd circle (at -6.8 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 270 RGMII_RXD1) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad K1 smd circle (at -7.6 -0.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 269 RGMII_RXD0) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J20 smd circle (at 7.6 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 49 FPDI_CLK+) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J19 smd circle (at 6.8 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 222 DDR3_DQ8) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J18 smd circle (at 6 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 229 DDR3_DQ12) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J17 smd circle (at 5.2 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 202 DDR3_A10) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J16 smd circle (at 4.4 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 186 DDR3_A11) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J15 smd circle (at 3.6 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J14 smd circle (at 2.8 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J13 smd circle (at 2 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J12 smd circle (at 1.2 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J11 smd circle (at 0.4 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J10 smd circle (at -0.4 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J9 smd circle (at -1.2 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J8 smd circle (at -2 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J7 smd circle (at -2.8 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J6 smd circle (at -3.6 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 2V5_3V3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J5 smd circle (at -4.4 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 282 ETH_MDC) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J4 smd circle (at -5.2 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 284 RGMII_TXD1) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J3 smd circle (at -6 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 245 ID_SC) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J2 smd circle (at -6.8 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad J1 smd circle (at -7.6 -1.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 273 RGMII_RX_DV) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H20 smd circle (at 7.6 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 228 DDR3_DQS1-) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H19 smd circle (at 6.8 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H18 smd circle (at 6 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 204 DDR3_CS) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H17 smd circle (at 5.2 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 203 DDR3_WE) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H16 smd circle (at 4.4 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 189 DDR3_A4) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H15 smd circle (at 3.6 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H14 smd circle (at 2.8 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 VCC1V35) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H13 smd circle (at 2 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H12 smd circle (at 1.2 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H11 smd circle (at 0.4 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H10 smd circle (at -0.4 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H9 smd circle (at -1.2 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H8 smd circle (at -2 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 264 VCC1V2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H7 smd circle (at -2.8 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 2V5_3V3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H6 smd circle (at -3.6 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 2V5_3V3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H5 smd circle (at -4.4 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 274 RGMII_RX_CLK) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H4 smd circle (at -5.2 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 287 RGMII_TX_CLK) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H3 smd circle (at -6 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 240 GPIO17) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H2 smd circle (at -6.8 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 275 RGMII_REF_CLK) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad H1 smd circle (at -7.6 -2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 244 ID_SD) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G20 smd circle (at 7.6 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 230 DDR3_DQ15) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G19 smd circle (at 6.8 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 225 DDR3_DQS1+) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G18 smd circle (at 6 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 46 FPDI_D0-) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G17 smd circle (at 5.2 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G16 smd circle (at 4.4 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 193 DDR3_BA1) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G15 smd circle (at 3.6 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G14 smd circle (at 2.8 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G13 smd circle (at 2 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G12 smd circle (at 1.2 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G11 smd circle (at 0.4 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G10 smd circle (at -0.4 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G9 smd circle (at -1.2 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G8 smd circle (at -2 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G7 smd circle (at -2.8 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G6 smd circle (at -3.6 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G5 smd circle (at -4.4 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 265 ETH_~RESET) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G4 smd circle (at -5.2 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G3 smd circle (at -6 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 168 CAM1_C_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G2 smd circle (at -6.8 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 CLK_25MHz) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad G1 smd circle (at -7.6 -2.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 141 GPIO15) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F20 smd circle (at 7.6 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 207 DDR3_CAS) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F19 smd circle (at 6.8 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 224 DDR3_DQ10) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F18 smd circle (at 6 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 195 DDR3_A0) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F17 smd circle (at 5.2 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 45 FPDI_D0+) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F16 smd circle (at 4.4 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 220 DDR3_DM0) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F15 smd circle (at 3.6 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F14 smd circle (at 2.8 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F13 smd circle (at 2 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F12 smd circle (at 1.2 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F11 smd circle (at 0.4 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F10 smd circle (at -0.4 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 2V5_3V3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F9 smd circle (at -1.2 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 2V5_3V3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F8 smd circle (at -2 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F7 smd circle (at -2.8 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F6 smd circle (at -3.6 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F5 smd circle (at -4.4 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 71 USB_FPGA_PULL_D+) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F4 smd circle (at -5.2 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 71 USB_FPGA_PULL_D+) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F3 smd circle (at -6 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 167 CAM1_C_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F2 smd circle (at -6.8 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 117 CAM0_C_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad F1 smd circle (at -7.6 -3.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 259 BTN3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E20 smd circle (at 7.6 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 227 DDR3_DQ11) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E19 smd circle (at 6.8 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 236 DDR3_DQ14) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E18 smd circle (at 6 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 196 DDR3_A3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E17 smd circle (at 5.2 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 FPDI_D1-) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E16 smd circle (at 4.4 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 180 DDR3_A8) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E15 smd circle (at 3.6 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 124 SD_PWR_ON) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E14 smd circle (at 2.8 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 137 GPIO2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E13 smd circle (at 2 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(R37-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E12 smd circle (at 1.2 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(R38-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E11 smd circle (at 0.4 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E10 smd circle (at -0.4 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E9 smd circle (at -1.2 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 292 "Net-(TP_E9-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E8 smd circle (at -2 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 293 "Net-(TP_E8-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E7 smd circle (at -2.8 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E6 smd circle (at -3.6 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 276 ETH_MDIO) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E5 smd circle (at -4.4 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 68 USB_FPGA_PULL_D-) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E4 smd circle (at -5.2 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 166 CAM1_D1_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E3 smd circle (at -6 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 68 USB_FPGA_PULL_D-) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E2 smd circle (at -6.8 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 116 CAM0_C_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad E1 smd circle (at -7.6 -4.4) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 135 BTN1) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D20 smd circle (at 7.6 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 197 DDR3_VREF) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D19 smd circle (at 6.8 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 191 DDR3_A2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D18 smd circle (at 6 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 FPDI_D1+) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D17 smd circle (at 5.2 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 FPDI_D2-) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D16 smd circle (at 4.4 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 296 "Net-(TP_D16-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D15 smd circle (at 3.6 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D14 smd circle (at 2.8 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D13 smd circle (at 2 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(R25-Pad2)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D12 smd circle (at 1.2 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(R26-Pad2)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D11 smd circle (at 0.4 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D10 smd circle (at -0.4 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D9 smd circle (at -1.2 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 134 US2_ID) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D8 smd circle (at -2 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 294 "Net-(TP_D8-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D7 smd circle (at -2.8 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D6 smd circle (at -3.6 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D5 smd circle (at -4.4 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 165 CAM1_D1_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D4 smd circle (at -5.2 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D3 smd circle (at -6 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 258 LED7) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D2 smd circle (at -6.8 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 136 BTN2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad D1 smd circle (at -7.6 -5.2) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 257 LED6) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C20 smd circle (at 7.6 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 226 DDR3_DQ9) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C19 smd circle (at 6.8 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C18 smd circle (at 6 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 FPDI_D2+) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C17 smd circle (at 5.2 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C16 smd circle (at 4.4 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 295 "Net-(TP_C16-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C15 smd circle (at 3.6 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C14 smd circle (at 2.8 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(R36-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C13 smd circle (at 2 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 290 SW1) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C12 smd circle (at 1.2 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C11 smd circle (at 0.4 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 GN0) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C10 smd circle (at -0.4 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 69 GN3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C9 smd circle (at -1.2 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C8 smd circle (at -2 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 70 GP5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C7 smd circle (at -2.8 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C6 smd circle (at -3.6 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C5 smd circle (at -4.4 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C4 smd circle (at -5.2 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 164 CAM1_D0_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C3 smd circle (at -6 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 LED3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C2 smd circle (at -6.8 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 255 LED4) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad C1 smd circle (at -7.6 -6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 256 LED5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B20 smd circle (at 7.6 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(R34-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B19 smd circle (at 6.8 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(R35-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B18 smd circle (at 6 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 138 GPIO3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B17 smd circle (at 5.2 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B16 smd circle (at 4.4 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B15 smd circle (at 3.6 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 140 GPIO4) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B14 smd circle (at 2.8 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B13 smd circle (at 2 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 291 SW2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B12 smd circle (at 1.2 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B11 smd circle (at 0.4 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 72 GP0) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B10 smd circle (at -0.4 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B9 smd circle (at -1.2 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 GP3) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B8 smd circle (at -2 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 73 GN5) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B7 smd circle (at -2.8 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B6 smd circle (at -3.6 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 USB_FPGA_D-) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B5 smd circle (at -4.4 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 261 /gpio/CAM0_D0_LP) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B4 smd circle (at -5.2 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 163 CAM1_D0_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B3 smd circle (at -6 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 LED1) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B2 smd circle (at -6.8 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 LED2) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad B1 smd circle (at -7.6 -6.8) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 114 CAM0_D1_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A19 smd circle (at 6.8 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(R22-Pad2)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A18 smd circle (at 6 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 170 "Net-(R23-Pad2)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A17 smd circle (at 5.2 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 237 Camera_GPIO) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A16 smd circle (at 4.4 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A15 smd circle (at 3.6 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A14 smd circle (at 2.8 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(R24-Pad2)") (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A13 smd circle (at 2 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 238 SDA0) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A12 smd circle (at 1.2 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 239 SCL0) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A11 smd circle (at 0.4 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A10 smd circle (at -0.4 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 110 PCIe_CLK_nREQ) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A9 smd circle (at -1.2 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 111 PCIe_nRST) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A8 smd circle (at -2 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 74 GN4) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A7 smd circle (at -2.8 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 75 GP4) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A6 smd circle (at -3.6 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 USB_FPGA_D+) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A5 smd circle (at -4.4 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 112 CAM0_D0_N) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A4 smd circle (at -5.2 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 113 CAM0_D0_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A3 smd circle (at -6 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 LED0) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad A2 smd circle (at -6.8 -7.6) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 115 CAM0_D1_P) (solder_mask_margin 0.05) (solder_paste_margin -0.025))
    (pad X smd oval (at 8.5 -8.5) (size 0.127 0.508) (layers F.Cu F.Mask))
    (pad X smd oval (at 8.5 -8.5) (size 0.508 0.127) (layers F.Cu F.Mask))
    (pad X smd oval (at -8.5 8.5) (size 0.127 0.508) (layers F.Cu F.Mask))
    (pad X smd oval (at -8.5 8.5) (size 0.508 0.127) (layers F.Cu F.Mask))
    (pad X smd oval (at 8.5 8.5) (size 0.508 0.127) (layers F.Cu F.Mask))
    (pad X smd oval (at 8.5 8.5) (size 0.127 0.508) (layers F.Cu F.Mask))
    (pad X smd oval (at -8.5 -8.5) (size 0.127 0.508) (layers F.Cu F.Mask))
    (pad X smd oval (at -8.5 -8.5) (size 0.508 0.127) (layers F.Cu F.Mask))
    (model ${KISYS3DMOD}/Package_BGA.3dshapes/BGA-256_17.0x17.0mm_Layout16x16_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module jumper:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder_Jumper_NC (layer B.Cu) (tedit 5DEA329A)
    (at 137.66 85.33 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr virtual)
    (fp_text reference RP3 (at 4.22 -0.04 270) (layer B.SilkS))
    (fp_text value 0 (at -1.011 0.042 180) (layer B.Fab) hide)
    (fp_text user %R (at -0.018 0.015 180) (layer Eco2.User) hide)
    (pad 2 smd roundrect (at 0.9675 0 180) (size 1.295 1.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 1 smd roundrect (at -0.9675 0 180) (size 1.295 1.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 27 /power/P3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl_disabled
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm locked (layer F.Cu) (tedit 61D41287)
    (at 101.49 77.58)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference 1.1V_1 (at -0.01 -0.03) (layer F.SilkS) hide)
    (fp_text value 1.1V (at -0.02 0.03 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 264 VCC1V2))
  )
  (module intergalaktik:intergalaktik locked (layer F.Cu) (tedit 0)
    (at 128.58 74.39)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen locked (layer F.Cu) (tedit 0)
    (at 145.5 80.81)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module nlnet:nlnet locked (layer F.Cu) (tedit 0)
    (at 138.83 108.3)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 105.43 100.41 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R33 (at 1.61 -0.03 90) (layer B.SilkS))
    (fp_text value 15k (at -0.035 0.03 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /flash/FPGA_INITN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "connectors:HRS_DF40C-100DP-0.4V(51)" (layer B.Cu) (tedit 6051FC47)
    (at 124.158 109.145)
    (fp_text reference J1 (at -11.425 0.075 90) (layer B.SilkS))
    (fp_text value "DF40C-100DP-0.4V(51)" (at 0.1 -0.05) (layer B.Fab))
    (pad 100 smd rect (at 9.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 99 smd rect (at 9.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 98 smd rect (at 9.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 97 smd rect (at 9.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 237 Camera_GPIO))
    (pad 96 smd rect (at 9 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 95 smd rect (at 9 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 94 smd rect (at 8.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 93 smd rect (at 8.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 92 smd rect (at 8.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 91 smd rect (at 8.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 90 smd rect (at 7.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 52 CM4_1.8V))
    (pad 89 smd rect (at 7.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 88 smd rect (at 7.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 52 CM4_1.8V))
    (pad 87 smd rect (at 7.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 86 smd rect (at 7 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 53 CM4_3.3V))
    (pad 85 smd rect (at 7 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 84 smd rect (at 6.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 53 CM4_3.3V))
    (pad 83 smd rect (at 6.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 82 smd rect (at 6.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 238 SDA0))
    (pad 81 smd rect (at 6.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 80 smd rect (at 5.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 239 SCL0))
    (pad 79 smd rect (at 5.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 78 smd rect (at 5.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 77 smd rect (at 5.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 76 smd rect (at 5 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 75 smd rect (at 5 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 124 SD_PWR_ON))
    (pad 74 smd rect (at 4.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 73 smd rect (at 4.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 72 smd rect (at 4.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 71 smd rect (at 4.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 70 smd rect (at 3.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 69 smd rect (at 3.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 137 GPIO2))
    (pad 68 smd rect (at 3.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 67 smd rect (at 3.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 138 GPIO3))
    (pad 66 smd rect (at 3 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 65 smd rect (at 3 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 64 smd rect (at 2.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 63 smd rect (at 2.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 140 GPIO4))
    (pad 62 smd rect (at 2.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 162 GPIO27))
    (pad 61 smd rect (at 2.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 139 GPIO14))
    (pad 60 smd rect (at 1.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 59 smd rect (at 1.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 58 smd rect (at 1.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 137 GPIO2))
    (pad 57 smd rect (at 1.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 141 GPIO15))
    (pad 56 smd rect (at 1 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 138 GPIO3))
    (pad 55 smd rect (at 1 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 139 GPIO14))
    (pad 54 smd rect (at 0.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 140 GPIO4))
    (pad 53 smd rect (at 0.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 52 smd rect (at 0.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 51 smd rect (at 0.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 141 GPIO15))
    (pad 50 smd rect (at -0.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 240 GPIO17))
    (pad 49 smd rect (at -0.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 142 GPIO18))
    (pad 48 smd rect (at -0.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 162 GPIO27))
    (pad 47 smd rect (at -0.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 143 GPIO23))
    (pad 46 smd rect (at -1 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 241 GPIO22))
    (pad 45 smd rect (at -1 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 144 GPIO24))
    (pad 44 smd rect (at -1.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 242 GPIO10))
    (pad 43 smd rect (at -1.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 42 smd rect (at -1.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 41 smd rect (at -1.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 145 GPIO25))
    (pad 40 smd rect (at -2.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 125 GPIO9))
    (pad 39 smd rect (at -2.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 146 GPIO8))
    (pad 38 smd rect (at -2.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 243 GPIO11))
    (pad 37 smd rect (at -2.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 147 GPIO7))
    (pad 36 smd rect (at -3 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 244 ID_SD))
    (pad 35 smd rect (at -3 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 245 ID_SC))
    (pad 34 smd rect (at -3.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 246 GPIO5))
    (pad 33 smd rect (at -3.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 32 smd rect (at -3.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 31 smd rect (at -3.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 106 GPIO12))
    (pad 30 smd rect (at -4.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 148 GPIO6))
    (pad 29 smd rect (at -4.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 107 GPIO16))
    (pad 28 smd rect (at -4.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 149 GPIO13))
    (pad 27 smd rect (at -4.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 108 GPIO20))
    (pad 26 smd rect (at -5 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 150 GPIO19))
    (pad 25 smd rect (at -5 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 109 GPIO21))
    (pad 24 smd rect (at -5.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 151 GPIO26))
    (pad 23 smd rect (at -5.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 22 smd rect (at -5.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 21 smd rect (at -5.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad S3 smd rect (at 10.275 1.355) (size 0.35 0.66) (layers B.Cu B.Paste B.Mask))
    (pad S4 smd rect (at 10.275 -1.355) (size 0.35 0.66) (layers B.Cu B.Paste B.Mask))
    (pad S1 smd rect (at -10.275 1.355) (size 0.35 0.66) (layers B.Cu B.Paste B.Mask))
    (pad S2 smd rect (at -10.275 -1.355) (size 0.35 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd rect (at -6.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 19 smd rect (at -6.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 262 ETH_nLED1))
    (pad 18 smd rect (at -6.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd rect (at -6.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 263 ETH_nLED2))
    (pad 16 smd rect (at -7 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at -7 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at -7.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -7.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -7.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 126 ETH_0P))
    (pad 11 smd rect (at -7.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 127 ETH_2P))
    (pad 10 smd rect (at -8.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 128 ETH_0N))
    (pad 9 smd rect (at -8.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 129 ETH_2N))
    (pad 8 smd rect (at -8.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -8.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -9 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 130 ETH_1N))
    (pad 5 smd rect (at -9 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 131 ETH_3N))
    (pad 4 smd rect (at -9.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 132 ETH_1P))
    (pad 3 smd rect (at -9.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 133 ETH_3P))
    (pad 2 smd rect (at -9.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -9.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/footprints/connectors/3D/DF40C-100DP.stp
      (offset (xyz 6.75 -0.85 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 -90))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 121.5 108.56 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R27 (at 1.325 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0.0625 -0.025 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /flash/FLASH_MOSI))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 6128DCBD)
    (at 97.62 75.644999 180)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (fp_text reference H4 (at -0.025 -1.45 180) (layer F.SilkS) hide)
    (fp_text value HOLE (at -0.075 0.05 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 3.3 3.3) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 6128DCAD)
    (at 145.62 75.645 180)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (fp_text reference H3 (at 0.025 1.101 180) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0.025 0.8 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 3.3 3.3) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 6128DC9C)
    (at 145.62 108.72 180)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (fp_text reference H1 (at 0.015 -1.46 180) (layer F.SilkS) hide)
    (fp_text value HOLE (at -0.14 -0.15 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 3.3 3.3) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 6128DC88)
    (at 97.619999 108.723599 180)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (fp_text reference H2 (at -0.1 -1.35 180) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 0.95 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 3.3 3.3) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module jumper:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder_Jumper_NC (layer B.Cu) (tedit 5DEA329A)
    (at 136.05 101.315 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr virtual)
    (fp_text reference RP1 (at 2.23 0.185 90) (layer B.SilkS))
    (fp_text value 0 (at -0.975 0.025 180) (layer B.Fab) hide)
    (fp_text user %R (at -0.018 0.015 180) (layer Eco2.User) hide)
    (pad 2 smd roundrect (at 0.9675 0 180) (size 1.295 1.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (pad 1 smd roundrect (at -0.9675 0 180) (size 1.295 1.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 32 /power/P1V1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl_disabled
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radiona:radiona locked (layer F.Cu) (tedit 59DE9037)
    (at 136.47 99.89)
    (descr "Imported from emard.svg")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference radiona (at 1.31 -0.73) (layer F.SilkS) hide)
    (fp_text value radiona (at 0 4.7) (layer F.SilkS) hide)
  )
  (module jumper:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder_Jumper_NC (layer B.Cu) (tedit 5DEA329A)
    (at 103.74 85.3)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr virtual)
    (fp_text reference RP2 (at -0.925 1.35 180) (layer B.SilkS))
    (fp_text value 0 (at -0.975 0.015 180) (layer B.Fab) hide)
    (fp_text user %R (at -0.018 0.015 180) (layer Eco2.User) hide)
    (pad 1 smd roundrect (at -0.9675 0) (size 1.295 1.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 28 /power/P2V5))
    (pad 2 smd roundrect (at 0.9675 0) (size 1.295 1.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 4 +2V5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl_disabled
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module L_1008_1210:L_1008_1210 (layer B.Cu) (tedit 5BC09943)
    (at 137.64 82.03 270)
    (descr "Inductor SMD 1008-1210 (2520-3225 Metric), square (rectangular) end terminal")
    (tags inductor)
    (attr smd)
    (fp_text reference L3 (at -1.98 2.06 180) (layer B.SilkS))
    (fp_text value 2.2uH (at 0 -0.02 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.27 0 270) (size 1.5 2.7) (layers B.Cu B.Paste B.Mask)
      (net 30 /power/L3) (solder_paste_margin -0.15))
    (pad 2 smd rect (at 1.27 0 270) (size 1.5 2.7) (layers B.Cu B.Paste B.Mask)
      (net 27 /power/P3V3) (solder_paste_margin -0.15))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module L_1008_1210:L_1008_1210 (layer B.Cu) (tedit 5BC09943)
    (at 140.31 100.69 180)
    (descr "Inductor SMD 1008-1210 (2520-3225 Metric), square (rectangular) end terminal")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at -2.34 1.94 180) (layer B.SilkS))
    (fp_text value 2.2uH (at -0.01 -0.085 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.27 0 180) (size 1.5 2.7) (layers B.Cu B.Paste B.Mask)
      (net 29 /power/L1) (solder_paste_margin -0.15))
    (pad 2 smd rect (at 1.27 0 180) (size 1.5 2.7) (layers B.Cu B.Paste B.Mask)
      (net 32 /power/P1V1) (solder_paste_margin -0.15))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module L_1008_1210:L_1008_1210 (layer B.Cu) (tedit 5BC09943)
    (at 99.48 85.925)
    (descr "Inductor SMD 1008-1210 (2520-3225 Metric), square (rectangular) end terminal")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at -1.915 1.975 180) (layer B.SilkS))
    (fp_text value 2.2uH (at 0.01 0.025 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.27 0) (size 1.5 2.7) (layers B.Cu B.Paste B.Mask)
      (net 31 /power/L2) (solder_paste_margin -0.15))
    (pad 2 smd rect (at 1.27 0) (size 1.5 2.7) (layers B.Cu B.Paste B.Mask)
      (net 28 /power/P2V5) (solder_paste_margin -0.15))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 100.63 75.53 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C49 (at 1.88 -0.04) (layer B.SilkS))
    (fp_text value 22nF (at 0.0825 -0.018 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 2V5_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 105.425 76.605 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C48 (at 1.93 -0.02 90) (layer B.SilkS))
    (fp_text value 22nF (at -0.02 -0.07) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 2V5_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 143.26 78.74)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C52 (at -2.13 0.01 180) (layer B.SilkS))
    (fp_text value 22nF (at -0.11 -0.06) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 111.54 107.64 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C51 (at -1.8 0 180) (layer B.SilkS))
    (fp_text value 22nF (at 0.1 0 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 109.98 107.64 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C50 (at -1.8 0 180) (layer B.SilkS))
    (fp_text value 22nF (at 0 0 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TSOT-25:TSOT-25 (layer B.Cu) (tedit 5B8526C8)
    (at 141.450001 81.335 90)
    (attr smd)
    (fp_text reference U7 (at 1.245 -2.56) (layer B.SilkS))
    (fp_text value TLV62569DBV (at -0.03 0.04 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.3 90) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0 -1.3 90) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.95 -1.3 90) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 30 /power/L3))
    (pad 4 smd rect (at 0.95 1.3 90) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at -0.95 1.3 90) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 /power/FB3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 102.4 75.5 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C53 (at 1.845 -0.055 180) (layer B.SilkS))
    (fp_text value 22nF (at 0.02 -0.08 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 2V5_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TSOT-25:TSOT-25 (layer B.Cu) (tedit 5B8526C8)
    (at 141.58 104.5)
    (attr smd)
    (fp_text reference U5 (at 1.245 -2.51 90) (layer B.SilkS))
    (fp_text value TLV62569DBV (at 0.075 0.025) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.3) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0 -1.3) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.95 -1.3) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 29 /power/L1))
    (pad 4 smd rect (at 0.95 1.3) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at -0.95 1.3) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 /power/FB1))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TSOT-25:TSOT-25 (layer B.Cu) (tedit 5B8526C8)
    (at 98.21 82.115 180)
    (attr smd)
    (fp_text reference U6 (at 1.22 -2.535 270) (layer B.SilkS))
    (fp_text value TLV62569DBV (at -0.03 -0.06 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.3 180) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0 -1.3 180) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.95 -1.3 180) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 /power/L2))
    (pad 4 smd rect (at 0.95 1.3 180) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at -0.95 1.3 180) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 /power/FB2))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module SOA008-150mil:SOA008-150-208mil (layer F.Cu) (tedit 5B892E95)
    (at 114.703 107.355001)
    (descr "Cypress SOA008 SOIC-8 150/208 mil")
    (tags "SOA008 SOIC-8 1.27 150 208 mil")
    (attr smd)
    (fp_text reference U3 (at -3.222 -3.065 180) (layer F.SilkS))
    (fp_text value IS25LP128F-JBLE (at -0.222 3.035 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.302 -1.905) (size 2.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /flash/FLASH_nCS))
    (pad 2 smd oval (at -3.302 -0.635) (size 2.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /flash/FLASH_MISO))
    (pad 3 smd oval (at -3.302 0.635) (size 2.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /flash/FLASH_nWP))
    (pad 4 smd oval (at -3.302 1.905) (size 2.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd oval (at 3.302 1.905) (size 2.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /flash/FLASH_MOSI))
    (pad 6 smd oval (at 3.302 0.635) (size 2.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /flash/FLASH_SCK))
    (pad 7 smd oval (at 3.302 -0.635) (size 2.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /flash/FLASH_nHOLD))
    (pad 8 smd oval (at 3.302 -1.905) (size 2.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.35x2.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIJ-8_5.3x5.3mm_P1.27mm.wrl_disabled
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 98.215 79.085)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.05 1.115) (layer B.SilkS))
    (fp_text value 22uF (at -0.175 0.015) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 137.650001 107.365)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -0.330001 0.875) (layer B.SilkS))
    (fp_text value 100pF (at 0.095 -0.009999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 /power/FB1))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 /power/P1V1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 137.725 104.989999)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 1.8 0.025 90) (layer B.SilkS))
    (fp_text value 22uF (at 0.1 0) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 /power/P1V1))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 137.715 103.355)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 1.8 0.05 90) (layer B.SilkS))
    (fp_text value 22uF (at 0.1 0.025) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 /power/P1V1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 141.575 107.53 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.075 1.05) (layer B.SilkS))
    (fp_text value 22uF (at 0.225 0.1) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 144.314999 85.265 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -0.385 0.975001) (layer B.SilkS))
    (fp_text value 100pF (at 0.05 -0.05 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 /power/P3V3))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /power/FB3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 141.940001 85.189999 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 1.81 -0.125) (layer B.SilkS))
    (fp_text value 22uF (at 0.025 0.025 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 /power/P3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 140.305 85.199999 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 1.81 0.03) (layer B.SilkS))
    (fp_text value 22uF (at 0.01 -0.02 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 /power/P3V3))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 144.480001 81.34 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 1.115 90) (layer B.SilkS))
    (fp_text value 22uF (at -0.075 -0.025 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 102.14 79.25 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at -0.025 0.775 180) (layer B.SilkS))
    (fp_text value 100pF (at 0.06 0.03) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /power/P2V5))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 /power/FB2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 102.065 81.625 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 1.8 -0.075 90) (layer B.SilkS))
    (fp_text value 22uF (at 0.085 -0.095) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /power/P2V5))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 102.075 83.26 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 1.835 0.01 90) (layer B.SilkS))
    (fp_text value 22uF (at 0.16 0.01) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /power/P2V5))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 132.64 103.75)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 1.88 -0.01 270) (layer B.SilkS))
    (fp_text value 2.2uF (at -0.01 0.115 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 117.23 98.07 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 1.87 0.02 180) (layer B.SilkS))
    (fp_text value 2.2uF (at -0.01 0.06 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 117.23 87.87 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 1.81 0.03 180) (layer B.SilkS))
    (fp_text value 2.2uF (at -0.06 0.05 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +2V5))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 117.23 93.07 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at -0.32 -1.09 90) (layer B.SilkS))
    (fp_text value 2.2uF (at -0.01 0.08 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 139.858999 98.248)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 1.871001 -0.068 90) (layer B.SilkS))
    (fp_text value 2.2uF (at 0.066 0.096) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 /power/P1V1))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 99.931 88.367 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at -1.859 0.067 90) (layer B.SilkS))
    (fp_text value 2.2uF (at -0.009 0.042) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /power/P2V5))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 135.24 82.64 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 1.83 -0.07 180) (layer B.SilkS))
    (fp_text value 2.2uF (at 0.029 0.057 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 /power/P3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 119.63 92.67 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 0.01 -0.82 90) (layer B.SilkS))
    (fp_text value 22nF (at 0 -0.01 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 114.83 92.67 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at 0.02 -0.82 90) (layer B.SilkS))
    (fp_text value 22nF (at 0 -0.02 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 2V5_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 115.630001 97.67 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at 0.01 0.79 90) (layer B.SilkS))
    (fp_text value 22nF (at 0 0.01 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 118.83 97.67 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 -0.83 90) (layer B.SilkS))
    (fp_text value 22nF (at -0.02 0.01 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 120.73 97.57 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 0 -0.82 90) (layer B.SilkS))
    (fp_text value 22nF (at -0.01 -0.07 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +2V5))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 113.63 97.470001 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C39 (at -0.03 0.79 90) (layer B.SilkS))
    (fp_text value 22nF (at 0 0.04 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +2V5))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 114.83 94.87)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -0.01 -0.78) (layer B.SilkS))
    (fp_text value 22nF (at -0.03 0.04) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 119.63 94.87 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -0.05 0.8) (layer B.SilkS))
    (fp_text value 22nF (at 0.01 -0.04) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 104 90.77 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 1.68 -0.15 90) (layer F.SilkS))
    (fp_text value 22nF (at -0.06 -0.025 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 110.69 73.3)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 1.31 -0.07 90) (layer B.SilkS))
    (fp_text value 22nF (at 0 -0.01 180) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 100.6 105.17 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0.52 -0.82) (layer B.SilkS))
    (fp_text value 22nF (at 0.02 0.005) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 131.975 106.13)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C54 (at -2.215 -0.03) (layer F.SilkS))
    (fp_text value 2.2uF (at -0.06 0.165) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 105.43 75.08 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C38 (at 1.86 -0.06 90) (layer B.SilkS))
    (fp_text value 2.2uF (at 0.03 0.01) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 2V5_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 107.850001 79.855 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D0 (at 1.875 -0.669999) (layer F.SilkS))
    (fp_text value RED (at -0.785 -0.379999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /blinkey/ALED0))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 106.14 79.88 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D1 (at 1.85 -0.65) (layer F.SilkS))
    (fp_text value ORANGE (at 0.02 -0.37 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /blinkey/ALED1))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 104.46 79.880001 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D2 (at 1.849999 -0.53) (layer F.SilkS))
    (fp_text value GREEN (at -0.170001 -0.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /blinkey/ALED2))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 102.78 79.88 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D3 (at 1.85 -0.54) (layer F.SilkS))
    (fp_text value BLUE (at -0.24 -0.36 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /blinkey/ALED3))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 109.305999 108.615 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R11 (at -1.595 -0.005999 270) (layer F.SilkS))
    (fp_text value 10k (at -0.045 0.055 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /flash/FLASH_nWP))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 109.04 104.08 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R12 (at -0.04 -0.84 180) (layer F.SilkS))
    (fp_text value 10k (at 0.025 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /flash/FLASH_nHOLD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 109.281 106.265 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R28 (at 0.015 0.741 270) (layer F.SilkS))
    (fp_text value 10k (at 0.032 0.06 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /flash/FLASH_MISO))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 119.956 106.315001 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R29 (at 0.014999 -0.814 270) (layer F.SilkS))
    (fp_text value 1k1 (at 0 -0.025 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /flash/FLASH_SCK))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 107.24 101.91 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R30 (at 1.3 -0.025 45) (layer F.SilkS))
    (fp_text value 4k7 (at 0.055 0.03 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 135) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.48 0 135) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /flash/FLASH_nCS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 104.42 100.41 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R32 (at 1.64 -0.04 270) (layer B.SilkS))
    (fp_text value 15k (at -0.09 0.020001 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 /flash/FPGA_DONE))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 107.6 82.36 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R40 (at -0.43 0.85 270) (layer F.SilkS) hide)
    (fp_text value 549 (at 0.075 0.024999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 LED0))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /blinkey/ALED0))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 105.88 82.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R41 (at -0.35 0.81 270) (layer F.SilkS) hide)
    (fp_text value 549 (at -0.049999 -0.025 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /blinkey/ALED1))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 LED1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 104.18 82.379999 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R42 (at -0.240001 0.85 90) (layer F.SilkS) hide)
    (fp_text value 549 (at 0.05 0.025 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 LED2))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /blinkey/ALED2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 102.485 82.38 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R43 (at -0.22 0.845 90) (layer F.SilkS) hide)
    (fp_text value 549 (at -0.025 0.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 LED3))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /blinkey/ALED3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 137.64 106.314999)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference RA1 (at -1.95 0.175001 90) (layer B.SilkS))
    (fp_text value 15k (at 0.05 0) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 /power/P1V1))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 /power/FB1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 102.15 80.3 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference RA2 (at -1.29 0.125 90) (layer B.SilkS))
    (fp_text value 15k (at 0.035 0.05) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 /power/FB2))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /power/P2V5))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 143.265001 85.275001 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference RA3 (at -1.164999 0.194999 180) (layer B.SilkS))
    (fp_text value 15k (at 0.034999 -0.005 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /power/FB3))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 /power/P3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 139.200001 106.765 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference RB1 (at 0.005 0.849999 270) (layer B.SilkS))
    (fp_text value 18k (at 0 -0.025 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 /power/FB1))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 100.59 79.85 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference RB2 (at -1.25 0.1 180) (layer B.SilkS))
    (fp_text value 4k7 (at 0.015 0.015 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 /power/FB2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 143.715002 83.714999 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference RB3 (at -1.284998 0.134999 270) (layer B.SilkS))
    (fp_text value 3k3 (at -0.065 -0.009999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /power/FB3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 106.26 91.19 270)
    (descr "SMD Crystal TXC 7M http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 2.61 -1.1) (layer F.SilkS))
    (fp_text value FNETHE025 (at -0.025 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V))
    (pad 2 smd rect (at 1.1 0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 -0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 CLK_25MHz))
    (pad 4 smd rect (at -1.1 -0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "connectors:HRS_DF40C-100DP-0.4V(51)" (layer B.Cu) (tedit 6051FC47)
    (at 124.158 75.145)
    (fp_text reference J2 (at -11.475 -0.025 90) (layer B.SilkS))
    (fp_text value "DF40C-100DP-0.4V(51)" (at -0.025 -0.1) (layer B.Fab))
    (pad 1 smd rect (at -9.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 134 US2_ID))
    (pad 2 smd rect (at -9.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 110 PCIe_CLK_nREQ))
    (pad 3 smd rect (at -9.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 54 USB_N))
    (pad 4 smd rect (at -9.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -9 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 55 USB_P))
    (pad 6 smd rect (at -9 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -8.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -8.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -8.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 111 PCIe_nRST))
    (pad 10 smd rect (at -8.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 80 PCIe_CLK_P))
    (pad 11 smd rect (at -7.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at -7.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 81 PCIe_CLK_N))
    (pad 13 smd rect (at -7.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -7.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -7 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 163 CAM1_D0_N))
    (pad 16 smd rect (at -7 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 82 PCIe_RX_P))
    (pad 17 smd rect (at -6.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 164 CAM1_D0_P))
    (pad 18 smd rect (at -6.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 83 PCIe_RX_N))
    (pad 19 smd rect (at -6.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 20 smd rect (at -6.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad S2 smd rect (at -10.275 -1.355) (size 0.35 0.66) (layers B.Cu B.Paste B.Mask))
    (pad S1 smd rect (at -10.275 1.355) (size 0.35 0.66) (layers B.Cu B.Paste B.Mask))
    (pad S4 smd rect (at 10.275 -1.355) (size 0.35 0.66) (layers B.Cu B.Paste B.Mask))
    (pad S3 smd rect (at 10.275 1.355) (size 0.35 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 21 smd rect (at -5.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 165 CAM1_D1_N))
    (pad 22 smd rect (at -5.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 84 PCIe_TX_P))
    (pad 23 smd rect (at -5.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 166 CAM1_D1_P))
    (pad 24 smd rect (at -5.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 85 PCIe_TX_N))
    (pad 25 smd rect (at -5 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 26 smd rect (at -5 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 27 smd rect (at -4.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 167 CAM1_C_N))
    (pad 28 smd rect (at -4.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 112 CAM0_D0_N))
    (pad 29 smd rect (at -4.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 168 CAM1_C_P))
    (pad 30 smd rect (at -4.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 113 CAM0_D0_P))
    (pad 31 smd rect (at -3.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 32 smd rect (at -3.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 33 smd rect (at -3.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 34 smd rect (at -3.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 114 CAM0_D1_N))
    (pad 35 smd rect (at -3 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 36 smd rect (at -3 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 115 CAM0_D1_P))
    (pad 37 smd rect (at -2.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 38 smd rect (at -2.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 39 smd rect (at -2.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 40 smd rect (at -2.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 116 CAM0_C_N))
    (pad 41 smd rect (at -1.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask))
    (pad 42 smd rect (at -1.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 117 CAM0_C_P))
    (pad 43 smd rect (at -1.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 56 HDMI1_HOTPLUG))
    (pad 44 smd rect (at -1.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 45 smd rect (at -1 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 57 HDMI1_SDA))
    (pad 46 smd rect (at -1 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 58 HDMI1_TX2_P))
    (pad 47 smd rect (at -0.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 59 HDMI1_SCL))
    (pad 48 smd rect (at -0.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 60 HDMI1_TX2_N))
    (pad 49 smd rect (at -0.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 61 HDMI1_CEC))
    (pad 50 smd rect (at -0.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 51 smd rect (at 0.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 76 HDMI0_CEC))
    (pad 52 smd rect (at 0.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 62 HDMI1_TX1_P))
    (pad 53 smd rect (at 0.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 77 HDMI0_HOTPLUG))
    (pad 54 smd rect (at 0.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 63 HDMI1_TX1_N))
    (pad 55 smd rect (at 1 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 56 smd rect (at 1 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 57 smd rect (at 1.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 118 DSI0_D0_N))
    (pad 58 smd rect (at 1.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 64 HDMI1_TX0_P))
    (pad 59 smd rect (at 1.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 119 DSI0_D0_P))
    (pad 60 smd rect (at 1.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 65 HDMI1_TX0_N))
    (pad 61 smd rect (at 2.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 62 smd rect (at 2.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 63 smd rect (at 2.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 120 DSI0_D1_N))
    (pad 64 smd rect (at 2.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 66 HDMI1_CLK_P))
    (pad 65 smd rect (at 3 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 121 DSI0_D1_P))
    (pad 66 smd rect (at 3 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 67 HDMI1_CLK_N))
    (pad 67 smd rect (at 3.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 68 smd rect (at 3.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 69 smd rect (at 3.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 122 DSI0_C_N))
    (pad 70 smd rect (at 3.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 36 HDMI0_TX2_P))
    (pad 71 smd rect (at 4.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 123 DSI0_C_P))
    (pad 72 smd rect (at 4.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 39 HDMI0_TX2_N))
    (pad 73 smd rect (at 4.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 74 smd rect (at 4.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 75 smd rect (at 5 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 152 DSI1_D0_N))
    (pad 76 smd rect (at 5 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 40 HDMI0_TX1_P))
    (pad 77 smd rect (at 5.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 153 DSI1_D0_P))
    (pad 78 smd rect (at 5.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 43 HDMI0_TX1_N))
    (pad 79 smd rect (at 5.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 80 smd rect (at 5.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 81 smd rect (at 6.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 154 DSI1_D1_N))
    (pad 82 smd rect (at 6.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 44 HDMI0_TX0_P))
    (pad 83 smd rect (at 6.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 155 DSI1_D1_P))
    (pad 84 smd rect (at 6.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 47 HDMI0_TX0_N))
    (pad 85 smd rect (at 7 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 86 smd rect (at 7 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 87 smd rect (at 7.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 156 DSI1_C_N))
    (pad 88 smd rect (at 7.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 48 HDMI0_CLK_P))
    (pad 89 smd rect (at 7.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 157 DSI1_C_P))
    (pad 90 smd rect (at 7.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 51 HDMI0_CLK_N))
    (pad 91 smd rect (at 8.2 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 92 smd rect (at 8.2 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 93 smd rect (at 8.6 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 158 DSI1_D2_N))
    (pad 94 smd rect (at 8.6 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 159 DSI1_D3_N))
    (pad 95 smd rect (at 9 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 160 DSI1_D2_P))
    (pad 96 smd rect (at 9 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 161 DSI1_D3_P))
    (pad 97 smd rect (at 9.4 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 98 smd rect (at 9.4 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 99 smd rect (at 9.8 1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 78 HDMI0_SDA))
    (pad 100 smd rect (at 9.8 -1.355) (size 0.23 0.66) (layers B.Cu B.Paste B.Mask)
      (net 79 HDMI0_SCL))
    (model ${KIPRJMOD}/footprints/connectors/3D/DF40C-100DP.stp
      (offset (xyz 6.75 -0.85 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 -90))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 127.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C37 (at -1.64 -0.02 90) (layer F.SilkS))
    (fp_text value 100n (at 0.03 0.07 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 HDMI0_TX2_P))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 FPDI_D2+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 128.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C36 (at -1.66 -0.01 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0.03 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 FPDI_D2-))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 HDMI0_TX2_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 129.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at -1.64 0.01 90) (layer F.SilkS))
    (fp_text value 100n (at -0.04 0.03 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 HDMI0_TX1_P))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 FPDI_D1+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 130.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C34 (at -1.65 0.04 90) (layer F.SilkS))
    (fp_text value 100n (at -0.03 0.04 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 FPDI_D1-))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 HDMI0_TX1_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 131.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at -1.65 -0.03 90) (layer F.SilkS))
    (fp_text value 100n (at -0.03 -0.03 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 HDMI0_TX0_P))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 FPDI_D0+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 132.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C32 (at -1.63 0.04 90) (layer F.SilkS))
    (fp_text value 100n (at -0.02 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 FPDI_D0-))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 HDMI0_TX0_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 133.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at -1.68 0.01 90) (layer F.SilkS))
    (fp_text value 100n (at 0.03 0.04 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 HDMI0_CLK_P))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 FPDI_CLK+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 134.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at -1.65 0.04 90) (layer F.SilkS))
    (fp_text value 100n (at -0.06 0.03 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 FPDI_CLK-))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 HDMI0_CLK_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 119.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C47 (at 1.65 0 90) (layer F.SilkS))
    (fp_text value 100n (at -0.03 0.02 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 HDMI1_TX2_P))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 GP5))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 120.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C46 (at 1.65 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0.03 -0.03 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 GN5))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 HDMI1_TX2_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 121.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C45 (at 1.65 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 HDMI1_TX1_P))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 GP4))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 122.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C44 (at 1.64 0.01 90) (layer F.SilkS))
    (fp_text value 100n (at -0.03 -0.03 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 GN4))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 HDMI1_TX1_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 123.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C43 (at 1.63 -0.01 90) (layer F.SilkS))
    (fp_text value 100n (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 HDMI1_TX0_P))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 GP3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 124.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C42 (at 1.63 0.09 90) (layer F.SilkS))
    (fp_text value 100n (at -0.005001 0.044999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 HDMI1_TX0_N))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 GN3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 125.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C41 (at 1.64 0.08 90) (layer F.SilkS))
    (fp_text value 100n (at 0.03 0.02 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 GP0))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 HDMI1_CLK_P))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 126.92 78.37 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C40 (at 1.64 0.01 90) (layer F.SilkS))
    (fp_text value 100n (at 0.03 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 GN0))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 HDMI1_CLK_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 108.59 76.030001 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D10 (at 0.81 1.33 180) (layer B.SilkS))
    (fp_text value 1N914 (at 0 -0.04 180) (layer B.Fab))
    (fp_text user %R (at -0.04 -0.07 180) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 71 USB_FPGA_PULL_D+))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 251 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 108.590002 78)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D11 (at -2.230002 0.04 180) (layer B.SilkS))
    (fp_text value 1N914 (at -0.01 -0.04 180) (layer B.Fab))
    (fp_text user %R (at -0.01 -0.04 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 71 USB_FPGA_PULL_D+))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 252 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 110.23 80.61 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D12 (at 2.03 0.54) (layer B.SilkS))
    (fp_text value 1N914 (at -0.04 -0.04 90) (layer B.Fab))
    (fp_text user %R (at 0.05 0.03 90) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 68 USB_FPGA_PULL_D-))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 253 "Net-(D12-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 108.25 80.59 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D13 (at 1.15 -1.3 90) (layer B.SilkS))
    (fp_text value 1N914 (at 0.03 -0.02 90) (layer B.Fab))
    (fp_text user %R (at 0 0.02 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 68 USB_FPGA_PULL_D-))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 254 "Net-(D13-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 111.25 76.41 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -1.32 -0.07 90) (layer B.SilkS))
    (fp_text value 27 (at -0.135001 -0.084999 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 USB_N))
    (pad 2 smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 USB_FPGA_D-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 111.24 75.4 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -1.35 -0.04 90) (layer B.SilkS))
    (fp_text value 27 (at -0.025001 -0.004999 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 USB_FPGA_D+))
    (pad 1 smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 55 USB_P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 109.24 74.509999 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0.48 0.81 180) (layer B.SilkS))
    (fp_text value 1k1 (at -0.055001 -0.014999 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 251 "Net-(D10-Pad1)"))
    (pad 2 smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 USB_FPGA_D+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 111.26 77.45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 1.36 -0.01 270) (layer B.SilkS))
    (fp_text value 15k (at -0.035001 -0.054999 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 USB_FPGA_D+))
    (pad 1 smd roundrect (at -0.51 0) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 252 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 111.75 79.960001 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.52 0.8 90) (layer B.SilkS))
    (fp_text value 1k1 (at 0.074999 -0.024999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 USB_FPGA_D-))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 253 "Net-(D12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 111.255001 78.464999)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 1.344999 0.045001 90) (layer B.SilkS))
    (fp_text value 15k (at 0.034999 -0.004999 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 254 "Net-(D13-Pad2)"))
    (pad 2 smd roundrect (at 0.51 0) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 USB_FPGA_D-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 124.97 79.36 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 1.37 0.02 270) (layer B.SilkS))
    (fp_text value 100k (at -0.025001 -0.094999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 HDMI0_CEC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 125.97 79.36 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 1.37 0.02 270) (layer B.SilkS))
    (fp_text value 100k (at -0.025001 -0.044999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 77 HDMI0_HOTPLUG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 122.97 79.37 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 1.6 -0.000295 270) (layer B.SilkS))
    (fp_text value 4k7 (at -0.065001 -0.064999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 HDMI1_SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 121.97 79.37137 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 1.59137 0.06 270) (layer B.SilkS))
    (fp_text value 4k7 (at -0.075001 -0.134999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 57 HDMI1_SDA))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 136.97 78.38 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 1.65 0.1 90) (layer F.SilkS))
    (fp_text value 4k7 (at 0.024999 0.064999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 HDMI0_SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 135.94 78.38 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 1.64 0.08 90) (layer F.SilkS))
    (fp_text value 4k7 (at -0.025001 0.034999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 HDMI0_SDA))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 123.97 79.37 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 1.6 0.05 270) (layer B.SilkS))
    (fp_text value 100k (at 0.024999 -0.014999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 61 HDMI1_CEC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 120.970293 79.371371 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 1.591371 0.019707 270) (layer B.SilkS))
    (fp_text value 100k (at 0.004999 -0.124999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 56 HDMI1_HOTPLUG))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 100.53 92.83 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C55 (at -1.64 0 270) (layer F.SilkS) hide)
    (fp_text value 22n (at 0.114999 0.024999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 /serdes/S_2_P))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 PCIe_TX_P))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 116.17 105.23 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C56 (at 1.87 -0.01 270) (layer B.SilkS))
    (fp_text value 22n (at 0.044999 -0.014999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 ETH_2P))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 /serdes/S_3_P))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 117.19 105.23 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C57 (at 1.83 -0.03 270) (layer B.SilkS))
    (fp_text value 22n (at 0.064999 -0.024999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 /serdes/S_6_P))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 132 ETH_1P))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.37 75.779999)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C58 (at 1.65 0.04) (layer F.SilkS))
    (fp_text value 22n (at 0.034999 -0.005001) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 /serdes/S_7_P))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 155 DSI1_D1_P))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 96.53 92.83 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C59 (at -1.64 -0.02 90) (layer F.SilkS) hide)
    (fp_text value 22n (at -0.015001 0.044999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 /serdes/CLK_0_P))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 PCIe_CLK_P))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 98.53 92.83 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C61 (at -1.64 0 90) (layer F.SilkS) hide)
    (fp_text value 22n (at 0.054999 -0.025001 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 PCIe_RX_P))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 /serdes/S_0_P))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 113.17 105.23 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C62 (at 1.85 0.02 270) (layer B.SilkS))
    (fp_text value 22n (at 0.014999 0.065001 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 133 ETH_3P))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 /serdes/S_1_P))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.37 77.78)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C63 (at 1.65 0) (layer F.SilkS))
    (fp_text value 22n (at -0.045001 -0.025001) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 157 DSI1_C_P))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 /serdes/CLK_1_P))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 120.19 105.23 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C64 (at 1.76 0.02 270) (layer B.SilkS))
    (fp_text value 22n (at 0.064999 -0.014999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 126 ETH_0P))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 94 /serdes/S_4_P))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.37 73.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C65 (at 1.65 0) (layer F.SilkS))
    (fp_text value 22n (at 0.104999 0.024999) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 /serdes/S_5_P))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 153 DSI1_D0_P))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 95.53 92.83 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C66 (at 1.63 0.01 270) (layer F.SilkS) hide)
    (fp_text value 22n (at 0.094999 0.054999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 PCIe_CLK_N))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /serdes/CLK_0_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 97.53 92.83 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C67 (at 1.64 -0.01 90) (layer F.SilkS) hide)
    (fp_text value 22n (at 0.054999 0.014999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 PCIe_RX_N))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /serdes/S_0_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 114.17 105.23 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C68 (at -1.86 -0.09 270) (layer B.SilkS))
    (fp_text value 22n (at 0.004999 -0.044999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 /serdes/S_1_N))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 131 ETH_3N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.37 78.78 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C69 (at -1.65 0) (layer F.SilkS))
    (fp_text value 22n (at 0 -0.025001) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /serdes/CLK_1_N))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 156 DSI1_C_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 119.19 105.23 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C70 (at -1.81 0.07 270) (layer B.SilkS))
    (fp_text value 22n (at 0.064999 -0.054999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 /serdes/S_4_N))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 128 ETH_0N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.37 74.77 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C71 (at -1.65 0) (layer F.SilkS))
    (fp_text value 22n (at 0.024999 0.014999) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 /serdes/S_5_N))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 152 DSI1_D0_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 99.53 92.83 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C72 (at 1.66 0.03 90) (layer F.SilkS) hide)
    (fp_text value 22n (at 0.024999 0.014999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 /serdes/S_2_N))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 PCIe_TX_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 115.17 105.23 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C73 (at -1.86 -0.02 270) (layer B.SilkS))
    (fp_text value 22n (at 0.054999 -0.054999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 129 ETH_2N))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 /serdes/S_3_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 118.19 105.23 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C74 (at -1.78 0.07 270) (layer B.SilkS))
    (fp_text value 22n (at 0.084999 -0.034999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 130 ETH_1N))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 /serdes/S_6_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.37 76.78 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C75 (at -1.65 -0.02) (layer F.SilkS))
    (fp_text value 22n (at 0.024999 0.074999) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 154 DSI1_D1_N))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 /serdes/S_7_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 95.53 85.91 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R18 (at -1.345001 -0.014999) (layer B.SilkS))
    (fp_text value 130 (at -0.025001 0.045001 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 260 "Net-(BTN1-Pad1)"))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Switch_EVPAA:Switch_EVPAA (layer F.Cu) (tedit 55A9C470)
    (at 97.125 86.2 90)
    (descr "Panasonic micro switch")
    (tags "EVPAA Switch")
    (attr smd)
    (fp_text reference BTN1 (at 1.515 -2.195 90) (layer F.SilkS))
    (fp_text value SW_Push (at 0.064999 1.624999 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.925 -0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(BTN1-Pad1)"))
    (pad 2 smd rect (at -1.925 0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 135 BTN1))
    (pad 1 smd rect (at 1.925 -0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(BTN1-Pad1)"))
    (pad 2 smd rect (at 1.925 0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 135 BTN1))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Switch_EVPAA:Switch_EVPAA (layer F.Cu) (tedit 55A9C470)
    (at 101.61 88.1 90)
    (descr "Panasonic micro switch")
    (tags "EVPAA Switch")
    (attr smd)
    (fp_text reference BTN2 (at 1.6 -2.19 90) (layer F.SilkS))
    (fp_text value SW_Push (at 0.004999 1.664999 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.925 0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 136 BTN2))
    (pad 1 smd rect (at 1.925 -0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(BTN1-Pad1)"))
    (pad 2 smd rect (at -1.925 0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 136 BTN2))
    (pad 1 smd rect (at -1.925 -0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(BTN1-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer B.Cu) (tedit 58641869)
    (at 114.17 81.85 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D8 (at -2.325001 0.005001) (layer B.SilkS))
    (fp_text value 3.6V (at 1.604999 -0.784999 90) (layer B.Fab))
    (fp_text user %R (at -0.065001 -0.054999 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 21 USB_FPGA_D+))
    (pad 2 smd rect (at 1.25 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer B.Cu) (tedit 58641869)
    (at 112.21 82.97 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D9 (at 1.61 1.29 270) (layer B.SilkS))
    (fp_text value 3.6V (at 1.614999 -0.764999 90) (layer B.Fab))
    (fp_text user %R (at -0.185001 -0.084999 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 26 USB_FPGA_D-))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 114.51 78.3)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 1.68 -0.01 180) (layer B.SilkS))
    (fp_text value 4k7 (at 0.714999 -0.374999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 134 US2_ID))
    (pad 2 smd roundrect (at 0.51 0) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 131.43 107.96)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -1.66 0.04 180) (layer F.SilkS))
    (fp_text value 4k7 (at 0.724999 0.374999) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 1 smd roundrect (at -0.51 0) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 SD_PWR_ON))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 118.9 78.42 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 1.66 0 90) (layer F.SilkS))
    (fp_text value 220 (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 113 CAM0_D0_P))
    (pad 2 smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 261 /gpio/CAM0_D0_LP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 127.44 85.35 225)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at -1.661701 0.035355 225) (layer B.SilkS))
    (fp_text value 300 (at -0.02 -0.03 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 225) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 160 DSI1_D2_P))
    (pad 2 smd roundrect (at 0.51 0 225) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 169 "Net-(R22-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 125.23 84.71 225)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at -1.668772 -0.127279 45) (layer B.SilkS))
    (fp_text value 300 (at -0.02 -0.01 45) (layer B.Fab))
    (fp_text user %R (at 0 0 45) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 225) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 161 DSI1_D3_P))
    (pad 2 smd roundrect (at 0.51 0 225) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 170 "Net-(R23-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 119.569376 83.280624 225)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 0.034473 0.770746 225) (layer B.SilkS))
    (fp_text value 300 (at 0 -0.05 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0 225) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 171 "Net-(R24-Pad2)"))
    (pad 1 smd roundrect (at -0.51 0 225) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 121 DSI0_D1_P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 124.69 82.21 225)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at -1.633417 -0.049497 225) (layer F.SilkS))
    (fp_text value 300 (at 0.05 0.03 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 225) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 172 "Net-(R25-Pad2)"))
    (pad 1 smd roundrect (at -0.51 0 225) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 DSI0_D0_P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 121 81.89 225)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 0.127279 0.820244 225) (layer B.SilkS))
    (fp_text value 300 (at -0.01 0.05 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0 225) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 173 "Net-(R26-Pad2)"))
    (pad 1 smd roundrect (at -0.51 0 225) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 123 DSI0_C_P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 126.2 86.86 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R34 (at 0.028284 0.876812 225) (layer B.SilkS))
    (fp_text value 300 (at 0 0.02 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 45) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 174 "Net-(R34-Pad1)"))
    (pad 2 smd roundrect (at 0.51 0 45) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 158 DSI1_D2_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 126.28 85.08 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R35 (at 1.689985 0.021213 225) (layer B.SilkS))
    (fp_text value 300 (at -0.080001 0 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0 45) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 159 DSI1_D3_N))
    (pad 1 smd roundrect (at -0.51 0 45) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 175 "Net-(R35-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 120.28 83.98 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R36 (at -0.091924 0.841457 225) (layer B.SilkS))
    (fp_text value 300 (at -0.05 -0.04 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 45) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 176 "Net-(R36-Pad1)"))
    (pad 2 smd roundrect (at 0.51 0 45) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 120 DSI0_D1_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 125.51 82.81 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R37 (at 1.633417 -0.26163 45) (layer F.SilkS))
    (fp_text value 300 (at -0.03 0.01 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 45) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 118 DSI0_D0_N))
    (pad 1 smd roundrect (at -0.51 0 45) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 177 "Net-(R37-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 121.72 82.6 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R38 (at 0.035355 0.855599 225) (layer B.SilkS))
    (fp_text value 300 (at -0.045001 -0.004999 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 45) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 178 "Net-(R38-Pad1)"))
    (pad 2 smd roundrect (at 0.51 0 45) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 122 DSI0_C_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 123.02 84.14 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R39 (at 0.02 -0.85 90) (layer F.SilkS))
    (fp_text value 70 (at 0 0.004999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 DSI0_C_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 129.69 82.16)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R49 (at 0 -0.785001) (layer F.SilkS))
    (fp_text value 70 (at -0.085001 0.064999) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 123 DSI0_C_P))
    (pad 2 smd roundrect (at 0.51 0) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 124.73 80.81 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R50 (at -1.661701 -0.049497 45) (layer F.SilkS))
    (fp_text value 70 (at -0.065001 0.004999 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0 45) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 DSI0_D0_P))
    (pad 2 smd roundrect (at 0.51 0 45) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 127.31 81.81 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R51 (at -0.007071 0.940452 45) (layer F.SilkS))
    (fp_text value 70 (at -0.055001 0.054999 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 45) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.51 0 45) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 118 DSI0_D0_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 121.21 86.85 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R52 (at -0.04 0.81 270) (layer B.SilkS))
    (fp_text value 70 (at -0.045001 -0.004999 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 121 DSI0_D1_P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 122.22 86.85 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R48 (at -1.66 -0.08 90) (layer B.SilkS))
    (fp_text value 70 (at -0.055001 -0.034999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 120 DSI0_D1_N))
    (pad 2 smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 138.35 106.32)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference RC1 (at 1.66 0.37 180) (layer F.SilkS))
    (fp_text value *DNP (at -0.015001 0.004999) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /power/FB1))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 179 "Net-(RC1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 138.76 108.4 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference RC2 (at -1.64 0) (layer B.SilkS))
    (fp_text value 91k (at 0.034999 -0.004999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 179 "Net-(RC1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 136.78 95.389999 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C76 (at 0.849999 -0.87 90) (layer B.SilkS))
    (fp_text value 22uF (at 0.46 0.05 -90) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 136.945001 91.465 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C77 (at -0.305 0.795001 270) (layer B.SilkS))
    (fp_text value 100pF (at 0.06 -0.06 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 233 /power/P1V35))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 234 /power/FB4))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 139.319998 91.540001 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C95 (at 1.889999 -0.020002) (layer B.SilkS))
    (fp_text value 22uF (at 0.2 -0.05 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 233 /power/P1V35))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 140.955 91.530001 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C96 (at 1.899999 -0.005) (layer B.SilkS))
    (fp_text value 22uF (at -0.03 -0.14 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 233 /power/P1V35))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 146.062001 93.674 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C97 (at 2.316 -0.527999 270) (layer B.SilkS))
    (fp_text value 2.2uF (at 0.245 0.15 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 233 /power/P1V35))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 145.8 89.23)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C98 (at -0.53 1.3) (layer B.SilkS))
    (fp_text value 2.2uF (at -0.19 0.02) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module L_1008_1210:L_1008_1210 (layer B.Cu) (tedit 5BC09943)
    (at 143.62 94.125001 90)
    (descr "Inductor SMD 1008-1210 (2520-3225 Metric), square (rectangular) end terminal")
    (tags inductor)
    (attr smd)
    (fp_text reference L4 (at -2.514999 -0.93) (layer B.SilkS))
    (fp_text value 2.2uH (at 0.01 -1.09 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.27 0 90) (size 1.5 2.7) (layers B.Cu B.Paste B.Mask)
      (net 233 /power/P1V35) (solder_paste_margin -0.15))
    (pad 1 smd rect (at -1.27 0 90) (size 1.5 2.7) (layers B.Cu B.Paste B.Mask)
      (net 235 /power/L4) (solder_paste_margin -0.15))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 137.99 91.46 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference RA4 (at -1.11 0.13 180) (layer B.SilkS))
    (fp_text value 15k (at 0.01 0.03 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 234 /power/FB4))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 233 /power/P1V35))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 137.544998 93.015001)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference RB4 (at -1.224999 0.054999 90) (layer B.SilkS))
    (fp_text value 12k (at 0.07 -0.04 -180) (layer B.Fab))
    (fp_text user %R (at 0 0 -180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 234 /power/FB4))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module jumper:R_0805_2012Metric_Pad1.29x1.40mm_HandSolder_Jumper_NC (layer B.Cu) (tedit 5DEA329A)
    (at 143 89.85 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr virtual)
    (fp_text reference RP4 (at 0.8 -1.27 270) (layer B.SilkS))
    (fp_text value 0 (at 1.639 0.001 270) (layer B.Fab) hide)
    (fp_text user %R (at -0.018 0.015 270) (layer Eco2.User) hide)
    (pad 1 smd roundrect (at -0.9675 0 90) (size 1.295 1.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 233 /power/P1V35))
    (pad 2 smd roundrect (at 0.9675 0 90) (size 1.295 1.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl_disabled
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TSOT-25:TSOT-25 (layer B.Cu) (tedit 5B8526C8)
    (at 139.81 95.39 270)
    (attr smd)
    (fp_text reference U8 (at -0.06 1.41 90) (layer B.SilkS))
    (fp_text value TLV62569DBV (at 0.254 0.127 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 5 smd rect (at -0.95 1.3 270) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 234 /power/FB4))
    (pad 4 smd rect (at 0.95 1.3 270) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at 0.95 -1.3 270) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 235 /power/L4))
    (pad 2 smd rect (at 0 -1.3 270) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 -1.3 270) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 146.92 90.49)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C92 (at 0.59 -1.16 90) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0.05 0.36) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 101.1 79.880001 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D4 (at 1.849999 -0.53 180) (layer F.SilkS))
    (fp_text value RED (at 0.049999 -0.32 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 247 /blinkey/ALED4))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 99.415001 79.880001 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D5 (at 1.849999 -0.614999 180) (layer F.SilkS))
    (fp_text value ORANGE (at 0.029999 -0.034999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 248 /blinkey/ALED5))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 97.735001 79.880001 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D6 (at 1.849999 -0.694999 180) (layer F.SilkS))
    (fp_text value GREEN (at -0.120001 -0.084999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 249 /blinkey/ALED6))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 96.055001 79.880001 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D7 (at 1.849999 -0.624999 180) (layer F.SilkS))
    (fp_text value BLUE (at -0.060001 -0.074999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 250 /blinkey/ALED7))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 100.83 82.36 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R44 (at -0.25 0.91 90) (layer F.SilkS) hide)
    (fp_text value 549 (at -0.03 0.03 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 255 LED4))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 247 /blinkey/ALED4))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 99.24 82.36 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R45 (at -0.28 0.9 90) (layer F.SilkS) hide)
    (fp_text value 549 (at 0.01 0.08 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 248 /blinkey/ALED5))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 256 LED5))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 97.58 82.36 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R46 (at -0.36 0.84 90) (layer F.SilkS) hide)
    (fp_text value 549 (at -0.03 0.03 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 257 LED6))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 249 /blinkey/ALED6))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 95.8 82.36 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R47 (at -0.4 0.88 90) (layer F.SilkS) hide)
    (fp_text value 549 (at -0.02 0.09 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 250 /blinkey/ALED7))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 258 LED7))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 138.34 98.04 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C88 (at -1.230366 0.028284 315) (layer F.SilkS))
    (fp_text value C_100n_0402 (at -0.318198 -0.33234 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 225) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 197 DDR3_VREF))
    (pad 2 smd roundrect (at 0.48 0 225) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 135.26 85.35 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C79 (at -0.02 -2.49 270) (layer B.SilkS))
    (fp_text value C_4u7_0402 (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 145.84 86.4)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C80 (at 1.68 0.1 180) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 134.26 85.35 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C81 (at -0.02 -2.19 90) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 138.69 87.27 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C82 (at -1.66 0.05 90) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 134.63 97.02 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C83 (at 1.65 -0.08) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 134.23 91.25)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C84 (at -1.67 0.05) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 137.69 87.27 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C85 (at -1.66 0.01 90) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 134.215 92.24)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C86 (at -1.635 -0.03) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 134.1 95.35)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C87 (at -1.67 0.04) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 146.58 87.4)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C89 (at 0 0.79) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 144.23 97.02)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C90 (at 1.89 0.56 180) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 146.92 91.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C91 (at -1.67 -0.06) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 135.47 98.47 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C93 (at 1.4 0.24 180) (layer B.SilkS))
    (fp_text value C_100n_0402 (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 197 DDR3_VREF))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 142.98 87.46 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C94 (at -1.74 -0.01 180) (layer B.SilkS))
    (fp_text value C_100n_0402 (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 232 "Net-(C94-Pad2)"))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 134 98.01 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C200 (at 1.9 -0.05) (layer B.SilkS))
    (fp_text value C_100n_0402 (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 197 DDR3_VREF))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 136.48 98.47 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C201 (at -0.05 -0.87 270) (layer B.SilkS))
    (fp_text value C_100n_0402 (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 197 DDR3_VREF))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 145.63 84.47 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R81 (at 0.28 0.9 90) (layer B.SilkS))
    (fp_text value R_240R_0402 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 201 "Net-(R81-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 139.74 88.58 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R82 (at 1.23 0.17) (layer B.SilkS))
    (fp_text value R_51R_0402 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 232 "Net-(C94-Pad2)"))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 209 DDR3_CLK+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 140.74 88.59 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R83 (at -1.26 -0.58 180) (layer B.SilkS))
    (fp_text value R_51R_0402 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 232 "Net-(C94-Pad2)"))
    (pad 2 smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 206 DDR3_CLK-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Switch_EVPAA:Switch_EVPAA (layer F.Cu) (tedit 55A9C470)
    (at 106.12 86.2 90)
    (descr "Panasonic micro switch")
    (tags "EVPAA Switch")
    (attr smd)
    (fp_text reference BTN3 (at 1.59 -2.21 90) (layer F.SilkS))
    (fp_text value SW_Push (at 0.59 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.925 -0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(BTN1-Pad1)"))
    (pad 2 smd rect (at -1.925 0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 259 BTN3))
    (pad 1 smd rect (at 1.925 -0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(BTN1-Pad1)"))
    (pad 2 smd rect (at 1.925 0.725 90) (size 1.15 1.05) (layers F.Cu F.Paste F.Mask)
      (net 259 BTN3))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 134.38 83.49 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C78 (at 1.65 -0.05 180) (layer F.SilkS))
    (fp_text value C_10u_0402 (at 0.034999 0.334999) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 109.42 102.92)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R31 (at 0 0.82) (layer B.SilkS))
    (fp_text value 15k (at -0.055001 -0.334999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 /flash/FPGA_PROGRAMN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 96.36 95.94 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C99 (at -1.61 0.01 90) (layer B.SilkS))
    (fp_text value C_4u7_0402 (at 0 -0.364999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 98.33 95.94 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C100 (at -1.83 0 90) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0.004999 -0.354999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 95.21 101.18 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C101 (at 0.04 0.72 90) (layer F.SilkS) hide)
    (fp_text value C_100n_0402 (at -0.035001 0.334999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 265 ETH_~RESET))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 97.35 95.94 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C102 (at -1.84 -0.01 90) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0.004999 -0.304999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 99.32 95.94 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C103 (at -1.85 0 90) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -0.354999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 100.31 95.95 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C104 (at -1.86 0 90) (layer B.SilkS))
    (fp_text value C_10n_0402 (at -0.005001 -0.354999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 102.03 101.17 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C105 (at -0.31 -0.81) (layer B.SilkS))
    (fp_text value C_4u7_0402 (at -0.005001 -0.364999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 101.29 95.8 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C106 (at -1.86 -0.03 90) (layer B.SilkS))
    (fp_text value C_10n_0402 (at 0.004999 -0.354999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 102.03 100.19 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C107 (at 1.84 -0.03) (layer B.SilkS))
    (fp_text value C_470n_0402 (at -0.035001 -0.344999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 102.27 95.34 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C108 (at -1.87 0.01 90) (layer B.SilkS))
    (fp_text value C_10n_0402 (at -0.015001 -0.354999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 97.2 104.26 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C109 (at 1.75 0 270) (layer B.SilkS))
    (fp_text value C_4u7_0402 (at -0.005001 -0.354999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 266 "Net-(C109-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 102.03 99.21 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C110 (at 0 1.16) (layer B.SilkS))
    (fp_text value C_10n_0402 (at 0.014999 -0.354999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 103.26 95.34 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C111 (at -1.82 0.01 90) (layer B.SilkS))
    (fp_text value C_10n_0402 (at 0 -0.354999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 98.18 104.26 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C112 (at 1.78 -0.02 270) (layer B.SilkS))
    (fp_text value C_10n_0402 (at -0.015001 -0.324999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 266 "Net-(C109-Pad1)"))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 102.04 98.23 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C113 (at -1.84 0.01) (layer B.SilkS))
    (fp_text value C_10n_0402 (at 0 -0.354999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 104.25 95.03 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C114 (at -1.82 0.01 90) (layer B.SilkS))
    (fp_text value C_10n_0402 (at 0.044999 -0.344999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 99.16 104.47 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C115 (at 2.01 0.05 270) (layer B.SilkS))
    (fp_text value C_10n_0402 (at 0.014999 -0.354999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 266 "Net-(C109-Pad1)"))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 102.05 97.25 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C116 (at -1.84 0.03) (layer B.SilkS))
    (fp_text value C_10n_0402 (at 0.034999 -0.314999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 101.36 103.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C117 (at 1.83 -0.55 90) (layer B.SilkS))
    (fp_text value C_4u7_0402 (at -0.005001 -0.364999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 267 /ethernet/AVDDL))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 100.37 103.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C118 (at -0.12 0.76 270) (layer B.SilkS))
    (fp_text value C_470n_0402 (at 0 -0.364999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 267 /ethernet/AVDDL))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 102.35 103.72 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C119 (at 1.88 -0.33 90) (layer B.SilkS))
    (fp_text value C_10n_0402 (at 0.054999 -0.354999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 267 /ethernet/AVDDL))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 97.87 98.99)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C120 (at 1.86 0.08) (layer B.SilkS))
    (fp_text value C_4u7_0402 (at 0 -0.364999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 268 /ethernet/AVDDL_PLL))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 103.34 103.72 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C121 (at 1.89 -0.02 90) (layer B.SilkS))
    (fp_text value C_10n_0402 (at -0.005001 -0.354999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 267 /ethernet/AVDDL))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 99.61 97.49)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C122 (at 0.12 0.81) (layer B.SilkS))
    (fp_text value C_100n_0402 (at 0 -0.354999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 268 /ethernet/AVDDL_PLL))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 95.99 98.99 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C123 (at 1.44 0.04 90) (layer B.SilkS))
    (fp_text value C_10n_0402 (at 0.034999 -0.294999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 268 /ethernet/AVDDL_PLL))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 99.72 101.5 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C124 (at -0.05 0.75 90) (layer B.SilkS))
    (fp_text value C_10n_0402 (at 0 -0.364999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5F68FEF0)
    (at 95.95 104.82 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB1 (at -1.85 -0.09 180) (layer B.SilkS))
    (fp_text value BLM18PG121SN1D (at 0.004999 -0.614999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 266 "Net-(C109-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5F68FEF0)
    (at 105.34 103.9)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB2 (at -0.05 0.94) (layer B.SilkS))
    (fp_text value BLM18PG121SN1D (at -0.07 -0.62) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 267 /ethernet/AVDDL))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5F68FEF0)
    (at 97.14 97.74)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB3 (at -1.8 -0.11 270) (layer B.SilkS))
    (fp_text value BLM18PG121SN1D (at -0.055001 -0.624999) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 264 VCC1V2))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 268 /ethernet/AVDDL_PLL))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 95.21 99.25 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R58 (at 0.02 0.71 90) (layer F.SilkS) hide)
    (fp_text value R_4k7_0402 (at 0 0.364999 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 265 ETH_~RESET))
    (pad 1 smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 105.81 93.82 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R61 (at 1.65 -0.02) (layer F.SilkS))
    (fp_text value R_2k2_0402 (at 0.014999 0.374999) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 276 ETH_MDIO))
    (pad 1 smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 95.2 103.09 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R65 (at 0 0.71 270) (layer F.SilkS) hide)
    (fp_text value R_12k1_0402 (at 0.004999 0.364999 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 280 "Net-(R65-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 107.48 108.9 135)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R66 (at 1.668772 -0.113137 315) (layer F.SilkS))
    (fp_text value R_1k_0402 (at 0 0.374999 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0 135) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 263 ETH_nLED2))
    (pad 2 smd roundrect (at 0.51 0 135) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 278 /ethernet/ETH_LED1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 106.34 109.2 135)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R67 (at -0.035355 -0.827315 315) (layer F.SilkS))
    (fp_text value R_1k_0402 (at 0 0.374999 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 135) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 279 /ethernet/ETH_LED2))
    (pad 1 smd roundrect (at -0.51 0 135) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 262 ETH_nLED1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ecp5-dc-scm:QFN-48-Microchip-QFN77-48LD-PL-2 (layer F.Cu) (tedit 600030D3)
    (at 100.01 99.21 90)
    (fp_text reference U4 (at -4.28 -4.14 180) (layer F.SilkS))
    (fp_text value KSZ9031RNXCA (at 1.97 2.67 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.427149 -2.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask)
      (net 266 "Net-(C109-Pad1)"))
    (pad 2 smd roundrect (at -3.427149 -2.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 126 ETH_0P))
    (pad 3 smd roundrect (at -3.427149 -1.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 128 ETH_0N))
    (pad 4 smd roundrect (at -3.427149 -1.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 267 /ethernet/AVDDL))
    (pad 5 smd roundrect (at -3.427149 -0.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 132 ETH_1P))
    (pad 6 smd roundrect (at -3.427149 -0.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 130 ETH_1N))
    (pad 7 smd roundrect (at -3.427149 0.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 127 ETH_2P))
    (pad 8 smd roundrect (at -3.427149 0.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 129 ETH_2N))
    (pad 9 smd roundrect (at -3.427149 1.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 267 /ethernet/AVDDL))
    (pad 10 smd roundrect (at -3.427149 1.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 133 ETH_3P))
    (pad 11 smd roundrect (at -3.427149 2.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 131 ETH_3N))
    (pad 12 smd roundrect (at -3.427149 2.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 266 "Net-(C109-Pad1)"))
    (pad 25 smd roundrect (at 3.427149 2.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 281 RGMII_TX_EN))
    (pad 26 smd roundrect (at 3.427149 2.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 264 VCC1V2))
    (pad 27 smd roundrect (at 3.427149 1.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 272 RGMII_RXD3))
    (pad 28 smd roundrect (at 3.427149 1.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 271 RGMII_RXD2))
    (pad 29 smd roundrect (at 3.427149 0.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 1 GND))
    (pad 30 smd roundrect (at 3.427149 0.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 264 VCC1V2))
    (pad 31 smd roundrect (at 3.427149 -0.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 270 RGMII_RXD1))
    (pad 32 smd roundrect (at 3.427149 -0.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 269 RGMII_RXD0))
    (pad 33 smd roundrect (at 3.427149 -1.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 273 RGMII_RX_DV))
    (pad 34 smd roundrect (at 3.427149 -1.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 53 CM4_3.3V))
    (pad 35 smd roundrect (at 3.427149 -2.25 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 274 RGMII_RX_CLK))
    (pad 36 smd roundrect (at 3.427149 -2.75 90) (size 0.818176 0.242474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 282 ETH_MDC))
    (pad 13 smd roundrect (at -2.75 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
    (pad 14 smd roundrect (at -2.25 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 264 VCC1V2))
    (pad 15 smd roundrect (at -1.75 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 279 /ethernet/ETH_LED2))
    (pad 16 smd roundrect (at -1.25 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 53 CM4_3.3V))
    (pad 17 smd roundrect (at -0.75 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 278 /ethernet/ETH_LED1))
    (pad 18 smd roundrect (at -0.25 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 264 VCC1V2))
    (pad 19 smd roundrect (at 0.25 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 283 RGMII_TXD0))
    (pad 20 smd roundrect (at 0.75 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 284 RGMII_TXD1))
    (pad 21 smd roundrect (at 1.25 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 285 RGMII_TXD2))
    (pad 22 smd roundrect (at 1.75 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 286 RGMII_TXD3))
    (pad 23 smd roundrect (at 2.25 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 264 VCC1V2))
    (pad 24 smd roundrect (at 2.75 3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 287 RGMII_TX_CLK))
    (pad 37 smd roundrect (at 2.75 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 276 ETH_MDIO))
    (pad 38 smd roundrect (at 2.25 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 277 ETH_INT_N))
    (pad 39 smd roundrect (at 1.75 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 264 VCC1V2))
    (pad 40 smd roundrect (at 1.25 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 53 CM4_3.3V))
    (pad 41 smd roundrect (at 0.75 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 275 RGMII_REF_CLK))
    (pad 42 smd roundrect (at 0.25 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 265 ETH_~RESET))
    (pad 43 smd roundrect (at -0.25 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
    (pad 44 smd roundrect (at -0.75 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 268 /ethernet/AVDDL_PLL))
    (pad 45 smd roundrect (at -1.25 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
    (pad 46 smd roundrect (at -1.75 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 288 /ethernet/PHY_CLK))
    (pad 47 smd roundrect (at -2.25 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
    (pad 48 smd roundrect (at -2.75 -3.427149 90) (size 0.242474 0.818176) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 280 "Net-(R65-Pad2)"))
    (pad 49 smd rect (at 0 0 90) (size 3 3) (layers F.Cu F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ecp5-dc-scm:OSC_ASEM1-16.000MHZ-LC-T (layer B.Cu) (tedit 60115861)
    (at 97.12 101.42)
    (fp_text reference Y2 (at -1.9 -0.06 270) (layer B.SilkS))
    (fp_text value ASEMB-25.000MHZ-LC-T (at 0 -0.05) (layer B.Fab))
    (pad 4 smd rect (at 0.95 1.05) (size 1 0.9) (layers B.Cu B.Paste B.Mask)
      (net 53 CM4_3.3V))
    (pad 3 smd rect (at 0.95 -1.05) (size 1 0.9) (layers B.Cu B.Paste B.Mask)
      (net 288 /ethernet/PHY_CLK))
    (pad 2 smd rect (at -0.95 -1.05) (size 1 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 1.05) (size 1 0.9) (layers B.Cu B.Paste B.Mask)
      (net 53 CM4_3.3V))
    (model ${KIPRJMOD}/lib/3d-models/ASEMB.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_Abracon_ABM8G-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 143.92 98.52 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R68 (at 1.64 -0.04 270) (layer B.SilkS))
    (fp_text value R_10k_0402 (at 0.004999 -0.364999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 184 VCC1V35))
    (pad 2 smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 197 DDR3_VREF))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 144.96 98.53 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R69 (at -1.62 -0.01 270) (layer B.SilkS))
    (fp_text value R_10k_0402 (at 0.014999 -0.364999 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 197 DDR3_VREF))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module usb_otg:USB-MICRO-B-FCI-10118192-0001LF (layer F.Cu) (tedit 60C67F9F)
    (at 108.02 74.44 180)
    (attr smd)
    (fp_text reference P1 (at -4.03 -4.08 180) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -0.6) (layer F.Fab))
    (pad 6 smd rect (at -3.1 -2.55 180) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.127))
    (pad 6 smd rect (at 3.1 -2.55 180) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.127))
    (pad 6 smd rect (at -1.2 0 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.127))
    (pad 6 smd rect (at 1.2 0 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.127))
    (pad 1 smd rect (at -1.3 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -0.65 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 USB_N))
    (pad 3 smd rect (at 0 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 55 USB_P))
    (pad 4 smd rect (at 0.65 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 134 US2_ID))
    (pad 5 smd rect (at 1.3 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.8 0 180) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.127))
    (pad 6 smd rect (at 3.8 0 180) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.127))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (offset (xyz 0 1.27 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 100.57 74.97 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RV2 (at 2 0.01 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 2V5_3V3))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +2V5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 102.12 74.96 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RV3 (at -1.98 0.01 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 2V5_3V3))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 CM4_3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ecp5-dc-scm:Testpoint_smd_1mm (layer B.Cu) (tedit 5E4A935B)
    (at 117.07 90.17)
    (attr virtual)
    (fp_text reference TP_E9 (at 1.76 -0.01) (layer B.SilkS))
    (fp_text value E9 (at 0 0.07) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0.0508) (size 1 1) (layers B.Cu B.Mask)
      (net 292 "Net-(TP_E9-Pad1)"))
  )
  (module ecp5-dc-scm:Testpoint_smd_1mm (layer F.Cu) (tedit 5E4A935B)
    (at 143.74 96.37)
    (attr virtual)
    (fp_text reference TP_1V35 (at -0.08 1.0192) (layer F.SilkS))
    (fp_text value 1V35 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 -0.0508) (size 1 1) (layers F.Cu F.Mask)
      (net 184 VCC1V35))
  )
  (module ecp5-dc-scm:Testpoint_smd_1mm (layer B.Cu) (tedit 5E4A935B)
    (at 120.4 88.9992)
    (attr virtual)
    (fp_text reference TP_C16 (at -1.36 -1.3892 135) (layer B.SilkS))
    (fp_text value C16 (at 0 0.5) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0.0508) (size 1 1) (layers B.Cu B.Mask)
      (net 295 "Net-(TP_C16-Pad1)"))
  )
  (module ecp5-dc-scm:Testpoint_smd_1mm (layer B.Cu) (tedit 5E4A935B)
    (at 122.01 89.0692)
    (attr virtual)
    (fp_text reference TP_D16 (at 1.53 -1.2292 45) (layer B.SilkS))
    (fp_text value D16 (at 0 0.5) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0.0508) (size 1 1) (layers B.Cu B.Mask)
      (net 296 "Net-(TP_D16-Pad1)"))
  )
  (gr_text GoJimmyPi (at 122.34 104.07) (layer F.SilkS))
  (gr_text RX (at 146.4 104.9 -90) (layer F.SilkS))
  (gr_text TX (at 146.4 99.71 -90) (layer F.SilkS))
  (gr_text "Tuned (mm)\n---------\nDDR3 - 35\nPCIe - 65\nGPDI0 - 20\nGPDI1 - 20\nCSI0 - 32\nCSI1 - 20\nS5,S7 - 100" (at 125.47 92.78) (layer B.SilkS))
  (gr_text "<<close for 1.2V" (at 142.68 105.9) (layer F.SilkS))
  (gr_text Ethernet (at 99.83 94.52) (layer F.SilkS))
  (gr_text 3.3V (at 136.49 78.4) (layer B.SilkS))
  (gr_text 1.35V (at 148.02 93.83 270) (layer B.SilkS))
  (gr_text GPDI0 (at 129.85 72.9) (layer B.SilkS))
  (gr_text DISP1 (at 131.81 77.45) (layer B.SilkS))
  (gr_text DISP0 (at 128 77.46) (layer B.SilkS))
  (gr_text GPDI1 (at 124.56 72.89) (layer B.SilkS))
  (gr_text CAM0 (at 120.98 72.89) (layer B.SilkS))
  (gr_text CAM1 (at 118.04 77.44) (layer B.SilkS))
  (gr_text USB (at 114.68 77.44) (layer B.SilkS))
  (gr_arc (start 146.209997 109.144996) (end 146.209999 112.144998) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 146.209993 75.145007) (end 149.21 75.145) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 97.099999 109.144999) (end 94.1 109.144999) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 97.100004 75.144996) (end 97.1 72.144992) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_text SERDES (at 123.59 106.74) (layer B.SilkS))
  (gr_text SERDES (at 116.54 106.74) (layer B.SilkS))
  (gr_text PCIe (at 117.14 72.88) (layer B.SilkS))
  (gr_text 25MHz (at 103.91 88.56 90) (layer F.SilkS))
  (gr_line (start 149.209999 109.144994) (end 149.21 75.145) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.1 109.144999) (end 94.1 75.145) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97.099999 112.144998) (end 146.209999 112.144998) (layer Edge.Cuts) (width 0.1))
  (dimension 40 (width 0.15) (layer Dwgs.User)
    (gr_text "40,000 mm" (at 88.73 92.15 90) (layer Dwgs.User))
    (feature1 (pts (xy 97.42 72.15) (xy 89.443579 72.15)))
    (feature2 (pts (xy 97.42 112.15) (xy 89.443579 112.15)))
    (crossbar (pts (xy 90.03 112.15) (xy 90.03 72.15)))
    (arrow1a (pts (xy 90.03 72.15) (xy 90.616421 73.276504)))
    (arrow1b (pts (xy 90.03 72.15) (xy 89.443579 73.276504)))
    (arrow2a (pts (xy 90.03 112.15) (xy 90.616421 111.023496)))
    (arrow2b (pts (xy 90.03 112.15) (xy 89.443579 111.023496)))
  )
  (dimension 55.000004 (width 0.15) (layer Dwgs.User)
    (gr_text "55,000 mm" (at 121.596963 117.469999 -0.0208348) (layer Dwgs.User))
    (feature1 (pts (xy 94.1 109.11) (xy 94.097223 116.746421)))
    (feature2 (pts (xy 149.1 109.13) (xy 149.097223 116.76642)))
    (crossbar (pts (xy 149.097436 116.18) (xy 94.097436 116.160001)))
    (arrow1a (pts (xy 94.097436 116.160001) (xy 95.224153 115.573989)))
    (arrow1b (pts (xy 94.097436 116.160001) (xy 95.223726 116.74683)))
    (arrow2a (pts (xy 149.097436 116.18) (xy 147.971146 115.59317)))
    (arrow2b (pts (xy 149.097436 116.18) (xy 147.970719 116.766011)))
  )
  (gr_text FLASH (at 114.57 110.89) (layer F.SilkS))
  (gr_text 1.1V (at 144.38 104.45 -90) (layer B.SilkS))
  (gr_text 2.5V (at 95.35 80.92 270) (layer B.SilkS))
  (gr_text "02.02.2022. v0.0.1" (at 135.79 111.04) (layer F.SilkS))
  (gr_text +2.5V (at 112.134999 87.125) (layer B.SilkS))
  (gr_text +3.3V (at 111.135 91.075) (layer B.SilkS))
  (gr_text +1.1V (at 110.635 95.75) (layer B.SilkS))
  (gr_text ULX4M-LD (at 138.76 104.42) (layer F.SilkS))
  (gr_text FPGA (at 116.93 84.55) (layer F.SilkS))
  (gr_text DDR3 (at 131.1 87.4 90) (layer F.SilkS))
  (gr_line (start 97.1 72.144992) (end 146.209986 72.145) (layer Edge.Cuts) (width 0.1))
  (zone (net 4) (net_name +2V5) (layer POWER.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.61 97.05) (xy 117.01 97.049999) (xy 117.05 99.87) (xy 116.75 100.49) (xy 114.93 102.37)
        (xy 113.43 103.875) (xy 113.36 103.875) (xy 107.784999 103.875)
      )
    )
  )
  (zone (net 264) (net_name VCC1V2) (layer POWER.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.359425 100.409991) (xy 114.09 103.7) (xy 114.62 104.12) (xy 126.659801 103.875) (xy 119.81 97.049999)
        (xy 119.81 91.65) (xy 114.61 91.65) (xy 114.61 96.85) (xy 117.41 96.85)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.336023 112.14) (xy 149.23 72.2) (xy 94.1 72.16) (xy 94.08 112.19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.557 98.079) (xy 119.16 98.079) (xy 119.160001 98.841) (xy 120.557 98.841)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.22 86.24) (xy 137.219998 84.335001) (xy 137.981997 84.334999) (xy 137.981999 86.24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.249 90.603) (xy 122.36 90.603) (xy 122.487 91.492) (xy 123.249 91.492)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.184 90.603) (xy 112.073 90.603) (xy 112.073 91.492) (xy 111.184 91.492)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.184 88.19) (xy 112.073 88.19) (xy 112.073 89.079) (xy 111.184 89.079)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.325 77.105) (xy 104.925 77.105) (xy 104.925 77.62725) (xy 104.325 77.627251)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.332125 76.105) (xy 104.917875 76.105) (xy 104.917875 75.605) (xy 104.332125 75.605)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.629 86.412) (xy 116.645001 86.412) (xy 116.645 87.428) (xy 115.629001 87.428)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.010001 76.86) (xy 101.810001 76.86) (xy 101.810001 75.66) (xy 103.01 75.66)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.9905 84.63) (xy 139.979077 82.832) (xy 138.328078 82.832) (xy 138.3395 84.63)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.370001 86.324) (xy 103.37 84.419) (xy 104.132 84.418999) (xy 104.132 86.324)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.419999 100.291) (xy 136.42 102.196) (xy 135.658 102.196001) (xy 135.658 100.291001)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.975 103.0405) (xy 139.773 103.029077) (xy 139.773 101.378077) (xy 137.975 101.3895)
      )
    )
  )
  (zone (net 35) (net_name 2V5_3V3) (layer POWER.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.126)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.409999 94.05) (xy 114.41 91.45) (xy 117.01 91.449999) (xy 117.010001 83.05) (xy 106.01 83.05)
        (xy 106.01 94.050001)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.32 112.14) (xy 149.2 72.206307) (xy 94.104744 72.274671) (xy 94.135256 112.06533)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer POWER.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.23 72.2) (xy 149.2 96.62) (xy 144.88 96.62) (xy 144.92 93.61) (xy 142.6025 93.7075)
        (xy 142.5775 93.4325) (xy 142.39 91.73) (xy 143.32 91.05) (xy 143.32 88.01) (xy 145.09 87.9)
        (xy 145.18 83.38) (xy 133.955 72.315)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer POWER.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.22 112.16) (xy 94.09 112.16) (xy 94.08 106.22) (xy 94.08 102.63) (xy 95.07 103.11)
        (xy 97.965 106.105051) (xy 100.01 106.24) (xy 100.324998 107.548312) (xy 102.935002 109.551689) (xy 109.8 109.58)
        (xy 111.77 107.6) (xy 112.339986 104.251958) (xy 125.5 104.23) (xy 133.15 104.2) (xy 136.260509 93.92)
        (xy 149.259491 93.92)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.019 90.234999) (xy 142.114 90.234999) (xy 142.113999 89.473) (xy 144.019 89.472999)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.269499 91.79) (xy 141.280923 93.588) (xy 142.931922 93.588) (xy 142.9205 91.79)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.52 90.91) (xy 125.725 104.19) (xy 125.955 79.18) (xy 138.45 79.21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.517 102.922) (xy 125.916 102.921999) (xy 125.916 85.523001) (xy 108.517 85.523)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.45 79.506834) (xy 99.95 79.457581) (xy 99.95 72.202419) (xy 114.45 72.213167)
      )
    )
  )
  (zone (net 53) (net_name CM4_3.3V) (layer POWER.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.126)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.0525 81.89125) (xy 94.1025 98.65625) (xy 94.097369 102.419982) (xy 94.87 102.42) (xy 98.69 106)
        (xy 99.520016 105.963108) (xy 100.34 106.02) (xy 100.4 106.8) (xy 100.91 107.36) (xy 103.13 109.27)
        (xy 109.325617 109.241678) (xy 112.22 104.17) (xy 107.290423 104.09) (xy 107.31 103.3) (xy 114.1925 96.941249)
        (xy 114.1925 94.34125) (xy 105.3925 94.34125) (xy 105.3925 82.34125) (xy 117.3925 82.34125) (xy 117.3925 91.34125)
        (xy 119.9925 91.34125) (xy 119.992499 96.74125) (xy 127.1325 103.91125) (xy 132.84 103.81) (xy 136.105 93.74)
        (xy 142.12 93.74) (xy 142.12 91.38) (xy 142.984397 90.95903) (xy 142.9 87.72) (xy 144.39 87.73)
        (xy 144.74 87.45) (xy 144.7 83.355841) (xy 133.293224 72.223777) (xy 94.12 72.14)
      )
    )
  )
)
