(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 94)
    (tracks 1368)
    (zones 0)
    (modules 279)
    (nets 144)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.25)
    (user_trace_width 0.28)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (user_trace_width 1.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 221 90)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(U2-Pad1)")
  (net 3 "Net-(U2-Pad5)")
  (net 4 "Net-(C10-Pad1)")
  (net 5 "Net-(U2-Pad8)")
  (net 6 "Net-(C2-Pad2)")
  (net 7 "Net-(J14-Pad1)")
  (net 8 "Net-(J17-Pad1)")
  (net 9 "Net-(J13-Pad1)")
  (net 10 "Net-(C3-Pad1)")
  (net 11 "Net-(C4-Pad2)")
  (net 12 "Net-(C10-Pad2)")
  (net 13 "Net-(C23-Pad1)")
  (net 14 "Net-(C22-Pad1)")
  (net 15 "Net-(C22-Pad2)")
  (net 16 "Net-(C37-Pad2)")
  (net 17 "Net-(C38-Pad1)")
  (net 18 "Net-(C40-Pad2)")
  (net 19 "Net-(C43-Pad2)")
  (net 20 "Net-(C45-Pad1)")
  (net 21 "Net-(C45-Pad2)")
  (net 22 "Net-(C46-Pad2)")
  (net 23 "Net-(C46-Pad1)")
  (net 24 "Net-(C47-Pad2)")
  (net 25 "Net-(C50-Pad1)")
  (net 26 "Net-(JP1-Pad2)")
  (net 27 "Net-(JP3-Pad2)")
  (net 28 "Net-(JP4-Pad2)")
  (net 29 "Net-(JP6-Pad2)")
  (net 30 "Net-(R39-Pad1)")
  (net 31 RtoL)
  (net 32 LtoR)
  (net 33 "Net-(C1-Pad1)")
  (net 34 "Net-(C3-Pad2)")
  (net 35 "Net-(C4-Pad1)")
  (net 36 "Net-(C5-Pad2)")
  (net 37 "Net-(C5-Pad1)")
  (net 38 "Net-(C6-Pad2)")
  (net 39 "Net-(C6-Pad1)")
  (net 40 "Net-(C16-Pad1)")
  (net 41 "Net-(C11-Pad1)")
  (net 42 "Net-(C17-Pad1)")
  (net 43 "Net-(C19-Pad1)")
  (net 44 "Net-(C21-Pad2)")
  (net 45 "Net-(C21-Pad1)")
  (net 46 "Net-(C24-Pad1)")
  (net 47 "Net-(C25-Pad1)")
  (net 48 "Net-(C26-Pad1)")
  (net 49 "Net-(C37-Pad1)")
  (net 50 "Net-(C38-Pad2)")
  (net 51 "Net-(C39-Pad1)")
  (net 52 "Net-(C44-Pad2)")
  (net 53 "Net-(C48-Pad2)")
  (net 54 "Net-(C49-Pad1)")
  (net 55 "Net-(C51-Pad2)")
  (net 56 "Net-(C51-Pad1)")
  (net 57 "Net-(C52-Pad2)")
  (net 58 "Net-(C52-Pad1)")
  (net 59 "Net-(C61-Pad2)")
  (net 60 "Net-(C61-Pad1)")
  (net 61 "Net-(C62-Pad1)")
  (net 62 "Net-(C62-Pad2)")
  (net 63 "Net-(C63-Pad1)")
  (net 64 "Net-(C64-Pad2)")
  (net 65 "Net-(C66-Pad1)")
  (net 66 "Net-(C67-Pad2)")
  (net 67 "Net-(J11-Pad1)")
  (net 68 "Net-(J12-Pad1)")
  (net 69 "Net-(J17-Pad2)")
  (net 70 "Net-(J18-Pad3)")
  (net 71 "Net-(J19-Pad1)")
  (net 72 "Net-(J21-Pad3)")
  (net 73 "Net-(J26-Pad1)")
  (net 74 "Net-(J26-Pad3)")
  (net 75 "Net-(J31-Pad1)")
  (net 76 "Net-(J36-Pad1)")
  (net 77 "Net-(JP2-Pad2)")
  (net 78 "Net-(JP5-Pad2)")
  (net 79 "Net-(R11-Pad2)")
  (net 80 "Net-(R12-Pad2)")
  (net 81 "Net-(R13-Pad2)")
  (net 82 "Net-(R14-Pad2)")
  (net 83 "Net-(R27-Pad1)")
  (net 84 "Net-(R28-Pad1)")
  (net 85 "Net-(R40-Pad1)")
  (net 86 "Net-(R41-Pad1)")
  (net 87 "Net-(R42-Pad1)")
  (net 88 "Net-(R51-Pad1)")
  (net 89 "Net-(R52-Pad1)")
  (net 90 "Net-(R55-Pad1)")
  (net 91 "Net-(R56-Pad1)")
  (net 92 "Net-(R63-Pad2)")
  (net 93 "Net-(R65-Pad2)")
  (net 94 "Net-(R79-Pad1)")
  (net 95 "Net-(R80-Pad1)")
  (net 96 "Net-(U3-Pad8)")
  (net 97 "Net-(U3-Pad5)")
  (net 98 "Net-(U3-Pad1)")
  (net 99 "Net-(U5-Pad8)")
  (net 100 "Net-(U5-Pad5)")
  (net 101 "Net-(U5-Pad1)")
  (net 102 "Net-(U6-Pad8)")
  (net 103 "Net-(U6-Pad5)")
  (net 104 "Net-(U6-Pad1)")
  (net 105 "Net-(U7-Pad8)")
  (net 106 "Net-(U7-Pad5)")
  (net 107 "Net-(U7-Pad1)")
  (net 108 "Net-(U8-Pad8)")
  (net 109 "Net-(U8-Pad5)")
  (net 110 "Net-(U8-Pad1)")
  (net 111 "Net-(C27-Pad2)")
  (net 112 "Net-(C30-Pad2)")
  (net 113 "Net-(J41-Pad1)")
  (net 114 "Net-(J43-Pad1)")
  (net 115 "Net-(J17-Pad3)")
  (net 116 "Net-(J18-Pad1)")
  (net 117 "Net-(J21-Pad2)")
  (net 118 "Net-(J21-Pad1)")
  (net 119 "Net-(J24-Pad1)")
  (net 120 "Net-(J25-Pad1)")
  (net 121 "Net-(C75-Pad1)")
  (net 122 "Net-(D5-Pad2)")
  (net 123 "Net-(D5-Pad1)")
  (net 124 "Net-(D6-Pad2)")
  (net 125 "Net-(J47-Pad1)")
  (net 126 "Net-(J48-Pad1)")
  (net 127 "Net-(Q1-Pad2)")
  (net 128 "Net-(Q1-Pad1)")
  (net 129 "Net-(Q4-Pad1)")
  (net 130 "Net-(Q4-Pad2)")
  (net 131 "Net-(J28-Pad1)")
  (net 132 "Net-(J39-Pad1)")
  (net 133 "Net-(J40-Pad1)")
  (net 134 "Net-(R104-Pad2)")
  (net 135 "Net-(R113-Pad2)")
  (net 136 "Net-(J27-Pad1)")
  (net 137 "Net-(J38-Pad1)")
  (net 138 "Net-(K1-Pad9)")
  (net 139 "Net-(K2-Pad4)")
  (net 140 "Net-(J10-Pad2)")
  (net 141 "Net-(J10-Pad1)")
  (net 142 "Net-(D7-Pad1)")
  (net 143 "Net-(D7-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class SMD ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class grounds ""
    (clearance 0.254)
    (trace_width 1)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
  )
  (net_class power ""
    (clearance 0.254)
    (trace_width 1)
    (via_dia 0.762)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class signal ""
    (clearance 0.2)
    (trace_width 0.6096)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net GND)
    (add_net LtoR)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C27-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C30-Pad2)")
    (add_net "Net-(C37-Pad1)")
    (add_net "Net-(C37-Pad2)")
    (add_net "Net-(C38-Pad1)")
    (add_net "Net-(C38-Pad2)")
    (add_net "Net-(C39-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C40-Pad2)")
    (add_net "Net-(C43-Pad2)")
    (add_net "Net-(C44-Pad2)")
    (add_net "Net-(C45-Pad1)")
    (add_net "Net-(C45-Pad2)")
    (add_net "Net-(C46-Pad1)")
    (add_net "Net-(C46-Pad2)")
    (add_net "Net-(C47-Pad2)")
    (add_net "Net-(C48-Pad2)")
    (add_net "Net-(C49-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C50-Pad1)")
    (add_net "Net-(C51-Pad1)")
    (add_net "Net-(C51-Pad2)")
    (add_net "Net-(C52-Pad1)")
    (add_net "Net-(C52-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C61-Pad1)")
    (add_net "Net-(C61-Pad2)")
    (add_net "Net-(C62-Pad1)")
    (add_net "Net-(C62-Pad2)")
    (add_net "Net-(C63-Pad1)")
    (add_net "Net-(C64-Pad2)")
    (add_net "Net-(C66-Pad1)")
    (add_net "Net-(C67-Pad2)")
    (add_net "Net-(C75-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J17-Pad1)")
    (add_net "Net-(J17-Pad2)")
    (add_net "Net-(J17-Pad3)")
    (add_net "Net-(J18-Pad1)")
    (add_net "Net-(J18-Pad3)")
    (add_net "Net-(J19-Pad1)")
    (add_net "Net-(J21-Pad1)")
    (add_net "Net-(J21-Pad2)")
    (add_net "Net-(J21-Pad3)")
    (add_net "Net-(J24-Pad1)")
    (add_net "Net-(J25-Pad1)")
    (add_net "Net-(J26-Pad1)")
    (add_net "Net-(J26-Pad3)")
    (add_net "Net-(J27-Pad1)")
    (add_net "Net-(J28-Pad1)")
    (add_net "Net-(J31-Pad1)")
    (add_net "Net-(J36-Pad1)")
    (add_net "Net-(J38-Pad1)")
    (add_net "Net-(J39-Pad1)")
    (add_net "Net-(J40-Pad1)")
    (add_net "Net-(J41-Pad1)")
    (add_net "Net-(J43-Pad1)")
    (add_net "Net-(J47-Pad1)")
    (add_net "Net-(J48-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(JP4-Pad2)")
    (add_net "Net-(JP5-Pad2)")
    (add_net "Net-(JP6-Pad2)")
    (add_net "Net-(K1-Pad9)")
    (add_net "Net-(K2-Pad4)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(R104-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R113-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R27-Pad1)")
    (add_net "Net-(R28-Pad1)")
    (add_net "Net-(R39-Pad1)")
    (add_net "Net-(R40-Pad1)")
    (add_net "Net-(R41-Pad1)")
    (add_net "Net-(R42-Pad1)")
    (add_net "Net-(R51-Pad1)")
    (add_net "Net-(R52-Pad1)")
    (add_net "Net-(R55-Pad1)")
    (add_net "Net-(R56-Pad1)")
    (add_net "Net-(R63-Pad2)")
    (add_net "Net-(R65-Pad2)")
    (add_net "Net-(R79-Pad1)")
    (add_net "Net-(R80-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U6-Pad1)")
    (add_net "Net-(U6-Pad5)")
    (add_net "Net-(U6-Pad8)")
    (add_net "Net-(U7-Pad1)")
    (add_net "Net-(U7-Pad5)")
    (add_net "Net-(U7-Pad8)")
    (add_net "Net-(U8-Pad1)")
    (add_net "Net-(U8-Pad5)")
    (add_net "Net-(U8-Pad8)")
    (add_net RtoL)
  )
  (net_class soic ""
    (clearance 0.1524)
    (trace_width 0.4)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 176.6 100.4 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R84 (at 12.7 0) (layer F.SilkS))
    (fp_text value 5k11 (at 5.2 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(C62-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Wide (layer F.Cu) (tedit 5A2795B7)
    (at 209.5 55.75 180)
    (descr "TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 5 -2.75) (layer F.SilkS))
    (fp_text value 2N4403 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 -2.54 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 142 "Net-(D7-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Disc_Vishay_100p (layer F.Cu) (tedit 5D533F69)
    (at 140.14 72.12 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (fp_text reference C51 (at -2.05 0 180) (layer F.SilkS))
    (fp_text value 100pF (at 2.52 -0.04 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(C51-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C51-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C320C104K5G5TA.step
      (offset (xyz 5.3 1.6 0))
      (scale (xyz 1.1 0.8 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 129.2 107.2)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C58 (at 2.4 3.5) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(C48-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C50-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC (layer F.Cu) (tedit 5F80C5DD)
    (at 109.87 93.79 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U9 (at 3.69 4.03 90) (layer F.SilkS))
    (fp_text value TL052 (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user 1 (at 5.71 -0.44 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (fp_text user 595-TL052ACP (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 5.715 6.535) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C40-Pad2)"))
    (pad 7 smd roundrect (at 4.445 6.535) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(C37-Pad1)"))
    (pad 6 smd roundrect (at 3.175 6.535) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(R40-Pad1)"))
    (pad 5 smd roundrect (at 1.905 6.535) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R41-Pad1)"))
    (pad 4 smd roundrect (at 1.905 1.085) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(C39-Pad1)"))
    (pad 3 smd roundrect (at 3.175 1.085) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R42-Pad1)"))
    (pad 2 smd roundrect (at 4.445 1.085) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R39-Pad1)"))
    (pad 1 smd roundrect (at 5.715 1.085) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C38-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C40-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(C39-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(C37-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(R42-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(R40-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R39-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "Net-(R41-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C38-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC (layer F.Cu) (tedit 5F80C5DD)
    (at 175.17 58.51 270)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U12 (at 3.49 3.92 90) (layer F.SilkS))
    (fp_text value OPA1656 (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user 1 (at 5.71 -0.44 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 8 smd roundrect (at 5.715 6.535 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C63-Pad1)"))
    (pad 7 smd roundrect (at 4.445 6.535 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C61-Pad2)"))
    (pad 6 smd roundrect (at 3.175 6.535 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C61-Pad1)"))
    (pad 5 smd roundrect (at 1.905 6.535 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 120 "Net-(J25-Pad1)"))
    (pad 4 smd roundrect (at 1.905 1.085 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C64-Pad2)"))
    (pad 3 smd roundrect (at 3.175 1.085 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(J17-Pad2)"))
    (pad 2 smd roundrect (at 4.445 1.085 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 "Net-(R104-Pad2)"))
    (pad 1 smd roundrect (at 5.715 1.085 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 "Net-(R79-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(C63-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(C64-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(C61-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(J17-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(C61-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "Net-(R104-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 "Net-(J25-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "Net-(R79-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC (layer F.Cu) (tedit 5F80C5DD)
    (at 167.52 121.52 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U13 (at 3.52 3.98 90) (layer F.SilkS))
    (fp_text value OPA1656 (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user 1 (at 5.71 -0.44 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 8 smd roundrect (at 5.715 6.535) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C66-Pad1)"))
    (pad 7 smd roundrect (at 4.445 6.535) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C62-Pad2)"))
    (pad 6 smd roundrect (at 3.175 6.535) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C62-Pad1)"))
    (pad 5 smd roundrect (at 1.905 6.535) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 "Net-(J24-Pad1)"))
    (pad 4 smd roundrect (at 1.905 1.085) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C67-Pad2)"))
    (pad 3 smd roundrect (at 3.175 1.085) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 117 "Net-(J21-Pad2)"))
    (pad 2 smd roundrect (at 4.445 1.085) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 135 "Net-(R113-Pad2)"))
    (pad 1 smd roundrect (at 5.715 1.085) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 "Net-(R80-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(C66-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(C67-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(C62-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "Net-(J21-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(C62-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(R113-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "Net-(J24-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "Net-(R80-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC (layer F.Cu) (tedit 5F80C5DD)
    (at 127.89 58.87)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U10 (at 3.71 4.03) (layer F.SilkS))
    (fp_text value OPA1656 (at 3.81 9.95) (layer F.Fab))
    (fp_text user 1 (at 5.71 -0.44 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 8 smd roundrect (at 5.715 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C47-Pad2)"))
    (pad 7 smd roundrect (at 4.445 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(C51-Pad2)"))
    (pad 6 smd roundrect (at 3.175 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(C51-Pad1)"))
    (pad 5 smd roundrect (at 1.905 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(R51-Pad1)"))
    (pad 4 smd roundrect (at 1.905 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(C49-Pad1)"))
    (pad 3 smd roundrect (at 3.175 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C43-Pad2)"))
    (pad 2 smd roundrect (at 4.445 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C45-Pad1)"))
    (pad 1 smd roundrect (at 5.715 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C45-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C47-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(C49-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(C51-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C43-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C51-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C45-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(R51-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C45-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC (layer F.Cu) (tedit 5F80C5DD)
    (at 127.9 113.48)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U11 (at 3.7 4.02) (layer F.SilkS))
    (fp_text value OPA1656 (at 3.81 9.95) (layer F.Fab))
    (fp_text user 1 (at 5.71 -0.44 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 8 smd roundrect (at 5.715 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(C48-Pad2)"))
    (pad 7 smd roundrect (at 4.445 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(C52-Pad2)"))
    (pad 6 smd roundrect (at 3.175 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(C52-Pad1)"))
    (pad 5 smd roundrect (at 1.905 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(R52-Pad1)"))
    (pad 4 smd roundrect (at 1.905 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(C50-Pad1)"))
    (pad 3 smd roundrect (at 3.175 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(C44-Pad2)"))
    (pad 2 smd roundrect (at 4.445 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C46-Pad1)"))
    (pad 1 smd roundrect (at 5.715 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C46-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(C48-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C50-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(C52-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(C44-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(C52-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C46-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "Net-(R52-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C46-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC-Single (layer F.Cu) (tedit 5F85D809)
    (at 87.82 106.01)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U8 (at 3.78 3.89) (layer F.SilkS))
    (fp_text value OPA1611 (at 3.81 9.95) (layer F.Fab))
    (fp_text user 1 (at 5.71 -0.44 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad "" smd roundrect (at 5.715 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 4.445 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(C25-Pad1)"))
    (pad 6 smd roundrect (at 3.175 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 "Net-(C27-Pad2)"))
    (pad "" smd roundrect (at 1.905 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at 1.905 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(C26-Pad1)"))
    (pad 3 smd roundrect (at 3.175 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(C19-Pad1)"))
    (pad 2 smd roundrect (at 4.445 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C22-Pad1)"))
    (pad "" smd roundrect (at 5.715 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "Net-(U8-Pad8)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(C26-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(C25-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(C19-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(C27-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C22-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 "Net-(U8-Pad5)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(U8-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC-Single (layer F.Cu) (tedit 5F85D809)
    (at 87.83 66.52)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U7 (at 3.77 3.98) (layer F.SilkS))
    (fp_text value OPA1611 (at 3.81 9.95) (layer F.Fab))
    (fp_text user 1 (at 5.71 -0.44 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad "" smd roundrect (at 5.715 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 4.445 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C23-Pad1)"))
    (pad 6 smd roundrect (at 3.175 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 "Net-(C30-Pad2)"))
    (pad "" smd roundrect (at 1.905 6.535 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at 1.905 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(C24-Pad1)"))
    (pad 3 smd roundrect (at 3.175 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(C17-Pad1)"))
    (pad 2 smd roundrect (at 4.445 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(C21-Pad1)"))
    (pad "" smd roundrect (at 5.715 1.085 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "Net-(U7-Pad8)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(C24-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C23-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(C17-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(C30-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(C21-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 "Net-(U7-Pad5)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "Net-(U7-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC-Lo (layer F.Cu) (tedit 5F85D75D)
    (at 58.19 66.42)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U3 (at 3.8 5.18) (layer F.SilkS))
    (fp_text value LT1115 (at 3.81 9.95) (layer F.Fab))
    (fp_text user 1 (at 5.71 0.8 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 4.81) (layer F.Fab))
    (pad "" smd roundrect (at 5.715 7.735 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 4.445 7.735 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(C16-Pad1)"))
    (pad 6 smd roundrect (at 3.175 7.735 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(R12-Pad2)"))
    (pad "" smd roundrect (at 1.905 7.735 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at 1.905 2.285 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(C11-Pad1)"))
    (pad 3 smd roundrect (at 3.175 2.285 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C2-Pad2)"))
    (pad 2 smd roundrect (at 4.445 2.285 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C3-Pad1)"))
    (pad "" smd roundrect (at 5.715 2.285 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 "Net-(U3-Pad8)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(C11-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(C16-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(R12-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C3-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 "Net-(U3-Pad5)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 "Net-(U3-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC-Lo (layer F.Cu) (tedit 5F85D75D)
    (at 58.19 120.42)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U5 (at 3.81 5.28) (layer F.SilkS))
    (fp_text value LT1115 (at 3.81 9.95) (layer F.Fab))
    (fp_text user 1 (at 5.71 0.8 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 4.81) (layer F.Fab))
    (pad "" smd roundrect (at 5.715 7.735 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 4.445 7.735 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)"))
    (pad 6 smd roundrect (at 3.175 7.735 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(R14-Pad2)"))
    (pad "" smd roundrect (at 1.905 7.735 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at 1.905 2.285 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C10-Pad2)"))
    (pad 3 smd roundrect (at 3.175 2.285 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 4.445 2.285 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(C6-Pad1)"))
    (pad "" smd roundrect (at 5.715 2.285 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 "Net-(U5-Pad8)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C1-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(R14-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(C6-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 "Net-(U5-Pad5)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 "Net-(U5-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC-Hi (layer F.Cu) (tedit 5F85D70F)
    (at 58.19 106.02)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U6 (at 3.81 2.88) (layer F.SilkS))
    (fp_text value LT1115 (at 3.81 9.95) (layer F.Fab))
    (fp_text user 1 (at 6.1 -1.1 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 2.81) (layer F.Fab))
    (pad "" smd roundrect (at 5.715 5.335 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 4.445 5.335 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)"))
    (pad 6 smd roundrect (at 3.175 5.335 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(R13-Pad2)"))
    (pad "" smd roundrect (at 1.905 5.335 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at 1.905 -0.115 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C10-Pad2)"))
    (pad 3 smd roundrect (at 3.175 -0.115 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 4.445 -0.115 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(C4-Pad1)"))
    (pad "" smd roundrect (at 5.715 -0.115 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "Net-(U6-Pad8)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C1-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(R13-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C4-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 "Net-(U6-Pad5)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "Net-(U6-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC-Hi (layer F.Cu) (tedit 5F85D70F)
    (at 58.19 52)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U2 (at 3.81 2.8) (layer F.SilkS))
    (fp_text value LT1115 (at 3.81 9.95) (layer F.Fab))
    (fp_text user 1 (at 6.1 -1.1 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 2.81) (layer F.Fab))
    (pad "" smd roundrect (at 5.715 5.335 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 4.445 5.335 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(C16-Pad1)"))
    (pad 6 smd roundrect (at 3.175 5.335 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(R11-Pad2)"))
    (pad "" smd roundrect (at 1.905 5.335 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at 1.905 -0.115 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(C11-Pad1)"))
    (pad 3 smd roundrect (at 3.175 -0.115 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C2-Pad2)"))
    (pad 2 smd roundrect (at 4.445 -0.115 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C5-Pad1)"))
    (pad "" smd roundrect (at 5.715 -0.115 270) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(U2-Pad8)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(C11-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(C16-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(R11-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C5-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(U2-Pad5)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(U2-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 114.2 98.4 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C39 (at 2.5 -3.6) (layer F.SilkS))
    (fp_text value 100n (at 2.4 0 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(C39-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 117.5 58.92 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R53 (at 6.38 2 90) (layer F.SilkS))
    (fp_text value 75k (at 5.2 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C45-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C45-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 131.7 137.9 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP5 (at 0 4.7) (layer F.SilkS) hide)
    (fp_text value 10dB (at -2.1 1.3 90) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(JP5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 149.7 53.4 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R73 (at -2.5 -0.1) (layer F.SilkS))
    (fp_text value 47 (at 5.08 -0.1) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(C51-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(J11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 150.2 123.6 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R72 (at 5 -2 90) (layer F.SilkS))
    (fp_text value 3k9 (at 5 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(C52-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(C52-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_Capacitors:C_Rect_L7.2mm_W3.5mm_P5.00mm_Kemet (layer F.Cu) (tedit 5F66BC51)
    (at 53.5 56.5 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.0mm Capacitor")
    (fp_text reference C5 (at 6.9 -0.05 180) (layer F.SilkS))
    (fp_text value 33n (at 2.525 0.1 180) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (fp_text user 80-PHE426DJ5330FR17T (at 0 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C5-Pad1)"))
    (model ${SMC_3D}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.5mm_P5.00mm_Kemet.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.2 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_Capacitors:C_Rect_L7.2mm_W3.5mm_P5.00mm_Kemet (layer F.Cu) (tedit 5F66BC51)
    (at 59.55 81.22)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.0mm Capacitor")
    (fp_text reference C3 (at 7.1 -0.14 90) (layer F.SilkS))
    (fp_text value 33n (at 2.6 0.06) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C3-Pad1)"))
    (model ${SMC_3D}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.5mm_P5.00mm_Kemet.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.2 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W4.5mm_P5.00mm_Wima (layer F.Cu) (tedit 5D533F69)
    (at 78.84 63.02)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (fp_text reference C17 (at 2.76 -3.22 180) (layer F.SilkS))
    (fp_text value 470p (at 2.73 0.01 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.7))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W4.5mm_P5.00mm_Wima (layer F.Cu) (tedit 5D533F69)
    (at 83.19 111.07 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (fp_text reference C19 (at 7.05 0.05 180) (layer F.SilkS))
    (fp_text value 470p (at 2.4 0.15) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.7))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W4.5mm_P5.00mm_Wima (layer F.Cu) (tedit 5D533F69)
    (at 167.5 75.3)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (fp_text reference C61 (at -2 -0.21 270) (layer F.SilkS))
    (fp_text value 100p (at 2.58 -0.01 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(C61-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(C61-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.7))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 69.24 62.92)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C16 (at 2.56 -3.42 180) (layer F.SilkS))
    (fp_text value 100n (at 2.5 -0.05 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(C16-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 64.45 44.02 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C9 (at -2.09 0.04 270) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0.04 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(C11-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(C16-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 53.5 60.5 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C11 (at 2.4 3.4 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(C11-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 100.25 67.5 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C23 (at 2.56 -3.5 270) (layer F.SilkS))
    (fp_text value 100n (at 2.56 0.08) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C23-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 93.5 60.1 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C33 (at 2.54 -3.48 180) (layer F.SilkS))
    (fp_text value 100n (at 2.4 0.02 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(C24-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C23-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 83.26 74.12 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C24 (at 7.02 -0.06 180) (layer F.SilkS))
    (fp_text value 100n (at 2.54 -0.04 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(C24-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 111.4 70 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C37 (at -2.3 -0.1 270) (layer F.SilkS))
    (fp_text value 100nF (at 2.55 -0.08 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C37-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(C37-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 114.25 81.5 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C40 (at 2.35 3.4 180) (layer F.SilkS))
    (fp_text value 100n (at 2.58 0.04 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C40-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 180.5 66.75 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C69 (at 2.75 -3.5 90) (layer F.SilkS))
    (fp_text value 100n (at 2.43 -0.11 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(C63-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 182.1 63.5 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C70 (at 2.5 -3.4 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0.01 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(C64-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(C63-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 168 55 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C71 (at 2.4 -3.4 270) (layer F.SilkS))
    (fp_text value 100n (at 2.82 0.31 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(C64-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 69.04 117.02)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C15 (at 2.56 -3.32) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0.1 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 64.49 136.07 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C10 (at -2.05 0 270) (layer F.SilkS))
    (fp_text value 100n (at 2.45 -0.1 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 53.5 114.5 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C12 (at 2.3 3.3 270) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 100.2 107.5 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C25 (at 2.5 -3.45 90) (layer F.SilkS))
    (fp_text value 100n (at 2.56 -0.02) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(C25-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 93.7 120.02 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C34 (at 2.55 3.3 180) (layer F.SilkS))
    (fp_text value 100n (at 2.55 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(C26-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(C25-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 84.69 117.02 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C26 (at 2.29 -3.58) (layer F.SilkS))
    (fp_text value 100n (at 2.45 0 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(C26-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 111.4 110 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C38 (at -2.1 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 2.64 0.02 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(C38-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C38-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 165.6 105.2 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C72 (at 6.9 -0.1 270) (layer F.SilkS))
    (fp_text value 100n (at 2.52 0.06 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(C66-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 182.1 115 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C73 (at -1.9 0) (layer F.SilkS))
    (fp_text value 100n (at 2.4 -0.1 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(C67-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(C66-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 181.69 123.62 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C74 (at 7.18 -0.11 180) (layer F.SilkS))
    (fp_text value 100n (at 2.5 -0.1 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(C67-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 68.14 86.62 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C20 (at -3.07 -2.47) (layer F.SilkS))
    (fp_text value 10u (at 1.77 0.03) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(C16-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 62.04 86.59 90)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C7 (at 2.29 -2.94 180) (layer F.SilkS))
    (fp_text value 10u (at -1.82 0.05 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(C16-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(C11-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 55.94 86.62 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C13 (at -2.62 3.14) (layer F.SilkS))
    (fp_text value 10u (at 1.79 -0.03 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(C11-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 97 79 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C29 (at 0.1 3.4 270) (layer F.SilkS))
    (fp_text value 10u (at 1.74 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C23-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 90.5 86 180)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C35 (at 0 3.5 180) (layer F.SilkS))
    (fp_text value 10u (at 1.72 0 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C23-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(C24-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 86.5 79 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C31 (at 0 -3.75 90) (layer F.SilkS))
    (fp_text value 10u (at 1.76 0.08 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(C24-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 131.54 86.5)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C42 (at 3.36 2.48 180) (layer F.SilkS))
    (fp_text value 10u (at -1.7 -0.2 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C40-Pad2)"))
    (pad 2 thru_hole circle (at 0 -1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 131.54 93.5)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C41 (at 3.56 -2.22) (layer F.SilkS))
    (fp_text value 10u (at -1.64 0.18 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(C39-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 160.6 69.6 180)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C63 (at 0 -3.6) (layer F.SilkS))
    (fp_text value 10u (at 1.95 -0.05 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(C63-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 160.6 63.52)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C64 (at 3.56 -0.12 270) (layer F.SilkS))
    (fp_text value 10u (at -1.7 0.1 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(C63-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(C64-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 160.6 57.3 180)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C65 (at -3.56 0.02 270) (layer F.SilkS))
    (fp_text value 10u (at 1.65 -0.1 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(C64-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 68.14 93.32 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C18 (at 3.38 -2.26 180) (layer F.SilkS))
    (fp_text value 10u (at -1.85 -0.05) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 62.04 93.32 90)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C8 (at -2.58 -2.94 180) (layer F.SilkS))
    (fp_text value 10u (at 1.9 0.15 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C10-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 55.94 93.32 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C14 (at 2.58 3.14 180) (layer F.SilkS))
    (fp_text value 10u (at -1.9 -0.05 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C10-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 97 101 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C28 (at 0 3.6 270) (layer F.SilkS))
    (fp_text value 10u (at -1.84 -0.02) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(C25-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 90.5 94)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C36 (at 0 3.5) (layer F.SilkS))
    (fp_text value 10u (at 1.82 -0.04 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(C25-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(C26-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 86.5 101 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C32 (at 0 -3.75 90) (layer F.SilkS))
    (fp_text value 10u (at -1.76 -0.08 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(C26-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 160.59 111.17)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C66 (at 3.61 0.03 270) (layer F.SilkS))
    (fp_text value 10u (at -1.84 0 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(C66-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 160.59 117.17 180)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C67 (at -3.71 0.07 270) (layer F.SilkS))
    (fp_text value 10u (at 1.84 -0.08 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(C66-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(C67-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 160.59 123.27)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C68 (at 3.61 -0.07 270) (layer F.SilkS))
    (fp_text value 10u (at -1.84 0 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(C67-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Disc_D8.5mm_W5.5mm_P7.50mm (layer F.Cu) (tedit 5D556843)
    (at 83.94 56.42 90)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=9*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 9mm width 5.0mm Capacitor")
    (fp_text reference C21 (at 9.25 -0.05) (layer F.SilkS))
    (fp_text value 10p (at 3.95 -0.05 180) (layer F.SilkS))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(C21-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D9.0mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Disc_D8.5mm_W5.5mm_P7.50mm (layer F.Cu) (tedit 5D556843)
    (at 83.94 124.32 270)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=9*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 9mm width 5.0mm Capacitor")
    (fp_text reference C22 (at 9.48 -0.06) (layer F.SilkS))
    (fp_text value 10p (at 3.75 -0.01 180) (layer F.SilkS))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(C22-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D9.0mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_Capacitors:C_Rect_L7.5mm_W5.5mm_P5.00mm_Vishay (layer F.Cu) (tedit 5D49A57C)
    (at 88.7 126.3)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.5*6.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.5mm width 6.5mm Capacitor")
    (fp_text reference C27 (at 2.5 3.7) (layer F.SilkS))
    (fp_text value 10n (at 2.5 0.1 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(C27-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C22-Pad2)"))
    (model ${SMC_3D}/Capacitor_THT.3dshapes/C_Rect_L7.5mm_W5.5mm_P5.00mm_Vishay.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_Capacitors:C_Rect_L7.5mm_W5.5mm_P5.00mm_Vishay (layer F.Cu) (tedit 5D49A57C)
    (at 88.55 53.7)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.5*6.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.5mm width 6.5mm Capacitor")
    (fp_text reference C30 (at 2.6 -3.6 180) (layer F.SilkS))
    (fp_text value 10n (at 2.65 -0.05 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(C30-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(C21-Pad2)"))
    (model ${SMC_3D}/Capacitor_THT.3dshapes/C_Rect_L7.5mm_W5.5mm_P5.00mm_Vishay.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:mkds_1,5-3 (layer F.Cu) (tedit 606A4C1F)
    (at 216 90 90)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J26 (at 0 -3.6 90) (layer F.Fab))
    (fp_text value Power (at 0.02 3.56 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2) (thermal_width 1.2))
    (pad 1 thru_hole circle (at -5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(J26-Pad1)"))
    (pad 3 thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(J26-Pad3)"))
    (model ${KIPRJMOD}/Lib/3D/pxc_1935174_03_PT-1-5-3-5-0-H_3D.stp
      (offset (xyz -30.09899954795837 -44.70399932861328 -38.86199941635132))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 90))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 40.54 68.77 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J4 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value IN (at -0.005 -2.74 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 40.54 63.52 270)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J5 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value gnd (at 0.05 2.3 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 143 45.1 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J11 (at 0 -2.148) (layer F.Fab))
    (fp_text value Warp (at 0 2.8 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 67 "Net-(J11-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 149.7 45.1 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J13 (at 0 -2.148) (layer F.Fab))
    (fp_text value Buffer (at 0 2.8 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(J13-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 187 45.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J19 (at 0 -2.148) (layer F.Fab))
    (fp_text value Top (at 0 2.575 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 71 "Net-(J19-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 180 45.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J25 (at 0 -2.148) (layer F.Fab))
    (fp_text value Wiper (at 0 2.575 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 120 "Net-(J25-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 216.54 72.52 270)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J31 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value Line (at -0.02 -2.66 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 75 "Net-(J31-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 216.54 78.52 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J32 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value gnd (at 0.02 2.66 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 216.54 58.52 270)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J28 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value Record (at -0.02 -2.66 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 131 "Net-(J28-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 216.54 52.52 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J29 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value gnd (at 0.02 2.66 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 40.54 111.27 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J1 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value IN (at 0.07 -2.74 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 "Net-(C1-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 40.54 116.52 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J2 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value gnd (at -0.08 -2.34 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 143 134.9)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J12 (at 0 -2.148) (layer F.Fab))
    (fp_text value Warp (at 0 2.9) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 68 "Net-(J12-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 149.7 134.9)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J14 (at 0 -2.148) (layer F.Fab))
    (fp_text value Buffer (at 0 2.9) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(J14-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 187 134.52 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J20 (at 0 -2.148) (layer F.Fab))
    (fp_text value Top (at -0.05 -2.65) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 141 "Net-(J10-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 180 134.52 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J24 (at 0 -2.148) (layer F.Fab))
    (fp_text value Wiper (at -0.05 -2.65) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 119 "Net-(J24-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 216.64 107.62 270)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J36 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value Line (at -0.34 -2.56 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 76 "Net-(J36-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 216.54 127.52 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J37 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value gnd (at 0.02 2.66 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 216.54 121.52 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J33 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value Record (at 0.02 2.66 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 140 "Net-(J10-Pad2)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 216.54 101.52 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J34 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value gnd (at 0 2.66 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 137.5 45.1 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J15 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 2.5 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 173 45.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J23 (at 0 -2.148) (layer F.Fab))
    (fp_text value Bottom (at 0 2.575 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 173 134.52 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J22 (at 0 -2.148) (layer F.Fab))
    (fp_text value Bottom (at -0.05 -2.65) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 137.5 134.9 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J16 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 -2.8) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 40.54 74.02 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J6 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value gnd (at 0 -2.3 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 40.5 106 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J3 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value gnd (at 0.02 -2.34 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:Oval_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56DE29)
    (at 216.54 66.77 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J30 (at -0.7 -2.3 90) (layer F.Fab))
    (fp_text value gnd (at 1.3 2.56 90) (layer F.SilkS))
    (fp_text user %R (at 3.65 -2.4 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 2.5 0 90) (size 5 2.5) (drill 1.2 (offset -1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0 90) (size 5 2.5) (drill 1.2 (offset 1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:Oval_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56DE29)
    (at 216.54 115.77 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J35 (at -0.7 -2.3 90) (layer F.Fab))
    (fp_text value gnd (at 1.3 2.66 90) (layer F.SilkS))
    (fp_text user %R (at 3.65 -2.4 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 2.5 0 90) (size 5 2.5) (drill 1.2 (offset -1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0 90) (size 5 2.5) (drill 1.2 (offset 1.25 0)) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 41 44.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (clearance 2)
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 60AFBFA6)
    (at 41 135.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (clearance 2)
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 198 44.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (clearance 2)
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 140.14 63.82 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C47 (at 6.95 -0.05 180) (layer F.SilkS))
    (fp_text value 100n (at 2.4 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C47-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 137.94 78.97 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C53 (at 0.03 -3.61 270) (layer F.SilkS))
    (fp_text value 10u (at -1.72 -0.06) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C47-Pad2)"))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 129.19 72.82)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C57 (at 2.6 -3.4) (layer F.SilkS))
    (fp_text value 100n (at 2.5 -0.02 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C47-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(C49-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 131.64 78.97 90)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C59 (at -3.53 -0.04 180) (layer F.SilkS))
    (fp_text value 10u (at 1.72 0.11) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C47-Pad2)"))
    (pad 2 thru_hole circle (at 0 -1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C49-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 123.24 67.22 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C49 (at 2.53 3.34 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0.1) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(C49-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 125.24 78.97 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C55 (at -0.04 3.63 90) (layer F.SilkS))
    (fp_text value 10u (at -1.72 -0.1) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C49-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 140.24 107.72 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C48 (at -2.02 0 180) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(C48-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 138.34 101.02 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C54 (at 0.03 -3.56 270) (layer F.SilkS))
    (fp_text value 10u (at -1.72 0.04) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(C48-Pad2)"))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 131.94 101.02 90)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C60 (at 3.52 0.06 180) (layer F.SilkS))
    (fp_text value 10u (at 1.77 0.06) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(C48-Pad2)"))
    (pad 2 thru_hole circle (at 0 -1 90) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C50-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 123.2 121.02 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C50 (at 2.7 -3.4 90) (layer F.SilkS))
    (fp_text value 100n (at 2.6 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C50-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 125.64 101.02 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C56 (at 0.1 3.5 90) (layer F.SilkS))
    (fp_text value 10u (at -1.77 -0.11) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C50-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 40.5 77.75 270)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 5.25 -2.25 270 unlocked) (layer F.SilkS))
    (fp_text value 1N4003 (at 5.08 2.47 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user %R (at 5.47 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 40.54 49.8 270)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D4 (at 5.2 -2.21 270 unlocked) (layer F.SilkS))
    (fp_text value 1N4003 (at 5.08 2.47 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user %R (at 5.47 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 40.54 102.25 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 5.12 2.21 270 unlocked) (layer F.SilkS))
    (fp_text value 1N4003 (at 5.08 2.47 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user %R (at 5.47 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 40.54 130.2 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D3 (at 5.2 2.21 270 unlocked) (layer F.SilkS))
    (fp_text value 1N4003 (at 5.08 2.47 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user %R (at 5.47 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 131.7 42.1)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0 4.9) (layer F.SilkS) hide)
    (fp_text value 10dB (at 2.2 1.1 90) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(JP3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 125.8 47.2 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 0 7.4) (layer F.SilkS) hide)
    (fp_text value "In | Out" (at -2.2 3 90) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(JP1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(C45-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 117.36 42.1 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP4 (at 0 -2.35 90) (layer F.SilkS) hide)
    (fp_text value 0dB (at -2 1.84 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(JP4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 125.8 132.8)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP2 (at 0 7.3) (layer F.SilkS) hide)
    (fp_text value "Out | In" (at 2.2 3.2 90) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(JP2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(C46-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 117.4 137.9 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value 0dB (at 2.1 2 180) (layer F.SilkS))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(JP6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5FA31278)
    (at 49.7 55 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.1 -2.3 90) (layer F.SilkS))
    (fp_text value 21R5 (at 5.1 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_width 1))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 148.5 83.72 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R67 (at 5.1 2) (layer F.SilkS))
    (fp_text value 10 (at 5.1 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C47-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J26-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 66.34 48.62 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 10.1 2.1 90) (layer F.SilkS))
    (fp_text value 2k26 (at 5.04 0.02) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 74.04 57.12 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R15 (at 5.12 2.16 90) (layer F.SilkS))
    (fp_text value 3k (at 5.06 -0.05 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 84.79 84.02 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R24 (at 5.05 2) (layer F.SilkS))
    (fp_text value 10 (at 5.05 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(C16-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 84.79 88.1 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R20 (at 5.05 2) (layer F.SilkS))
    (fp_text value 10 (at 4.95 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(C11-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(C24-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 78.34 69.02 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R21 (at 8.18 -2.16 270) (layer F.SilkS))
    (fp_text value 2k8 (at 4.89 0.04 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 78.34 46.92 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R25 (at 5.14 -2.13 90) (layer F.SilkS))
    (fp_text value 32k4 (at 5.13 -0.01 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(C21-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(C21-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 98.54 47.42 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R28 (at 4.99 2.07) (layer F.SilkS))
    (fp_text value 316k (at 4.94 -0.08) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(C21-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(R28-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 100.1 62.26 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R30 (at 5.86 2.2 270) (layer F.SilkS))
    (fp_text value 2k (at 5.095 0.01 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(R28-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(C30-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 106.04 84.02 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R35 (at 5.04 2.02) (layer F.SilkS))
    (fp_text value 10 (at 4.84 0.02) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C23-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J26-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 106.04 88.1 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R36 (at 4.94 2.02) (layer F.SilkS))
    (fp_text value 10 (at 4.74 0.02) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(C24-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(J26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 111.4 76 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R34 (at 4.65 -2.25) (layer F.SilkS))
    (fp_text value 240k (at 5 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(C17-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(C37-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 113.8 63.2 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R40 (at 5.1 -2.2) (layer F.SilkS))
    (fp_text value 33k (at 5.05 0.05) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C37-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(R40-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 103.64 58.77)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R44 (at 5.15 2.15) (layer F.SilkS))
    (fp_text value 1M (at 5.15 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(R40-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(C30-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 117.5 83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R41 (at 5 2 90) (layer F.SilkS))
    (fp_text value 1M (at 5.05 0.1 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "Net-(R41-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 113.8 54.2 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R45 (at 5.14 -2.18) (layer F.SilkS))
    (fp_text value 75k (at 5.14 -0.08) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 RtoL))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C43-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 176.54 88.02 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R37 (at 5.04 2.02) (layer F.SilkS))
    (fp_text value 10 (at 5.04 -0.08) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C40-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J26-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 149.7 50 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R75 (at -2.5 0) (layer F.SilkS))
    (fp_text value 56k (at 5 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 183.3 55.2 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R79 (at 4.9 2) (layer F.SilkS))
    (fp_text value 2k2 (at 5.04 0.07) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "Net-(R104-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "Net-(R79-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 187 50 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R81 (at 3.2 -2.1 90) (layer F.SilkS))
    (fp_text value 47 (at 5.04 -0.03 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "Net-(R79-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(J19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 176.6 79.8 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R83 (at 12.7 0) (layer F.SilkS))
    (fp_text value 5k11 (at 5.05 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(C61-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 175.6 70 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R85 (at 5.4 -2.2) (layer F.SilkS))
    (fp_text value 5k11 (at 5.1 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(C61-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(C61-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 185.75 75.25 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R88 (at 4.95 -2.15) (layer F.SilkS))
    (fp_text value 47 (at 4.9 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(C61-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 138 "Net-(K1-Pad9)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 176.5 84 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R87 (at 5.04 2.12) (layer F.SilkS))
    (fp_text value 10 (at 4.94 0.02) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(C63-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J26-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 161.75 95 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R89 (at 5.02 -2.15 90) (layer F.SilkS))
    (fp_text value 10 (at 5.12 -0.04 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(C64-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(J26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 125.49 84.92 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R49 (at 5.28 -2.2 90) (layer F.SilkS))
    (fp_text value 75k (at 5.3 -0.1 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 LtoR))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C45-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 150.09 66.52 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R59 (at 5.2 -2.09 90) (layer F.SilkS))
    (fp_text value 3k9 (at 5.1 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(JP3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C51-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 145.59 56.32 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R71 (at 5.18 2.09 90) (layer F.SilkS))
    (fp_text value 3k9 (at 5.1 0.05 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C51-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(C51-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 124.94 51.42)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R55 (at 5.16 -2.05) (layer F.SilkS))
    (fp_text value 3k9 (at 5.1 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(JP1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "Net-(R55-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 135.1 55.52 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R57 (at 5.1 1.98) (layer F.SilkS))
    (fp_text value 3k9 (at 5.1 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "Net-(R55-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C51-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 154.5 56.3 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R78 (at 5.1 2 90) (layer F.SilkS))
    (fp_text value 1k5 (at 5.15 0.05 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J13-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 "Net-(J17-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 69.69 46.92 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 5 -2.14 90) (layer F.SilkS))
    (fp_text value 75 (at 4.95 -0.04 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(R11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 121.3 56 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R60 (at 7.1 2.2 90) (layer F.SilkS))
    (fp_text value 3k9 (at 5.1 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(JP4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(R51-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 103.64 49.7)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R47 (at 5.1 2.18) (layer F.SilkS))
    (fp_text value 75k (at 4.96 0.18) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C43-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 145.55 69.38 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R63 (at 5.32 2.05 90) (layer F.SilkS))
    (fp_text value 3k9 (at 5.2 0.05 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "Net-(R63-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C51-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 150.14 79.57 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R64 (at 4.83 -2.14 90) (layer F.SilkS))
    (fp_text value 3k9 (at 5 -0.05 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "Net-(R63-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 117.5 56 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R51 (at 4.2 -2.1 270) (layer F.SilkS))
    (fp_text value 3k9 (at 5.15 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 RtoL))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(R51-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 66.34 77.32 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 10.14 -2.13 90) (layer F.SilkS))
    (fp_text value 2k26 (at 5.16 0.03) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 138.34 87.02)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R68 (at 5.1 2.2) (layer F.SilkS))
    (fp_text value 10 (at 5.1 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(J26-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(C49-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 69.74 79.12 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 4.86 2.15 90) (layer F.SilkS))
    (fp_text value 75 (at 5.01 0.08 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(R12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 74.04 68.92 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R16 (at 5.2 -2.2 90) (layer F.SilkS))
    (fp_text value 3k (at 4.95 0.15 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5F9EC42C)
    (at 53.2 68.9 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 4.95 -2.26 90) (layer F.SilkS))
    (fp_text value 21R5 (at 5.04 -0.02 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_width 1))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 148.5 96.42 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R69 (at 5 -2.1) (layer F.SilkS))
    (fp_text value 10 (at 5.06 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(C48-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J26-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 122.04 95.07 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R50 (at 4.87 -2.04 90) (layer F.SilkS))
    (fp_text value 75k (at 5 0.2 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 RtoL))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C46-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 145.84 113.42 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R61 (at 4.98 2.04 90) (layer F.SilkS))
    (fp_text value 3k9 (at 5 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(JP5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(C52-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 117.5 109.6 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R54 (at 5.16 2.13 90) (layer F.SilkS))
    (fp_text value 75k (at 5 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C46-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C46-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 135.1 128.7 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R56 (at 5.05 -2.19) (layer F.SilkS))
    (fp_text value 3k9 (at 4.96 -0.1) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(JP2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "Net-(R56-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 124.96 124.6)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R58 (at 5.02 2.07 180) (layer F.SilkS))
    (fp_text value 3k9 (at 5.1 0.1) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "Net-(R56-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(C52-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 69.74 133.12 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R14 (at 5.01 2.1 90) (layer F.SilkS))
    (fp_text value 75 (at 5.1 0.1 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(R14-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 113.8 125.8 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R46 (at 5.04 2.07) (layer F.SilkS))
    (fp_text value 75k (at 5.08 -0.03) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 LtoR))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(C44-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 121.3 124 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R62 (at 7.5 -2.1 90) (layer F.SilkS))
    (fp_text value 3k9 (at 4.9 -0.04 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(JP6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "Net-(R52-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 113.8 130.3 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R48 (at 5.04 2.07) (layer F.SilkS))
    (fp_text value 75k (at 5.08 -0.03) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(C44-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 145.84 110.62 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R65 (at 6.12 -2.09 90) (layer F.SilkS))
    (fp_text value 3k9 (at 5.3 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "Net-(R65-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(C52-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 150.14 100.42 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R66 (at 5.08 2.14 90) (layer F.SilkS))
    (fp_text value 3k9 (at 4.8 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "Net-(R65-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 66.34 102.57 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 10.1 2.45 90) (layer F.SilkS))
    (fp_text value 2k26 (at 4.95 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 117.5 124 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R52 (at 4 2.1 90) (layer F.SilkS))
    (fp_text value 3k9 (at 5 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 LtoR))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "Net-(R52-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 69.74 100.96 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 5.2 -2.17 90) (layer F.SilkS))
    (fp_text value 75 (at 5.3 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(R13-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 73.94 111.12 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R18 (at 5 2.15 90) (layer F.SilkS))
    (fp_text value 3k (at 5.1 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 138.34 93.12)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R70 (at 5 -2) (layer F.SilkS))
    (fp_text value 10 (at 5.08 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(J26-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C50-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5F9EC449)
    (at 53.2 109.1 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 3.7 2.3 90) (layer F.SilkS))
    (fp_text value 21R5 (at 5.04 0.04 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_width 1))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5FA312C2)
    (at 49.5 125 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 4.8 2.2 90) (layer F.SilkS))
    (fp_text value 21R5 (at 5.09 -0.02 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_width 1))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 66.34 131.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 10.04 -2.1 90) (layer F.SilkS))
    (fp_text value 2k26 (at 5.08 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(C6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 73.94 122.97 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R17 (at 5.3 -2.1 90) (layer F.SilkS))
    (fp_text value 3k (at 5 0.05 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 84.79 96.02 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R23 (at 5.05 -2.1) (layer F.SilkS))
    (fp_text value 10 (at 4.95 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(C25-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 84.79 91.9 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R19 (at 5.05 -2) (layer F.SilkS))
    (fp_text value 10 (at 5.08 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 78.18 111.11 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R22 (at 9.41 2.22 90) (layer F.SilkS))
    (fp_text value 2k8 (at 4.85 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 78.34 133.12 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R26 (at 5.25 2.1 90) (layer F.SilkS))
    (fp_text value 32k4 (at 5.1 0.05 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C22-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C22-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 99.09 132.47 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R27 (at 5.09 -2.23) (layer F.SilkS))
    (fp_text value 316k (at 4.85 0.05) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C22-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(R27-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 100.2 117.5 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R29 (at 5.9 -2.1 90) (layer F.SilkS))
    (fp_text value 2k (at 5.18 -0.06 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(R27-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(C27-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 106.04 96.02 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R31 (at 5 -2.1) (layer F.SilkS))
    (fp_text value 10 (at 5.1 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(C25-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J26-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 106.04 91.9 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R33 (at 5.1 -2.1) (layer F.SilkS))
    (fp_text value 10 (at 5.1 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(C26-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(J26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 111.4 104 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R32 (at 5.4 2.25) (layer F.SilkS))
    (fp_text value 240k (at 5 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(C19-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C38-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 113.8 116.8 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R39 (at 4.74 2) (layer F.SilkS))
    (fp_text value 33k (at 4.94 -0.03) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(C38-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R39-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 103.64 121.2)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R43 (at 5.51 -2.02) (layer F.SilkS))
    (fp_text value 1M (at 5.08 -0.02) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R39-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(C27-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 117.5 96.6 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R42 (at 5 -2.3 90) (layer F.SilkS))
    (fp_text value 1M (at 5.1 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(R42-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 139.54 126.5)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R74 (at 12.76 0) (layer F.SilkS))
    (fp_text value 47 (at 4.96 0.1) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(C52-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "Net-(J12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 176.54 92.02 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R38 (at 5.04 -1.98) (layer F.SilkS))
    (fp_text value 10 (at 5.04 0.02) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(C39-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(J26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 149.7 129.7 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R76 (at -2.5 0) (layer F.SilkS))
    (fp_text value 56k (at 5.2 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J14-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 167 124.8)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R80 (at 5.2 2.1) (layer F.SilkS))
    (fp_text value 2k2 (at 4.9 0.1) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(R113-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "Net-(R80-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 187 130 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R82 (at 2.7 2.1 90) (layer F.SilkS))
    (fp_text value 47 (at 5 -0.1 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "Net-(R80-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 141 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 167.1 110.5)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R86 (at 5.2 -2) (layer F.SilkS))
    (fp_text value 5k11 (at 5 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(C62-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(C62-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 180.5 100.34 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R91 (at 5.25 -2.25 90) (layer F.SilkS))
    (fp_text value 47 (at 5.05 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 139 "Net-(K2-Pad4)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(C62-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 180.69 84.89 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R90 (at 5.08 2.14 90) (layer F.SilkS))
    (fp_text value 10 (at 5.08 -0.06 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(C66-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J26-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 176.54 96 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R92 (at 4.84 -2.2) (layer F.SilkS))
    (fp_text value 10 (at 5.04 -0.03) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(C67-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(J26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 154.5 123.7 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R77 (at 5.2 -2.1 90) (layer F.SilkS))
    (fp_text value 1k5 (at 4.94 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J14-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(J21-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_Capacitors:C_Rect_L7.2mm_W3.5mm_P5.00mm_Kemet (layer F.Cu) (tedit 5F66BC51)
    (at 59.6 98.8)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.0mm Capacitor")
    (fp_text reference C4 (at 7.1 0.05 90) (layer F.SilkS))
    (fp_text value 33n (at 2.5 0) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C4-Pad1)"))
    (model ${SMC_3D}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.5mm_P5.00mm_Kemet.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.2 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_Capacitors:C_Rect_L7.2mm_W3.5mm_P5.00mm_Kemet (layer F.Cu) (tedit 5F66BC51)
    (at 53.5 124 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.0mm Capacitor")
    (fp_text reference C6 (at 7.3 0.1 180) (layer F.SilkS))
    (fp_text value 33n (at 2.5 0 180) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(C6-Pad1)"))
    (model ${SMC_3D}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.5mm_P5.00mm_Kemet.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.2 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:SO-LOMC (layer F.Cu) (tedit 5E18F70F)
    (at 61.99 63.02 270)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 0.28 -0.01 180) (layer F.SilkS))
    (fp_text value OPA1642 (at 0 3.4 90) (layer F.Fab))
    (fp_text user 1 (at -4.25 -1.9 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.725 -1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(C16-Pad1)"))
    (pad 7 smd roundrect (at 2.725 -0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(R12-Pad2)"))
    (pad 6 smd roundrect (at 2.725 0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C3-Pad1)"))
    (pad 5 smd roundrect (at 2.725 1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C2-Pad2)"))
    (pad 4 smd roundrect (at -2.725 1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(C11-Pad1)"))
    (pad 3 smd roundrect (at -2.725 0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C2-Pad2)"))
    (pad 2 smd roundrect (at -2.725 -0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C5-Pad1)"))
    (pad 1 smd roundrect (at -2.725 -1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:SO-LOMC (layer F.Cu) (tedit 5E18F70F)
    (at 61.99 117.02 270)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U4 (at 0.18 -0.01 180) (layer F.SilkS))
    (fp_text value OPA1642 (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (fp_text user 1 (at -4.25 -1.9 270 unlocked) (layer F.SilkS))
    (pad 1 smd roundrect (at -2.725 -1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(R13-Pad2)"))
    (pad 2 smd roundrect (at -2.725 -0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(C4-Pad1)"))
    (pad 3 smd roundrect (at -2.725 0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C1-Pad1)"))
    (pad 4 smd roundrect (at -2.725 1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C10-Pad2)"))
    (pad 5 smd roundrect (at 2.725 1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C1-Pad1)"))
    (pad 6 smd roundrect (at 2.725 0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(C6-Pad1)"))
    (pad 7 smd roundrect (at 2.725 -0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(R14-Pad2)"))
    (pad 8 smd roundrect (at 2.725 -1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 217 45.5 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J27 (at 0 -2.148) (layer F.Fab))
    (fp_text value HP (at -0.05 2.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 136 "Net-(J27-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 217 134.5)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J38 (at 0 -2.148) (layer F.Fab))
    (fp_text value HP (at 0.05 2.5) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 137 "Net-(J38-Pad1)"))
  )
  (module SMC_generic:C_Rect_L7.2mm_W4.5mm_P5.00mm_Wima (layer F.Cu) (tedit 5D533F69)
    (at 174.8 105.25 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (fp_text reference C62 (at -2 0 90) (layer F.SilkS))
    (fp_text value 100p (at 2.65 0.2 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(C62-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(C62-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.7))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 206 45.5 270)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J39 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value vHP (at -2.5 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 132 "Net-(J39-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 206 134.5 270)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J40 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value vHP (at 2.5 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 133 "Net-(J40-Pad1)"))
  )
  (module SMC_generic:C_Rect_L7.2mm_W2.5mm_P5.00mm_Kemet (layer F.Cu) (tedit 5D53486E)
    (at 107.4 44.5)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C43 (at 2.5 -3.32) (layer F.SilkS))
    (fp_text value 15n (at 2.56 -0.02 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C43-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W3.0mm_P5.00mm_Blue.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W2.5mm_P5.00mm_Kemet (layer F.Cu) (tedit 5D53486E)
    (at 107.5 135.5)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C44 (at 2.46 3.5) (layer F.SilkS))
    (fp_text value 15n (at 2.5 0.08 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(C44-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W3.0mm_P5.00mm_Blue.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W2.5mm_P5.00mm_Kemet (layer F.Cu) (tedit 5D53486E)
    (at 123.24 63.92 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C45 (at 2.52 -3.34 90) (layer F.SilkS))
    (fp_text value 15n (at 2.5 -0.04 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C45-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C45-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W3.0mm_P5.00mm_Blue.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W2.5mm_P5.00mm_Kemet (layer F.Cu) (tedit 5D53486E)
    (at 123.2 112.7 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C46 (at 2.5 -3.3 90) (layer F.SilkS))
    (fp_text value 15n (at 2.5 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C46-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C46-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W3.0mm_P5.00mm_Blue.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Disc_Vishay_100p (layer F.Cu) (tedit 5D533F69)
    (at 140.24 121.02 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (fp_text reference C52 (at -2.18 0.06 180) (layer F.SilkS))
    (fp_text value 100pF (at 2.52 -0.04 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(C52-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(C52-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/C320C104K5G5TA.step
      (offset (xyz 5.3 1.6 0))
      (scale (xyz 1.1 0.8 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 96 137)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J41 (at 0 -2.148) (layer F.Fab))
    (fp_text value Ph-out (at 0 2) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 113 "Net-(J41-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 102 137)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J42 (at 0 -2.148) (layer F.Fab))
    (fp_text value W-in (at 0 2) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 32 LtoR))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 96 43 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J43 (at 0 -2.148) (layer F.Fab))
    (fp_text value Ph-out (at 0 2 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 114 "Net-(J43-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 102 43 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J44 (at 0 -2.148) (layer F.Fab))
    (fp_text value W-in (at 0 2 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 RtoL))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 90 137)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J45 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 2) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 90 43 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J46 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 2 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 97 127.7 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R93 (at -1.8 0 180) (layer F.SilkS))
    (fp_text value 47 (at 5.1 -0.1 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(C27-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 "Net-(J41-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 96.9 52.1 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R94 (at -1.6 -0.05 180) (layer F.SilkS))
    (fp_text value 47 (at 5.08 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "Net-(J43-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(C30-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 156.7 47.08 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J17 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Mono/Stereo (at -2.1 1.78 270) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J17-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J17-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(J17-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 166 138 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J18 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Balance (at -2.2 2.5 90) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(J18-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J18-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 156.7 132.92)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J21 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Stereo/Mono (at 2.1 1.78 270) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(J21-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(J21-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 "Net-(J21-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 154.5 69.4 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R95 (at 5.1 2 90) (layer F.SilkS))
    (fp_text value 3k (at 5.1 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J17-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 161.5 52.16 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R96 (at 5.3 2.1 90) (layer F.SilkS))
    (fp_text value 2k (at 4.9 -0.1 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(J17-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(J18-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 157 84.84 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R97 (at 5.16 2.1 90) (layer F.SilkS))
    (fp_text value 3k (at 5.1 0.05 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J14-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 152.25 95 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R98 (at 4.9 -2.2 90) (layer F.SilkS))
    (fp_text value 3k (at 5.2 -0.1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "Net-(J21-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 161.5 127.84 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R99 (at 4.96 -2.2 90) (layer F.SilkS))
    (fp_text value 2k (at 5.26 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "Net-(J21-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "Net-(J18-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 154.5 110.6 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R100 (at 5.1 -2 90) (layer F.SilkS))
    (fp_text value 3k (at 5 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J14-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "Net-(J21-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:Relay_DPDT_Kemet_EC2-n (layer F.Cu) (tedit 605E0406)
    (at 206 63 270)
    (descr "Relay Omron G6S-2, see http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6s.pdf")
    (tags "Relay Omron G6S-2")
    (fp_text reference K1 (at 2.5 12 90) (layer F.SilkS))
    (fp_text value G6S-2 (at 2.5 14.9 90) (layer F.Fab))
    (fp_text user %R (at 2.54 6.35 90) (layer F.Fab))
    (fp_text user + (at 0 1.9 180 unlocked) (layer F.SilkS))
    (fp_text user - (at 5.1 1.9 180 unlocked) (layer F.SilkS))
    (pad 9 thru_hole circle (at 5.08 7.62 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 138 "Net-(K1-Pad9)"))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 71 "Net-(J19-Pad1)"))
    (pad 12 thru_hole circle (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 143 "Net-(D7-Pad2)"))
    (pad 10 thru_hole circle (at 5.08 5.08 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 132 "Net-(J39-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 142 "Net-(D7-Pad1)"))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 136 "Net-(J27-Pad1)"))
    (pad 8 thru_hole circle (at 5.08 10.16 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 75 "Net-(J31-Pad1)"))
    (pad 5 thru_hole circle (at 0 10.16 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 131 "Net-(J28-Pad1)"))
    (model ${KIPRJMOD}/lib/3D/EC2-5SNU.step
      (offset (xyz -1.2 1.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module SMC_generic:Relay_DPDT_Kemet_EC2-n (layer F.Cu) (tedit 605E0406)
    (at 206 112 270)
    (descr "Relay Omron G6S-2, see http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6s.pdf")
    (tags "Relay Omron G6S-2")
    (fp_text reference K2 (at 2.5 11.9 90) (layer F.SilkS))
    (fp_text value G6S-2 (at 2.5 14.9 90) (layer F.Fab))
    (fp_text user %R (at 2.54 6.35 90) (layer F.Fab))
    (fp_text user + (at 0 1.9 180 unlocked) (layer F.SilkS))
    (fp_text user - (at 5.1 1.9 180 unlocked) (layer F.SilkS))
    (pad 9 thru_hole circle (at 5.08 7.62 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 141 "Net-(J10-Pad1)"))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 139 "Net-(K2-Pad4)"))
    (pad 12 thru_hole circle (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 143 "Net-(D7-Pad2)"))
    (pad 10 thru_hole circle (at 5.08 5.08 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 137 "Net-(J38-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 142 "Net-(D7-Pad1)"))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 133 "Net-(J40-Pad1)"))
    (pad 8 thru_hole circle (at 5.08 10.16 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 140 "Net-(J10-Pad2)"))
    (pad 5 thru_hole circle (at 0 10.16 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 76 "Net-(J36-Pad1)"))
    (model ${KIPRJMOD}/lib/3D/EC2-5SNU.step
      (offset (xyz -1.2 1.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 204.5 90 270)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C75 (at 0 3.4 90) (layer F.SilkS))
    (fp_text value 10u (at -1.8 0.1 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 1 270) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(C75-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Wide (layer F.Cu) (tedit 5A2795B7)
    (at 207 83 180)
    (descr "TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 5 -2.75) (layer F.SilkS))
    (fp_text value 2N7000 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "Net-(D5-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -2.54 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 "Net-(C75-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Wide (layer F.Cu) (tedit 5A2795B7)
    (at 201.9 97)
    (descr "TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 0.1 -2.75) (layer F.SilkS))
    (fp_text value 2N5551 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(J48-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 "Net-(C75-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Wide (layer F.Cu) (tedit 5A2795B7)
    (at 209.5 123 180)
    (descr "TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 5 -2.75) (layer F.SilkS))
    (fp_text value 2N5551 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 "Net-(Q4-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 143 "Net-(D7-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -2.54 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 "Net-(Q4-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 200.9 60 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R101 (at 3.7 1.7) (layer F.SilkS))
    (fp_text value 220k (at 3.81 -0.05) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 136 "Net-(J27-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 200.9 71 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R102 (at 3.95 -1.7) (layer F.SilkS))
    (fp_text value 220k (at 3.75 -0.1) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 132 "Net-(J39-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 209.5 60.5 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R103 (at 4.75 -2.1 90) (layer F.SilkS))
    (fp_text value 135 (at 5 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J26-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 198.89 95.05 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R105 (at 5 -2.09 90) (layer F.SilkS))
    (fp_text value 30k (at 5 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J26-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(J48-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 189.67 95.05 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R106 (at 5 -2.07 90) (layer F.SilkS))
    (fp_text value 5M1 (at 5 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 "Net-(C75-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J26-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 209.5 51.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R107 (at 5 2) (layer F.SilkS))
    (fp_text value 1k (at 5 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 "Net-(D5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 199.34 74.5)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R108 (at 5.25 -2.25) (layer F.SilkS))
    (fp_text value 560 (at 5 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J26-Pad3)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 185.2 95.05 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R109 (at 5 -2.1 90) (layer F.SilkS))
    (fp_text value 560 (at 5 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 "Net-(C75-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 125 "Net-(J47-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 194.29 95.05 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R110 (at 5.15 -2.09 90) (layer F.SilkS))
    (fp_text value 270 (at 5.08 0.05 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(J48-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 199.34 105)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R111 (at 5.16 2.2) (layer F.SilkS))
    (fp_text value 560 (at 5.1 -0.1) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(D6-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(J26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 209.5 128.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R112 (at 5.1 -2.25) (layer F.SilkS))
    (fp_text value 1k (at 5.16 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 "Net-(Q4-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 209.5 119.5 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R114 (at 5.1 2.2 90) (layer F.SilkS))
    (fp_text value 135 (at 5.1 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(J26-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 200.95 109 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R115 (at 3.9 1.75) (layer F.SilkS))
    (fp_text value 220k (at 3.81 0) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 133 "Net-(J40-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 200.95 120 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R116 (at 3.8 -1.75) (layer F.SilkS))
    (fp_text value 220k (at 3.75 0) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 137 "Net-(J38-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 195.3 78)
    (descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
    (tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
    (fp_text reference D5 (at 4.02 1.75) (layer F.SilkS))
    (fp_text value BZX76C10 (at 3.81 1.92) (layer F.Fab))
    (fp_text user K (at 0 1.75) (layer F.SilkS))
    (fp_text user K (at 0 -1.75) (layer F.Fab))
    (fp_text user %R (at 4.038 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 122 "Net-(D5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 123 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 202.92 100.6 180)
    (descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
    (tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
    (fp_text reference D6 (at 4.16 1.6) (layer F.SilkS))
    (fp_text value BZX76C10 (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 4.038 0) (layer F.Fab))
    (fp_text user K (at 0 -1.75) (layer F.Fab))
    (fp_text user K (at 0 -1.75) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 124 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 183.3 50.9 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R104 (at 5 2) (layer F.SilkS))
    (fp_text value 10k (at 5 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "Net-(R104-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 167 129.1)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R113 (at 5.1 2.1) (layer F.SilkS))
    (fp_text value 10k (at 5 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(R113-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 187 80)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference J47 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value NO (at 0 2.05) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 125 "Net-(J47-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 187 101 180)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference J48 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value NC (at 0 2.05) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(J48-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 198 135.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (clearance 2)
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 187 66.5 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(J19-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(J28-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 187 113.5)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 140 "Net-(J10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 141 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 190.5 68.05 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R117 (at 3.8 1.7 90) (layer F.SilkS))
    (fp_text value 220k (at 3.75 0 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 75 "Net-(J31-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 190.5 63 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R118 (at 5.75 1.65 90) (layer F.SilkS))
    (fp_text value 220k (at 3.81 0.1 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 131 "Net-(J28-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 190.5 117 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R119 (at 5.7 -1.7 90) (layer F.SilkS))
    (fp_text value 220k (at 3.81 0 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 140 "Net-(J10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 190.5 112 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R120 (at 3.9 -1.8 90) (layer F.SilkS))
    (fp_text value 220k (at 3.81 0 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 76 "Net-(J36-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_multi_socket (layer F.Cu) (tedit 6090875B)
    (at 47.5 107 90)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*9mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 9mm Capacitor")
    (fp_text reference C1 (at 7.5 0 90) (layer F.SilkS))
    (fp_text value 220p (at 7.5 5.75 90) (layer F.SilkS) hide)
    (fp_text user %R (at 7.5 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 5 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 33 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 12.5 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.5 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 33 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 33 "Net-(C1-Pad1)"))
    (model ${KIPRJMOD}/lib/3D/C_Rect_L18.0mm_W5.0mm_P15.00mm_Kemet.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_multi_socket (layer F.Cu) (tedit 6090875B)
    (at 47.5 88 90)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*9mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 9mm Capacitor")
    (fp_text reference C2 (at 7.5 0 90) (layer F.SilkS))
    (fp_text value 220p (at 7.5 5.75 90) (layer F.SilkS) hide)
    (fp_text user %R (at 7.5 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 15 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 2.5 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 12.5 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 5 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 10 0 90) (size 2.54 2.54) (drill 1.4478) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (model ${KIPRJMOD}/lib/3D/C_Rect_L18.0mm_W5.0mm_P15.00mm_Kemet.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial_MM_0338 (layer F.Cu) (tedit 60908A99)
    (at 47.5 111 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 2.1 90) (layer F.SilkS))
    (fp_text value 100 (at 5.1 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16 0 270) (size 2.54 2.54) (drill 1.4732) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.54 2.54) (drill 1.4732) (layers *.Cu *.Mask)
      (net 33 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial_MM_0338 (layer F.Cu) (tedit 60908A99)
    (at 47.5 69 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.1 -2.1 90) (layer F.SilkS))
    (fp_text value 100 (at 5.1 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 1.4732) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 2.54 2.54) (drill 1.4732) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 210 84.9 270)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D7 (at 5.2 -0.05 90) (layer F.SilkS))
    (fp_text value 1N4003 (at 5.08 2.47 90) (layer F.Fab))
    (fp_text user %R (at 5.47 0 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user K (at -1.9 -0.05 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 142 "Net-(D7-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 143 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 211.5 42)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J7 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 211.5 138 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J8 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_text https://audiokarma.org/forums/index.php?threads/ultra-high-spec-opamp-mc-mm-phono-warp-elliptic-filter-line-headphone-amps.937686 (at 92 90 90) (layer B.SilkS))
  (gr_text "May 2021" (at 71.7 42.1) (layer F.SilkS))
  (gr_text "Phono to\nWarp switch" (at 82 42.5 180) (layer F.SilkS))
  (gr_text "Phono to\nWarp switch" (at 82 137.5) (layer F.SilkS))
  (gr_line (start 221 40) (end 221 140) (layer Edge.Cuts) (width 0.05))
  (gr_text Right (at 213.8 65.52 90) (layer F.SilkS))
  (gr_text Left (at 213.8 114.57 90) (layer F.SilkS))
  (gr_text LEFT (at 44 111.3 270) (layer F.SilkS))
  (gr_text RIGHT (at 44 68.7 270) (layer F.SilkS))
  (gr_text In (at 149.69 41.12 180) (layer F.SilkS))
  (gr_text Out (at 142.69 41.12 180) (layer F.SilkS))
  (gr_text In (at 149.93 139.08) (layer F.SilkS))
  (gr_text Out (at 142.98 139) (layer F.SilkS))
  (gr_text "Volume Pot" (at 179.65 40.89 180) (layer F.SilkS))
  (gr_text "Volume Pot" (at 180.025 139.17) (layer F.SilkS))
  (gr_text "A High-Gain Opamp Based Preamp for LOMC Cartridges" (at 44.5 90 90) (layer B.SilkS))
  (gr_text -15v (at 218.75 94.9 90) (layer B.SilkS))
  (gr_text +15v (at 218.75 85 90) (layer B.SilkS))
  (gr_text "LOMC Preamp\nv3.2, May 2021" (at 79.5 90 90) (layer B.SilkS))
  (gr_text "LOMC Pre v3.2" (at 56.9 42.2) (layer F.SilkS))
  (gr_text -15v (at 215.5 98.2) (layer F.SilkS))
  (gr_text +15v (at 215.5 81.9) (layer F.SilkS))
  (gr_line (start 36.5 140) (end 36.5 40) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 221 40) (end 36.5 40) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 36.5 140) (end 221 140) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 139.5) (xy 37 131.9) (xy 41 131.9) (xy 44.6 135.5) (xy 44.6 139.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 48.1) (xy 41 48.1) (xy 44.6 44.5) (xy 44.6 40.5) (xy 37 40.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.4 44.5) (xy 201.6 44.5) (xy 201.6 40) (xy 194.4 40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.4 135.5) (xy 201.6 135.5) (xy 201.6 140) (xy 194.4 140)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 90.5) (xy 175.1 90.6) (xy 176.54 92.02) (xy 177.6 92) (xy 177.6 88.1)
        (xy 176.5 88.1) (xy 175.1 89.5) (xy 37 89.5) (xy 37 40.52) (xy 220.5 40.5)
        (xy 220.5 139.5) (xy 37 139.5)
      )
    )
  )
)
