<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="41.58" y2="0" width="0" layer="20"/>
<wire x1="41.58" y1="0" x2="41.58" y2="50.79" width="0" layer="20"/>
<wire x1="41.58" y1="50.79" x2="0" y2="50.79" width="0" layer="20"/>
<wire x1="0" y1="50.79" x2="0" y2="0" width="0" layer="20"/>
<text>Isp Programming Board</text>
<text>By Duncan Young</text>
</plain>
<libraries>
<library name="DUNK">
<packages>
<package name="LED-0603">
</package>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
<package name="DIL08">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="AVRISP-BOX">
</package>
<package name="0805">
</package>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="blinkinlabs">
<description>Library of parts that we use for our Blinkinlabs designs. Some parts copied (and modified) from the excellent
Sparkfun and Adafruit libraries.</description>
<packages>
<package name="OSHW-LOGO-L">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="DUNK" package="LED-0603" value="BLUE">
<attribute name="PROD_ID" value="DIO-08575"/>
</element>
<element name="IC1" library="DUNK" package="DIL28-3" value="ATMEGA48/88/168-PU"/>
<element name="IC2" library="DUNK" package="DIL08" value="TINY13-20PU"/>
<element name="IC3" library="DUNK" package="DIL14" value="ATTINY24/44/84-PU"/>
<element name="ISP1" library="DUNK" package="AVRISP-BOX" value="ISPBOXHEADER-BOX"/>
<element name="LOGO1" library="blinkinlabs" package="OSHW-LOGO-L" value="OSHW-LOGOL"/>
<element name="R1" library="DUNK" package="0805" value="0.75">
<attribute name="PROD_ID" value="RES-08474"/>
</element>
<element name="Y1" library="DUNK" package="HC49US" value=""/>
</elements>
<signals>
<signal name="AGND">
<contactref element="IC1" pad="22"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="4"/>
<contactref element="ISP1" pad="6"/>
<contactref element="D1" pad="C"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="7"/>
<contactref element="IC2" pad="8"/>
<contactref element="ISP1" pad="2"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="ISP1" pad="5"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="19"/>
<contactref element="IC2" pad="7"/>
<contactref element="ISP1" pad="3"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="18"/>
<contactref element="IC2" pad="6"/>
<contactref element="ISP1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="17"/>
<contactref element="IC2" pad="5"/>
<contactref element="ISP1" pad="4"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="X1">
<contactref element="IC1" pad="9"/>
<contactref element="IC2" pad="3"/>
<contactref element="Y1" pad="1"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="X2">
<contactref element="IC1" pad="10"/>
<contactref element="IC2" pad="2"/>
<contactref element="Y1" pad="2"/>
<contactref element="IC3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
