(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 54)
    (zones 0)
    (modules 8)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.2032)
    (zone_clearance 0.4064)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.7112)
    (via_drill 0.3556)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0254)
    (solder_mask_min_width 0.127)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VCC)
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.7112)
    (via_drill 0.3556)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /VCC)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 5BF9F74F)
    (at 147.193 99.719 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 0 270) (layer B.SilkS))
    (fp_text value C (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module apa106:APA106 (layer F.Cu) (tedit 5C0A0508)
    (at 145.415 100.33)
    (fp_text reference L1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value APA106 (at 0 -3.81) (layer F.Fab))
    (fp_text user In (at 1.27 -2.54) (layer F.SilkS) hide)
    (fp_text user Vcc (at 1.397 -1.27) (layer F.SilkS) hide)
    (fp_text user Gnd (at 1.397 0) (layer F.SilkS) hide)
    (fp_text user Out (at 1.397 1.27) (layer F.SilkS) hide)
    (pad 4 thru_hole roundrect (at 0 1.27) (size 1.27 1.016) (drill 0.6604) (layers *.Cu *.Mask) (roundrect_rratio 0.5)
      (net 4 "Net-(J2-Pad1)"))
    (pad 3 thru_hole roundrect (at 0 0) (size 1.27 1.016) (drill 0.6604) (layers *.Cu *.Mask) (roundrect_rratio 0.5)
      (net 1 GND))
    (pad 2 thru_hole roundrect (at 0 -1.27) (size 1.27 1.016) (drill 0.6604) (layers *.Cu *.Mask) (roundrect_rratio 0.5)
      (net 2 /VCC))
    (pad 1 thru_hole roundrect (at 0 -2.54) (size 1.27 1.016) (drill 0.6604) (layers *.Cu *.Mask) (roundrect_rratio 0.5)
      (net 3 "Net-(J1-Pad1)"))
  )
  (module apa106:narrow_01x03_header (layer F.Cu) (tedit 5C0A002E)
    (at 149.225 99.695)
    (fp_text reference J2 (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 -5.08) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 -1.905) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 4 "Net-(J2-Pad1)"))
    (pad 3 thru_hole roundrect (at 0 1.905) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 1 GND))
    (pad 2 thru_hole roundrect (at 0 0) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 2 /VCC))
  )
  (module apa106:narrow_01x03_header (layer F.Cu) (tedit 5C0A002E)
    (at 142.24 99.695)
    (fp_text reference J1 (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 -5.08) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 -1.905) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 3 "Net-(J1-Pad1)"))
    (pad 3 thru_hole roundrect (at 0 1.905) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 1 GND))
    (pad 2 thru_hole roundrect (at 0 0) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 2 /VCC))
  )
  (module apa106:narrow_01x03_header (layer F.Cu) (tedit 5C0A002E)
    (at 142.24 107.823)
    (fp_text reference J1 (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 -5.08) (layer F.Fab))
    (pad 2 thru_hole roundrect (at 0 0) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 2 /VCC))
    (pad 3 thru_hole roundrect (at 0 1.905) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 -1.905) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 3 "Net-(J1-Pad1)"))
  )
  (module apa106:narrow_01x03_header (layer F.Cu) (tedit 5C0A002E)
    (at 149.225 107.823)
    (fp_text reference J2 (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 -5.08) (layer F.Fab))
    (pad 2 thru_hole roundrect (at 0 0) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 2 /VCC))
    (pad 3 thru_hole roundrect (at 0 1.905) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 -1.905) (size 1.651 1.27) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.4)
      (net 4 "Net-(J2-Pad1)"))
  )
  (module apa106:APA106 (layer F.Cu) (tedit 5C0A0519)
    (at 145.415 108.458)
    (fp_text reference L1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value APA106 (at 0 -3.81) (layer F.Fab))
    (fp_text user Out (at 1.397 1.27) (layer F.SilkS) hide)
    (fp_text user Gnd (at 1.397 0) (layer F.SilkS) hide)
    (fp_text user Vcc (at 1.397 -1.27) (layer F.SilkS) hide)
    (fp_text user In (at 1.27 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole roundrect (at 0 -2.54) (size 1.27 1.016) (drill 0.6604) (layers *.Cu *.Mask) (roundrect_rratio 0.5)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole roundrect (at 0 -1.27) (size 1.27 1.016) (drill 0.6604) (layers *.Cu *.Mask) (roundrect_rratio 0.5)
      (net 2 /VCC))
    (pad 3 thru_hole roundrect (at 0 0) (size 1.27 1.016) (drill 0.6604) (layers *.Cu *.Mask) (roundrect_rratio 0.5)
      (net 1 GND))
    (pad 4 thru_hole roundrect (at 0 1.27) (size 1.27 1.016) (drill 0.6604) (layers *.Cu *.Mask) (roundrect_rratio 0.5)
      (net 4 "Net-(J2-Pad1)"))
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 5BF9F74F)
    (at 147.193 107.847 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 0 270) (layer B.SilkS))
    (fp_text value C (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /VCC))
    (pad 2 smd roundrect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 142.113 96.901) (end 149.352 96.901) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 142.113 98.044) (end 142.113 96.901) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 142.113 101.346) (end 140.97 101.346) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 149.352 101.346) (end 149.352 102.489) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 149.352 98.044) (end 150.495 98.044) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 140.97 101.346) (end 140.97 98.044) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 149.352 102.489) (end 142.113 102.489) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 150.495 98.044) (end 150.495 101.346) (layer Edge.Cuts) (width 0.0254))
  (gr_text DO (at 147.574 97.79) (layer F.SilkS))
  (gr_text V (at 143.51 99.695) (layer B.SilkS))
  (gr_text V (at 147.955 99.695) (layer F.SilkS))
  (gr_text DI (at 143.637 97.79) (layer B.SilkS))
  (gr_text G (at 147.955 101.6) (layer F.SilkS))
  (gr_text G (at 143.51 101.6) (layer B.SilkS))
  (gr_line (start 150.495 106.172) (end 150.495 109.474) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 149.352 110.617) (end 142.113 110.617) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 140.97 109.474) (end 140.97 106.172) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 149.352 106.172) (end 150.495 106.172) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 149.352 109.474) (end 149.352 110.617) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 142.113 109.474) (end 140.97 109.474) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 142.113 106.172) (end 142.113 105.029) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 142.113 105.029) (end 149.352 105.029) (layer Edge.Cuts) (width 0.0254))
  (gr_text G (at 147.955 109.728) (layer F.SilkS))
  (gr_text DI (at 143.637 105.918) (layer B.SilkS))
  (gr_text G (at 143.51 109.728) (layer B.SilkS))
  (gr_text V (at 147.955 107.823) (layer F.SilkS))
  (gr_text V (at 143.51 107.823) (layer B.SilkS))
  (gr_text DO (at 147.574 105.918) (layer F.SilkS))
)
