(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 27)
    (no_connects 0)
    (area 135.814999 45.009999 168.985001 76.275001)
    (thickness 1.6)
    (drawings 5)
    (tracks 39)
    (zones 0)
    (modules 5)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.5 0.35)
    (user_via 0.6 0.4)
    (user_via 0.8 0.6)
    (user_via 1 0.8)
    (user_via 1.7 1.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad9)")
  (net 5 "Net-(J1-Pad1)")
  (net 6 "Net-(J1-Pad5)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-PadCD)")
  (net 10 "Net-(J1-PadWP)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J1-PadCD)")
    (add_net "Net-(J1-PadWP)")
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57FE9B14)
    (at 147.574 58.674 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 1u (at 3.175 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorConnectors:SquantorConnectors-SDCMF-10915W010 (layer F.Cu) (tedit 57FFF36D)
    (at 163.83 60.96 90)
    (attr smd)
    (fp_text reference J1 (at 13.716 -14.605 90) (layer F.SilkS))
    (fp_text value SDCMF-10915W010 (at 0.381 2.286 90) (layer F.Fab))
    (pad 1 smd rect (at 7.366 -13.462 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 4.826 -13.462 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 2.286 -13.462 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.254 -13.462 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 5 smd rect (at -2.794 -13.462 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -5.334 -13.462 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -7.874 -13.462 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at -9.398 -13.462 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at 9.906 -13.462 180) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad9)"))
    (pad WP smd rect (at -11.938 -13.462 180) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-PadWP)"))
    (pad CD smd rect (at -10.668 -13.462 180) (size 1.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-PadCD)"))
    (pad S4 smd rect (at 12.192 -11.43 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S3 smd rect (at 13.97 2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S2 smd rect (at -13.208 2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S1 smd rect (at -13.208 -11.43 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad D1 thru_hole circle (at 9.906 -10.414 180) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad D2 thru_hole circle (at -11.176 -10.414 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module SquantorConnectors:SquantorConnectors-1X10_SMALL (layer B.Cu) (tedit 58010A96)
    (at 137.16 60.96 270)
    (attr virtual)
    (fp_text reference JP2 (at -9.525 -2.54 270) (layer B.SilkS))
    (fp_text value PINHD-1X10TH_NORMAL (at -1.27 -2.54 270) (layer B.Fab))
    (pad 1 thru_hole rect (at -11.43 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 4 "Net-(J1-Pad9)"))
    (pad 2 thru_hole circle (at -8.89 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 5 "Net-(J1-Pad1)"))
    (pad 3 thru_hole circle (at -6.35 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 3 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at -3.81 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at -1.27 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 2 +3V3))
    (pad 6 thru_hole circle (at 1.27 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 6 "Net-(J1-Pad5)"))
    (pad 7 thru_hole circle (at 3.81 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 6.35 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at 8.89 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 9 "Net-(J1-PadCD)"))
    (pad 10 thru_hole circle (at 11.43 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 10 "Net-(J1-PadWP)"))
  )
  (module SquantorConnectors:SquantorConnectors-1X10_SMALL (layer B.Cu) (tedit 58010A9D)
    (at 144.78 60.96 270)
    (attr virtual)
    (fp_text reference JP1 (at -9.6012 2.4638 270) (layer B.SilkS))
    (fp_text value PINHD-1X10TH_NORMAL (at -1.27 2.54 270) (layer B.Fab))
    (pad 1 thru_hole rect (at -11.43 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 4 "Net-(J1-Pad9)"))
    (pad 2 thru_hole circle (at -8.89 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 5 "Net-(J1-Pad1)"))
    (pad 3 thru_hole circle (at -6.35 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 3 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at -3.81 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at -1.27 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 2 +3V3))
    (pad 6 thru_hole circle (at 1.27 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 6 "Net-(J1-Pad5)"))
    (pad 7 thru_hole circle (at 3.81 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 6.35 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at 8.89 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 9 "Net-(J1-PadCD)"))
    (pad 10 thru_hole circle (at 11.43 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask B.Paste B.SilkS)
      (net 10 "Net-(J1-PadWP)"))
  )
  (module Symbols:OSHW-Logo2_9.8x8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 161.925 61.595 270)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_9.8x8mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (gr_line (start 135.89 76.2) (end 168.91 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.89 45.085) (end 135.89 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 45.085) (end 135.89 45.085) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 45.085) (end 168.91 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text V2016.10.14 (at 156.21 61.595 90) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.89 45.085) (xy 168.91 45.085) (xy 168.91 76.2) (xy 135.89 76.2)
      )
    )
  )
)
