(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 38)
    (no_connects 0)
    (area 141.656999 98.8438 209.005201 117.903001)
    (thickness 1.6)
    (drawings 39)
    (tracks 258)
    (zones 0)
    (modules 12)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 Vin)
  (net 4 "Net-(GS1-Pad2)")
  (net 5 "Net-(P1-Pad2)")
  (net 6 "Net-(P1-Pad1)")
  (net 7 "Net-(P1-Pad4)")
  (net 8 "Net-(P1-Pad3)")
  (net 9 "Net-(P1-Pad6)")
  (net 10 "Net-(P1-Pad5)")
  (net 11 ICSPCLK)
  (net 12 "Net-(P1-Pad7)")
  (net 13 ICSPDAT)
  (net 14 "Net-(P2-Pad2)")
  (net 15 MCLR/VPP)
  (net 16 "Net-(P2-Pad3)")
  (net 17 "Net-(P2-Pad6)")
  (net 18 "Net-(P2-Pad5)")
  (net 19 "Net-(P2-Pad8)")
  (net 20 "Net-(P2-Pad7)")
  (net 21 "Net-(P2-Pad10)")
  (net 22 "Net-(P2-Pad9)")
  (net 23 "Net-(U2-Pad2)")
  (net 24 "Net-(U3-Pad4)")
  (net 25 "Net-(U4-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class "power track" ""
    (clearance 0.2032)
    (trace_width 0.3048)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
    (add_net ICSPCLK)
    (add_net ICSPDAT)
    (add_net MCLR/VPP)
    (add_net "Net-(GS1-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P2-Pad10)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P2-Pad9)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U4-Pad6)")
    (add_net VDD)
    (add_net Vin)
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 5A48CC8A)
    (at 166.4208 112.6236)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 2.2352 -3.9116) (layer F.SilkS))
    (fp_text value PIC16F1829 (at 16.9164 -7.1628) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.7 -2.925) (size 2 0.4) (layers F.Cu F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -3.7 -2.275) (size 2 0.4) (layers F.Cu F.Mask)
      (net 14 "Net-(P2-Pad2)"))
    (pad 3 smd rect (at -3.7 -1.625) (size 2 0.4) (layers F.Cu F.Mask)
      (net 16 "Net-(P2-Pad3)"))
    (pad 4 smd rect (at -3.7 -0.975) (size 2 0.4) (layers F.Cu F.Mask)
      (net 15 MCLR/VPP))
    (pad 5 smd rect (at -3.7 -0.325) (size 2 0.4) (layers F.Cu F.Mask)
      (net 18 "Net-(P2-Pad5)"))
    (pad 6 smd rect (at -3.7 0.325) (size 2 0.4) (layers F.Cu F.Mask)
      (net 17 "Net-(P2-Pad6)"))
    (pad 7 smd rect (at -3.7 0.975) (size 2 0.4) (layers F.Cu F.Mask)
      (net 20 "Net-(P2-Pad7)"))
    (pad 8 smd rect (at -3.7 1.625) (size 2 0.4) (layers F.Cu F.Mask)
      (net 19 "Net-(P2-Pad8)"))
    (pad 9 smd rect (at -3.7 2.275) (size 2 0.4) (layers F.Cu F.Mask)
      (net 22 "Net-(P2-Pad9)"))
    (pad 10 smd rect (at -3.7 2.925) (size 2 0.4) (layers F.Cu F.Mask)
      (net 21 "Net-(P2-Pad10)"))
    (pad 11 smd rect (at 3.7 2.925) (size 2 0.4) (layers F.Cu F.Mask)
      (net 6 "Net-(P1-Pad1)"))
    (pad 12 smd rect (at 3.7 2.275) (size 2 0.4) (layers F.Cu F.Mask)
      (net 5 "Net-(P1-Pad2)"))
    (pad 13 smd rect (at 3.7 1.625) (size 2 0.4) (layers F.Cu F.Mask)
      (net 8 "Net-(P1-Pad3)"))
    (pad 14 smd rect (at 3.7 0.975) (size 2 0.4) (layers F.Cu F.Mask)
      (net 7 "Net-(P1-Pad4)"))
    (pad 15 smd rect (at 3.7 0.325) (size 2 0.4) (layers F.Cu F.Mask)
      (net 10 "Net-(P1-Pad5)"))
    (pad 16 smd rect (at 3.7 -0.325) (size 2 0.4) (layers F.Cu F.Mask)
      (net 9 "Net-(P1-Pad6)"))
    (pad 17 smd rect (at 3.7 -0.975) (size 2 0.4) (layers F.Cu F.Mask)
      (net 12 "Net-(P1-Pad7)"))
    (pad 18 smd rect (at 3.7 -1.625) (size 2 0.4) (layers F.Cu F.Mask)
      (net 11 ICSPCLK))
    (pad 19 smd rect (at 3.7 -2.275) (size 2 0.4) (layers F.Cu F.Mask)
      (net 13 ICSPDAT))
    (pad 20 smd rect (at 3.7 -2.925) (size 2 0.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module GS3 (layer F.Cu) (tedit 5A47CA9A)
    (at 169.5 105.2 180)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference GS1 (at 1.3716 0 270) (layer F.SilkS))
    (fp_text value GS3 (at -10.8 -3.1 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 180) (size 1 1.1) (layers F.Cu F.Mask)
      (net 3 Vin))
    (pad 2 smd rect (at 0 0 180) (size 1 1.1) (layers F.Cu F.Mask)
      (net 4 "Net-(GS1-Pad2)"))
    (pad 3 smd rect (at 0 1.27 180) (size 1 1.1) (layers F.Cu F.Mask)
      (net 1 VDD))
  )
  (module custom2:Solder-20 (layer B.Cu) (tedit 5A15AAF1)
    (at 170.8404 110.7948 270)
    (fp_text reference P1 (at -6.604 0 540) (layer B.Fab) hide)
    (fp_text value CONN_02X05 (at 0 0 270) (layer B.Fab))
    (fp_text user 20 (at -5.08 -2.794 540) (layer B.SilkS))
    (fp_text user 18 (at -2.54 -2.794 540) (layer B.SilkS))
    (fp_text user 16 (at 0 -2.794 540) (layer B.SilkS))
    (fp_text user 14 (at 2.54 -2.794 540) (layer B.SilkS))
    (fp_text user 19 (at -5.08 2.794 540) (layer B.SilkS))
    (fp_text user 17 (at -2.54 2.794 540) (layer B.SilkS))
    (fp_text user 15 (at 0 2.794 540) (layer B.SilkS))
    (fp_text user 13 (at 2.54 2.794 540) (layer B.SilkS))
    (fp_text user 12 (at 5.08 -2.794 540) (layer B.SilkS))
    (fp_text user 11 (at 5.08 2.794 540) (layer B.SilkS))
    (pad 9 smd rect (at -5.08 1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 13 ICSPDAT))
    (pad 10 smd rect (at -5.08 -1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -2.54 1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 12 "Net-(P1-Pad7)"))
    (pad 8 smd rect (at -2.54 -1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 11 ICSPCLK))
    (pad 5 smd rect (at 0 1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 10 "Net-(P1-Pad5)"))
    (pad 6 smd rect (at 0 -1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 9 "Net-(P1-Pad6)"))
    (pad 3 smd rect (at 2.54 1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 8 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 2.54 -1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 7 "Net-(P1-Pad4)"))
    (pad 1 smd rect (at 5.08 1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 6 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 5.08 -1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 5 "Net-(P1-Pad2)"))
  )
  (module custom2:Solder-10 (layer B.Cu) (tedit 5A15AA3C)
    (at 161.8488 110.7948 270)
    (fp_text reference P2 (at -6.604 0 540) (layer B.Fab) hide)
    (fp_text value CONN_02X05 (at 0 0 270) (layer B.Fab))
    (fp_text user 10 (at 5.08 2.794 540) (layer B.SilkS))
    (fp_text user 8 (at 2.54 2.54 540) (layer B.SilkS))
    (fp_text user 6 (at 0 2.54 540) (layer B.SilkS))
    (fp_text user 4 (at -2.54 2.54 540) (layer B.SilkS))
    (fp_text user 9 (at 5.08 -2.54 540) (layer B.SilkS))
    (fp_text user 7 (at 2.54 -2.54 540) (layer B.SilkS))
    (fp_text user 5 (at 0 -2.54 540) (layer B.SilkS))
    (fp_text user 3 (at -2.54 -2.54 540) (layer B.SilkS))
    (fp_text user 2 (at -5.08 2.54 540) (layer B.SilkS))
    (fp_text user 1 (at -5.08 -2.54 540) (layer B.SilkS))
    (pad 2 smd rect (at -5.08 1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 14 "Net-(P2-Pad2)"))
    (pad 1 smd rect (at -5.08 -1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 1 VDD))
    (pad 4 smd rect (at -2.54 1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 15 MCLR/VPP))
    (pad 3 smd rect (at -2.54 -1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 16 "Net-(P2-Pad3)"))
    (pad 6 smd rect (at 0 1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 17 "Net-(P2-Pad6)"))
    (pad 5 smd rect (at 0 -1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 18 "Net-(P2-Pad5)"))
    (pad 8 smd rect (at 2.54 1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 19 "Net-(P2-Pad8)"))
    (pad 7 smd rect (at 2.54 -1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 20 "Net-(P2-Pad7)"))
    (pad 10 smd rect (at 5.08 1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 21 "Net-(P2-Pad10)"))
    (pad 9 smd rect (at 5.08 -1.27 270) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 22 "Net-(P2-Pad9)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5A15A807)
    (at 176.022 103.1748)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference ICSP (at -1.27 -1.3208) (layer F.SilkS))
    (fp_text value PICKIT3_ICSP (at 7.7724 -0.762) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 MCLR/VPP))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(GS1-Pad2)"))
    (pad 3 thru_hole rect (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 ICSPDAT))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 ICSPCLK))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(U4-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06_Pitch2.54mm (layer F.Cu) (tedit 5A15A57A)
    (at 153.924 103.124)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference REF** (at 1.27 -3.302) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x06_Pitch2.54mm (at 39.878 11.684) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06_Pitch2.54mm (layer F.Cu) (tedit 5A15A4F2)
    (at 143.764 103.124)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference REF** (at 1.27 -3.302) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x06_Pitch2.54mm (at 50.038 10.16) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06_Pitch2.54mm (layer F.Cu) (tedit 5A15A4CA)
    (at 148.844 103.124)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference REF** (at 1.27 -3.302) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x06_Pitch2.54mm (at 44.958 8.636) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5A146186)
    (at 161.2392 103.7844)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U3 (at 2.7432 0.1524) (layer F.SilkS))
    (fp_text value MCP1755 (at 21.0312 3.048) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Mask)
      (net 3 Vin))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Mask)
      (net 3 Vin))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Mask)
      (net 24 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-5 (layer F.Cu) (tedit 5A14616D)
    (at 169.3164 105.156)
    (descr "module CMS SOT223 5 pins, http://ww1.microchip.com/downloads/en/DeviceDoc/51751a.pdf")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 2.8956 -2.286) (layer F.SilkS))
    (fp_text value LP38692 (at 12.8016 -1.2192) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at -3.05 2.25) (size 2.2 1) (layers F.Cu F.Mask)
      (net 3 Vin))
    (pad 2 smd rect (at -3.05 -0.75) (size 2.2 1) (layers F.Cu F.Mask)
      (net 23 "Net-(U2-Pad2)"))
    (pad 5 smd rect (at 3.25 0) (size 1.8 3.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.05 0.75) (size 2.2 1) (layers F.Cu F.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at -3.05 -2.25) (size 2.2 1) (layers F.Cu F.Mask)
      (net 3 Vin))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223-5.wrl
      (at (xyz 0.0024606299 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A15A147)
    (at 159.8676 108.3564 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -0.0254 -1.5494 270) (layer F.SilkS))
    (fp_text value C (at 1.3716 -19.5072 360) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A144884)
    (at 159.8676 113.538 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value C (at 3.81 21.336 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text DEV_ (at 162.179 116.84) (layer F.SilkS))
  (gr_text https://pierremuth.wordpress.com (at 166.37 101.854) (layer B.SilkS))
  (gr_text Vpp (at 174.498 103.251 90) (layer F.SilkS))
  (gr_text clk (at 174.498 113.284 90) (layer F.SilkS))
  (gr_text dat (at 174.498 110.871 90) (layer F.SilkS))
  (gr_text Gnd (at 174.498 108.204 90) (layer F.SilkS))
  (gr_text raw (at 169.4 102.5) (layer F.SilkS))
  (gr_text reg (at 169.5 107.7) (layer F.SilkS))
  (gr_text Vin (at 174.498 105.664 90) (layer F.SilkS))
  (gr_text PIC16F1829 (at 166.497 116.84) (layer F.Mask))
  (gr_text F (at 142.24 115.824) (layer B.SilkS))
  (gr_text E (at 142.24 113.284) (layer B.SilkS))
  (gr_text D (at 142.24 110.744) (layer B.SilkS))
  (gr_text C (at 142.24 108.204) (layer B.SilkS))
  (gr_text B (at 142.24 105.41) (layer B.SilkS))
  (gr_text A (at 142.24 103.124) (layer B.SilkS))
  (gr_text 6 (at 156.464 101.6) (layer B.SilkS))
  (gr_text 5 (at 153.924 101.6) (layer B.SilkS))
  (gr_text 4 (at 151.384 101.6) (layer B.SilkS))
  (gr_text 3 (at 148.844 101.6) (layer B.SilkS))
  (gr_text 2 (at 146.304 101.6) (layer B.SilkS))
  (gr_text 1 (at 143.764 101.6) (layer B.SilkS))
  (gr_text F (at 142.24 115.824) (layer F.SilkS))
  (gr_text E (at 142.24 113.284) (layer F.SilkS))
  (gr_text D (at 142.24 110.744) (layer F.SilkS))
  (gr_text C (at 142.24 108.204) (layer F.SilkS))
  (gr_text B (at 142.24 105.41) (layer F.SilkS))
  (gr_text A (at 142.24 103.124) (layer F.SilkS))
  (gr_text 6 (at 156.464 101.6) (layer F.SilkS))
  (gr_text 5 (at 153.924 101.6) (layer F.SilkS))
  (gr_text 4 (at 151.384 101.6) (layer F.SilkS))
  (gr_text 3 (at 148.844 101.6) (layer F.SilkS))
  (gr_text 2 (at 146.304 101.6) (layer F.SilkS))
  (gr_text 1 (at 143.764 101.6) (layer F.SilkS))
  (gr_line (start 141.732 101.092) (end 141.986 101.092) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.732 117.602) (end 141.732 101.092) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 117.602) (end 141.732 117.602) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 101.092) (end 177.8 117.602) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 101.092) (end 141.986 101.092) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 158.0388 101.346) (xy 177.546 101.346) (xy 177.546 117.4496) (xy 158.0388 117.4496)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 177.546 101.346) (xy 158.0388 101.346) (xy 158.0388 117.4496) (xy 177.546 117.4496)
      )
    )
  )
)
