(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu20.10.1)
  (general
    (thickness 1.6)
    (drawings 56)
    (tracks 219)
    (zones 0)
    (modules 4)
    (nets 37)
  )
  (page USLetter)
  (title_block
    (title "WP-2 IC Card Programming Adapter")
    (date 2021-04-02)
    (rev 004)
    (company "Brian K. White - b.kenyon.w@gmail.com")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (uvia_size 0.5)
    (uvia_drill 0.3)
    (uvias_allowed no)
    (uvia_min_size 0.5)
    (uvia_min_drill 0.3)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.22)
    (aux_axis_origin 139.686 99.695)
    (grid_origin 139.686 99.695)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_WP-2_IC_CARD_programming_adapter"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /~OE)
  (net 3 /D0)
  (net 4 /D1)
  (net 5 /D2)
  (net 6 /D3)
  (net 7 /D4)
  (net 8 /D5)
  (net 9 /D6)
  (net 10 /D7)
  (net 11 /A17)
  (net 12 /A16)
  (net 13 /A15)
  (net 14 /A14)
  (net 15 /A13)
  (net 16 /A12)
  (net 17 /A11)
  (net 18 /A10)
  (net 19 /A9)
  (net 20 /A8)
  (net 21 /A7)
  (net 22 /A6)
  (net 23 /A5)
  (net 24 /A4)
  (net 25 /A3)
  (net 26 /A2)
  (net 27 /A1)
  (net 28 /A0)
  (net 29 /R~W)
  (net 30 /~CE1)
  (net 31 /CE2)
  (net 32 VDD)
  (net 33 /A15_A14)
  (net 34 /A14_~WE)
  (net 35 /A17_CE2)
  (net 36 /~WE~_A15)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.5)
    (uvia_drill 0.3)
    (diff_pair_width 0.2)
    (diff_pair_gap 0.2)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A14_~WE)
    (add_net /A15)
    (add_net /A15_A14)
    (add_net /A16)
    (add_net /A17)
    (add_net /A17_CE2)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CE2)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /R~W)
    (add_net /~CE1)
    (add_net /~OE)
    (add_net /~WE~_A15)
    (add_net GND)
    (add_net VDD)
  )
  (module 0_LOCAL:Pin_Header_Straight_1x38_Pitch1.27mm (layer F.Cu) (tedit 6066AB1F)
    (at 136.511 99.695)
    (descr "Through hole straight pin header, 1x38, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x38 1.27mm single row")
    (fp_text reference J1 (at 1.27 0 -90) (layer F.SilkS) hide)
    (fp_text value Conn_01x38_Male (at -1.27 0 -90) (layer F.Fab))
    (fp_text user %R (at 1.27 0 -90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 -23.495) (size 1 1) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -22.225) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 -20.955) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 31 /CE2))
    (pad 4 thru_hole circle (at 0 -19.685) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 30 /~CE1))
    (pad 5 thru_hole circle (at 0 -18.415) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 /~OE))
    (pad 6 thru_hole circle (at 0 -17.145) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 /D0))
    (pad 7 thru_hole circle (at 0 -15.875) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 /D1))
    (pad 8 thru_hole circle (at 0 -14.605) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 /D2))
    (pad 9 thru_hole circle (at 0 -13.335) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 /D3))
    (pad 10 thru_hole circle (at 0 -12.065) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 /D4))
    (pad 11 thru_hole circle (at 0 -10.795) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 /D5))
    (pad 12 thru_hole circle (at 0 -9.525) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 9 /D6))
    (pad 13 thru_hole circle (at 0 -8.255) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 /D7))
    (pad 14 thru_hole circle (at 0 -6.985) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at 0 -5.715) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 0 -4.445) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 0 -3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 /A17))
    (pad 18 thru_hole circle (at 0 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 12 /A16))
    (pad 19 thru_hole circle (at 0 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 13 /A15))
    (pad 20 thru_hole circle (at 0 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 /A14))
    (pad 21 thru_hole circle (at 0 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 15 /A13))
    (pad 22 thru_hole circle (at 0 3.175) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 16 /A12))
    (pad 23 thru_hole circle (at 0 4.445) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 /A11))
    (pad 24 thru_hole circle (at 0 5.715) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 18 /A10))
    (pad 25 thru_hole circle (at 0 6.985) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 19 /A9))
    (pad 26 thru_hole circle (at 0 8.255) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 20 /A8))
    (pad 27 thru_hole circle (at 0 9.525) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 21 /A7))
    (pad 28 thru_hole circle (at 0 10.795) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 22 /A6))
    (pad 29 thru_hole circle (at 0 12.065) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 23 /A5))
    (pad 30 thru_hole circle (at 0 13.335) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 24 /A4))
    (pad 31 thru_hole circle (at 0 14.605) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 25 /A3))
    (pad 32 thru_hole circle (at 0 15.875) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 26 /A2))
    (pad 33 thru_hole circle (at 0 17.145) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 27 /A1))
    (pad 34 thru_hole circle (at 0 18.415) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 28 /A0))
    (pad 35 thru_hole circle (at 0 19.685) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 29 /R~W))
    (pad 36 thru_hole circle (at 0 20.955) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at 0 22.225) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad 38 thru_hole circle (at 0 23.495) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 32 VDD))
    (model ${KIPRJMOD}/3d/PinHeader_1x38_P1.27mm_Vertical.step
      (offset (xyz 0 23.495 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/WP-2_IC_Card_v003_ROM_assembly.step_x
      (offset (xyz -1.1303 0 9.499599999999999))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
    (model ${KIPRJMOD}/WP-2_IC_Card_ROM_carried.step_x
      (offset (xyz -1.1303 0 9.499599999999999))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
    (model ${KIPRJMOD}/WP-2_IC_Card_ROM_no_carrier.step_x
      (offset (xyz -1.1303 0 9.499599999999999))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
    (model ${KIPRJMOD}/WP-2_IC_Card_RAM.step_x
      (offset (xyz -1.397 0 9.5504))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
    (model ${KIPRJMOD}/WP-2_IC_Card_ROM.step_x
      (offset (xyz -1.397 0 9.5504))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module 0_LOCAL:2x8_jumper_block (layer F.Cu) (tedit 6066AA18)
    (at 140.829 80.645)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_02x08_Odd_Even (at 1.27 20.11) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89 90) (layer F.Fab))
    (pad 16 thru_hole circle (at 2.54 17.78) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 29 /R~W))
    (pad 15 thru_hole circle (at 0 17.78) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 14 /A14))
    (pad 14 thru_hole circle (at 2.54 15.24) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 34 /A14_~WE))
    (pad 13 thru_hole circle (at 0 15.24) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 34 /A14_~WE))
    (pad 12 thru_hole circle (at 2.54 12.7) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 31 /CE2))
    (pad 11 thru_hole circle (at 0 12.7) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 11 /A17))
    (pad 10 thru_hole circle (at 2.54 10.16) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 35 /A17_CE2))
    (pad 9 thru_hole circle (at 0 10.16) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 35 /A17_CE2))
    (pad 8 thru_hole circle (at 2.54 7.62) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 13 /A15))
    (pad 7 thru_hole circle (at 0 7.62) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 29 /R~W))
    (pad 6 thru_hole circle (at 2.54 5.08) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 36 /~WE~_A15))
    (pad 5 thru_hole circle (at 0 5.08) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 36 /~WE~_A15))
    (pad 4 thru_hole circle (at 2.54 2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 14 /A14))
    (pad 3 thru_hole circle (at 0 2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 13 /A15))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 33 /A15_A14))
    (pad 1 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 33 /A15_A14))
    (model ${KIPRJMOD}/3d/PinHeader_2x08_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/3d/Jumper.stp
      (offset (xyz 1.27 -3.7719 2.54))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/3d/Jumper.stp
      (offset (xyz 1.27 -8.851900000000001 2.54))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/3d/Jumper.stp
      (offset (xyz 1.27 -13.9319 2.54))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/3d/Jumper.stp
      (offset (xyz 1.27 -19.0119 2.54))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 0_LOCAL:JP2_tight_storage (layer F.Cu) (tedit 5FBC7AAA)
    (at 141.591 111.125 90)
    (fp_text reference REF** (at 0 -1.25 -90) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -2 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 1.1938 0 90) (size 0.9144 0.9144) (drill 0.9144) (layers *.Cu))
    (pad "" np_thru_hole circle (at -1.1938 0 90) (size 0.9144 0.9144) (drill 0.9144) (layers *.Cu))
  )
  (module 0_LOCAL:2x16x600 (layer F.Cu) (tedit 5F9A5FE1)
    (at 139.686 99.695)
    (descr "32-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference J2 (at -3.81 -19.05) (layer F.SilkS) hide)
    (fp_text value Conn_02x16_Counter_Clockwise (at 0 21.44) (layer F.Fab))
    (fp_text user %R (at -3.81 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at -7.62 -19.05) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1))
    (pad 17 thru_hole circle (at 7.62 19.05) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 6 /D3))
    (pad 2 thru_hole circle (at -7.62 -16.51) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 12 /A16))
    (pad 18 thru_hole circle (at 7.62 16.51) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 7 /D4))
    (pad 3 thru_hole circle (at -7.62 -13.97) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 33 /A15_A14))
    (pad 19 thru_hole circle (at 7.62 13.97) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 8 /D5))
    (pad 4 thru_hole circle (at -7.62 -11.43) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 16 /A12))
    (pad 20 thru_hole circle (at 7.62 11.43) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 9 /D6))
    (pad 5 thru_hole circle (at -7.62 -8.89) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 21 /A7))
    (pad 21 thru_hole circle (at 7.62 8.89) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 10 /D7))
    (pad 6 thru_hole circle (at -7.62 -6.35) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 22 /A6))
    (pad 22 thru_hole circle (at 7.62 6.35) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 30 /~CE1))
    (pad 7 thru_hole circle (at -7.62 -3.81) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 23 /A5))
    (pad 23 thru_hole circle (at 7.62 3.81) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 18 /A10))
    (pad 8 thru_hole circle (at -7.62 -1.27) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 24 /A4))
    (pad 24 thru_hole circle (at 7.62 1.27) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 2 /~OE))
    (pad 9 thru_hole circle (at -7.62 1.27) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 25 /A3))
    (pad 25 thru_hole circle (at 7.62 -1.27) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 17 /A11))
    (pad 10 thru_hole circle (at -7.62 3.81) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 26 /A2))
    (pad 26 thru_hole circle (at 7.62 -3.81) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 19 /A9))
    (pad 11 thru_hole circle (at -7.62 6.35) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 27 /A1))
    (pad 27 thru_hole circle (at 7.62 -6.35) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 20 /A8))
    (pad 12 thru_hole circle (at -7.62 8.89) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 28 /A0))
    (pad 28 thru_hole circle (at 7.62 -8.89) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 15 /A13))
    (pad 13 thru_hole circle (at -7.62 11.43) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 3 /D0))
    (pad 29 thru_hole circle (at 7.62 -11.43) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 34 /A14_~WE))
    (pad 14 thru_hole circle (at -7.62 13.97) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 4 /D1))
    (pad 30 thru_hole circle (at 7.62 -13.97) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 35 /A17_CE2))
    (pad 15 thru_hole circle (at -7.62 16.51) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 5 /D2))
    (pad 31 thru_hole circle (at 7.62 -16.51) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 36 /~WE~_A15))
    (pad 16 thru_hole circle (at -7.62 19.05) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 32 thru_hole circle (at 7.62 -19.05) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 32 VDD))
    (model ${KIPRJMOD}/3d/PinHeader_1x16_P2.54mm_Vertical.step
      (offset (xyz 7.62 19.05 -1.7272))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${KIPRJMOD}/3d/PinHeader_1x16_P2.54mm_Vertical.step
      (offset (xyz -7.62 19.05 -1.7272))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
  )
  (gr_text RAM (at 145.274 81.915 90) (layer F.SilkS))
  (gr_text RAM (at 145.274 86.995 90) (layer F.SilkS))
  (gr_text RAM (at 145.274 92.075 90) (layer F.SilkS))
  (gr_text RAM (at 145.274 97.155 90) (layer F.SilkS))
  (gr_text ROM (at 139.051 81.915 90) (layer F.SilkS))
  (gr_text ROM (at 139.051 86.995 90) (layer F.SilkS))
  (gr_text ROM (at 139.051 92.075 90) (layer F.SilkS))
  (gr_text ROM (at 139.051 97.155 90) (layer F.SilkS))
  (gr_line (start 139.051 75.565) (end 139.051 78.74) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 139.686 78.74) (end 139.051 78.74) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.051 120.65) (end 139.051 123.825) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.971 120.65) (end 133.971 123.825) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.971 78.74) (end 133.971 75.565) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.686 79.375) (end 147.941 79.375) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 147.941 80.01) (end 148.576 80.01) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 138.416 75.565) (end 139.051 75.565) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_text 1 (at 138.4795 76.2 90) (layer F.SilkS))
  (gr_line (start 131.431 79.375) (end 133.336 79.375) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 133.336 78.74) (end 133.336 79.375) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 131.431 80.01) (end 131.431 79.375) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 134.606 75.565) (end 134.606 74.93) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.431 120.015) (end 133.336 120.015) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 133.336 120.65) (end 133.971 120.65) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 131.431 119.38) (end 130.796 119.38) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 134.606 123.825) (end 133.971 123.825) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.686 120.015) (end 147.941 120.015) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 138.416 123.825) (end 138.416 124.46) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 139.686 120.65) (end 139.686 120.015) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 147.941 119.38) (end 147.941 120.015) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.796 119.38) (end 130.796 80.01) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.416 124.46) (end 134.606 124.46) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.576 80.01) (end 148.576 119.38) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.606 74.93) (end 138.416 74.93) (layer Edge.Cuts) (width 0.1))
  (gr_text 38 (at 138.4795 123.19 90) (layer F.SilkS))
  (gr_text "WP-2_IC_Card_programming_adapter v004" (at 134.606 99.695 90) (layer B.SilkS))
  (gr_text 1 (at 133.971 80.645) (layer F.SilkS))
  (gr_text github.com/bkw777/WP-2_IC_Card (at 145.02 99.695 90) (layer B.SilkS))
  (gr_text "WP-2 IC CARD" (at 139.686 109.855 90) (layer F.SilkS))
  (gr_text 38 (at 134.5425 123.19 -90) (layer F.SilkS))
  (gr_text 1 (at 134.5425 76.2 -90) (layer F.SilkS))
  (gr_text "Programming Adapter" (at 142.861 109.855 90) (layer F.SilkS))
)
