<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<hole x="8.89" y="13.9954" drill="2.54"/>
<hole x="44.45" y="58.42" drill="2.54" locked="yes"/>
<hole x="8.89" y="20.574" drill="1.3208" locked="yes"/>
<hole x="8.89" y="58.674" drill="1.3208" locked="yes"/>
<hole x="37.846" y="58.674" drill="1.3208" locked="yes"/>
<hole x="44.45" y="13.97" drill="1.3208" locked="yes"/>
<wire x1="14.224" y1="0" x2="1.3008" y2="0" width="0.254" layer="20"/>
<wire x1="1.3008" y1="0" x2="0" y2="1.3008" width="0.254" layer="20" curve="-90"/>
<wire x1="0" y1="1.3008" x2="0" y2="21.971" width="0.254" layer="20"/>
<wire x1="14.224" y1="0" x2="14.224" y2="8.89" width="0.254" layer="20"/>
<wire x1="14.224" y1="8.89" x2="16.256" y2="8.89" width="0.254" layer="20"/>
<wire x1="16.256" y1="8.89" x2="16.256" y2="0.0635" width="0.254" layer="20"/>
<wire x1="16.256" y1="0.0635" x2="52.0467375" y2="0" width="0.254" layer="20"/>
<wire x1="52.0467375" y1="0" x2="53.34" y2="1.2932625" width="0.254" layer="20" curve="90"/>
<wire x1="53.34" y1="1.2932625" x2="53.34" y2="21.844" width="0.254" layer="20"/>
<wire x1="0" y1="50.546" x2="0" y2="70.982496875" width="0.254" layer="20"/>
<wire x1="0" y1="70.982496875" x2="1.407503125" y2="72.39" width="0.254" layer="20" curve="-90"/>
<wire x1="1.407503125" y1="72.39" x2="37.1475" y2="72.39" width="0.254" layer="20"/>
<wire x1="37.1475" y1="72.39" x2="37.1475" y2="63.5" width="0.254" layer="20"/>
<wire x1="37.1475" y1="63.5" x2="39.0525" y2="63.5" width="0.254" layer="20"/>
<wire x1="39.0525" y1="63.5" x2="39.0525" y2="72.39" width="0.254" layer="20"/>
<wire x1="53.34" y1="50.546" x2="53.34" y2="71.0967375" width="0.254" layer="20"/>
<wire x1="53.34" y1="71.0967375" x2="52.0467375" y2="72.39" width="0.254" layer="20" curve="90"/>
<wire x1="52.0467375" y1="72.39" x2="49.9745" y2="72.39" width="0.254" layer="20"/>
<wire x1="49.9745" y1="72.39" x2="49.9745" y2="70.1675" width="0.254" layer="20"/>
<wire x1="49.9745" y1="70.1675" x2="46.5455" y2="70.1675" width="0.254" layer="20"/>
<wire x1="46.5455" y1="70.1675" x2="46.5455" y2="72.39" width="0.254" layer="20"/>
<wire x1="46.5455" y1="72.39" x2="39.0525" y2="72.39" width="0.254" layer="20"/>
<wire x1="0" y1="21.971" x2="3.81" y2="21.971" width="0.254" layer="20"/>
<wire x1="3.81" y1="21.971" x2="3.81" y2="23.8125" width="0.254" layer="20"/>
<wire x1="3.81" y1="23.8125" x2="0" y2="23.8125" width="0.254" layer="20"/>
<wire x1="0" y1="23.8125" x2="0" y2="48.514" width="0.254" layer="20"/>
<wire x1="0" y1="48.514" x2="3.81" y2="48.514" width="0.254" layer="20"/>
<wire x1="3.81" y1="48.514" x2="3.81" y2="50.546" width="0.254" layer="20"/>
<wire x1="3.81" y1="50.546" x2="0" y2="50.546" width="0.254" layer="20"/>
<wire x1="53.34" y1="21.844" x2="49.53" y2="21.844" width="0.254" layer="20"/>
<wire x1="49.53" y1="21.844" x2="49.53" y2="23.876" width="0.254" layer="20"/>
<wire x1="49.53" y1="23.876" x2="53.34" y2="23.876" width="0.254" layer="20"/>
<wire x1="53.34" y1="23.876" x2="53.34" y2="48.514" width="0.254" layer="20"/>
<wire x1="53.34" y1="48.514" x2="49.53" y2="48.514" width="0.254" layer="20"/>
<wire x1="49.53" y1="48.514" x2="49.53" y2="50.546" width="0.254" layer="20"/>
<wire x1="49.53" y1="50.546" x2="53.34" y2="50.546" width="0.254" layer="20"/>
<text>TVS</text>
<text>Power
Indicator</text>
<text>RV-Project.Com </text>
<text>Ver 3.2B
1/7/2019</text>
<text>Ch4/S1 = ON
Ch3/S2 = Open
Ch1/S3 = OFF
Ch2/S4 = Close</text>
<text>Trim Case Rib</text>
<text>Trim Case Rib</text>
<text>Replaces MaxxAir
Thermostat Boards
00-03550K
00-A3550K
</text>
<text>GND   12V</text>
<text>ON       OFF</text>
<text>Power</text>
<text>Fan Remote Control</text>
<text>Made in USA</text>
<text>OPEN</text>
<text>CLOSE</text>
<text>OFF</text>
<text>ON</text>
<text>ON</text>
<text>OFF</text>
<text>CLOSE</text>
<text>OPEN</text>
<text>IGO</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="1206-CAP">
</package>
<package name="SOD-123">
<description>100V/150mA 1N4148 - Super Cheap</description>
</package>
<package name="FUSE476">
</package>
<package name="WURTHRJ11">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="SOT23-3">
</package>
<package name="1206-RES">
</package>
<package name="ASK_MICRO_RECEIVER_DECODER_433MHZ">
</package>
<package name="PCB_KEYPAD_PRINT">
</package>
<package name="TAYDA_A5104_SLIDE_SWITCH">
</package>
<package name="GODZILLA_LARGE">
</package>
<package name="DG301-2P">
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="SMD_ELECTROLYTIC_4MMDIA">
</package>
<package name="SOT223/SOT89_COMBO">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="EB2RELAY">
</package>
<package name="GODZILLA_MEDIUM">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="a-lib" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="a-lib" package="SOD-123" value="TVS-SSOD123">
<attribute name="NAME"/>
</element>
<element name="F1" library="a-lib" package="FUSE476" value="1A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="a-lib" package="WURTHRJ11" value="RJ11VERTICALMOUNTWURTH">
<attribute name="PARTNUM" value="615006138521 "/>
</element>
<element name="LED1" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="a-lib" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q2" library="a-lib" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q3" library="a-lib" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q4" library="a-lib" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="R2" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX1" library="a-lib" package="ASK_MICRO_RECEIVER_DECODER_433MHZ" value=""/>
<element name="S1" library="a-lib" package="PCB_KEYPAD_PRINT" value="SPST_KEYPAD_MEMBRANE_SWITCH">
<attribute name="NAME"/>
</element>
<element name="S2" library="a-lib" package="PCB_KEYPAD_PRINT" value="SPST_KEYPAD_MEMBRANE_SWITCH">
<attribute name="NAME"/>
</element>
<element name="S3" library="a-lib" package="PCB_KEYPAD_PRINT" value="SPST_KEYPAD_MEMBRANE_SWITCH">
<attribute name="NAME"/>
</element>
<element name="S4" library="a-lib" package="PCB_KEYPAD_PRINT" value="SPST_KEYPAD_MEMBRANE_SWITCH">
<attribute name="NAME"/>
</element>
<element name="SW1" library="a-lib" package="TAYDA_A5104_SLIDE_SWITCH" value=""/>
<element name="R6" library="SparkFun-Resistors" package="0805" value="3k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="3k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="a-lib" package="DG301-2P" value="A668">
<attribute name="PITCH" value="5MM"/>
</element>
<element name="D4" library="a-lib" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="a-lib" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="a-lib" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="a-lib" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="a-lib" package="SMD_ELECTROLYTIC_4MMDIA" value="10uF@16V">
<attribute name="NAME"/>
</element>
<element name="C1" library="a-lib" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="a-lib" package="SOT223/SOT89_COMBO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K2" library="a-lib" package="EB2RELAY" value="SMD_DPDT_RELAY_10PINEB2">
<attribute name="NAME"/>
<attribute name="PARTNUM" value="EB2-5NU"/>
<attribute name="VOLTAGE" value="5v"/>
</element>
<element name="K3" library="a-lib" package="EB2RELAY" value="SMD_DPDT_RELAY_10PINEB2">
<attribute name="NAME"/>
<attribute name="PARTNUM" value="EB2-5NU"/>
<attribute name="VOLTAGE" value="5v"/>
</element>
<element name="K4" library="a-lib" package="EB2RELAY" value="SMD_DPDT_RELAY_10PINEB2">
<attribute name="NAME"/>
<attribute name="PARTNUM" value="EB2-5NU"/>
<attribute name="VOLTAGE" value="5v"/>
</element>
<element name="K1" library="a-lib" package="EB2RELAY" value="SMD_DPDT_RELAY_10PINEB2">
<attribute name="NAME"/>
<attribute name="PARTNUM" value="EB2-5NU"/>
<attribute name="VOLTAGE" value="5v"/>
</element>
<element name="LOGO2" library="a-lib" package="GODZILLA_LARGE" value="Godziwa Large">
<attribute name="VALUE" value="Godziwa Large"/>
</element>
<element name="LOGO1" library="a-lib" package="GODZILLA_MEDIUM" value="CLIPART_LOGOGODZIWA_MEDIUM">
<attribute name="VAULE" value="Godziwa Medium"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J2" pad="P$4"/>
<contactref element="S4" pad="P$2"/>
<contactref element="S2" pad="P$2"/>
<contactref element="K2" pad="4"/>
<contactref element="K4" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="S4" pad="P$1"/>
<contactref element="R6" pad="2"/>
<contactref element="K4" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="S2" pad="P$1"/>
<contactref element="R7" pad="2"/>
<contactref element="K2" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="P$5"/>
<contactref element="S1" pad="P$1"/>
<contactref element="S3" pad="P$1"/>
<contactref element="K1" pad="3"/>
<contactref element="K3" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="J2" pad="P$2"/>
<contactref element="S3" pad="P$2"/>
<contactref element="R6" pad="1"/>
<contactref element="K3" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="J2" pad="P$3"/>
<contactref element="S1" pad="P$2"/>
<contactref element="R7" pad="1"/>
<contactref element="K1" pad="4"/>
</signal>
<signal name="5V">
<contactref element="RX1" pad="VCC"/>
<contactref element="R5" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="C3" pad="+"/>
<contactref element="U1" pad="1"/>
<contactref element="K2" pad="1"/>
<contactref element="K1" pad="1"/>
<contactref element="K3" pad="1"/>
<contactref element="K4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="Q2" pad="3"/>
<contactref element="D2" pad="A"/>
<contactref element="K2" pad="10"/>
</signal>
<signal name="N$8">
<contactref element="Q1" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="K1" pad="10"/>
</signal>
<signal name="N$9">
<contactref element="Q3" pad="3"/>
<contactref element="D3" pad="A"/>
<contactref element="K3" pad="10"/>
</signal>
<signal name="N$10">
<contactref element="Q4" pad="3"/>
<contactref element="D4" pad="A"/>
<contactref element="K4" pad="10"/>
</signal>
<signal name="GND">
<contactref element="Q4" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="RX1" pad="GND"/>
<contactref element="LED1" pad="K"/>
<contactref element="C2" pad="2"/>
<contactref element="D5" pad="A"/>
<contactref element="J2" pad="P$6"/>
<contactref element="J1" pad="P$1"/>
<contactref element="C3" pad="-"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R3" pad="2"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="Q2" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R2" pad="1"/>
<contactref element="RX1" pad="OUT3"/>
</signal>
<signal name="N$17">
<contactref element="RX1" pad="OUT1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="RX1" pad="OUT2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R5" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$22">
<contactref element="F1" pad="P$1"/>
<contactref element="D5" pad="C"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="J2" pad="P$1"/>
<contactref element="J1" pad="P$2"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R1" pad="1"/>
<contactref element="RX1" pad="OUT4"/>
</signal>
<signal name="N$12">
<contactref element="Q4" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="SW1" pad="2"/>
<contactref element="F1" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
