(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 58)
    (no_connects 19)
    (area 174.549999 100.889999 236.295001 130.250001)
    (thickness 1.6)
    (drawings 24)
    (tracks 180)
    (zones 0)
    (modules 19)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 VCC)
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D3-Pad1)")
  (net 5 "Net-(D4-Pad1)")
  (net 6 "Net-(D5-Pad1)")
  (net 7 "Net-(D6-Pad1)")
  (net 8 "Net-(D7-Pad1)")
  (net 9 "Net-(D8-Pad1)")
  (net 10 "Net-(P1-Pad7)")
  (net 11 GND)
  (net 12 "Net-(P1-Pad3)")
  (net 13 "Net-(P1-Pad5)")
  (net 14 "Net-(P1-Pad9)")
  (net 15 "Net-(P1-Pad11)")
  (net 16 "Net-(P1-Pad13)")
  (net 17 "Net-(P1-Pad15)")
  (net 18 "Net-(P1-Pad17)")
  (net 19 "Net-(D1-Pad2)")
  (net 20 "Net-(D2-Pad2)")
  (net 21 "Net-(D3-Pad2)")
  (net 22 "Net-(D4-Pad2)")
  (net 23 "Net-(D5-Pad2)")
  (net 24 "Net-(D6-Pad2)")
  (net 25 "Net-(D7-Pad2)")
  (net 26 "Net-(D8-Pad2)")
  (net_class Default "Esta é a classe de net default."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad17)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad9)")
    (add_net VCC)
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5984B110)
    (at 231.14 118.11)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D8 (at 1.27 -3.175) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 "Net-(D8-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 26 "Net-(D8-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_THT:Resistor_Array_SIP9 (layer F.Cu) (tedit 57FA3974)
    (at 194.31 108.585)
    (descr "9-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 11.43 -2.4) (layer F.SilkS))
    (fp_text value R_Network08 (at 11.43 2.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad3)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad5)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad7)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad9)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad11)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad13)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad15)"))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(P1-Pad17)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Array_SIP9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x09 (layer F.Cu) (tedit 5984B1BC)
    (at 194.31 105.41 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value CONN_02X09 (at 2.54 27.94 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(D4-Pad1)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(D7-Pad1)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(P1-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(D8-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x09.wrl
      (at (xyz 0.05 -0.4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5984B0EE)
    (at 177.8 118.11)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at 1.27 -3.175) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 19 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5984B0F3)
    (at 185.42 118.11)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at 1.27 -3.175) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 20 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5984B0FB)
    (at 193.04 118.11)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.27 -3.175) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 21 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5984B0FF)
    (at 200.66 118.11)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D4 (at 1.27 -3.175) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 22 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5984B104)
    (at 208.28 118.11)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D5 (at 1.27 -3.175 180) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 23 "Net-(D5-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5984B108)
    (at 215.9 118.11)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D6 (at 1.27 -3.175) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 24 "Net-(D6-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5984B10C)
    (at 223.52 118.11)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D7 (at 1.27 -3.175) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 8 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 25 "Net-(D7-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_THT:Resistor_Array_SIP9 (layer F.Cu) (tedit 57FA3974)
    (at 194.31 111.76)
    (descr "9-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN2 (at 11.43 -2.4) (layer F.SilkS))
    (fp_text value R_Network08 (at 11.43 2.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(D2-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(D3-Pad2)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(D4-Pad2)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(D5-Pad2)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(D6-Pad2)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(D7-Pad2)"))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(D8-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Array_SIP9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5984B0B6)
    (at 176.53 128.27 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.81 2.54 180) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad3)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5984B0BD)
    (at 184.15 128.27 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW2 (at 3.81 2.54 180) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad5)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad5)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5984B0C3)
    (at 191.77 128.27 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW3 (at 3.81 2.54 180) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad7)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad7)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5984B0C9)
    (at 199.39 128.27 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW4 (at 3.81 2.54 180) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad9)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad9)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5984B0CD)
    (at 207.01 128.27 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW5 (at 3.81 2.54 180) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad11)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad11)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5984B0D4)
    (at 214.63 128.27 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW6 (at 3.81 2.54 180) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad13)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad13)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5984B0D8)
    (at 222.25 128.27 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW7 (at 3.81 2.54 180) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad15)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad15)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5984B0DE)
    (at 229.87 128.27 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW8 (at 3.81 2.54 180) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(P1-Pad17)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(P1-Pad17)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 217.805 112.395) (end 217.805 113.665) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 191.135 112.395) (end 192.405 112.395) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.07 113.665) (end 191.135 113.665) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 192.405 107.315) (end 192.405 112.395) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 216.535 107.315) (end 216.535 112.395) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.805 113.665) (end 231.775 113.665) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 192.405 100.965) (end 216.535 100.965) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.5 105.41) (end 190.5 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 218.44 105.41) (end 218.44 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 236.22 128.27) (end 236.22 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.53 130.175) (end 234.315 130.175) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.625 118.11) (end 174.625 128.27) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 176.53 128.27) (end 176.53 130.175) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 234.315 128.27) (end 236.22 128.27) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 231.775 118.11) (end 231.775 113.665) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 179.07 118.11) (end 174.625 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 216.535 105.41) (end 218.44 105.41) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 192.405 105.41) (end 192.405 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 216.535 102.87) (end 216.535 100.965) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 192.405 102.87) (end 190.5 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text - (at 191.77 102.87) (layer F.SilkS))
  (gr_text L (at 217.17 102.87) (layer F.SilkS))
  (gr_text + (at 191.77 105.41) (layer F.SilkS))
  (gr_text B (at 217.17 105.41) (layer F.SilkS))
)
