<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>+5V</text>
<text>+5V</text>
<text>GND</text>
<text>GND</text>
<text>VIN</text>
<text>SOLDER 5V
SUBMODULE
HERE</text>
<text>ON</text>
<text>1000MA</text>
<text>250MA</text>
<text>50MA</text>
<text>POS</text>
<text>NEG</text>
<text>5V REGULATOR TEST BOARD | TIM KOSTKA | 2016-OCT-19</text>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="36.83" y2="0" width="0" layer="20"/>
<wire x1="36.83" y1="0" x2="36.83" y2="25.4" width="0" layer="20"/>
<wire x1="36.83" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<text>JST
BATTERY</text>
<text>1 OHM</text>
<text>1 OHM</text>
<text>100 OHM</text>
<text>10 OHM</text>
<text>10 OHM</text>
<text>1 OHM</text>
<text>1 OHM</text>
<text>1 OHM</text>
<text>0.1 OHM</text>
</plain>
<libraries>
<library name="kcl_pdb360">
<packages>
<package name="CASTELLATION-BASE">
</package>
</packages>
</library>
<library name="kcl_passives">
<packages>
<package name="RES2512R">
<description>Vishay CRCW series, reflow.</description>
</package>
</packages>
</library>
<library name="kcl_connectors_auto">
<packages>
<package name="SAM-TSW-102-XX-X-S">
</package>
<package name="SAM-TSW-103-XX-X-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J5" library="kcl_pdb360" package="CASTELLATION-BASE" value="TPCASTELLATION-BASE"/>
<element name="J7" library="kcl_pdb360" package="CASTELLATION-BASE" value="TPCASTELLATION-BASE"/>
<element name="J8" library="kcl_pdb360" package="CASTELLATION-BASE" value="TPCASTELLATION-BASE"/>
<element name="J9" library="kcl_pdb360" package="CASTELLATION-BASE" value="TPCASTELLATION-BASE"/>
<element name="J10" library="kcl_pdb360" package="CASTELLATION-BASE" value="TPCASTELLATION-BASE"/>
<element name="R1" library="kcl_passives" package="RES2512R" value="1">
<attribute name="PN" value="CRCW25121R00FKEG"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="kcl_passives" package="RES2512R" value="1">
<attribute name="PN" value="CRCW25121R00FKEG"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="kcl_passives" package="RES2512R" value="1">
<attribute name="PN" value="CRCW25121R00FKEG"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="kcl_passives" package="RES2512R" value="1">
<attribute name="PN" value="CRCW25121R00FKEG"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="kcl_passives" package="RES2512R" value="1">
<attribute name="PN" value="CRCW25121R00FKEG"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="kcl_passives" package="RES2512R" value="10">
<attribute name="PN" value="CRCW251210R0FKEG"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="kcl_passives" package="RES2512R" value="10">
<attribute name="PN" value="CRCW251210R0FKEG"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="kcl_passives" package="RES2512R" value="100">
<attribute name="PN" value="CRCW2512100RFKEG"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="kcl_connectors_auto" package="SAM-TSW-103-XX-X-S" value="CONN3TSW-S">
<attribute name="PN" value="TSW-101-07-F-S"/>
</element>
<element name="J2" library="kcl_connectors_auto" package="SAM-TSW-103-XX-X-S" value="CONN3TSW-S">
<attribute name="PN" value="TSW-101-07-F-S"/>
</element>
<element name="J3" library="kcl_connectors_auto" package="SAM-TSW-103-XX-X-S" value="CONN3TSW-S">
<attribute name="PN" value="TSW-101-07-F-S"/>
</element>
<element name="J4" library="kcl_connectors_auto" package="SAM-TSW-102-XX-X-S" value="CONN2TSW-S">
<attribute name="PN" value="TSW-100-07-F-S"/>
</element>
<element name="R9" library="kcl_passives" package="RES2512R" value="0.1">
<attribute name="PN" value="RUT6432FR100CS"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="kcl_connectors_auto" package="SAM-TSW-102-XX-X-S" value="CONN2TSW-S">
<attribute name="PN" value="TSW-100-07-F-S"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J5" pad="1"/>
<contactref element="J7" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="J3" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="VIN">
<contactref element="J10" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="J8" pad="1"/>
<contactref element="J9" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="1"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R9" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="J6" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
