(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 100)
    (no_connects 0)
    (area 93.924999 61.924999 158.075001 117.075001)
    (thickness 1.6)
    (drawings 62)
    (tracks 473)
    (zones 0)
    (modules 38)
    (nets 63)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2.6)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 155 65)
    (visible_elements 7FFFDE7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +5V)
  (net 4 /GPIO2)
  (net 5 /GPIO3)
  (net 6 /GPIO4)
  (net 7 /GPIO17)
  (net 8 /GPIO27)
  (net 9 /GPIO22)
  (net 10 /GPIO23)
  (net 11 /GPIO24)
  (net 12 /GPIO10)
  (net 13 /GPIO25)
  (net 14 /ID_SD)
  (net 15 /ID_SC)
  (net 16 /GPIO6)
  (net 17 /GPIO13)
  (net 18 /GPIO19)
  (net 19 /GPIO16)
  (net 20 /GPIO26)
  (net 21 /GPIO20)
  (net 22 /GPIO21)
  (net 23 "Net-(ID_EEPROM1-Pad7)")
  (net 24 "Net-(temp1-Pad3)")
  (net 25 /PD3)
  (net 26 "Net-(ATMEGA1-Pad2)")
  (net 27 "Net-(ATMEGA1-Pad7)")
  (net 28 "Net-(ATMEGA1-Pad8)")
  (net 29 "Net-(ATMEGA1-Pad9)")
  (net 30 /PD6)
  (net 31 "Net-(ATMEGA1-Pad11)")
  (net 32 "Net-(ATMEGA1-Pad12)")
  (net 33 /PB1)
  (net 34 "Net-(ATMEGA1-Pad14)")
  (net 35 /ADC6)
  (net 36 "Net-(ATMEGA1-Pad22)")
  (net 37 "Net-(ATMEGA1-Pad23)")
  (net 38 "Net-(ATMEGA1-Pad24)")
  (net 39 "Net-(ATMEGA1-Pad25)")
  (net 40 "Net-(ATMEGA1-Pad26)")
  (net 41 "Net-(ATMEGA1-Pad27)")
  (net 42 "Net-(ATMEGA1-Pad28)")
  (net 43 "Net-(ATMEGA1-Pad29)")
  (net 44 "Net-(ATMEGA1-Pad30)")
  (net 45 "Net-(ATMEGA1-Pad31)")
  (net 46 "Net-(ATMEGA1-Pad32)")
  (net 47 /UART_TXD)
  (net 48 "Net-(ATMEGA1-Pad10)")
  (net 49 "Net-(ATMEGA1-Pad20)")
  (net 50 "Net-(led1-PadDOUT)")
  (net 51 "Net-(led2-PadDOUT)")
  (net 52 "Net-(led3-PadDOUT)")
  (net 53 "Net-(led4-PadDOUT)")
  (net 54 "Net-(led5-PadDOUT)")
  (net 55 "Net-(P1-Pad10)")
  (net 56 "Net-(P1-Pad12)")
  (net 57 "Net-(P1-Pad21)")
  (net 58 "Net-(P1-Pad23)")
  (net 59 "Net-(P1-Pad24)")
  (net 60 "Net-(P1-Pad26)")
  (net 61 "Net-(P1-Pad29)")
  (net 62 "Net-(P1-Pad32)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ADC6)
    (add_net /GPIO10)
    (add_net /GPIO13)
    (add_net /GPIO16)
    (add_net /GPIO17)
    (add_net /GPIO19)
    (add_net /GPIO2)
    (add_net /GPIO20)
    (add_net /GPIO21)
    (add_net /GPIO22)
    (add_net /GPIO23)
    (add_net /GPIO24)
    (add_net /GPIO25)
    (add_net /GPIO26)
    (add_net /GPIO27)
    (add_net /GPIO3)
    (add_net /GPIO4)
    (add_net /GPIO6)
    (add_net /ID_SC)
    (add_net /ID_SD)
    (add_net /PB1)
    (add_net /PD3)
    (add_net /PD6)
    (add_net /UART_TXD)
    (add_net GND)
    (add_net "Net-(ATMEGA1-Pad10)")
    (add_net "Net-(ATMEGA1-Pad11)")
    (add_net "Net-(ATMEGA1-Pad12)")
    (add_net "Net-(ATMEGA1-Pad14)")
    (add_net "Net-(ATMEGA1-Pad2)")
    (add_net "Net-(ATMEGA1-Pad20)")
    (add_net "Net-(ATMEGA1-Pad22)")
    (add_net "Net-(ATMEGA1-Pad23)")
    (add_net "Net-(ATMEGA1-Pad24)")
    (add_net "Net-(ATMEGA1-Pad25)")
    (add_net "Net-(ATMEGA1-Pad26)")
    (add_net "Net-(ATMEGA1-Pad27)")
    (add_net "Net-(ATMEGA1-Pad28)")
    (add_net "Net-(ATMEGA1-Pad29)")
    (add_net "Net-(ATMEGA1-Pad30)")
    (add_net "Net-(ATMEGA1-Pad31)")
    (add_net "Net-(ATMEGA1-Pad32)")
    (add_net "Net-(ATMEGA1-Pad7)")
    (add_net "Net-(ATMEGA1-Pad8)")
    (add_net "Net-(ATMEGA1-Pad9)")
    (add_net "Net-(ID_EEPROM1-Pad7)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad21)")
    (add_net "Net-(P1-Pad23)")
    (add_net "Net-(P1-Pad24)")
    (add_net "Net-(P1-Pad26)")
    (add_net "Net-(P1-Pad29)")
    (add_net "Net-(P1-Pad32)")
    (add_net "Net-(led1-PadDOUT)")
    (add_net "Net-(led2-PadDOUT)")
    (add_net "Net-(led3-PadDOUT)")
    (add_net "Net-(led4-PadDOUT)")
    (add_net "Net-(led5-PadDOUT)")
    (add_net "Net-(temp1-Pad3)")
  )
  (module .pretty:Keypad_Ethernet (layer F.Cu) (tedit 5945996E)
    (at 119 79 90)
    (descr "JST J2100 series connector, dual row, center locking, S08B-J21DK-GG, side entry type, through hole")
    (tags "connector jst j2100 horizontal")
    (fp_text reference P3 (at 2.45 3.4 180) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 2.7 6.3 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.45 -5.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 /GPIO25))
    (pad 3 thru_hole circle (at 2 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GPIO10))
    (pad 5 thru_hole circle (at 4 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 11 /GPIO24))
    (pad 7 thru_hole circle (at 6 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GPIO22))
    (pad 2 thru_hole circle (at -1 -2.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GPIO4))
    (pad 4 thru_hole circle (at 1 -2.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GPIO17))
    (pad 6 thru_hole circle (at 3 -2.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GPIO27))
    (pad 8 thru_hole circle (at 5 -2.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 /GPIO23))
    (pad "" thru_hole circle (at -3.8 2.5 90) (size 3.5 3.5) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 8.8 2.5 90) (size 3.5 3.5) (drill 3.25) (layers *.Cu *.Mask))
    (model Connectors_JST.3dshapes/JST_J2100_S08B-J21DK-GG_2x04x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 59482FB8)
    (at 98 75 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference temp1 (at 0 3.2 270) (layer F.SilkS))
    (fp_text value LM75BD (at 0 3.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /GPIO2))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /GPIO3))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(temp1-Pad3)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 594598EB)
    (at 148 76 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference ID_EEPROM1 (at 0 -3.5 180) (layer F.SilkS))
    (fp_text value CAT24C32 (at 0 3.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /ID_SD))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /ID_SC))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(ID_EEPROM1-Pad7)"))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:ATMEGA328P (layer F.Cu) (tedit 59459B36)
    (at 128.5 106 270)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference ATMEGA1 (at 0 0 270) (layer F.SilkS))
    (fp_text value ATMEGA328P-A (at 0 6.05 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.25 -2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 /PD3))
    (pad 2 smd rect (at -4.25 -2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(ATMEGA1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 -0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at -4.25 0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 7 smd rect (at -4.25 2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(ATMEGA1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(ATMEGA1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(ATMEGA1-Pad9)"))
    (pad 10 smd rect (at -2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(ATMEGA1-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(ATMEGA1-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(ATMEGA1-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 /PB1))
    (pad 14 smd rect (at 1.2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(ATMEGA1-Pad14)"))
    (pad 15 smd rect (at 2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /GPIO6))
    (pad 16 smd rect (at 2.8 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /GPIO13))
    (pad 17 smd rect (at 4.25 2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /GPIO19))
    (pad 18 smd rect (at 4.25 2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 19 smd rect (at 4.25 1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 /ADC6))
    (pad 20 smd rect (at 4.25 0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(ATMEGA1-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 -1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(ATMEGA1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(ATMEGA1-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(ATMEGA1-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(ATMEGA1-Pad25)"))
    (pad 26 smd rect (at 2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(ATMEGA1-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(ATMEGA1-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(ATMEGA1-Pad28)"))
    (pad 29 smd rect (at -0.4 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(ATMEGA1-Pad29)"))
    (pad 30 smd rect (at -1.2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(ATMEGA1-Pad30)"))
    (pad 31 smd rect (at -2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(ATMEGA1-Pad31)"))
    (pad 32 smd rect (at -2.8 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(ATMEGA1-Pad32)"))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59459A8D)
    (at 98 80 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -3.5 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59459AB1)
    (at 124.5 98 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 20p (at -3 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(ATMEGA1-Pad7)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59459AA9)
    (at 122.5 98 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value 20p (at -3 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(ATMEGA1-Pad8)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Neo_RGB_LED locked (layer F.Cu) (tedit 5945988D)
    (at 144 89.5 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/HB/Data-Sheets/CLMVBFKA.pdf)
    (tags "LED Cree PLCC-4")
    (attr smd)
    (fp_text reference led1 (at 0 -3.5 450) (layer F.SilkS))
    (fp_text value Neo_LED_RGB_IC (at 0 4 270) (layer F.Fab) hide)
    (pad VDD smd rect (at 2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad DOUT smd rect (at 2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(led1-PadDOUT)"))
    (pad DIN smd rect (at -2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 30 /PD6))
    (pad VSS smd rect (at -2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_Cree-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Neo_RGB_LED locked (layer F.Cu) (tedit 59459897)
    (at 135 89.5 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/HB/Data-Sheets/CLMVBFKA.pdf)
    (tags "LED Cree PLCC-4")
    (attr smd)
    (fp_text reference led2 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value Neo_LED_RGB_IC (at 0 4 270) (layer F.Fab) hide)
    (pad VDD smd rect (at 2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad DOUT smd rect (at 2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(led2-PadDOUT)"))
    (pad DIN smd rect (at -2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(led1-PadDOUT)"))
    (pad VSS smd rect (at -2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_Cree-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Neo_RGB_LED locked (layer F.Cu) (tedit 594598A6)
    (at 126 89.5 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/HB/Data-Sheets/CLMVBFKA.pdf)
    (tags "LED Cree PLCC-4")
    (attr smd)
    (fp_text reference led3 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value Neo_LED_RGB_IC (at 0 4 270) (layer F.Fab) hide)
    (pad VDD smd rect (at 2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad DOUT smd rect (at 2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(led3-PadDOUT)"))
    (pad DIN smd rect (at -2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(led2-PadDOUT)"))
    (pad VSS smd rect (at -2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_Cree-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Neo_RGB_LED locked (layer F.Cu) (tedit 594598AA)
    (at 117 89.5 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/HB/Data-Sheets/CLMVBFKA.pdf)
    (tags "LED Cree PLCC-4")
    (attr smd)
    (fp_text reference led4 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value Neo_LED_RGB_IC (at 0 4 270) (layer F.Fab) hide)
    (pad VDD smd rect (at 2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad DOUT smd rect (at 2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(led4-PadDOUT)"))
    (pad DIN smd rect (at -2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(led3-PadDOUT)"))
    (pad VSS smd rect (at -2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_Cree-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Neo_RGB_LED locked (layer F.Cu) (tedit 5945991C)
    (at 108 89.5 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/HB/Data-Sheets/CLMVBFKA.pdf)
    (tags "LED Cree PLCC-4")
    (attr smd)
    (fp_text reference led5 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value Neo_LED_RGB_IC (at 0 4 270) (layer F.Fab) hide)
    (pad VDD smd rect (at 2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad DOUT smd rect (at 2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(led5-PadDOUT)"))
    (pad DIN smd rect (at -2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(led4-PadDOUT)"))
    (pad VSS smd rect (at -2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_Cree-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:raspiMountingHole locked (layer F.Cu) (tedit 58890667)
    (at 155 114)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference MountHole1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 3.1))
  )
  (module .pretty:raspiMountingHole locked (layer F.Cu) (tedit 594598C1)
    (at 155 65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference MountHole2 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 3.1))
  )
  (module .pretty:raspiMountingHole locked (layer F.Cu) (tedit 59459904)
    (at 97 65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference MountHole3 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 3.1))
  )
  (module .pretty:raspiMountingHole locked (layer F.Cu) (tedit 58890667)
    (at 97 114)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference MountHole4 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 3.1))
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm locked (layer F.Cu) (tedit 59459909)
    (at 102 66.4 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference P1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value RPiGPIO (at 1.27 50.59 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /GPIO2))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GPIO3))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GPIO4))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /UART_TXD))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GPIO17))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GPIO27))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GPIO22))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /GPIO23))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /GPIO24))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GPIO10))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(P1-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /GPIO25))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(P1-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(P1-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(P1-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /ID_SD))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /ID_SC))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(P1-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GPIO6))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(P1-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /GPIO13))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /GPIO19))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /GPIO16))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /GPIO26))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /GPIO20))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /GPIO21))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module .pretty:Piezo_CT-1205h-smt (layer F.Cu) (tedit 5945992A)
    (at 105.5 105.5 270)
    (descr "Diode, Universal, SMA, SMB, Handsoldering,")
    (tags "Diode Universal SMA SMB Handsoldering ")
    (attr smd)
    (fp_text reference PB1 (at 0 -3 270) (layer F.SilkS))
    (fp_text value Piezo (at 0 3 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 5.8 0 270) (size 4 3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -5.8 0 270) (size 4 3) (layers F.Cu F.Paste F.Mask)
      (net 33 /PB1))
    (model Diodes_SMD.3dshapes/D_SMA-SMB_Universal_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module .pretty:R_0805_HandSoldering (layer F.Cu) (tedit 594599C4)
    (at 139 76 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7 90) (layer F.Fab) hide)
    (fp_text value 3.9K (at 4.5 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /ID_SD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:R_0805_HandSoldering (layer F.Cu) (tedit 594599C1)
    (at 142 76 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.7 90) (layer F.Fab) hide)
    (fp_text value 3.9K (at 4.5 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /ID_SC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:R_0805_HandSoldering (layer F.Cu) (tedit 594599CA)
    (at 136 76 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7 90) (layer F.Fab) hide)
    (fp_text value 1K (at 4 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(ID_EEPROM1-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:R_0805_HandSoldering (layer F.Cu) (tedit 5945993F)
    (at 113.5 103.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.7 270) (layer F.Fab) hide)
    (fp_text value 1K (at 0 -2 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /PD6))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(ATMEGA1-Pad10)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:R_0805_HandSoldering (layer F.Cu) (tedit 59459927)
    (at 113.5 109 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.7 90) (layer F.Fab) hide)
    (fp_text value 1K (at 0 2 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /PD6))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(ATMEGA1-Pad10)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:R_0805_HandSoldering (layer F.Cu) (tedit 59459948)
    (at 135.5 101.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.7 270) (layer F.Fab) hide)
    (fp_text value 1K (at 0 1.75 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 /UART_TXD))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(ATMEGA1-Pad30)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:R_0805_HandSoldering (layer F.Cu) (tedit 59459945)
    (at 135.5 110.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.7 90) (layer F.Fab) hide)
    (fp_text value 10K (at 0 1.75 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /GPIO16))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(ATMEGA1-Pad29)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5945995E)
    (at 143.5 108 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference ADC6 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value aux_conn (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /ADC6))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module .pretty:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5945994F)
    (at 150.44 99.07)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference PD3 (at -1.94 1.43 90) (layer F.SilkS))
    (fp_text value aux_conn (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at -1.94 1.43 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /PD3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module .pretty:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59459953)
    (at 154.44 99.07)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference GPIO20 (at 2.56 1.43 90) (layer F.SilkS))
    (fp_text value aux_conn (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 2.56 1.43 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /GPIO20))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module .pretty:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59459957)
    (at 154.5 108 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference GPIO21 (at -2.5 0 270) (layer F.SilkS))
    (fp_text value aux_conn (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at -2.5 0 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /GPIO21))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module .pretty:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5945995A)
    (at 150.5 108 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference GPIO26 (at 2 0 270) (layer F.SilkS))
    (fp_text value aux_conn (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at 2 0 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /GPIO26))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module .pretty:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5945999E)
    (at 143.5 99)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference ISP1 (at -2.44 -0.02 90) (layer F.SilkS))
    (fp_text value ISP (at 1.27 7.41) (layer F.Fab) hide)
    (fp_text user %R (at -2.45 -0.02 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /GPIO13))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /GPIO19))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GPIO6))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /GPIO16))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module .pretty:Crystal_SMD_HC49-SD (layer F.Cu) (tedit 59459923)
    (at 118.5 106 90)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference OSC1 (at 0 -3.55 90) (layer F.Fab) hide)
    (fp_text value "16 MHz Crystal" (at 0 3.55 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -4.25 0 90) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(ATMEGA1-Pad7)"))
    (pad 2 smd rect (at 4.25 0 90) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(ATMEGA1-Pad8)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_HC49-SD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 594598AF)
    (at 150.5 88.25)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(ID_EEPROM1-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module .pretty:Test_Point_2Pads (layer F.Cu) (tedit 594598B3)
    (at 153.75 90.75 90)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference PP1 (at 1.25 1.75 270) (layer F.SilkS))
    (fp_text value horizTest (at 1.27 2 90) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0 90) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd circle (at 2.54 0 90) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(ID_EEPROM1-Pad7)"))
  )
  (module .pretty:makerspace_4,8mm (layer B.Cu) (tedit 0)
    (at 112 89.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module .pretty:ci_wide_6mm (layer B.Cu) (tedit 0)
    (at 104.75 89.25 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module .pretty:tiger_paw_10mm (layer B.Cu) (tedit 0)
    (at 143 89.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module .pretty:AluCap_8mmDia_Nichicon (layer F.Cu) (tedit 5948263F)
    (at 106 75.5)
    (descr "Diode, Universal, SMA, SMB, Handsoldering,")
    (tags "Diode Universal SMA SMB Handsoldering ")
    (attr smd)
    (fp_text reference C2 (at 0 0) (layer F.SilkS))
    (fp_text value 1000uF (at 0 2.05) (layer F.Fab) hide)
    (fp_text user + (at -2.5 -3.5) (layer F.SilkS))
    (fp_text user + (at 2.5 -3.5) (layer F.SilkS))
    (fp_text user - (at -2.5 3.5) (layer F.SilkS))
    (fp_text user - (at 2.5 3.5) (layer F.SilkS))
    (pad 1 smd rect (at 0 -4.15) (size 1.25 3.5) (drill (offset 0 0.9)) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0 4.15) (size 1.25 3.5) (drill (offset 0 -0.9)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Diodes_SMD.3dshapes/D_SMA-SMB_Universal_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text "CATS Keypad Connector\nNot For Ethernet Use" (at 128.8 76.5 90) (layer F.SilkS))
  (gr_text + (at 152.3 85.7) (layer F.SilkS))
  (gr_text VCC (at 146 96.5) (layer F.SilkS))
  (gr_text + (at 150.5 96.5) (layer F.SilkS))
  (gr_text + (at 154.5 96.5) (layer F.SilkS))
  (gr_text + (at 154.5 110.5) (layer F.SilkS))
  (gr_text + (at 150.5 110.5) (layer F.SilkS))
  (gr_text + (at 143.5 110.5) (layer F.SilkS))
  (gr_text "Stefan Abare - Giandre Acosta - Maurice Barnett\nThor Brockman - Brice Grooms - Brad Hord\nJoshua McMillan - Owen Phillips - Garrett Ross" (at 129.9 89.5 270) (layer B.SilkS))
  (gr_text "CATS HAT V0.2.2" (at 127.97 115.39) (layer F.SilkS))
  (dimension 18 (width 0.3) (layer Dwgs.User)
    (gr_text "18.000 mm" (at 149 125.71) (layer Dwgs.User))
    (feature1 (pts (xy 158 117) (xy 158 127.06)))
    (feature2 (pts (xy 140 117) (xy 140 127.06)))
    (crossbar (pts (xy 140 124.36) (xy 158 124.36)))
    (arrow1a (pts (xy 158 124.36) (xy 156.873496 124.946421)))
    (arrow1b (pts (xy 158 124.36) (xy 156.873496 123.773579)))
    (arrow2a (pts (xy 140 124.36) (xy 141.126504 124.946421)))
    (arrow2b (pts (xy 140 124.36) (xy 141.126504 123.773579)))
  )
  (dimension 2 (width 0.3) (layer Dwgs.User)
    (gr_text "2.000 mm" (at 139 93.39) (layer Dwgs.User))
    (feature1 (pts (xy 140 97) (xy 140 92.04)))
    (feature2 (pts (xy 138 97) (xy 138 92.04)))
    (crossbar (pts (xy 138 94.74) (xy 140 94.74)))
    (arrow1a (pts (xy 140 94.74) (xy 138.873496 95.326421)))
    (arrow1b (pts (xy 140 94.74) (xy 138.873496 94.153579)))
    (arrow2a (pts (xy 138 94.74) (xy 139.126504 95.326421)))
    (arrow2b (pts (xy 138 94.74) (xy 139.126504 94.153579)))
  )
  (dimension 44 (width 0.3) (layer Dwgs.User)
    (gr_text "44.000 mm" (at 116 125.72) (layer Dwgs.User))
    (feature1 (pts (xy 138 117) (xy 138 127.07)))
    (feature2 (pts (xy 94 117) (xy 94 127.07)))
    (crossbar (pts (xy 94 124.37) (xy 138 124.37)))
    (arrow1a (pts (xy 138 124.37) (xy 136.873496 124.956421)))
    (arrow1b (pts (xy 138 124.37) (xy 136.873496 123.783579)))
    (arrow2a (pts (xy 94 124.37) (xy 95.126504 124.956421)))
    (arrow2b (pts (xy 94 124.37) (xy 95.126504 123.783579)))
  )
  (dimension 55 (width 0.3) (layer Dwgs.User)
    (gr_text "55.000 mm" (at 168.35 89.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 157.6 117) (xy 169.7 117)))
    (feature2 (pts (xy 157.6 62) (xy 169.7 62)))
    (crossbar (pts (xy 167 62) (xy 167 117)))
    (arrow1a (pts (xy 167 117) (xy 166.413579 115.873496)))
    (arrow1b (pts (xy 167 117) (xy 167.586421 115.873496)))
    (arrow2a (pts (xy 167 62) (xy 166.413579 63.126504)))
    (arrow2b (pts (xy 167 62) (xy 167.586421 63.126504)))
  )
  (target plus (at 126 89.5) (size 5) (width 0.15) (layer Edge.Cuts))
  (gr_line (start 136.5 117) (end 97 117) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 29 (width 0.3) (layer Dwgs.User)
    (gr_text "29.000 mm" (at 111.5 74.35) (layer Dwgs.User))
    (feature1 (pts (xy 126 65) (xy 126 75.7)))
    (feature2 (pts (xy 97 65) (xy 97 75.7)))
    (crossbar (pts (xy 97 73) (xy 126 73)))
    (arrow1a (pts (xy 126 73) (xy 124.873496 73.586421)))
    (arrow1b (pts (xy 126 73) (xy 124.873496 72.413579)))
    (arrow2a (pts (xy 97 73) (xy 98.126504 73.586421)))
    (arrow2b (pts (xy 97 73) (xy 98.126504 72.413579)))
  )
  (gr_line (start 141.5 117) (end 155 117) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 6.4 (width 0.3) (layer Dwgs.User)
    (gr_text "6.400 mm" (at 155 54.45) (layer Dwgs.User))
    (feature1 (pts (xy 158.2 65) (xy 158.2 53.1)))
    (feature2 (pts (xy 151.8 65) (xy 151.8 53.1)))
    (crossbar (pts (xy 151.8 55.8) (xy 158.2 55.8)))
    (arrow1a (pts (xy 158.2 55.8) (xy 157.073496 56.386421)))
    (arrow1b (pts (xy 158.2 55.8) (xy 157.073496 55.213579)))
    (arrow2a (pts (xy 151.8 55.8) (xy 152.926504 56.386421)))
    (arrow2b (pts (xy 151.8 55.8) (xy 152.926504 55.213579)))
  )
  (dimension 2.74 (width 0.3) (layer Dwgs.User)
    (gr_text "2.740 mm" (at 151.33 65 90) (layer Dwgs.User))
    (feature1 (pts (xy 155 63.63) (xy 149.98 63.63)))
    (feature2 (pts (xy 155 66.37) (xy 149.98 66.37)))
    (crossbar (pts (xy 152.68 66.37) (xy 152.68 63.63)))
    (arrow1a (pts (xy 152.68 63.63) (xy 153.266421 64.756504)))
    (arrow1b (pts (xy 152.68 63.63) (xy 152.093579 64.756504)))
    (arrow2a (pts (xy 152.68 66.37) (xy 153.266421 65.243496)))
    (arrow2b (pts (xy 152.68 66.37) (xy 152.093579 65.243496)))
  )
  (gr_line (start 138 98) (end 138 115.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 115.5) (end 140 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 98) (end 140 115.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 141.5 115.5) (end 141.5 117) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 136.5 115.5) (end 138 115.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139 98) (end 138 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139 98) (end 139 97) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 17 (width 0.3) (layer Dwgs.User)
    (gr_text "17.000 mm" (at 151.35 105.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 142.5 114) (xy 152.7 114)))
    (feature2 (pts (xy 142.5 97) (xy 152.7 97)))
    (crossbar (pts (xy 150 97) (xy 150 114)))
    (arrow1a (pts (xy 150 114) (xy 149.413579 112.873496)))
    (arrow1b (pts (xy 150 114) (xy 150.586421 112.873496)))
    (arrow2a (pts (xy 150 97) (xy 149.413579 98.126504)))
    (arrow2b (pts (xy 150 97) (xy 150.586421 98.126504)))
  )
  (dimension 11.5 (width 0.3) (layer Dwgs.User)
    (gr_text "11.500 mm" (at 129.15 111.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 135.5 105.5) (xy 127.8 105.5)))
    (feature2 (pts (xy 135.5 117) (xy 127.8 117)))
    (crossbar (pts (xy 130.5 117) (xy 130.5 105.5)))
    (arrow1a (pts (xy 130.5 105.5) (xy 131.086421 106.626504)))
    (arrow1b (pts (xy 130.5 105.5) (xy 129.913579 106.626504)))
    (arrow2a (pts (xy 130.5 117) (xy 131.086421 115.873496)))
    (arrow2b (pts (xy 130.5 117) (xy 129.913579 115.873496)))
  )
  (gr_line (start 98 97.5) (end 95 97.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99 82.5) (end 99 96.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98 81.5) (end 95 81.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 98 82.5) (end 98 81.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 98 96.5) (end 99 96.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94 65) (end 94 80.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94 98.5) (end 94 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 95 98.5) (end 94 98.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 95 80.5) (end 95 81.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 5 (width 0.3) (layer Dwgs.User)
    (gr_text "5.000 mm" (at 96.5 100.85) (layer Dwgs.User))
    (feature1 (pts (xy 99 97.5) (xy 99 102.2)))
    (feature2 (pts (xy 94 97.5) (xy 94 102.2)))
    (crossbar (pts (xy 94 99.5) (xy 99 99.5)))
    (arrow1a (pts (xy 99 99.5) (xy 97.873496 100.086421)))
    (arrow1b (pts (xy 99 99.5) (xy 97.873496 98.913579)))
    (arrow2a (pts (xy 94 99.5) (xy 95.126504 100.086421)))
    (arrow2b (pts (xy 94 99.5) (xy 95.126504 98.913579)))
  )
  (dimension 5 (width 0.3) (layer Dwgs.User)
    (gr_text "5.000 mm" (at 96.5 77.150001) (layer Dwgs.User))
    (feature1 (pts (xy 99 81.5) (xy 99 75.800001)))
    (feature2 (pts (xy 94 81.5) (xy 94 75.800001)))
    (crossbar (pts (xy 94 78.500001) (xy 99 78.500001)))
    (arrow1a (pts (xy 99 78.500001) (xy 97.873496 79.086422)))
    (arrow1b (pts (xy 99 78.500001) (xy 97.873496 77.91358)))
    (arrow2a (pts (xy 94 78.500001) (xy 95.126504 79.086422)))
    (arrow2b (pts (xy 94 78.500001) (xy 95.126504 77.91358)))
  )
  (dimension 19.5 (width 0.3) (layer Dwgs.User)
    (gr_text "19.500 mm" (at 86.15 71.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 97 81.5) (xy 84.8 81.5)))
    (feature2 (pts (xy 97 62) (xy 84.8 62)))
    (crossbar (pts (xy 87.5 62) (xy 87.5 81.5)))
    (arrow1a (pts (xy 87.5 81.5) (xy 86.913579 80.373496)))
    (arrow1b (pts (xy 87.5 81.5) (xy 88.086421 80.373496)))
    (arrow2a (pts (xy 87.5 62) (xy 86.913579 63.126504)))
    (arrow2b (pts (xy 87.5 62) (xy 88.086421 63.126504)))
  )
  (dimension 19.5 (width 0.3) (layer Dwgs.User)
    (gr_text "19.500 mm" (at 86.15 107.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 97 97.5) (xy 84.8 97.5)))
    (feature2 (pts (xy 97 117) (xy 84.8 117)))
    (crossbar (pts (xy 87.5 117) (xy 87.5 97.5)))
    (arrow1a (pts (xy 87.5 97.5) (xy 88.086421 98.626504)))
    (arrow1b (pts (xy 87.5 97.5) (xy 86.913579 98.626504)))
    (arrow2a (pts (xy 87.5 117) (xy 88.086421 115.873496)))
    (arrow2b (pts (xy 87.5 117) (xy 86.913579 115.873496)))
  )
  (dimension 58 (width 0.3) (layer Dwgs.User)
    (gr_text "58.000 mm" (at 126 122.35) (layer Dwgs.User))
    (feature1 (pts (xy 155 117) (xy 155 123.7)))
    (feature2 (pts (xy 97 117) (xy 97 123.7)))
    (crossbar (pts (xy 97 121) (xy 155 121)))
    (arrow1a (pts (xy 155 121) (xy 153.873496 121.586421)))
    (arrow1b (pts (xy 155 121) (xy 153.873496 120.413579)))
    (arrow2a (pts (xy 97 121) (xy 98.126504 121.586421)))
    (arrow2b (pts (xy 97 121) (xy 98.126504 120.413579)))
  )
  (dimension 49 (width 0.3) (layer Dwgs.User)
    (gr_text "49.000 mm" (at 162.35 89.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 158 114) (xy 163.7 114)))
    (feature2 (pts (xy 158 65) (xy 163.7 65)))
    (crossbar (pts (xy 161 65) (xy 161 114)))
    (arrow1a (pts (xy 161 114) (xy 160.413579 112.873496)))
    (arrow1b (pts (xy 161 114) (xy 161.586421 112.873496)))
    (arrow2a (pts (xy 161 65) (xy 160.413579 66.126504)))
    (arrow2b (pts (xy 161 65) (xy 161.586421 66.126504)))
  )
  (dimension 58 (width 0.3) (layer Dwgs.User)
    (gr_text "58.000 mm" (at 126 58.65) (layer Dwgs.User))
    (feature1 (pts (xy 155 62) (xy 155 57.3)))
    (feature2 (pts (xy 97 62) (xy 97 57.3)))
    (crossbar (pts (xy 97 60) (xy 155 60)))
    (arrow1a (pts (xy 155 60) (xy 153.873496 60.586421)))
    (arrow1b (pts (xy 155 60) (xy 153.873496 59.413579)))
    (arrow2a (pts (xy 97 60) (xy 98.126504 60.586421)))
    (arrow2b (pts (xy 97 60) (xy 98.126504 59.413579)))
  )
  (dimension 49 (width 0.3) (layer Dwgs.User)
    (gr_text "49.000 mm" (at 90.65 89.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 94 65) (xy 89.3 65)))
    (feature2 (pts (xy 94 114) (xy 89.3 114)))
    (crossbar (pts (xy 92 114) (xy 92 65)))
    (arrow1a (pts (xy 92 65) (xy 92.586421 66.126504)))
    (arrow1b (pts (xy 92 65) (xy 91.413579 66.126504)))
    (arrow2a (pts (xy 92 114) (xy 92.586421 112.873496)))
    (arrow2b (pts (xy 92 114) (xy 91.413579 112.873496)))
  )
  (gr_arc (start 97 114) (end 97 117) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155 114) (end 158 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 71) (end 158 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 65) (end 158 71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 97 65) (end 94 65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155 65) (end 155 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97 62) (end 155 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 158 62) (xy 94 62) (xy 94 117) (xy 158 117)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 158 117) (xy 140 117) (xy 140 97) (xy 138 97) (xy 138 117)
        (xy 94 117) (xy 94 97.5) (xy 99.2 97.5) (xy 99.2 81.6) (xy 94 81.6)
        (xy 94 62) (xy 158 62)
      )
    )
  )
)
