(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 45)
    (tracks 27)
    (zones 0)
    (modules 25)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.4 1.4)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 133 77)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(R10-Pad1)")
  (net 2 "Net-(R11-Pad1)")
  (net 3 "Net-(R1-Pad1)")
  (net 4 "Net-(R2-Pad1)")
  (net 5 "Net-(R3-Pad1)")
  (net 6 "Net-(R4-Pad1)")
  (net 7 "Net-(R5-Pad1)")
  (net 8 "Net-(R6-Pad1)")
  (net 9 "Net-(R9-Pad1)")
  (net 10 "Net-(R7-Pad1)")
  (net 11 "Net-(R8-Pad1)")
  (net 12 "Net-(R12-Pad1)")
  (net 13 "Net-(C1-Pad1)")
  (net 14 "Net-(C1-Pad2)")
  (net 15 "Net-(C2-Pad2)")
  (net 16 "Net-(C2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class signal ""
    (clearance 0.15)
    (trace_width 0.6096)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
  )
  (module Load-PCB:C_Load-5p (layer F.Cu) (tedit 6043B8C3)
    (at 108.375 65)
    (descr "C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 10.00mm  length 13mm width 8mm Capacitor")
    (fp_text reference C1 (at 5 0) (layer F.SilkS))
    (fp_text value C (at 5 5.25) (layer F.Fab))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 10 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.step
      (offset (xyz 2.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:C_Load-5p (layer F.Cu) (tedit 6043B8C3)
    (at 157.625 65 180)
    (descr "C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 10.00mm  length 13mm width 8mm Capacitor")
    (fp_text reference C2 (at 5 0) (layer F.SilkS))
    (fp_text value C (at 5 5.25) (layer F.Fab))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.step
      (offset (xyz 2.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 135.1 54.2 15)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 1.7 -1.1 15 unlocked) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37 15) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 15) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 15) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 140.9 64.1)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 1.8 1.5) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 130.9 69.8 195)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 1.2 -1.8 15) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37 15) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 15) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 195) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 195) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 127.3 67.7 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 1.8 -1.5) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 125.1 64.1 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 1.9 -1.6) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 125.1 59.9 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 1.7 1.5) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 127.2 56.3 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 1.5 1.5) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 130.9 54.2 165)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 1.7 1.1 -15 unlocked) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37 165) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 165) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 165) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 165) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 138.8 56.3)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 1.6 -1.6) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 140.9 59.9)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 1.6 -1.35) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 138.7 67.7)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 1.7 1.5 180) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:R_Axial_Load_L6.3mm_D2.5mm_P2.54mm (layer F.Cu) (tedit 6018694E)
    (at 135.05 69.75 345)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 1.25 1.85 165) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37 165) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 165) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 345) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 345) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:Grayhill_56_12 (layer F.Cu) (tedit 60196EF8)
    (at 133 62 270)
    (fp_text reference SW1 (at -2 -0.1) (layer F.SilkS) hide)
    (fp_text value SW_Rotary2x6 (at 0 7.345 90) (layer F.Fab))
    (fp_text user 1 (at 5.65 1.5 90) (layer F.SilkS))
    (fp_text user 2 (at 4.2 4.1 90) (layer F.SilkS))
    (fp_text user 3 (at 1.55 5.7 90) (layer F.SilkS))
    (fp_text user 4 (at -1.55 5.7 90) (layer F.SilkS))
    (fp_text user 5 (at -4.15 4.1 90) (layer F.SilkS))
    (fp_text user 6 (at -5.65 1.55 90) (layer F.SilkS))
    (fp_text user 7 (at -5.6 -1.5 90) (layer F.SilkS))
    (fp_text user 8 (at -4.15 -4.15 90) (layer F.SilkS))
    (fp_text user 9 (at -1.5 -5.6 90) (layer F.SilkS))
    (fp_text user 10 (at 1.5 -5.6 90) (layer F.SilkS))
    (fp_text user 11 (at 4.15 -4.2 90) (layer F.SilkS))
    (fp_text user 12 (at 5.67 -1.55 90) (layer F.SilkS))
    (fp_text user 1 (at 5.65 1.5 90) (layer B.SilkS))
    (fp_text user 2 (at 4.2 4.1 90) (layer B.SilkS))
    (fp_text user 3 (at 1.55 5.7 90) (layer B.SilkS))
    (fp_text user 4 (at -1.55 5.7 90) (layer B.SilkS))
    (fp_text user 5 (at -4.15 4.1 90) (layer B.SilkS))
    (fp_text user 6 (at -5.65 1.55 90) (layer B.SilkS))
    (fp_text user 7 (at -5.6 -1.5 90) (layer B.SilkS))
    (fp_text user 8 (at -4.15 -4.15 90) (layer B.SilkS))
    (fp_text user 9 (at -1.5 -5.6 90) (layer B.SilkS))
    (fp_text user 10 (at 1.5 -5.6 90) (layer B.SilkS))
    (fp_text user 11 (at 4.15 -4.2 90) (layer B.SilkS))
    (fp_text user 12 (at 5.67 -1.55 90) (layer B.SilkS))
    (pad 14 thru_hole circle (at 0 -2.415 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad2)"))
    (pad 13 thru_hole circle (at 0 2.415 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C1-Pad2)"))
    (pad 12 thru_hole circle (at 4.491555 -1.203508 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R12-Pad1)"))
    (pad 11 thru_hole circle (at 3.288046 -3.288046 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(R11-Pad1)"))
    (pad 10 thru_hole circle (at 1.203508 -4.491555 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(R10-Pad1)"))
    (pad 9 thru_hole circle (at -1.203508 -4.491555 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R9-Pad1)"))
    (pad 8 thru_hole circle (at -3.288046 -3.288046 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R8-Pad1)"))
    (pad 7 thru_hole circle (at -4.491555 -1.203508 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R7-Pad1)"))
    (pad 6 thru_hole circle (at -4.491555 1.203508 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R6-Pad1)"))
    (pad 5 thru_hole circle (at -3.288046 3.288046 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(R5-Pad1)"))
    (pad 4 thru_hole circle (at -1.203508 4.491555 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(R4-Pad1)"))
    (pad 3 thru_hole circle (at 1.203508 4.491555 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 3.288046 3.288046 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(R2-Pad1)"))
    (pad 1 thru_hole circle (at 4.491555 1.203508 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(R1-Pad1)"))
    (model ${KIPRJMOD}/lib/3D/56sdp30-01-2-xxx.stp
      (offset (xyz 0 0 7.9))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 108.5 55.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 157.5 55.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Load-PCB:PinHeader_1x1_Horizontal locked (layer F.Cu) (tedit 60454BA3)
    (at 116.375 72.9 270)
    (descr "Through hole angled pin header, 1x01, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x01 2.54mm single row")
    (fp_text reference P1 (at 2.7 -2.125 90) (layer F.SilkS))
    (fp_text value Pad (at 4.385 2.27 90) (layer F.Fab))
    (fp_text user %R (at 2.77 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:PinHeader_1x1_Horizontal locked (layer F.Cu) (tedit 60454BA3)
    (at 149.625 72.9 270)
    (descr "Through hole angled pin header, 1x01, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x01 2.54mm single row")
    (fp_text reference P2 (at 2.7 2.025 90) (layer F.SilkS))
    (fp_text value Pad (at 4.385 2.27 90) (layer F.Fab))
    (fp_text user %R (at 2.77 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:PinHeader_1x1_Horizontal locked (layer F.Cu) (tedit 60454BA3)
    (at 106.375 72.9 270)
    (descr "Through hole angled pin header, 1x01, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x01 2.54mm single row")
    (fp_text reference P3 (at 2.7 -2.225 90) (layer F.SilkS))
    (fp_text value Pad (at 4.385 2.27 90) (layer F.Fab))
    (fp_text user %R (at 2.77 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:PinHeader_1x1_Horizontal locked (layer F.Cu) (tedit 60454BA3)
    (at 159.625 72.9 270)
    (descr "Through hole angled pin header, 1x01, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x01 2.54mm single row")
    (fp_text reference P4 (at 2.7 2.025 90) (layer F.SilkS))
    (fp_text value Pad (at 4.385 2.27 90) (layer F.Fab))
    (fp_text user %R (at 2.77 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Load-PCB:THTPad_D1.7_Drill1 locked (layer F.Cu) (tedit 6045521B)
    (at 116.375 75.5 270)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference P5 (at 0 -1.998 90) (layer F.SilkS) hide)
    (fp_text value PadB (at 0 2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C1-Pad2)"))
  )
  (module Load-PCB:THTPad_D1.7_Drill1 locked (layer F.Cu) (tedit 6045521B)
    (at 106.375 75.5 270)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference P6 (at 0 -1.998 90) (layer F.SilkS) hide)
    (fp_text value PadB (at 0 2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(C1-Pad1)"))
  )
  (module Load-PCB:THTPad_D1.7_Drill1 locked (layer F.Cu) (tedit 6045521B)
    (at 149.625 75.475 90)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference P7 (at 0 -1.998 90) (layer F.SilkS) hide)
    (fp_text value PadB (at 0 2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad2)"))
  )
  (module Load-PCB:THTPad_D1.7_Drill1 locked (layer F.Cu) (tedit 6045521B)
    (at 159.65 75.5 90)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference P8 (at 0 -1.998 90) (layer F.SilkS) hide)
    (fp_text value PadB (at 0 2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C2-Pad1)"))
  )
  (gr_line (start 161 77) (end 105 77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 161 52) (end 161 77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105 52) (end 161 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105 77) (end 105 52) (layer Edge.Cuts) (width 0.05))
  (gr_text P4 (at 157.8 73.9) (layer B.SilkS))
  (gr_text P2 (at 147.8 73.9) (layer B.SilkS))
  (gr_text P1 (at 118.1 73.9) (layer B.SilkS))
  (gr_text P3 (at 108.2 73.9) (layer B.SilkS))
  (gr_text R12 (at 135.5 71.4) (layer B.SilkS))
  (gr_text R11 (at 139.9 69) (layer B.SilkS))
  (gr_text R10 (at 142.1 65.4) (layer B.SilkS))
  (gr_text R9 (at 141.9 58.6) (layer B.SilkS))
  (gr_text R8 (at 140 54.9) (layer B.SilkS))
  (gr_text R7 (at 136 52.9) (layer B.SilkS))
  (gr_text R6 (at 130 52.8) (layer B.SilkS))
  (gr_text R5 (at 125.9 54.9) (layer B.SilkS))
  (gr_text R4 (at 123.7 58.6) (layer B.SilkS))
  (gr_text R3 (at 123.7 65.5) (layer B.SilkS))
  (gr_text R2 (at 125.8 69) (layer B.SilkS))
  (gr_text R1 (at 129.9 71.3) (layer B.SilkS))
  (zone (net 16) (net_name "Net-(C2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.9 52.8) (xy 136.9 53.6) (xy 136.9 70.1) (xy 137.5 71.2) (xy 150.6 71.2)
        (xy 159.3 76.3) (xy 160.5 75.6) (xy 160.5 73.8) (xy 160.5 72) (xy 158.6 64.7)
        (xy 157.9 64)
      )
    )
  )
  (zone (net 13) (net_name "Net-(C1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.1 70) (xy 129.1 53.6) (xy 128.1 52.8) (xy 108 64) (xy 107.4 64.7)
        (xy 105.5 72) (xy 105.5 73.8) (xy 105.5 75.5) (xy 106.8 76.3) (xy 115.5 71.2)
        (xy 128.5 71.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.7 71.2) (xy 126.7 68.3) (xy 124.3 64.6) (xy 124.3 59.7) (xy 126.8 55.5)
        (xy 129.9 53.5) (xy 136.1 53.5) (xy 139.2 55.5) (xy 141.6 59.6) (xy 141.6 64.2)
        (xy 139.3 68.2) (xy 135.2 71.2)
      )
    )
  )
)
