<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="83.82" y1="-5.969" x2="83.82" y2="129.54" width="0" layer="20"/>
<wire x1="83.82" y1="129.54" x2="0" y2="129.54" width="0" layer="20"/>
<wire x1="0" y1="129.54" x2="0" y2="-5.969" width="0" layer="20"/>
<wire x1="0" y1="-5.969" x2="83.82" y2="-5.969" width="0" layer="20"/>
<text>OpenAg
Signal PCB v1.1</text>
<text>RESET</text>
<text>Mega</text>
<text>GND</text>
<text>GND</text>
<text>+5V</text>
<text>+5V</text>
<text>2-sided PC board</text>
<text>0.062"-Thick material</text>
<text>1/2-Ounce copper</text>
<text>Exclude solder mask from vias</text>
<text>Exclude silkscreen from pads</text>
<text>Blue solder mask</text>
<text>Omit any lettering too small to
clearly render on silkscreen layers</text>
<text>k</text>
<text>1</text>
<text>1</text>
<text>+5V</text>
<text>GND</text>
<text>D6</text>
<text>GND</text>
<text>+5V</text>
<text>D7</text>
<text>GND</text>
<text>+5V</text>
<text>D8</text>
<text>GND</text>
<text>+5V</text>
<text>D9</text>
<text>GND</text>
<text>+5V</text>
<text>D10</text>
<text>GND</text>
<text>+5V</text>
<text>D5</text>
<text>GND</text>
<text>+5</text>
<text>D4</text>
<text>GND</text>
<text>+5V</text>
<text>D3</text>
<text>GND</text>
<text>+5V</text>
<text>A7</text>
<text>GND</text>
<text>+5V</text>
<text>SD</text>
<text>CK</text>
<text>GND</text>
<text>+5V</text>
<text>SD</text>
<text>CK</text>
<text>GND</text>
<text>+5V</text>
<text>SD</text>
<text>CK</text>
<text>GND</text>
<text>+5V</text>
<text>SD</text>
<text>CK</text>
<text>GND</text>
<text>+5V</text>
<text>SD</text>
<text>CK</text>
<text>GND</text>
<text>+5V</text>
<text>SD</text>
<text>CK</text>
<text>GND</text>
<text>+5V</text>
<text>SD</text>
<text>CK</text>
<text>GND</text>
<text>+5V</text>
<text>RX</text>
<text>TX</text>
<text>GND</text>
<text>+5V</text>
<text>RX</text>
<text>TX</text>
<text>G</text>
<text>+5V</text>
<text>RX</text>
<text>TX</text>
<text>+5V</text>
<text>A6</text>
<text>GND</text>
<text>+5V</text>
<text>A5</text>
<text>GND</text>
<text>+5V</text>
<text>A4</text>
<text>GND</text>
<text>+5V</text>
<text>A3</text>
<text>GND</text>
<text>+5V</text>
<text>A2</text>
<text>GND</text>
<text>+5V</text>
<text>A1</text>
<text>GND</text>
<text>+5V</text>
<text>A0</text>
<text>VCC</text>
<text>PRB</text>
<text>PGND</text>
<text>VCC</text>
<text>PRB</text>
<text>PGND</text>
<text>RX</text>
<text>TX</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>GND</text>
<text>1</text>
<text>2</text>
<text>GND</text>
<text>RST</text>
<text>SCK</text>
<text>MISO</text>
<text>MOSI</text>
<text>STP3</text>
<text>STP4</text>
<text>UM1f</text>
<text>UM1d</text>
<text>UM1e</text>
<text>UM1a</text>
<text>UM1b</text>
<text>UM1c</text>
<text>UM2xa</text>
<text>JP1</text>
<text>JP2</text>
<text>UM2Xb</text>
<text>UM2Xd</text>
<text>UM2Xc</text>
<text>MAN1</text>
</plain>
<libraries>
<library name="REM_Connectors_Molex">
<packages>
<package name="MOLEX_0705430003">
</package>
</packages>
</library>
<library name="REM_Arduino">
<packages>
<package name="ARDUINO_UNO_REV3_SOCKET">
</package>
</packages>
</library>
<library name="REM_AtlasScientific">
<packages>
<package name="ATLAS_SCIENTIFIC_STAMP">
</package>
</packages>
</library>
<library name="REM_DigitalIsolators_SiliconLabs">
<packages>
<package name="SO8ISO">
</package>
</packages>
</library>
<library name="REM_DC_to_DC_Converters_Recom">
<packages>
<package name="RECOM_R1SE_0505_R">
</package>
</packages>
</library>
<library name="REM_VoltageRegulators_ST_Microelectronics">
<packages>
<package name="SOT89">
</package>
</packages>
</library>
<library name="REM_Connectors_Tyco">
<packages>
<package name="BNC_FEMALE_PANEL_RGT_ANGLE_MNT">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="aggregate-parts">
<description>Generated from &lt;b&gt;PartXfer.sch&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="M0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="REM_Capacitors_SurfaceMount_TDK">
<packages>
<package name="M0805">
</package>
</packages>
</library>
<library name="REM_Switches_Grayhill">
<packages>
<package name="GRAYHILL_95CW06C3JRT">
</package>
</packages>
</library>
<library name="arduino_Uno_Rev3-02-TH">
<description>Generated from &lt;b&gt;arduino_Uno_Rev3-02-TH.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="LED_CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="Tyco_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 22/02/2012 09:45:50</description>
<packages>
<package name="RESC1608X60N">
</package>
</packages>
</library>
<library name="adafruitNew">
<packages>
<package name="1X08-BIG">
</package>
</packages>
</library>
<library name="REM_Capacitors_SurfaceMount_AVX">
<packages>
<package name="M2917">
</package>
</packages>
</library>
<library name="REM_Connectors_Generic">
<packages>
<package name="PAD070">
</package>
</packages>
</library>
<library name="REM_ArduinoMega">
<packages>
<package name="ARDUINO_MEGA_2560_R3_CONNECTORS">
<description>Arduino Mega 2560 Rev. 3, side connection headers pattern</description>
</package>
</packages>
</library>
<library name="REM_TactSwitches_Panasonic">
<packages>
<package name="PANASONIC-EVP-AA502W">
</package>
</packages>
</library>
<library name="REM_LEDs_StanleyElectric">
<packages>
<package name="BILED-0605">
</package>
</packages>
</library>
<library name="SmartPrj">
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="I2C_6" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="I2C_7" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="SERIAL_3" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="SERIAL_2" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="SERIAL_1" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="D3" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="D4" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="D5" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="D6" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="D7" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="I2C_5" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="D8" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="I2C_4" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="I2C_3" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="I2C_1" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="I2C_2" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="A3" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="A2" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="A1" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="A0" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="A7" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="A6" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="D9" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="D10" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="A5" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="A4" library="REM_Connectors_Molex" package="MOLEX_0705430003" value="MOLEX_0705430003">
<attribute name="NAME"/>
</element>
<element name="UM1" library="REM_ArduinoMega" package="ARDUINO_MEGA_2560_R3_CONNECTORS" value="ARDUINO_MEGA_2560_R3_SIDES">
<attribute name="NAME"/>
</element>
<element name="UM2" library="REM_Arduino" package="ARDUINO_UNO_REV3_SOCKET" value="ARDUINO_UNO_REV3_SOCKET">
<attribute name="VAL" value="Arduino_Uno_Rev_3"/>
<attribute name="NAME"/>
</element>
<element name="STP1" library="REM_AtlasScientific" package="ATLAS_SCIENTIFIC_STAMP" value="ATLAS_SCIENTIFIC_STAMP">
<attribute name="NAME"/>
</element>
<element name="STP2" library="REM_AtlasScientific" package="ATLAS_SCIENTIFIC_STAMP" value="ATLAS_SCIENTIFIC_STAMP">
<attribute name="NAME"/>
</element>
<element name="SIG_ISO1" library="REM_DigitalIsolators_SiliconLabs" package="SO8ISO" value="SI8600AC-B-IS">
<attribute name="NAME"/>
</element>
<element name="SIG_ISO2" library="REM_DigitalIsolators_SiliconLabs" package="SO8ISO" value="SI8600AC-B-IS">
<attribute name="NAME"/>
</element>
<element name="DCDC1" library="REM_DC_to_DC_Converters_Recom" package="RECOM_R1SE_0505_R" value="RECOM_R1SE_0505_R">
<attribute name="NAME"/>
</element>
<element name="DCDC2" library="REM_DC_to_DC_Converters_Recom" package="RECOM_R1SE_0505_R" value="RECOM_R1SE_0505_R">
<attribute name="NAME"/>
</element>
<element name="REG1" library="REM_VoltageRegulators_ST_Microelectronics" package="SOT89" value="LD2981ABU50TR">
<attribute name="NAME"/>
</element>
<element name="REG2" library="REM_VoltageRegulators_ST_Microelectronics" package="SOT89" value="LD2981ABU50TR">
<attribute name="NAME"/>
</element>
<element name="P1" library="REM_Connectors_Tyco" package="BNC_FEMALE_PANEL_RGT_ANGLE_MNT" value="BNC_TE_1_1337542_0">
<attribute name="NAME"/>
</element>
<element name="P2" library="REM_Connectors_Tyco" package="BNC_FEMALE_PANEL_RGT_ANGLE_MNT" value="BNC_TE_1_1337542_0">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun" package="0805" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="0805" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="0805" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="0805" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="aggregate-parts" package="M0805" value="C-N-100.0N-X7R-25V-10P-0805">
<attribute name="VAL" value="100nF"/>
<attribute name="NAME"/>
</element>
<element name="C9" library="aggregate-parts" package="M0805" value="C-N-100.0N-X7R-25V-10P-0805">
<attribute name="VAL" value="100nF"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun" package="0805" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun" package="0805" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="aggregate-parts" package="M0805" value="C-N-100.0N-X7R-25V-10P-0805">
<attribute name="VAL" value="100nF"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="aggregate-parts" package="M0805" value="C-N-100.0N-X7R-25V-10P-0805">
<attribute name="VAL" value="100nF"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="SparkFun" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="SparkFun" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ4" library="SparkFun" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="REM_Capacitors_SurfaceMount_TDK" package="M0805" value="2.2uF">
<attribute name="VALUE" value="2.2uF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="REM_Capacitors_SurfaceMount_TDK" package="M0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="REM_Switches_Grayhill" package="GRAYHILL_95CW06C3JRT" value="95CW06C3JRT">
<attribute name="NAME"/>
</element>
<element name="PWR" library="arduino_Uno_Rev3-02-TH" package="LED_CHIPLED_0805" value="LED_LEDCHIPLED_0805">
<attribute name="NAME"/>
<attribute name="VAL"/>
</element>
<element name="R11" library="Tyco_By_element14_Batch_1" package="RESC1608X60N" value="1K Ohms">
<attribute name="OC_NEWARK" value="51R8603"/>
<attribute name="TOLERANCE" value="± 1%"/>
<attribute name="MPN" value="CPF0603F1K1C1"/>
<attribute name="SUPPLIER" value="Tyco"/>
<attribute name="OC_FARNELL" value="1527476"/>
<attribute name="WATTAGE" value="0.063W"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="adafruitNew" package="1X08-BIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="adafruitNew" package="1X08-BIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="REM_Capacitors_SurfaceMount_AVX" package="M2917" value="T495X477K010ATE100">
<attribute name="VAL" value="470uF"/>
<attribute name="NAME"/>
</element>
<element name="C12" library="aggregate-parts" package="M0805" value="C-N-100.0N-X7R-25V-10P-0805">
<attribute name="VAL" value="100nF"/>
<attribute name="NAME"/>
</element>
<element name="C13" library="aggregate-parts" package="M0805" value="C-N-100.0N-X7R-25V-10P-0805">
<attribute name="VAL" value="100nF"/>
<attribute name="NAME"/>
</element>
<element name="C14" library="aggregate-parts" package="M0805" value="C-N-100.0N-X7R-25V-10P-0805">
<attribute name="VAL" value="100nF"/>
<attribute name="NAME"/>
</element>
<element name="C15" library="aggregate-parts" package="M0805" value="C-N-100.0N-X7R-25V-10P-0805">
<attribute name="VAL" value="100nF"/>
<attribute name="NAME"/>
</element>
<element name="C16" library="aggregate-parts" package="M0805" value="C-N-100.0N-X7R-25V-10P-0805">
<attribute name="VAL" value="100nF"/>
<attribute name="NAME"/>
</element>
<element name="5VA" library="REM_Connectors_Generic" package="PAD070" value="PAD070">
<attribute name="NAME"/>
</element>
<element name="5VB" library="REM_Connectors_Generic" package="PAD070" value="PAD070">
<attribute name="NAME"/>
</element>
<element name="GNDC" library="REM_Connectors_Generic" package="PAD070" value="PAD070">
<attribute name="NAME"/>
</element>
<element name="GNDD" library="REM_Connectors_Generic" package="PAD070" value="PAD070">
<attribute name="NAME"/>
</element>
<element name="SW2" library="REM_TactSwitches_Panasonic" package="PANASONIC-EVP-AA502W" value="EVP-AA502W">
<attribute name="VAL" value="EVP-AA502W"/>
</element>
<element name="SW3" library="REM_TactSwitches_Panasonic" package="PANASONIC-EVP-AA502W" value="EVP-AA502W">
<attribute name="VAL" value="EVP-AA502W"/>
</element>
<element name="STATUS" library="REM_LEDs_StanleyElectric" package="BILED-0605" value="LED-REDGRN-BRBG1211C">
<attribute name="RNUMBER" value="R00816"/>
<attribute name="VAL" value="BRBG1211C"/>
<attribute name="NAME"/>
</element>
<element name="R12" library="Tyco_By_element14_Batch_1" package="RESC1608X60N" value="1K Ohms">
<attribute name="OC_NEWARK" value="51R8603"/>
<attribute name="TOLERANCE" value="± 1%"/>
<attribute name="MPN" value="CPF0603F1K1C1"/>
<attribute name="SUPPLIER" value="Tyco"/>
<attribute name="OC_FARNELL" value="1527476"/>
<attribute name="WATTAGE" value="0.063W"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="Tyco_By_element14_Batch_1" package="RESC1608X60N" value="1K Ohms">
<attribute name="OC_NEWARK" value="51R8603"/>
<attribute name="TOLERANCE" value="± 1%"/>
<attribute name="MPN" value="CPF0603F1K1C1"/>
<attribute name="SUPPLIER" value="Tyco"/>
<attribute name="OC_FARNELL" value="1527476"/>
<attribute name="WATTAGE" value="0.063W"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GNDA" library="REM_Connectors_Generic" package="PAD070" value="PAD070">
<attribute name="NAME"/>
</element>
<element name="GNDB" library="REM_Connectors_Generic" package="PAD070" value="PAD070">
<attribute name="NAME"/>
</element>
<element name="ICSP" library="SmartPrj" package="2X03" value="3x2M">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="SIG_ISO1" pad="5"/>
<contactref element="SIG_ISO2" pad="5"/>
<contactref element="C10" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="UM2" pad="PWR_GND3"/>
<contactref element="UM2" pad="PWR_GND2"/>
<contactref element="UM2" pad="IOH14"/>
<contactref element="DCDC1" pad="1"/>
<contactref element="DCDC2" pad="1"/>
<contactref element="A7" pad="1"/>
<contactref element="A6" pad="1"/>
<contactref element="A5" pad="1"/>
<contactref element="A4" pad="1"/>
<contactref element="A3" pad="1"/>
<contactref element="A2" pad="1"/>
<contactref element="A1" pad="1"/>
<contactref element="A0" pad="1"/>
<contactref element="UM1" pad="GND1"/>
<contactref element="UM1" pad="GND2"/>
<contactref element="D10" pad="1"/>
<contactref element="D9" pad="1"/>
<contactref element="D8" pad="1"/>
<contactref element="D7" pad="1"/>
<contactref element="D6" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="I2C_1" pad="1"/>
<contactref element="I2C_2" pad="1"/>
<contactref element="I2C_3" pad="1"/>
<contactref element="I2C_4" pad="1"/>
<contactref element="I2C_5" pad="1"/>
<contactref element="I2C_6" pad="1"/>
<contactref element="I2C_7" pad="1"/>
<contactref element="UM1" pad="GND3"/>
<contactref element="SERIAL_3" pad="1"/>
<contactref element="SERIAL_1" pad="1"/>
<contactref element="SERIAL_2" pad="1"/>
<contactref element="SW1" pad="1B"/>
<contactref element="SW1" pad="1A"/>
<contactref element="PWR" pad="C"/>
<contactref element="C11" pad="N"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="GNDC" pad="1"/>
<contactref element="GNDD" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="GNDA" pad="1"/>
<contactref element="GNDB" pad="1"/>
<contactref element="ICSP" pad="6"/>
</signal>
<signal name="VCOM">
<contactref element="SIG_ISO1" pad="8"/>
<contactref element="SIG_ISO2" pad="8"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="UM1" pad="IRF"/>
<contactref element="UM2" pad="PWR_IOREF"/>
</signal>
<signal name="N$9">
<contactref element="R3" pad="1"/>
<contactref element="SIG_ISO2" pad="3"/>
<contactref element="STP2" pad="3"/>
</signal>
<signal name="GND_ISO1">
<contactref element="SIG_ISO1" pad="4"/>
<contactref element="STP1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="DCDC1" pad="4"/>
<contactref element="REG1" pad="2"/>
<contactref element="REG1" pad="TAB"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="GND_ISO2">
<contactref element="SIG_ISO2" pad="4"/>
<contactref element="STP2" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="DCDC2" pad="4"/>
<contactref element="REG2" pad="2"/>
<contactref element="REG2" pad="TAB"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="V_ISO1">
<contactref element="SIG_ISO1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="STP1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="REG1" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="V_ISO2">
<contactref element="SIG_ISO2" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="STP2" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="REG2" pad="1"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="STP1" pad="5"/>
<contactref element="P1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="STP1" pad="6"/>
<contactref element="P1" pad="2"/>
<contactref element="SW2" pad="2"/>
<contactref element="SW2" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="STP2" pad="5"/>
<contactref element="P2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="STP2" pad="6"/>
<contactref element="P2" pad="2"/>
<contactref element="SW3" pad="2"/>
<contactref element="SW3" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="DCDC1" pad="5"/>
<contactref element="REG1" pad="3"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="DCDC2" pad="5"/>
<contactref element="REG2" pad="3"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="A7">
<contactref element="A7" pad="3"/>
<contactref element="UM1" pad="ADL7"/>
</signal>
<signal name="A6">
<contactref element="UM1" pad="ADL6"/>
<contactref element="A6" pad="3"/>
</signal>
<signal name="A5">
<contactref element="A5" pad="3"/>
<contactref element="UM1" pad="ADL5"/>
<contactref element="UM2" pad="AD5"/>
</signal>
<signal name="A4">
<contactref element="A4" pad="3"/>
<contactref element="UM1" pad="ADL4"/>
<contactref element="UM2" pad="AD4"/>
</signal>
<signal name="A3">
<contactref element="A3" pad="3"/>
<contactref element="UM1" pad="ADL3"/>
<contactref element="UM2" pad="AD3"/>
</signal>
<signal name="A2">
<contactref element="A2" pad="3"/>
<contactref element="UM1" pad="ADL2"/>
<contactref element="UM2" pad="AD2"/>
</signal>
<signal name="A1">
<contactref element="A1" pad="3"/>
<contactref element="UM1" pad="ADL1"/>
<contactref element="UM2" pad="AD1"/>
</signal>
<signal name="A0">
<contactref element="A0" pad="3"/>
<contactref element="UM1" pad="ADL0"/>
<contactref element="UM2" pad="AD0"/>
</signal>
<signal name="+5V">
<contactref element="D10" pad="2"/>
<contactref element="D9" pad="2"/>
<contactref element="UM1" pad="P5V"/>
<contactref element="D8" pad="2"/>
<contactref element="D7" pad="2"/>
<contactref element="D6" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="D4" pad="2"/>
<contactref element="D3" pad="2"/>
<contactref element="A0" pad="2"/>
<contactref element="A1" pad="2"/>
<contactref element="A2" pad="2"/>
<contactref element="A3" pad="2"/>
<contactref element="A4" pad="2"/>
<contactref element="A5" pad="2"/>
<contactref element="A6" pad="2"/>
<contactref element="A7" pad="2"/>
<contactref element="I2C_1" pad="2"/>
<contactref element="I2C_2" pad="2"/>
<contactref element="I2C_3" pad="2"/>
<contactref element="I2C_4" pad="2"/>
<contactref element="I2C_5" pad="2"/>
<contactref element="I2C_6" pad="2"/>
<contactref element="I2C_7" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="SERIAL_3" pad="2"/>
<contactref element="SERIAL_2" pad="2"/>
<contactref element="SERIAL_1" pad="2"/>
<contactref element="UM2" pad="PWR_5V"/>
<contactref element="DCDC2" pad="2"/>
<contactref element="DCDC1" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="C11" pad="P"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="5VB" pad="1"/>
<contactref element="5VA" pad="1"/>
<contactref element="ICSP" pad="2"/>
</signal>
<signal name="D3">
<contactref element="UM1" pad="IO3"/>
<contactref element="D3" pad="3"/>
<contactref element="UM2" pad="IOL3"/>
</signal>
<signal name="D4">
<contactref element="D4" pad="3"/>
<contactref element="UM1" pad="IO4"/>
<contactref element="UM2" pad="IOL4"/>
</signal>
<signal name="D5">
<contactref element="UM1" pad="IO5"/>
<contactref element="D5" pad="3"/>
<contactref element="UM2" pad="IOL5"/>
</signal>
<signal name="D6">
<contactref element="UM1" pad="IO6"/>
<contactref element="D6" pad="3"/>
<contactref element="UM2" pad="IOL6"/>
</signal>
<signal name="D7">
<contactref element="UM1" pad="IO7"/>
<contactref element="D7" pad="3"/>
<contactref element="UM2" pad="IOL7"/>
</signal>
<signal name="D8">
<contactref element="D8" pad="3"/>
<contactref element="UM1" pad="IO8"/>
<contactref element="UM2" pad="IOH8"/>
</signal>
<signal name="D9">
<contactref element="UM1" pad="IO9"/>
<contactref element="D9" pad="3"/>
<contactref element="UM2" pad="IOH9"/>
</signal>
<signal name="D10">
<contactref element="UM1" pad="IO10"/>
<contactref element="D10" pad="3"/>
<contactref element="UM2" pad="IOH10"/>
</signal>
<signal name="MTX3">
<contactref element="UM1" pad="IO14"/>
<contactref element="SERIAL_3" pad="4"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="MRX3">
<contactref element="UM1" pad="IO15"/>
<contactref element="SERIAL_3" pad="3"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="MTX2">
<contactref element="UM1" pad="IO16"/>
<contactref element="SERIAL_2" pad="4"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="MRX2">
<contactref element="UM1" pad="IO17"/>
<contactref element="SERIAL_2" pad="3"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="MTX1">
<contactref element="UM1" pad="IO18"/>
<contactref element="SERIAL_1" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="MRX1">
<contactref element="UM1" pad="IO19"/>
<contactref element="SERIAL_1" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SDA1">
<contactref element="UM1" pad="IO20"/>
<contactref element="SIG_ISO1" pad="7"/>
<contactref element="SIG_ISO2" pad="7"/>
<contactref element="R6" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="SJ2" pad="3"/>
<contactref element="SJ3" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="SCL1">
<contactref element="SJ1" pad="3"/>
<contactref element="UM1" pad="IO21"/>
<contactref element="SIG_ISO1" pad="6"/>
<contactref element="SIG_ISO2" pad="6"/>
<contactref element="R5" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="SJ4" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SCLB">
<contactref element="I2C_6" pad="4"/>
<contactref element="I2C_7" pad="4"/>
<contactref element="I2C_5" pad="4"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="SDAB">
<contactref element="I2C_6" pad="3"/>
<contactref element="I2C_7" pad="3"/>
<contactref element="I2C_5" pad="3"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="UM1" pad="SCL"/>
<contactref element="R9" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="SJ4" pad="1"/>
<contactref element="UM2" pad="IOH17"/>
</signal>
<signal name="SDA">
<contactref element="UM1" pad="SDA"/>
<contactref element="R10" pad="2"/>
<contactref element="SJ2" pad="1"/>
<contactref element="SJ3" pad="1"/>
<contactref element="UM2" pad="IOH16"/>
</signal>
<signal name="SDAA">
<contactref element="I2C_1" pad="3"/>
<contactref element="I2C_2" pad="3"/>
<contactref element="I2C_3" pad="3"/>
<contactref element="I2C_4" pad="3"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="SCLA">
<contactref element="I2C_1" pad="4"/>
<contactref element="I2C_2" pad="4"/>
<contactref element="I2C_3" pad="4"/>
<contactref element="I2C_4" pad="4"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="UM1" pad="AREF"/>
<contactref element="UM2" pad="IOH15"/>
</signal>
<signal name="IO13">
<contactref element="UM1" pad="IO13"/>
<contactref element="UM2" pad="IOH13"/>
<contactref element="STATUS" pad="3"/>
</signal>
<signal name="IO12">
<contactref element="UM1" pad="IO12"/>
<contactref element="UM2" pad="IOH12"/>
<contactref element="STATUS" pad="1"/>
</signal>
<signal name="IO11">
<contactref element="UM1" pad="IO11"/>
<contactref element="UM2" pad="IOH11"/>
</signal>
<signal name="IO0">
<contactref element="UM1" pad="IO0"/>
<contactref element="UM2" pad="IOL0"/>
</signal>
<signal name="IO1">
<contactref element="UM1" pad="IO1"/>
<contactref element="UM2" pad="IOL1"/>
</signal>
<signal name="IO2">
<contactref element="UM1" pad="IO2"/>
<contactref element="UM2" pad="IOL2"/>
</signal>
<signal name="VIN">
<contactref element="UM1" pad="VIN"/>
<contactref element="UM2" pad="PWR_VIN"/>
</signal>
<signal name="RST">
<contactref element="UM1" pad="RST"/>
<contactref element="UM2" pad="PWR_RESET"/>
<contactref element="SW1" pad="2B"/>
<contactref element="SW1" pad="2A"/>
<contactref element="ICSP" pad="5"/>
</signal>
<signal name="P3V">
<contactref element="UM1" pad="P3V"/>
<contactref element="UM2" pad="PWR_3_3V"/>
</signal>
<signal name="NC1">
<contactref element="UM1" pad="NC1"/>
<contactref element="UM2" pad="PWR_NC"/>
</signal>
<signal name="N$3">
<contactref element="R11" pad="2"/>
<contactref element="PWR" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="JP2" pad="8"/>
<contactref element="UM1" pad="ADH7"/>
</signal>
<signal name="N$21">
<contactref element="JP2" pad="7"/>
<contactref element="UM1" pad="ADH6"/>
</signal>
<signal name="N$22">
<contactref element="JP2" pad="6"/>
<contactref element="UM1" pad="ADH5"/>
</signal>
<signal name="N$23">
<contactref element="JP2" pad="5"/>
<contactref element="UM1" pad="ADH4"/>
</signal>
<signal name="N$24">
<contactref element="JP2" pad="4"/>
<contactref element="UM1" pad="ADH3"/>
</signal>
<signal name="N$25">
<contactref element="JP2" pad="3"/>
<contactref element="UM1" pad="ADH2"/>
</signal>
<signal name="N$26">
<contactref element="JP2" pad="2"/>
<contactref element="UM1" pad="ADH1"/>
</signal>
<signal name="N$27">
<contactref element="JP2" pad="1"/>
<contactref element="UM1" pad="ADH0"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="SIG_ISO1" pad="3"/>
<contactref element="STP1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="SIG_ISO1" pad="2"/>
<contactref element="STP1" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="SW3" pad="1"/>
<contactref element="SW3" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="SIG_ISO2" pad="2"/>
<contactref element="STP2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="STATUS" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R13" pad="2"/>
<contactref element="STATUS" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="ICSP" pad="3"/>
<contactref element="UM1" pad="33"/>
</signal>
<signal name="MISO">
<contactref element="ICSP" pad="1"/>
<contactref element="UM1" pad="31"/>
</signal>
<signal name="MOSI">
<contactref element="ICSP" pad="4"/>
<contactref element="UM1" pad="32"/>
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
<signal name="N$17">
</signal>
</signals>
</board>
</drawing>
</eagle>
