(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(U1-RES-Pad3)")
  (net 2 "unconnected-(U1-ADC_IN-Pad5)")
  (net 3 "unconnected-(U1-RES-Pad10)")
  (net 4 "Net-(J1-Pin_4)")
  (net 5 "Net-(J1-Pin_3)")
  (net 6 "GND")
  (net 7 "Net-(J2-Pin_3)")
  (net 8 "Net-(J2-Pin_1)")
  (net 9 "Net-(J2-Pin_2)")
  (net 10 "Net-(J2-Pin_4)")
  (net 11 "+3V3")
  (footprint "Sensor_Motion:Analog_LGA-16_3.25x3mm_P0.5mm_LayoutBorder3x5y" (layer "F.Cu")
    (at 19.1375 17.9)
    (descr "LGA, 16 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ADXL363.pdf#page=44)")
    (tags "LGA NoLead CC-16-4")
    (property "Sheetfile" "ADLX-Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Micropower 3-Axis Accelerometer, Thermometer, 2/4/8g range, SPI, LGA-16")
    (property "ki_keywords" "3-axis accelerometer spi mems thermometer")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.5) (layer "F.Fab"))
    (fp_text value "ADXL362B" (at 0 2.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.2875 -1) (size 0.925 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+3V3") (pinfunction "V_{DD_I/O}") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.2875 -0.5) (size 0.925 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "3" smd roundrect (at -1.2875 0) (size 0.925 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "unconnected-(U1-RES-Pad3)") (pinfunction "RES") (pintype "passive"))
    (pad "4" smd roundrect (at -1.2875 0.5) (size 0.925 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J2-Pin_1)") (pinfunction "SCLK") (pintype "input"))
    (pad "5" smd roundrect (at -1.2875 1) (size 0.925 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "unconnected-(U1-ADC_IN-Pad5)") (pinfunction "ADC_IN") (pintype "input"))
    (pad "6" smd roundrect (at -0.5 1.275) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J2-Pin_2)") (pinfunction "MOSI") (pintype "input"))
    (pad "7" smd roundrect (at 0 1.275) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J2-Pin_3)") (pinfunction "MISO") (pintype "output"))
    (pad "8" smd roundrect (at 0.5 1.275) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J2-Pin_4)") (pinfunction "~{CS}") (pintype "input"))
    (pad "9" smd roundrect (at 1.2875 1) (size 0.925 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pin_4)") (pinfunction "INT2") (pintype "output"))
    (pad "10" smd roundrect (at 1.2875 0.5) (size 0.925 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "unconnected-(U1-RES-Pad10)") (pinfunction "RES") (pintype "passive"))
    (pad "11" smd roundrect (at 1.2875 0) (size 0.925 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pin_3)") (pinfunction "INT1") (pintype "output"))
    (pad "12" smd roundrect (at 1.2875 -0.5) (size 0.925 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "13" smd roundrect (at 1.2875 -1) (size 0.925 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "14" smd roundrect (at 0.5 -1.275) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+3V3") (pinfunction "V_{S}") (pintype "power_in"))
    (pad "15" smd roundrect (at 0 -1.275) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "16" smd roundrect (at -0.5 -1.275) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Sensor_Motion.3dshapes/LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 19.1875 13.9)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ADLX-Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -2.7 0.05) (layer "F.Fab"))
    (fp_text value "C" (at 2.35 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (at 14.0375 14 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "ADLX-Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at -2.0825 0) (layer "B.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at 0 -9.95) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81 90) (layer "B.Fab"))
    (pad "1" thru_hole oval (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J2-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J2-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J2-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J2-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (at 24.2875 14.01 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "ADLX-Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 1.9975 -0.04) (layer "B.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at 0 -9.95) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole rect (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_2") (pintype "passive") (zone_connect 2))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J1-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 12.1375 12.1) (end 26.1375 23.1)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "MOSI" (at 12.2875 15.55 270) (layer "F.SilkS"))
  (gr_text "CS" (at 12.2875 21.05 270) (layer "F.SilkS"))
  (gr_text "3v3" (at 25.9875 14.55 90) (layer "F.SilkS"))
  (gr_text "MISO" (at 12.2875 18.15 270) (layer "F.SilkS"))
  (gr_text "SCLK" (at 12.3375 13 270) (layer "F.SilkS"))
  (gr_text "INT1" (at 25.9875 19.9 90) (layer "F.SilkS"))
  (gr_text "INT2" (at 25.9375 22.5 90) (layer "F.SilkS"))
  (gr_text "GND" (at 25.9875 17.3 90) (layer "F.SilkS"))
  (zone (net 6) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.25)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 12.3 12.2)
        (xy 26.0375 12.25)
        (xy 26.0375 23.15)
        (xy 12.2375 23.05)
      )
    )
  )
)
