(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 6)
    (zones 0)
    (modules 3)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 154.94 98.32 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.25 -2 90) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm (layer F.Cu) (tedit 5EB70B43)
    (at 148.01 90.77)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference J1 (at 0 -2.47) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.47) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm (layer F.Cu) (tedit 5EB70B43)
    (at 166.37 90.77)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference J2 (at 0 -2.47) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.47) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 2 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 169.37 96.67) (end 169.37 87.77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.33 97.67) (end 169.37 96.67) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 145.01 96.67) (end 145.01 87.77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 146.05 97.67) (end 145.01 96.67) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 145.01 87.77) (end 169.37 87.77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.33 102.87) (end 168.33 97.67) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 146.05 102.87) (end 146.05 97.67) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 146.05 102.87) (end 168.33 102.87) (layer Edge.Cuts) (width 0.05))
)
