(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 73)
    (tracks 407)
    (zones 0)
    (modules 38)
    (nets 80)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.762)
    (user_trace_width 2.794)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /RX_GPS)
  (net 3 /TX_GPS)
  (net 4 /PPS)
  (net 5 +3V3)
  (net 6 +5V)
  (net 7 /P1_ID)
  (net 8 /MAG~RST)
  (net 9 /P1_TX_SDA)
  (net 10 /P1_RX_SDA)
  (net 11 /P1_TX_SCL)
  (net 12 /P1_RX_SCL)
  (net 13 /P0_ID)
  (net 14 /P0_TX_SDA)
  (net 15 /P0_RX_SDA)
  (net 16 /P0_TX_SCL)
  (net 17 /P0_RX_SCL)
  (net 18 /P0_INT)
  (net 19 /P2_SCL)
  (net 20 /P2_SDA)
  (net 21 /P1_SCL)
  (net 22 /P0_SDA)
  (net 23 /P1_SDA)
  (net 24 /P0_SCL)
  (net 25 /P1_INT)
  (net 26 /P2_INT)
  (net 27 "Net-(J1601-PadS1)")
  (net 28 "/USB C Power/CC2")
  (net 29 "Net-(J1601-PadA8)")
  (net 30 "Net-(J1601-PadB6)")
  (net 31 "Net-(J1601-PadA7)")
  (net 32 "Net-(J1601-PadA6)")
  (net 33 "Net-(J1601-PadB7)")
  (net 34 "/USB C Power/CC1")
  (net 35 "Net-(J1601-PadB8)")
  (net 36 "Net-(U101-Pad14)")
  (net 37 "Net-(U101-Pad11)")
  (net 38 "Net-(U101-Pad10)")
  (net 39 "Net-(U101-Pad9)")
  (net 40 "Net-(U101-Pad8)")
  (net 41 "Net-(U101-Pad7)")
  (net 42 "Net-(U101-Pad6)")
  (net 43 "Net-(U101-Pad4)")
  (net 44 "Net-(U101-Pad1)")
  (net 45 "Net-(U104-Pad31)")
  (net 46 "Net-(U104-Pad45)")
  (net 47 "Net-(U104-Pad30)")
  (net 48 "Net-(U104-Pad29)")
  (net 49 "Net-(U104-Pad26)")
  (net 50 "Net-(U104-Pad28)")
  (net 51 "Net-(U104-Pad27)")
  (net 52 "Net-(U104-Pad35)")
  (net 53 "Net-(U104-Pad25)")
  (net 54 "Net-(U104-Pad44)")
  (net 55 "Net-(U104-Pad47)")
  (net 56 "Net-(U104-Pad42)")
  (net 57 "Net-(U104-Pad33)")
  (net 58 "Net-(U104-Pad32)")
  (net 59 "Net-(U104-Pad7)")
  (net 60 "Net-(U104-Pad22)")
  (net 61 "Net-(U104-Pad2)")
  (net 62 "Net-(U104-Pad4)")
  (net 63 "Net-(U104-Pad3)")
  (net 64 "Net-(U104-Pad13)")
  (net 65 "Net-(U104-Pad11)")
  (net 66 "Net-(U104-Pad23)")
  (net 67 "Net-(U104-Pad24)")
  (net 68 "Net-(U104-Pad10)")
  (net 69 "Net-(U104-Pad19)")
  (net 70 "Net-(U104-Pad12)")
  (net 71 "Net-(U104-Pad14)")
  (net 72 "Net-(U104-Pad8)")
  (net 73 "Net-(U901-Pad9)")
  (net 74 "Net-(U901-Pad10)")
  (net 75 "Net-(U901-Pad11)")
  (net 76 "/Pocket 6DoF 1/INT")
  (net 77 "Net-(U1001-Pad9)")
  (net 78 "Net-(U1001-Pad10)")
  (net 79 "Net-(U1001-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net +3V3)
    (add_net +5V)
    (add_net /MAG~RST)
    (add_net /P0_ID)
    (add_net /P0_INT)
    (add_net /P0_RX_SCL)
    (add_net /P0_RX_SDA)
    (add_net /P0_SCL)
    (add_net /P0_SDA)
    (add_net /P0_TX_SCL)
    (add_net /P0_TX_SDA)
    (add_net /P1_ID)
    (add_net /P1_INT)
    (add_net /P1_RX_SCL)
    (add_net /P1_RX_SDA)
    (add_net /P1_SCL)
    (add_net /P1_SDA)
    (add_net /P1_TX_SCL)
    (add_net /P1_TX_SDA)
    (add_net /P2_INT)
    (add_net /P2_SCL)
    (add_net /P2_SDA)
    (add_net /PPS)
    (add_net "/Pocket 6DoF 1/INT")
    (add_net /RX_GPS)
    (add_net /TX_GPS)
    (add_net "/USB C Power/CC1")
    (add_net "/USB C Power/CC2")
    (add_net GND)
    (add_net "Net-(J1601-PadA6)")
    (add_net "Net-(J1601-PadA7)")
    (add_net "Net-(J1601-PadA8)")
    (add_net "Net-(J1601-PadB6)")
    (add_net "Net-(J1601-PadB7)")
    (add_net "Net-(J1601-PadB8)")
    (add_net "Net-(J1601-PadS1)")
    (add_net "Net-(U1001-Pad10)")
    (add_net "Net-(U1001-Pad11)")
    (add_net "Net-(U1001-Pad9)")
    (add_net "Net-(U101-Pad1)")
    (add_net "Net-(U101-Pad10)")
    (add_net "Net-(U101-Pad11)")
    (add_net "Net-(U101-Pad14)")
    (add_net "Net-(U101-Pad4)")
    (add_net "Net-(U101-Pad6)")
    (add_net "Net-(U101-Pad7)")
    (add_net "Net-(U101-Pad8)")
    (add_net "Net-(U101-Pad9)")
    (add_net "Net-(U104-Pad10)")
    (add_net "Net-(U104-Pad11)")
    (add_net "Net-(U104-Pad12)")
    (add_net "Net-(U104-Pad13)")
    (add_net "Net-(U104-Pad14)")
    (add_net "Net-(U104-Pad19)")
    (add_net "Net-(U104-Pad2)")
    (add_net "Net-(U104-Pad22)")
    (add_net "Net-(U104-Pad23)")
    (add_net "Net-(U104-Pad24)")
    (add_net "Net-(U104-Pad25)")
    (add_net "Net-(U104-Pad26)")
    (add_net "Net-(U104-Pad27)")
    (add_net "Net-(U104-Pad28)")
    (add_net "Net-(U104-Pad29)")
    (add_net "Net-(U104-Pad3)")
    (add_net "Net-(U104-Pad30)")
    (add_net "Net-(U104-Pad31)")
    (add_net "Net-(U104-Pad32)")
    (add_net "Net-(U104-Pad33)")
    (add_net "Net-(U104-Pad35)")
    (add_net "Net-(U104-Pad4)")
    (add_net "Net-(U104-Pad42)")
    (add_net "Net-(U104-Pad44)")
    (add_net "Net-(U104-Pad45)")
    (add_net "Net-(U104-Pad47)")
    (add_net "Net-(U104-Pad7)")
    (add_net "Net-(U104-Pad8)")
    (add_net "Net-(U901-Pad10)")
    (add_net "Net-(U901-Pad11)")
    (add_net "Net-(U901-Pad9)")
  )
  (net_class RF ""
    (clearance 0.254)
    (trace_width 2.794)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (module KwanSystems:GCTUSBTypeC_PTH (layer F.Cu) (tedit 5F3D494F)
    (at 73.66 107.95 270)
    (descr "Part GCT USB4105. Digikey 2073-USB4105-GF-ACT-ND")
    (tags USB)
    (attr smd)
    (fp_text reference J1601 (at 9.144 2.794 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Receptacle_USB2.0 (at -4.826 4.572 90) (layer F.Fab))
    (fp_text user "PCB edge" (at -6.604 0.762 90) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at -2.89 -6.28 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.89 -6.28 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad A1 smd rect (at -3.2 -7.6425 270) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A12 smd rect (at 3.2 -7.6425 270) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B12 smd rect (at -3.2 -7.0675 270) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A4 smd rect (at -2.4 -7.6425 270) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad B9 smd rect (at -2.4 -7.0675 270) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad B8 smd rect (at -1.75 -7.355 270) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J1601-PadB8)"))
    (pad A5 smd rect (at -1.25 -7.355 270) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 34 "/USB C Power/CC1"))
    (pad B7 smd rect (at -0.75 -7.355 270) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J1601-PadB7)"))
    (pad A6 smd rect (at -0.25 -7.355 270) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J1601-PadA6)"))
    (pad A7 smd rect (at 0.25 -7.355 270) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J1601-PadA7)"))
    (pad B6 smd rect (at 0.75 -7.355 270) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J1601-PadB6)"))
    (pad A8 smd rect (at 1.25 -7.355 270) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J1601-PadA8)"))
    (pad B5 smd rect (at 1.75 -7.355 270) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 28 "/USB C Power/CC2"))
    (pad B4 smd rect (at 2.4 -7.0675 270) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad A9 smd rect (at 2.4 -7.6425 270) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad B1 smd rect (at 3.2 -7.0675 270) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 -6.78 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 27 "Net-(J1601-PadS1)"))
    (pad S1 thru_hole oval (at -4.32 -2.6 270) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 27 "Net-(J1601-PadS1)"))
    (pad S1 thru_hole oval (at 4.32 -2.6 270) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 27 "Net-(J1601-PadS1)"))
    (pad S1 thru_hole oval (at 4.32 -6.78 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 27 "Net-(J1601-PadS1)"))
    (model /home/jeppesen/workspace/kicad/KwanSystems.pretty/USB4105-GF-A--3DModel-STEP-46669.STEP
      (offset (xyz 0 3.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 83.82 109.728)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1602 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1k (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "/USB C Power/CC2"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 83.82 106.68)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1601 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1k (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "/USB C Power/CC1"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:Symbol_KiCAD-Logo_CopperAndSilkScreenTop_small (layer F.Cu) (tedit 0)
    (at 121.666 123.952)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (fp_text reference G101 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value DesignedWithKicad (at 0.75 0 180) (layer F.SilkS) hide)
  )
  (module KwanSystems:Teensy2x24 (layer F.Cu) (tedit 5EF62457)
    (at 77.47 115.57 90)
    (fp_text reference U104 (at -0.2 -2.5 90) (layer F.Fab))
    (fp_text value Teensy4.1 (at 0 -4.1 90) (layer F.Fab))
    (fp_text user MicroSD (at 7.62 58.42 90) (layer F.SilkS))
    (fp_text user USB (at 12.192 5.588 90) (layer F.SilkS))
    (pad 31 thru_hole oval (at 15.24 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(U104-Pad31)"))
    (pad 45 thru_hole oval (at 15.24 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(U104-Pad45)"))
    (pad 46 thru_hole oval (at 15.24 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 30 thru_hole oval (at 15.24 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(U104-Pad30)"))
    (pad 29 thru_hole oval (at 15.24 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(U104-Pad29)"))
    (pad 26 thru_hole oval (at 15.24 55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(U104-Pad26)"))
    (pad 28 thru_hole oval (at 15.24 50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(U104-Pad28)"))
    (pad 27 thru_hole oval (at 15.24 53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(U104-Pad27)"))
    (pad 39 thru_hole oval (at 15.24 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /P1_SDA))
    (pad 40 thru_hole oval (at 15.24 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /P0_SDA))
    (pad 37 thru_hole oval (at 15.24 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /PPS))
    (pad 35 thru_hole oval (at 15.24 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(U104-Pad35)"))
    (pad 25 thru_hole circle (at 15.24 58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(U104-Pad25)"))
    (pad 41 thru_hole oval (at 15.24 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /P0_SCL))
    (pad 44 thru_hole oval (at 15.24 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(U104-Pad44)"))
    (pad 47 thru_hole oval (at 15.24 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(U104-Pad47)"))
    (pad 48 thru_hole oval (at 15.24 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 42 thru_hole oval (at 15.24 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(U104-Pad42)"))
    (pad 34 thru_hole oval (at 15.24 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 43 thru_hole oval (at 15.24 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /P0_INT))
    (pad 36 thru_hole oval (at 15.24 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /P0_ID))
    (pad 38 thru_hole oval (at 15.24 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /P1_SCL))
    (pad 33 thru_hole oval (at 15.24 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(U104-Pad33)"))
    (pad 32 thru_hole oval (at 15.24 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(U104-Pad32)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(U104-Pad7)"))
    (pad 21 thru_hole oval (at 0 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /RX_GPS))
    (pad 22 thru_hole oval (at 0 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(U104-Pad22)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /MAG~RST))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P1_ID))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(U104-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(U104-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(U104-Pad3)"))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /P2_SCL))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(U104-Pad13)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(U104-Pad11)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /P2_SDA))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /TX_GPS))
    (pad 23 thru_hole oval (at 0 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(U104-Pad23)"))
    (pad 24 thru_hole oval (at 0 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(U104-Pad24)"))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /P2_INT))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(U104-Pad10)"))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(U104-Pad19)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(U104-Pad12)"))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(U104-Pad14)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /P1_INT))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(U104-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x24_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x24_P2.54mm_Vertical.step
      (offset (xyz 15.24 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (offset (xyz 0 -38.1 9.5504))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (offset (xyz 15.24 -38.1 9.5504))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model "/home/jeppesen/workspace/kicad/KwanSystems.pretty/Teensy 4.1 (Without Headers).step"
      (offset (xyz 7.62 -29.21 10.2616))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.step
      (offset (xyz 0 0 11.049))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.step
      (offset (xyz 15.24 0 11.049))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/jeppesen/workspace/kicad/KwanSystems.pretty/TeensyView.step
      (offset (xyz -97.155 -165.1 20.32))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
    (model ${KISYS3DMOD}/Package_BGA.3dshapes/BGA-100_11.0x11.0mm_Layout10x10_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD.step
      (offset (xyz 7.62 -15.24 22.86))
      (scale (xyz 1 2.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 87.63 97.79 90)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference J112 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_02x06_Male (at 1.27 15.03 90) (layer F.Fab))
    (fp_text user %R (at 1.27 6.35) (layer F.Fab))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /P0_ID))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /MAG~RST))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /P0_TX_SDA))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /P0_RX_SDA))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /P0_TX_SCL))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /P0_RX_SCL))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /TX_GPS))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /RX_GPS))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /PPS))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /P0_INT))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.33 118.11 270)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference J102 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_02x06_Male (at 1.27 15.03 90) (layer F.Fab))
    (fp_text user %R (at 1.27 6.35) (layer F.Fab))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P1_ID))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /MAG~RST))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /P1_TX_SDA))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /P1_RX_SDA))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /P1_TX_SCL))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /P1_RX_SCL))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /TX_GPS))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /RX_GPS))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /PPS))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /P1_INT))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-8_3x3mm_P0.65mm (layer F.Cu) (tedit 5F459F09)
    (at 95.25 107.95 90)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U112 (at 0 -2.55 90) (layer F.SilkS) hide)
    (fp_text value P82B96 (at 0 2.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 2.15 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 7 smd rect (at 2.15 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 /P0_SCL))
    (pad 6 smd rect (at 2.15 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 /P0_TX_SCL))
    (pad 5 smd rect (at 2.15 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 /P0_RX_SCL))
    (pad 4 smd rect (at -2.15 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.15 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 /P0_RX_SDA))
    (pad 2 smd rect (at -2.15 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 /P0_TX_SDA))
    (pad 1 smd rect (at -2.15 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 /P0_SDA))
  )
  (module KwanSystems:SolderJumper-2_Bridged (layer F.Cu) (tedit 5F4584FB)
    (at 96.266 107.95 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference J117 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 16 /P0_TX_SCL))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 24 /P0_SCL))
  )
  (module KwanSystems:SolderJumper-2_Bridged (layer F.Cu) (tedit 5F4584FB)
    (at 94.234 107.95 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference J111 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 15 /P0_RX_SDA))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 22 /P0_SDA))
  )
  (module KwanSystems:SolderJumper-2_Bridged (layer F.Cu) (tedit 5F4584FB)
    (at 103.886 107.95 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference J107 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 11 /P1_TX_SCL))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 21 /P1_SCL))
  )
  (module KwanSystems:SolderJumper-2_Bridged (layer F.Cu) (tedit 5F4584FB)
    (at 101.854 107.95 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference J101 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 10 /P1_RX_SDA))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 23 /P1_SDA))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 97.79 107.95 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R141 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /P0_SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 92.71 107.95 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R140 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /P0_SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 100.33 107.95 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R139 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /P1_SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 105.41 107.95 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R138 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /P1_SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.11 113.03 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R117 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /P2_SDA))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 115.57 113.03 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R116 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /P2_SCL))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:Axis (layer F.Cu) (tedit 590A7BBF)
    (at 130.81 123.19 90)
    (descr "Built for the MPU-9250 using guidelines found in http://cds.linear.com/docs/en/packaging/Carsem%20MLP%20users%20guide.pdf")
    (fp_text reference G105 (at -1.3 1.5 90) (layer F.Fab) hide)
    (fp_text value Axis (at -1.8 2.75 90) (layer F.SilkS) hide)
    (fp_text user Z (at 3.302 -3.302 180) (layer B.SilkS))
    (fp_text user Y (at 0 -3.302) (layer B.SilkS))
    (fp_text user X (at 3.2 1.016 180) (layer B.SilkS))
    (fp_text user Z (at 3.302 -3.302 180) (layer F.SilkS))
    (fp_text user X (at 3.2 1.016 180) (layer F.SilkS))
    (fp_text user Y (at 0 -3.302 180) (layer F.SilkS))
  )
  (module KwanSystems:StKwansSoldermask (layer B.Cu) (tedit 5F40003C)
    (at 132.08 107.95 180)
    (fp_text reference G104 (at -3.683 2.7432) (layer B.Mask) hide)
    (fp_text value KwanSystems (at 4.2926 -3.7084) (layer B.Mask) hide)
    (fp_text user github.com/kwan3217/kicad (at 21.082 -36.83 unlocked) (layer B.Cu) hide)
    (fp_text user stkwans.blogspot.com (at 21.082 -3.556 unlocked) (layer B.SilkS))
    (fp_text user "a division of Kwan Systems" (at 25.654 -1.778 unlocked) (layer B.SilkS))
    (fp_text user "St Kwan's Home for" (at 27.432 3.048 unlocked) (layer B.SilkS))
    (fp_text user "the Terminally ADD" (at 26.416 0.508 unlocked) (layer B.SilkS))
  )
  (module KwanSystems:STANDOFF_NONPLATED (layer F.Cu) (tedit 5AD79727)
    (at 134.62 91.44 90)
    (fp_text reference J129 (at 0 2 90) (layer F.SilkS) hide)
    (fp_text value STANDOFF (at -0.05 -1.7 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
  )
  (module KwanSystems:STANDOFF_NONPLATED (layer F.Cu) (tedit 5AD79727)
    (at 78.74 91.44 90)
    (fp_text reference J127 (at 0 2 90) (layer F.SilkS) hide)
    (fp_text value STANDOFF (at -0.05 -1.7 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
  )
  (module KwanSystems:STANDOFF_NONPLATED (layer F.Cu) (tedit 5AD79727)
    (at 134.62 124.46 90)
    (fp_text reference J125 (at 0 2 90) (layer F.SilkS) hide)
    (fp_text value STANDOFF (at -0.05 -1.7 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
  )
  (module KwanSystems:STANDOFF_NONPLATED (layer F.Cu) (tedit 5AD79727)
    (at 78.74 124.46 90)
    (fp_text reference J120 (at 0 2 90) (layer F.SilkS) hide)
    (fp_text value STANDOFF (at -0.05 -1.7 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/PocketCableCutout.wrl
      (offset (xyz 55.4228 2.54 6.0452))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/PocketCableCutout.wrl
      (offset (xyz 55.4228 2.54 3.0226))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/PocketCableCutout.wrl
      (offset (xyz 55.4228 2.54 9.0678))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/PocketCableCutout.wrl
      (offset (xyz 55.4228 2.54 12.0904))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/PocketCableCutout.wrl
      (offset (xyz 55.4228 2.54 15.113))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/PocketMicroSDOverlap.wrl
      (offset (xyz 55.4228 2.54 18.1356))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/PocketMicroSDOverlap.wrl
      (offset (xyz 55.4228 2.54 21.1582))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/PocketMicroSDOverlap.wrl
      (offset (xyz 55.4228 2.54 24.1808))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/PocketCover.wrl
      (offset (xyz 55.4228 2.54 -4.826))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/PocketPTHCutout.wrl
      (offset (xyz 55.4228 2.54 -1.778))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/PocketCover.wrl
      (offset (xyz 55.4228 2.54 27.20339999999999))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
  )
  (module KwanSystems:StKwansSoldermask (layer F.Cu) (tedit 5F3FF60D)
    (at 128.27 93.98)
    (fp_text reference G102 (at -3.683 -2.7432) (layer F.Mask) hide)
    (fp_text value KwanSystems (at 4.2926 3.7084) (layer F.Mask) hide)
    (fp_text user github.com/kwan3217/kicad (at -24.13 2.54 unlocked) (layer F.SilkS))
    (fp_text user stkwans.blogspot.com (at -21.59 0.508 unlocked) (layer F.SilkS))
    (fp_text user "a division of Kwan Systems" (at -20.32 -1.27 unlocked) (layer F.SilkS))
    (fp_text user "St Kwan's Home for" (at -15.24 -3.81 unlocked) (layer F.SilkS))
    (fp_text user "the Terminally ADD" (at -15.24 -2.54 unlocked) (layer F.SilkS))
  )
  (module KwanSystems:OSHW-Symbol_6.7x6mm_SolderMask (layer B.Cu) (tedit 0)
    (at 84.328 107.696 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference G103 (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW (at 0.75 0) (layer B.Fab) hide)
  )
  (module KwanSystems:Symbol_KiCAD-Logo_CopperAndSilkScreenTop_small (layer B.Cu) (tedit 0)
    (at 80.518 96.266 180)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (fp_text reference G101 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value DesignedWithKicad (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.968 107.95 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1108 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.032 107.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1106 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.936 105.41 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1008 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.936 106.426 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1005 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.936 108.966 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C908 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.936 109.982 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C905 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:BME280 (layer F.Cu) (tedit 5F3D9117)
    (at 127 107.95 90)
    (fp_text reference U1101 (at -0.05 2.5 90) (layer F.SilkS) hide)
    (fp_text value BME280 (at 4.064 0.762 90) (layer F.Fab) hide)
    (pad 6 smd rect (at -1.025 0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 7 smd rect (at -1.025 -0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -1.025 0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.025 0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 /P2_SCL))
    (pad 1 smd rect (at 1.025 -0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.025 0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 20 /P2_SDA))
    (pad 8 smd rect (at -1.025 -0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.025 -0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model /home/jeppesen/workspace/kicad/KwanSystems.pretty/BME280--3DModel-STEP-56544.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module KwanSystems:LGA-14L (layer F.Cu) (tedit 5F3D6253)
    (at 120.65 106.172 90)
    (fp_text reference U1001 (at -3.302 -0.762 270) (layer F.Fab))
    (fp_text value LSM6DSO (at 4.826 -0.762 90) (layer F.Fab) hide)
    (fp_text user >Name (at -2 -1.5 90) (layer F.Fab) hide)
    (fp_text user Z (at -0.45 0.25 90) (layer Dwgs.User))
    (fp_text user X (at 0.35 0.25 90) (layer Dwgs.User))
    (fp_text user Y (at -0.4 -0.5 90) (layer Dwgs.User))
    (pad 1 smd rect (at -1.1625 -0.75 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -1.1625 -0.25 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -1.1625 0.25 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at -1.1625 0.75 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 "/Pocket 6DoF 1/INT") (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -0.5 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at 0 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 7 smd rect (at 0.5 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 8 smd rect (at 1.1625 0.75 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.0508))
    (pad 9 smd rect (at 1.1625 0.25 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U1001-Pad9)") (solder_mask_margin 0.0508))
    (pad 10 smd rect (at 1.1625 -0.25 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U1001-Pad10)") (solder_mask_margin 0.0508))
    (pad 11 smd rect (at 1.1625 -0.75 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U1001-Pad11)") (solder_mask_margin 0.0508))
    (pad 12 smd rect (at 0.5 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.0508))
    (pad 13 smd rect (at 0 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /P2_SCL) (solder_mask_margin 0.0508))
    (pad 14 smd rect (at -0.5 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /P2_SDA) (solder_mask_margin 0.0508))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-14_3x2.5mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:LGA-14L (layer F.Cu) (tedit 5F3D6253)
    (at 120.65 109.728 90)
    (fp_text reference U901 (at 3.048 0.405 270) (layer F.Fab))
    (fp_text value LSM6DSO (at 4.826 -0.762 90) (layer F.Fab) hide)
    (fp_text user >Name (at -2 -1.5 90) (layer F.Fab) hide)
    (fp_text user Z (at -0.45 0.25 90) (layer Dwgs.User))
    (fp_text user X (at 0.35 0.25 90) (layer Dwgs.User))
    (fp_text user Y (at -0.4 -0.5 90) (layer Dwgs.User))
    (pad 1 smd rect (at -1.1625 -0.75 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -1.1625 -0.25 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -1.1625 0.25 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at -1.1625 0.75 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /P2_INT) (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -0.5 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at 0 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 7 smd rect (at 0.5 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 8 smd rect (at 1.1625 0.75 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.0508))
    (pad 9 smd rect (at 1.1625 0.25 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U901-Pad9)") (solder_mask_margin 0.0508))
    (pad 10 smd rect (at 1.1625 -0.25 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U901-Pad10)") (solder_mask_margin 0.0508))
    (pad 11 smd rect (at 1.1625 -0.75 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U901-Pad11)") (solder_mask_margin 0.0508))
    (pad 12 smd rect (at 0.5 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.0508))
    (pad 13 smd rect (at 0 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /P2_SCL) (solder_mask_margin 0.0508))
    (pad 14 smd rect (at -0.5 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /P2_SDA) (solder_mask_margin 0.0508))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-14_3x2.5mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:AK09970 (layer F.Cu) (tedit 5F3D3F3B)
    (at 114.046 107.95 90)
    (fp_text reference U101 (at 0 0.3 90) (layer Dwgs.User))
    (fp_text value AK09970 (at 0.2 -0.3 90) (layer Dwgs.User))
    (fp_text user Z (at -0.6 0.7 90) (layer Dwgs.User))
    (fp_text user Y (at -0.7 -0.9 90) (layer Dwgs.User))
    (fp_text user X (at 0.8 0.7 90) (layer Dwgs.User))
    (pad 16 smd rect (at -1.5375 0.75) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 8 /MAG~RST))
    (pad 15 smd rect (at -1.5375 0.25) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 14 smd rect (at -1.5375 -0.25) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U101-Pad14)"))
    (pad 13 smd rect (at -1.5375 -0.75) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -0.75 -1.5375 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -0.25 -1.5375 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U101-Pad11)"))
    (pad 10 smd rect (at 0.25 -1.5375 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U101-Pad10)"))
    (pad 9 smd rect (at 0.75 -1.5375 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U101-Pad9)"))
    (pad 8 smd rect (at 1.5375 -0.75 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U101-Pad8)"))
    (pad 7 smd rect (at 1.5375 -0.25 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U101-Pad7)"))
    (pad 6 smd rect (at 1.5375 0.25 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U101-Pad6)"))
    (pad 5 smd rect (at 1.5375 0.75 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 20 /P2_SDA))
    (pad 4 smd rect (at 0.75 1.5375 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U101-Pad4)"))
    (pad 3 smd rect (at 0.25 1.5375 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 19 /P2_SCL))
    (pad 2 smd rect (at -0.25 1.5375 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -0.75 1.5375 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U101-Pad1)"))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Package_SO:TSSOP-8_3x3mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 102.87 107.95 90)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U102 (at 0 -2.55 90) (layer F.SilkS) hide)
    (fp_text value P82B96 (at 0 2.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 2.15 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 7 smd rect (at 2.15 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 /P1_SCL))
    (pad 6 smd rect (at 2.15 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /P1_TX_SCL))
    (pad 5 smd rect (at 2.15 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /P1_RX_SCL))
    (pad 4 smd rect (at -2.15 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.15 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /P1_RX_SDA))
    (pad 2 smd rect (at -2.15 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /P1_TX_SDA))
    (pad 1 smd rect (at -2.15 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 /P1_SDA))
  )
  (gr_text "Assembly\nDate" (at 115.062 96.52) (layer B.Mask))
  (gr_text "Serial\nNumber" (at 115.062 91.567) (layer B.Mask))
  (gr_text 3V3 (at 97.79 123.19 270) (layer F.SilkS))
  (gr_text RGPS (at 95.25 123.19 270) (layer F.SilkS))
  (gr_text RSCL (at 92.71 123.19 270) (layer F.SilkS))
  (gr_text ID (at 87.63 125.73 270) (layer F.SilkS))
  (gr_text TGPS (at 95.25 125.73 270) (layer F.SilkS))
  (gr_text GND (at 100.33 123.19 270) (layer F.SilkS))
  (gr_text M~RST (at 87.63 123.19 270) (layer F.SilkS))
  (gr_text RSDA (at 90.17 123.19 270) (layer F.SilkS))
  (gr_text TSDA (at 90.17 125.73 270) (layer F.SilkS))
  (gr_text PPS (at 97.79 125.73 270) (layer F.SilkS))
  (gr_text INT (at 100.33 125.73 270) (layer F.SilkS))
  (gr_text TSCL (at 92.71 125.73 270) (layer F.SilkS))
  (gr_text github.com/kwan3217/kicad (at 92.71 124.46) (layer B.Cu))
  (gr_text P1 (at 85.09 119.38) (layer F.SilkS))
  (gr_text P0 (at 85.09 96.52) (layer F.SilkS))
  (gr_text TSDA (at 97.79 90.17 90) (layer F.SilkS))
  (gr_text TSCL (at 95.25 90.17 90) (layer F.SilkS))
  (gr_text ID (at 100.33 90.17 90) (layer F.SilkS))
  (gr_text INT (at 87.63 90.17 90) (layer F.SilkS))
  (gr_text PPS (at 90.17 90.17 90) (layer F.SilkS))
  (gr_text TGPS (at 92.71 90.17 90) (layer F.SilkS))
  (gr_text M~RST (at 100.33 92.71 90) (layer F.SilkS))
  (gr_text RSDA (at 97.79 92.71 90) (layer F.SilkS))
  (gr_text RSCL (at 95.25 92.71 90) (layer F.SilkS))
  (gr_text RGPS (at 92.71 92.71 90) (layer F.SilkS))
  (gr_text 3V3 (at 90.17 92.71 90) (layer F.SilkS))
  (gr_text GND (at 87.63 92.71 90) (layer F.SilkS))
  (gr_text "Pocket Board\nv1.0\n2020 Oct 09" (at 116.84 120.65) (layer B.SilkS))
  (gr_text "Wearable Pocketometer" (at 119.38 124.46) (layer B.Mask))
  (gr_text "Pocket Board\nv1.0\n2020 Oct 09" (at 106.68 121.92) (layer F.SilkS))
  (gr_text "Wearable Pocketometer" (at 116.84 118.11) (layer F.SilkS))
  (gr_line (start 76.2 88.9) (end 137.16 88.9) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 76.2 124.46) (end 73.66 124.46) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 76.2 91.44) (end 76.2 88.9) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 137.16 91.44) (end 139.7 91.44) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 137.16 124.46) (end 137.16 127) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.2 127) (end 137.16 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 73.66 91.44) (end 73.66 124.46) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.7 124.46) (end 139.7 91.44) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 88.9) (xy 139.7 127) (xy 73.66 127) (xy 73.66 88.9)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 88.9) (xy 139.7 127) (xy 73.66 127) (xy 73.66 88.9)
      )
    )
  )
)
