(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 43)
    (no_connects 2)
    (area 52.267 115.429 106.276096 149.709)
    (thickness 1.6)
    (drawings 9)
    (tracks 164)
    (zones 0)
    (modules 22)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 5V+)
  (net 3 Vin)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(C5-Pad1)")
  (net 9 EventIN)
  (net 10 "Net-(J2-Pad2)")
  (net 11 USB-)
  (net 12 USB+)
  (net 13 "Net-(J2-Pad5)")
  (net 14 "Net-(J2-Pad6)")
  (net 15 "Net-(J2-Pad7)")
  (net 16 "Net-(J2-Pad8)")
  (net 17 Uart0TX)
  (net 18 Uart0RX)
  (net 19 Uart1TX)
  (net 20 Uart1RX)
  (net 21 "Net-(J2-Pad17)")
  (net 22 "Net-(J2-Pad19)")
  (net 23 "Net-(J2-Pad20)")
  (net 24 "Net-(m-usb1-Pad1)")
  (net 25 "Net-(R1-Pad2)")
  (net 26 "Net-(R3-Pad2)")
  (net 27 "Net-(Uart0-Pad4)")
  (net 28 "Net-(Uart0-Pad5)")
  (net 29 "Net-(Uart0-Pad6)")
  (net 30 "Net-(Uart1-Pad4)")
  (net 31 "Net-(Uart1-Pad5)")
  (net 32 "Net-(Uart1-Pad6)")
  (net 33 "Net-(D2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net EventIN)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(Uart0-Pad4)")
    (add_net "Net-(Uart0-Pad5)")
    (add_net "Net-(Uart0-Pad6)")
    (add_net "Net-(Uart1-Pad4)")
    (add_net "Net-(Uart1-Pad5)")
    (add_net "Net-(Uart1-Pad6)")
    (add_net "Net-(m-usb1-Pad1)")
    (add_net USB+)
    (add_net USB-)
    (add_net Uart0RX)
    (add_net Uart0TX)
    (add_net Uart1RX)
    (add_net Uart1TX)
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5V+)
    (add_net "Net-(C3-Pad2)")
    (add_net Vin)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A16800B)
    (at 79.248 138.43 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.524 180) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 5V+))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A167F55)
    (at 84.328 138.684 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 Vin))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 81.026 132.588 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 3.3uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_3220 (layer F.Cu) (tedit 590CF5B9)
    (at 69.596 142.494 180)
    (descr "Diode SMD 3220, reflow soldering http://datasheets.avx.com/schottky.pdf")
    (tags "Diode 3220")
    (attr smd)
    (fp_text reference D1 (at 0 -3.6 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3.7 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab))
    (pad 1 smd rect (at -4 0 270) (size 3.9 3.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 4 0 270) (size 3.9 3.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_3220.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 100.838 141.224)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "vIN and event" (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Vin))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 EventIN))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x10_Pitch2.00mm_SMD (layer F.Cu) (tedit 58CD5450)
    (at 80.264 122.936 90)
    (descr "surface-mounted straight socket strip, 2x10, 2.00mm pitch, double rows")
    (tags "Surface mounted socket strip SMD 2x10 2.00mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 -11.06 90) (layer F.SilkS))
    (fp_text value "Multi Connector" (at 0 11.06 90) (layer F.Fab))
    (fp_text user %R (at 0 -11.06 90) (layer F.Fab))
    (pad 1 smd rect (at 3.125 -9 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 5V+))
    (pad 2 smd rect (at -3.125 -9 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at 3.125 -7 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 11 USB-))
    (pad 4 smd rect (at -3.125 -7 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 12 USB+))
    (pad 5 smd rect (at 3.125 -5 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad5)"))
    (pad 6 smd rect (at -3.125 -5 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at 3.125 -3 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad7)"))
    (pad 8 smd rect (at -3.125 -3 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad8)"))
    (pad 9 smd rect (at 3.125 -1 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 9 EventIN))
    (pad 10 smd rect (at -3.125 -1 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 3.125 1 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 17 Uart0TX))
    (pad 12 smd rect (at -3.125 1 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 18 Uart0RX))
    (pad 13 smd rect (at 3.125 3 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -3.125 3 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 19 Uart1TX))
    (pad 15 smd rect (at 3.125 5 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 20 Uart1RX))
    (pad 16 smd rect (at -3.125 5 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 3.125 7 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad17)"))
    (pad 18 smd rect (at -3.125 7 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 3.125 9 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J2-Pad19)"))
    (pad 20 smd rect (at -3.125 9 90) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J2-Pad20)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x10_Pitch2.00mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Taiyo-Yuden_NR-80xx (layer F.Cu) (tedit 5990349D)
    (at 91.44 141.986)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-80xx, 8.0mmx8.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L1 (at 0 -5) (layer F.SilkS))
    (fp_text value 15uH (at 0 5.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.8 0) (size 1.8 7.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 2.8 0) (size 1.8 7.7) (layers F.Cu F.Paste F.Mask)
      (net 2 5V+))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_NR-80xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_USB:USB_Micro-B_Molex_47346-0001 (layer F.Cu) (tedit 594C50D0)
    (at 56.642 141.478 270)
    (descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
    (tags "Micro B USB SMD")
    (attr smd)
    (fp_text reference m-usb1 (at 0 -4.5 450) (layer F.SilkS))
    (fp_text value Micro_USB (at 0 3.4 450) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 1.47 450) (layer Dwgs.User))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -2.66 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(m-usb1-Pad1)"))
    (pad 2 smd rect (at -0.65 -2.66 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 11 USB-))
    (pad 3 smd rect (at 0 -2.66 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 12 USB+))
    (pad 4 smd rect (at 0.65 -2.66 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.3 -2.66 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.4625 -2.3 270) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.4625 -2.3 270) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.91 0 270) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.91 0 270) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -0.84 0 270) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.84 0 270) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connectors_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 77.978 132.588 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 20K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 87.63 132.842 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value RT8284N (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R3-Pad2)"))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R1-Pad2)"))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 Vin))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53261-0771_07x1.25mm_Angled (layer F.Cu) (tedit 58A3B7FB)
    (at 59.182 129.032 270)
    (descr "Molex PicoBlade, single row, side entry type, surface mount, PN:53261-0771")
    (tags "connector molex picoblade smt")
    (attr smd)
    (fp_text reference Uart0 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value Uart0 (at 0 5 270) (layer F.Fab))
    (fp_text user %R (at 0 2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -3.75 -1.45 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.5 -1.45 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 Uart0TX))
    (pad 3 smd rect (at -1.25 -1.45 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 Uart0RX))
    (pad 4 smd rect (at 0 -1.45 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(Uart0-Pad4)"))
    (pad 5 smd rect (at 1.25 -1.45 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Uart0-Pad5)"))
    (pad 6 smd rect (at 2.5 -1.45 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Uart0-Pad6)"))
    (pad 7 smd rect (at 3.75 -1.45 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 5V+))
    (pad "" smd rect (at -6.25 1.45 270) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 6.25 1.45 270) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_PicoBlade_53261-0771_07x1.25mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53261-0771_07x1.25mm_Angled (layer F.Cu) (tedit 58A3B7FB)
    (at 99.06 132.334 90)
    (descr "Molex PicoBlade, single row, side entry type, surface mount, PN:53261-0771")
    (tags "connector molex picoblade smt")
    (attr smd)
    (fp_text reference Uart1 (at 0 -3.5 90) (layer F.SilkS))
    (fp_text value Uart1 (at 0 5 90) (layer F.Fab))
    (fp_text user %R (at 0 2.5 90) (layer F.Fab))
    (pad 1 smd rect (at -3.75 -1.45 90) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.5 -1.45 90) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 Uart1TX))
    (pad 3 smd rect (at -1.25 -1.45 90) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 Uart1RX))
    (pad 4 smd rect (at 0 -1.45 90) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(Uart1-Pad4)"))
    (pad 5 smd rect (at 1.25 -1.45 90) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(Uart1-Pad5)"))
    (pad 6 smd rect (at 2.5 -1.45 90) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Uart1-Pad6)"))
    (pad 7 smd rect (at 3.75 -1.45 90) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 5V+))
    (pad "" smd rect (at -6.25 1.45 90) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 6.25 1.45 90) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_PicoBlade_53261-0771_07x1.25mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 92.456 119.634 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.25 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.35 270) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A167FC4)
    (at 95.504 125.984 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.032 0 360) (layer F.SilkS))
    (fp_text value 90k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 5V+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 5A16818E)
    (at 63.246 120.904)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 5A168189)
    (at 97.536 120.904)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 75.946 129.286 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A1764D1)
    (at 90.678 129.032)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.54 0.762) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 80.518 130.048 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 45.3K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 5V+))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 74.93 135.636)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 81.026 136.144 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 Vin))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo2_9.8x8mm_SilkScreen (layer F.Cu) (tedit 5A17695B)
    (at 68.326 132.842)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_9.8x8mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (gr_text "Multi\nLite V2" (at 81.534 144.78) (layer F.SilkS))
  (gr_arc (start 57.658 120.396) (end 55.118 120.396) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100.584 120.396) (end 100.584 117.856) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 57.658 145.288) (end 57.658 147.828) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100.584 145.288) (end 103.124 145.288) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.124 120.396) (end 103.124 145.288) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 55.118 120.396) (end 55.118 145.288) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.584 117.856) (end 57.658 117.856) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 57.658 147.828) (end 100.584 147.828) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.388 146.558) (xy 55.372 145.542) (xy 55.626 119.888) (xy 57.404 118.11) (xy 100.584 118.11)
        (xy 102.87 120.142) (xy 102.616 145.542) (xy 102.616 146.05) (xy 100.838 147.574) (xy 57.404 147.574)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.388 146.558) (xy 55.372 145.542) (xy 55.626 119.888) (xy 57.404 118.11) (xy 100.584 118.11)
        (xy 102.87 120.142) (xy 102.616 145.542) (xy 102.616 146.05) (xy 100.838 147.574) (xy 57.404 147.574)
      )
    )
  )
)
