(kicad_pcb (version 4) (host pcbnew "(2015-08-26 BZR 6129, Git 2e41367)-product")
  (general
    (links 44)
    (no_connects 0)
    (area 151.674999 100.174999 186.325001 115.825001)
    (thickness 1.6)
    (drawings 36)
    (tracks 173)
    (zones 0)
    (modules 17)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 ~RESET)
  (net 4 XTAL1)
  (net 5 XTAL2)
  (net 6 "Net-(LED5-Pad1)")
  (net 7 "Net-(Q5-Pad1)")
  (net 8 "Net-(LED1-Pad1)")
  (net 9 "Net-(LED2-Pad1)")
  (net 10 "Net-(Q12-Pad2)")
  (net 11 US_~EU)
  (net 12 MOSI)
  (net 13 SCK)
  (net 14 "Net-(J1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net MOSI)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(LED5-Pad1)")
    (add_net "Net-(Q12-Pad2)")
    (add_net "Net-(Q5-Pad1)")
    (add_net SCK)
    (add_net US_~EU)
    (add_net XTAL1)
    (add_net XTAL2)
    (add_net ~RESET)
  )
  (net_class "MOAR POWAR" ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad1)")
  )
  (module Custom_Library:Battery_Holder_CR2_TH locked (layer B.Cu) (tedit 5A47D136)
    (at 169 108 180)
    (fp_text reference BT1 (at -15.5 3.5 450) (layer B.SilkS))
    (fp_text value CR2 (at -15.5 -3.75 270) (layer B.SilkS))
    (pad "" np_thru_hole circle (at -14.69 6.73 180) (size 1.98 1.98) (drill 1.98) (layers *.Cu *.Mask B.SilkS))
    (pad 1 thru_hole rect (at -14.69 0 180) (size 2.4 3) (drill 1.19) (layers *.Cu *.Mask B.SilkS)
      (net 1 +BATT))
    (pad 2 thru_hole oval (at 14.69 0 180) (size 2.4 3) (drill 1.19) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
  )
  (module Custom_Library:1206 (layer F.Cu) (tedit 5A47F5A0)
    (at 163.5 114)
    (fp_text reference C2 (at -2.75 -0.25 90) (layer F.SilkS))
    (fp_text value "150uF 6.3V" (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 1.6 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Custom_Library:0805_LED (layer F.Cu) (tedit 5A47F28B)
    (at 158 102 180)
    (fp_text reference LED5 (at 2.25 0 270) (layer F.SilkS))
    (fp_text value GREEN (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(LED5-Pad1)"))
    (pad 2 smd rect (at 1.05 0 180) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
  )
  (module Custom_Library:Pushbutton_5mm_SMD (layer F.Cu) (tedit 5A4715B9)
    (at 181.25 112.75)
    (fp_text reference SW1 (at -0.5 -3.25) (layer F.SilkS))
    (fp_text value RESET (at 0 4) (layer F.SilkS))
    (pad 1 smd rect (at -3.2 -1.9) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.2 1.9) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 3 ~RESET))
    (pad 1 smd rect (at 3.2 -1.9) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.2 1.9) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 3 ~RESET))
  )
  (module Custom_Library:XTAL_SMD_PBRC-M (layer F.Cu) (tedit 5A47CFF3)
    (at 174 112.5 90)
    (fp_text reference XTL1 (at 3 0 180) (layer F.SilkS))
    (fp_text value 8MHz (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -1.075 90) (size 1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 XTAL1))
    (pad 2 smd rect (at 0 -1.075 90) (size 1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 -1.075 90) (size 1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 XTAL2))
    (pad 1 smd rect (at -1.5 1.075 90) (size 1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 XTAL1))
    (pad 2 smd rect (at 0 1.075 90) (size 1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 1.075 90) (size 1 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 XTAL2))
    (pad 1 smd rect (at -1.5 0 90) (size 0.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 XTAL1))
    (pad 2 smd rect (at 0 0 90) (size 0.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 0 90) (size 0.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 XTAL2))
  )
  (module Custom_Library:0805 (layer F.Cu) (tedit 5A47F5A5)
    (at 169 114)
    (fp_text reference C1 (at -2.25 -0.25 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 1.05 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Custom_Library:0805 (layer F.Cu) (tedit 588A45A8)
    (at 158 114)
    (fp_text reference R1 (at -2.25 0 90) (layer F.SilkS))
    (fp_text value 1k (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 MOSI))
  )
  (module Custom_Library:0805 (layer F.Cu) (tedit 5A47149C)
    (at 169 105 180)
    (fp_text reference R3 (at 2.25 0 270) (layer F.SilkS))
    (fp_text value US/~EU (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 US_~EU))
    (pad 2 smd rect (at 1.05 0 180) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Custom_Library:0805 (layer F.Cu) (tedit 5A4714A4)
    (at 163 105 180)
    (fp_text reference R5 (at 2.25 0 270) (layer F.SilkS))
    (fp_text value 1k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 SCK))
    (pad 2 smd rect (at 1.05 0 180) (size 0.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(LED5-Pad1)"))
  )
  (module Custom_Library:SOT-23 (layer F.Cu) (tedit 5A4714F4)
    (at 158 110.5 90)
    (fp_text reference Q5 (at 0.5 -2 90) (layer F.SilkS))
    (fp_text value MMBT2907 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at -1.1 0.95 90) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd rect (at 1.1 0 90) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q12-Pad2)"))
  )
  (module Custom_Library:SOT-23-6 (layer F.Cu) (tedit 5A4714ED)
    (at 158 105.5 270)
    (fp_text reference Q12 (at 0 2 270) (layer F.SilkS))
    (fp_text value CMXT2222A (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(LED2-Pad1)"))
    (pad 5 smd rect (at 1.1 0 270) (size 1.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q12-Pad2)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q12-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(LED1-Pad1)"))
  )
  (module Custom_Library:SOIC-8_Wide (layer F.Cu) (tedit 5A47F2A4)
    (at 166 109.5 90)
    (fp_text reference IC1 (at -3 0.75 180) (layer F.SilkS))
    (fp_text value ATTINY85-M (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.905 3.6 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 3 ~RESET))
    (pad 2 smd rect (at -0.635 3.6 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 4 XTAL1))
    (pad 3 smd rect (at 0.635 3.6 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 5 XTAL2))
    (pad 4 smd rect (at 1.905 3.6 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.905 -3.6 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 12 MOSI))
    (pad 6 smd rect (at 0.635 -3.6 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 11 US_~EU))
    (pad 7 smd rect (at -0.635 -3.6 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 13 SCK))
    (pad 8 smd rect (at -1.905 -3.6 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
  )
  (module Custom_Library:LED_VSMB2943SL (layer F.Cu) (tedit 5A47EB7F)
    (at 153.5 112.5 270)
    (fp_text reference LED1 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value VSMB2943SLX01 (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(LED1-Pad1)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
  )
  (module Custom_Library:LED_VSMB2943SL (layer F.Cu) (tedit 5A47F658)
    (at 153.5 103.5 270)
    (fp_text reference LED2 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value VSMB2943SLX01 (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(LED2-Pad1)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
  )
  (module Custom_Library:1206 (layer F.Cu) (tedit 5A46CFB3)
    (at 153.5 112.5 270)
    (fp_text reference LED3 (at 0 2.5 450) (layer F.SilkS))
    (fp_text value "DNP SFH 4646-Z" (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(LED1-Pad1)"))
    (pad 2 smd rect (at 1.6 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
  )
  (module Custom_Library:1206 (layer F.Cu) (tedit 5A46CF96)
    (at 153.5 103.5 270)
    (fp_text reference LED4 (at 0 2.5 450) (layer F.SilkS))
    (fp_text value "DNP SFH 4646-Z" (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(LED2-Pad1)"))
    (pad 2 smd rect (at 1.6 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
  )
  (module Custom_Library:Pin_Header_01x06_Staggered (layer F.Cu) (tedit 5A471541)
    (at 169 102)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at -7 -3 90) (layer F.SilkS))
    (fp_text value ICSP (at -8.25 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -6.35 -0.2) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at -3.81 0.2) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at -1.27 -0.2) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 13 SCK))
    (pad 4 thru_hole oval (at 1.27 0.2) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 11 US_~EU))
    (pad 5 thru_hole oval (at 3.81 -0.2) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 12 MOSI))
    (pad 6 thru_hole oval (at 6.35 0.2) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 ~RESET))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "Dec 2017" (at 177.5 103.75) (layer F.SilkS))
  (gr_text "TV-B-Gone\nMini v1" (at 172 106.75) (layer F.SilkS))
  (gr_text "Based on the\noriginal TV-B-Gone\nkit by Lady Ada and\nCornfield Electronics" (at 181 112) (layer B.SilkS))
  (gr_line (start 184.25 101.25) (end 183.13 101.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 182.13 101.25) (end 182.13 100.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 185.25 101.25) (end 184.25 101.25) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.13 100.25) (end 152.75 100.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.25 114.75) (end 186.25 101.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.75 115.75) (end 185.25 115.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.75 101.25) (end 151.75 114.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.75 101.25) (end 151.75 101.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.75 114.75) (end 152.75 115.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 185.25 114.75) (end 186.25 114.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.500001) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 151 98) (xy 189 98) (xy 189 117) (xy 151 117)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.500001))
    (polygon
      (pts
        (xy 172.25 112) (xy 175 112) (xy 175 113) (xy 172.25 113)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.500001) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 154 99) (xy 188 99) (xy 188 118) (xy 154 118)
      )
    )
  )
  (zone (net 1) (net_name +BATT) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.500001) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 157.75 98) (xy 157.75 105) (xy 156 105) (xy 154 107) (xy 154 109)
        (xy 156 111) (xy 157.75 111) (xy 157.75 119) (xy 150 118) (xy 150 99)
      )
    )
  )
  (zone (net 1) (net_name +BATT) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.500001) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 157 99) (xy 149 100) (xy 149 116) (xy 157 117) (xy 157 111)
        (xy 154 109) (xy 154 107) (xy 157 105)
      )
    )
  )
  (zone (net 9) (net_name "Net-(LED2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.500001) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 155.75 98.5) (xy 155.75 103.25) (xy 151.25 103.25) (xy 151.25 98.5)
      )
    )
  )
  (zone (net 8) (net_name "Net-(LED1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.500001) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 156 108.75) (xy 154.25 108.75) (xy 153 108.25) (xy 151.25 108.25) (xy 151.25 112.25)
        (xy 156 112.25)
      )
    )
  )
)
