(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 135.274999 102.074999 174.375001 110.225001)
    (thickness 1.6)
    (drawings 12)
    (tracks 135)
    (zones 0)
    (modules 27)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFBF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "ground pad" (layer B.Cu) (tedit 57900340)
    (at 172.085 107.9246)
    (fp_text reference REF** (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value "ground pad" (at 0 0.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask B.SilkS))
  )
  (module "ground pad" (layer B.Cu) (tedit 5790033B)
    (at 172.0342 104.0638)
    (fp_text reference REF** (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value "ground pad" (at 0 0.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask B.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer B.Cu) (tedit 578FCF7F)
    (at 139.05 106.15)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0.95 1.636) (layer B.SilkS))
    (fp_text value Pin_Header_Straight_1x08 (at 1.6 2.186) (layer B.Fab))
    (pad 1 connect rect (at 0 1.516) (size 0.8 0.4) (layers B.Cu B.Mask))
    (pad 2 smd rect (at 0 1.016) (size 0.8 0.4) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at 0 0.516) (size 0.8 0.4) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 0 0.016) (size 0.8 0.4) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 0 -0.484) (size 0.8 0.4) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 0 -0.984) (size 0.8 0.4) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at 0 -1.484) (size 0.8 0.4) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 0 -1.984) (size 0.8 0.4) (layers B.Cu B.Paste B.Mask))
  )
  (module pins (layer F.Cu) (tedit 578E74DD)
    (at 153.4 106.05)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E69FD)
    (at 153.4 103.35)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R1 (at -1.381 1.3742) (layer F.SilkS))
    (fp_text value R (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E6A0B)
    (at 153.45 108.75 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference C1 (at 1.2278 1.2064 180) (layer F.SilkS))
    (fp_text value C (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E69E7)
    (at 149.7 108.75 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference C6 (at 1.11 1.1556 180) (layer F.SilkS))
    (fp_text value C (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E69CE)
    (at 149.65 103.35)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R6 (at -1.3902 1.3742) (layer F.SilkS))
    (fp_text value R (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pins (layer F.Cu) (tedit 578E74D7)
    (at 149.65 106.05)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module pins (layer F.Cu) (tedit 578E691A)
    (at 142.15 106.1)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E69AC)
    (at 142.15 103.4)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R4 (at -1.2054 1.248) (layer F.SilkS))
    (fp_text value R (at 0.0138 0.994) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E6959)
    (at 142.2 108.8 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference C4 (at 0.849 1.231 180) (layer F.SilkS))
    (fp_text value C (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E69BA)
    (at 145.95 108.8 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference C7 (at 1.2208 1.2564 180) (layer F.SilkS))
    (fp_text value C (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E69A0)
    (at 145.9 103.4)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R7 (at -1.0692 1.2988) (layer F.SilkS))
    (fp_text value R (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pins (layer F.Cu) (tedit 578E74D4)
    (at 145.9 106.1)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module pins (layer F.Cu) (tedit 578E74E3)
    (at 168.5 106)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E6A9A)
    (at 168.5 103.3)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R5 (at -1.1648 1.2972) (layer F.SilkS))
    (fp_text value R (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E7507)
    (at 168.55 108.7 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference "" (at 0.0254 -1.2954 180) (layer F.SilkS))
    (fp_text value C (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E6A41)
    (at 161.05 108.65 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference C8 (at 1.2586 1.1572 180) (layer F.SilkS))
    (fp_text value C (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E6A36)
    (at 161 103.25)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R8 (at -1.361 1.3472) (layer F.SilkS))
    (fp_text value R (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pins (layer F.Cu) (tedit 578E74F4)
    (at 161 105.95)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module pins (layer F.Cu) (tedit 578E74FF)
    (at 157.15 105.95)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E6A27)
    (at 157.15 103.25)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R3 (at -1.194 1.3218) (layer F.SilkS))
    (fp_text value R (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E6A1C)
    (at 157.2 108.65 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference C3 (at 1.1932 1.2588 180) (layer F.SilkS))
    (fp_text value C (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E6A7E)
    (at 164.8 108.7 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference C2 (at 1.4018 1.2834 180) (layer F.SilkS))
    (fp_text value C (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E6A70)
    (at 164.75 103.3)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R2 (at -1.428 1.3734) (layer F.SilkS))
    (fp_text value R (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pins (layer F.Cu) (tedit 578E74EB)
    (at 164.75 106)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text "R5\n" (at 168.529 103.5304) (layer B.SilkS))
  (gr_text "R2\n" (at 164.6428 103.378) (layer B.SilkS))
  (gr_text "R8\n" (at 160.8582 103.4796) (layer B.SilkS))
  (gr_text "R3\n" (at 157.099 103.4034) (layer B.SilkS))
  (gr_text "R1\n" (at 153.289 103.3272) (layer B.SilkS))
  (gr_text "R6\n" (at 149.7076 103.5558) (layer B.SilkS))
  (gr_text R7 (at 145.8214 103.5558) (layer B.SilkS))
  (gr_text R4 (at 141.9098 103.6574) (layer B.SilkS))
  (gr_line (start 135.35 102.15) (end 135.35 110.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.3 102.15) (end 135.35 102.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.3 110.15) (end 174.3 102.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.3 110.15) (end 135.35 110.15) (angle 90) (layer Edge.Cuts) (width 0.15))
)
