(kicad_pcb (version 20171130) (host pcbnew 5.1.7-1.fc32)
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 73)
    (zones 0)
    (modules 18)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Earth)
  (net 2 /B+)
  (net 3 /A_in)
  (net 4 "Net-(C2-Pad1)")
  (net 5 /A)
  (net 6 /A_out)
  (net 7 /f2)
  (net 8 /f1)
  (net 9 /G1)
  (net 10 /C)
  (net 11 /G3)
  (net 12 /G2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.75)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A)
    (add_net /A_in)
    (add_net /A_out)
    (add_net /B+)
    (add_net /C)
    (add_net /G1)
    (add_net /G2)
    (add_net /G3)
    (add_net /f1)
    (add_net /f2)
    (add_net Earth)
    (add_net "Net-(C2-Pad1)")
  )
  (module VT9-PT:VT9-PT (layer F.Cu) (tedit 5F8D2425)
    (at 111.76 55.88 90)
    (descr "Valve ECC-83-2 flat pins")
    (tags "Valve ECC-83-2 flat pins")
    (fp_text reference V1 (at 0 -24 90) (layer F.SilkS))
    (fp_text value EF86 (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 -18.2 90) (layer F.Fab))
    (pad 9 thru_hole oval (at -10.086093 -7.255322 108) (size 2.03 3.05) (drill oval 1.02 2.03) (layers *.Cu *.Mask)
      (net 9 /G1))
    (pad 8 thru_hole oval (at -10.086093 -13.744678 72) (size 2.03 3.05) (drill oval 1.02 2.03) (layers *.Cu *.Mask)
      (net 11 /G3))
    (pad 7 thru_hole oval (at -6.271745 -18.994678 36) (size 2.03 3.05) (drill oval 1.02 2.03) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 6 thru_hole oval (at -0.1 -21) (size 2.03 3.05) (drill oval 1.02 2.03) (layers *.Cu *.Mask)
      (net 5 /A))
    (pad 5 thru_hole oval (at 6.071745 -18.994678 324) (size 2.03 3.05) (drill oval 1.02 2.03) (layers *.Cu *.Mask)
      (net 7 /f2))
    (pad 4 thru_hole oval (at 9.886093 -13.744678 288) (size 2.03 3.05) (drill oval 1.02 2.03) (layers *.Cu *.Mask)
      (net 8 /f1))
    (pad 3 thru_hole oval (at 9.886093 -7.255322 252) (size 2.03 3.05) (drill oval 1.02 2.03) (layers *.Cu *.Mask)
      (net 10 /C))
    (pad 2 thru_hole oval (at 6.071745 -2.005322 216) (size 2.03 3.05) (drill oval 1.02 2.03) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole oval (at -0.1 0 180) (size 2.03 3.05) (drill oval 1.02 2.03) (layers *.Cu *.Mask)
      (net 12 /G2))
    (pad "" thru_hole circle (at 0 -10.5 90) (size 7.5 7.5) (drill 5.5) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/VT9-PT.pretty/VT9_PT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 107.95 61.1525 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 36K (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 9 /G1))
    (pad 1 smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 107.95 56.0725 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 1M (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 1 Earth))
    (pad 1 smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 82.3575 53.34 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.82) (layer B.SilkS))
    (fp_text value 2M (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 1 Earth))
    (pad 1 smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 2 /B+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VT9-PT:TerminalBlock_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5F8D165F)
    (at 81.28 71.12)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J7 (at 1.27 -4.37) (layer F.SilkS))
    (fp_text value plate (at 1.27 4.37) (layer F.Fab))
    (fp_text user %R (at 1.27 2) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /A))
    (pad 1 thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 /B+))
    (model ${KIPRJMOD}/VT9-PT.pretty/OSTVN02A150.wrl
      (offset (xyz -1 -3 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module VT9-PT:TerminalBlock_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5F8D165F)
    (at 106.68 71.12)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J6 (at 1.27 -4.37) (layer F.SilkS))
    (fp_text value cathode (at 1.27 4.37) (layer F.Fab))
    (fp_text user %R (at 1.27 2) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /C))
    (model ${KIPRJMOD}/VT9-PT.pretty/OSTVN02A150.wrl
      (offset (xyz -1 -3 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module VT9-PT:TerminalBlock_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5F8D165F)
    (at 88.9 71.12)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J5 (at 1.27 -4.37) (layer F.SilkS))
    (fp_text value grids (at 1.27 4.37) (layer F.Fab))
    (fp_text user %R (at 1.27 2) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /G3))
    (pad 1 thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /G2))
    (model ${KIPRJMOD}/VT9-PT.pretty/OSTVN02A150.wrl
      (offset (xyz -1 -3 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module VT9-PT:TerminalBlock_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5F8D165F)
    (at 109.22 40.64 180)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J4 (at 1.27 -4.37) (layer F.SilkS))
    (fp_text value A_audio (at 1.27 4.37) (layer F.Fab))
    (fp_text user %R (at 1.27 2) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /A_out))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 /A_in))
    (model ${KIPRJMOD}/VT9-PT.pretty/OSTVN02A150.wrl
      (offset (xyz -1 -3 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module VT9-PT:TerminalBlock_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5F8D1695)
    (at 96.52 71.12)
    (descr "Terminal Block TE 282834-3, 3 pins, pitch 2.54mm, size 8.08x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-3 pitch 2.54mm size 8.08x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J3 (at 2.54 -4.37) (layer F.SilkS))
    (fp_text value A (at 2.54 4.37) (layer F.Fab))
    (fp_text user %R (at 2.54 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 /G1))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /C))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /A))
    (model ${KIPRJMOD}/VT9-PT.pretty/OSTVN03A150.wrl
      (offset (xyz -1 -4 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module VT9-PT:TerminalBlock_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5F8D165F)
    (at 93.345 40.64 180)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J2 (at 1.27 -4.37) (layer F.SilkS))
    (fp_text value Filament (at 1.27 4.37) (layer F.Fab))
    (fp_text user %R (at 1.27 2) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 /f2))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 /f1))
    (model ${KIPRJMOD}/VT9-PT.pretty/OSTVN02A150.wrl
      (offset (xyz -1 -3 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module VT9-PT:TerminalBlock_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5F8D165F)
    (at 76.2 58.42 270)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J1 (at 1.27 -4.37 90) (layer F.SilkS))
    (fp_text value Power (at 1.27 4.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 /B+))
    (model ${KIPRJMOD}/VT9-PT.pretty/OSTVN02A150.wrl
      (offset (xyz -1 -3 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 114.3 71.12)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.35) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.35) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 114.3 40.64)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.35) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.35) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 76.2 40.64)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.35) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.35) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 76.2 71.12)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.35) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.35) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 94.615 55.675 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 1.85 90) (layer B.SilkS))
    (fp_text value 0.022uF (at 0 -1.85 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 /A))
    (pad 1 smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 6 /A_out))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 114.3 46.56 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.85 90) (layer B.SilkS))
    (fp_text value 0.022uF (at 0 -1.85 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 /A_in))
    (pad 1 smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_10x10.5 (layer F.Cu) (tedit 5BCA39D1)
    (at 82.55 49.53 180)
    (descr "SMD capacitor, aluminum electrolytic, Vishay 1010, 10.0x10.5mm, http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C1 (at 0 -6.3) (layer F.SilkS))
    (fp_text value 10uF (at 0 6.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 4.2 0 180) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 1 Earth))
    (pad 1 smd roundrect (at -4.2 0 180) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 2 /B+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Filament (at 92.075 43.18 180) (layer B.SilkS))
  (gr_text Audio (at 107.95 43.18 180) (layer B.SilkS))
  (gr_text Cathode (at 107.95 68.58) (layer B.SilkS))
  (gr_text A (at 101.6 68.58) (layer B.SilkS))
  (gr_text C (at 99.06 68.58) (layer B.SilkS))
  (gr_text G1 (at 96.52 68.58) (layer B.SilkS))
  (gr_text B+ (at 81.28 69.215) (layer B.SilkS))
  (gr_text A (at 83.82 69.215) (layer B.SilkS))
  (gr_text 2 (at 88.9 69.215) (layer B.SilkS))
  (gr_text 3 (at 91.44 69.215) (layer B.SilkS))
  (gr_text Grids (at 90.17 67.945) (layer B.SilkS))
  (gr_text Plate (at 82.55 67.945) (layer B.SilkS))
  (gr_text "EF86 Preamp\nProto Board V1" (at 83.82 66.04) (layer F.SilkS))
  (gr_line (start 73.66 73.66) (end 73.66 38.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.84 73.66) (end 73.66 73.66) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.84 38.1) (end 116.84 73.66) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.66 38.1) (end 116.84 38.1) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.84 73.66) (xy 73.66 73.66) (xy 73.66 38.1) (xy 116.84 38.1)
      )
    )
  )
  (zone (net 1) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.84 73.66) (xy 73.66 73.66) (xy 73.66 38.1) (xy 116.84 38.1)
      )
    )
  )
)
